IEEE8021-PE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32,
    Counter64
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    MacAddress,
    TEXTUAL-CONVENTION,
    TimeStamp,
    TruthValue
        FROM SNMPv2-TC
    ieee802dot1mibs
        FROM LLDP-V2-TC-MIB
    PortList
        FROM Q-BRIDGE-MIB;

ieee8021BridgePEMib MODULE-IDENTITY
    LAST-UPDATED    "201201220000Z" -- January 22, 2012, 0000Z
    ORGANIZATION    "IEEE 802.1 Working Group"
    CONTACT-INFO
            "WG-URL: http:////www.ieee802.org/1/
            WG-EMail: stds-802-1-L@IEEE.ORG

             Contact: Tony Jeffree
              Postal: C/O IEEE 802.1 Working Group
                      IEEE Standards Association
                      445 Hoes Lane
                      Piscataway
                      NJ 08854
                      USA
              E-mail: stds-802-1-L@IEEE.ORG"
    DESCRIPTION
        "The PE MIB module for managing devices that support
        Bridge Port Extension.

        Unless otherwise indicated, the references in this MIB
        module are to IEEE Std 802.1BR-2012.

        Copyright (C) IEEE.
        This version of this MIB module is part of 
        IEEE 802.1BR-2012; see the specification itself
        for full legal notices."
    
    REVISION         "201201220000Z" -- January 22, 2012, 0000Z
    DESCRIPTION
        "Initial version published as part of IEEE Std. 802.1BR-2012"

    ::= { ieee802dot1mibs 25 }


-- =============================================================
-- subtrees in the PE MIB
-- =============================================================

ieee8021BridgePENotifications  OBJECT IDENTIFIER
    ::= { ieee8021BridgePEMib 1 }

ieee8021BridgePEObjects  OBJECT IDENTIFIER
    ::= { ieee8021BridgePEMib 2 }

ieee8021BridgePEConformance  OBJECT IDENTIFIER
    ::= { ieee8021BridgePEMib 3 }


-- Textual Conventions

IEEE802BridgePEEChannelIDTC ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "Textual convention of an E-Channel Identifier."
    SYNTAX          Unsigned32 (1..4194302)

IEEE802BridgePETrafficClassValueTC ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS current
    DESCRIPTION
        "Indicates a traffic class. Values 0-7 correspond to
        traffic classes."
    SYNTAX Unsigned32 (0..7)

IEEE802BridgePETrafficSelectionAlgorithmTC ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "Indicates the Traffic Selection Algorithm
        0: Strict Priority
        1: Credit-based shaper
        2: Enhanced transmission selection
        3-254: Reserved for furture standardization
        255: Vendor specific"
    SYNTAX INTEGER {
        tsaStrictPriority(0),
        tsaCreditBasedShaper(1),
        tsaEnhancedTransmission(2),
        tsaVendorSpecific(255)
        }

IEEE802BridgePETrafficClassBandwidthValue ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS current
    DESCRIPTION
        "Indicates the bandwidth in percent assigned to a
        traffic class."
      SYNTAX Unsigned32 (0..100)

IEEE8021PbbComponentIdentifier ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS       current
    DESCRIPTION
        "The component identifier is used to distinguish between the
        multiple virtual bridge instances within a PB or PBB.  Each
        virtual bridge instance is called a component.  In simple
        situations where there is only a single component the default
        value is 1.  The component is identified by a component
        identifier unique within the BEB and by a MAC address unique
        within the PBBN.  Each component is associated with a Backbone
        Edge Bridge (BEB) Configuration managed object."    
    SYNTAX       Unsigned32 (1..4294967295)

IEEE8021BridgePortNumber ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS       current
    DESCRIPTION
        "An integer that uniquely identifies a bridge port, as
        specified in 17.3.2.2 of IEEE 802.1ap.
        This value is used within the spanning tree
        protocol to identify this port to neighbor bridges."    
    SYNTAX       Unsigned32 (1..65535)

IEEE8021BridgePortNumberOrZero ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS       current
    DESCRIPTION
        "An integer that uniquely identifies a bridge port, as
        specified in 17.3.2.2 of IEEE 802.1ap.  The value 0
        means no port number, and this must be clarified in the
        DESCRIPTION clause of any object defined using this
        TEXTUAL-CONVENTION."    
    SYNTAX       Unsigned32 (0..65535)

-- PE port table entry managed object

ieee8021BridgePEPortTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Ieee8021BridgePEPortEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table that contains per port information
        related to Port Extension.  A row is created in this
        table for any port on a Controlling Bridge that is
        extended using Port Extension, including those ports
        that provide communication to the Port Extenders
        themselves."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEObjects 1 }

ieee8021BridgePEPortEntry OBJECT-TYPE
    SYNTAX          Ieee8021BridgePEPortEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of per port Port Extension objects."
    INDEX           {
                        ieee8021BridgePEPortComponentId,
                        ieee8021BridgePEPort,
                        ieee8021BridgePEPortType
                    } 
    ::= { ieee8021BridgePEPortTable 1 }

Ieee8021BridgePEPortEntry ::= SEQUENCE {
        ieee8021BridgePEPortComponentId          
            IEEE8021PbbComponentIdentifier,
        ieee8021BridgePEPort                     
            IEEE8021BridgePortNumber,
        ieee8021BridgePEPortType                 
            INTEGER,
        ieee8021BridgePEPortUpstreamCSPAddress   
            MacAddress,
        ieee8021BridgePEPortEcid                 
            IEEE802BridgePEEChannelIDTC,
        ieee8021BridgePEPortNumber               
            IEEE8021BridgePortNumberOrZero,
        ieee8021BridgePECounterDiscontinuityTime 
            TimeStamp,
        ieee8021BridgePEPortRxrqErrorsBridge     
            Counter64,
        ieee8021BridgePEPortRxrspErrorsBridge    
            Counter64,
        ieee8021BridgePEPortRxrqErrorsPE         
            Counter64,
        ieee8021BridgePEPortRxrspErrorsPE        
            Counter64,
        ieee8021BridgePEPCP
            TruthValue,
        ieee8021BridgePEROW
            TruthValue,
        ieee8021BridgePEDEI
            TruthValue,
        ieee8021BridgePECN
            TruthValue,
        ieee8021BridgePEPFC
            TruthValue,
        ieee8021BridgePEExtPortEChannelsSupported
            Unsigned32,
        ieee8021BridgePERemoteRepEChannelsSupported
            Unsigned32,
        ieee8021BridgePETCsSupported
            Unsigned32,
        ieee8021BridgePEUtVLANsSupported
            Unsigned32
}

ieee8021BridgePEPortComponentId OBJECT-TYPE
    SYNTAX          IEEE8021PbbComponentIdentifier
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The component identifier is used to distinguish between the
        multiple virtual bridge instances within a PBB. In simple
        situations where there is only a single component the default
        value is 1." 
    ::= { ieee8021BridgePEPortEntry 1 }

ieee8021BridgePEPort OBJECT-TYPE
    SYNTAX          IEEE8021BridgePortNumber
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The port number of the port for which this entry
        contains bridge management information." 
    ::= { ieee8021BridgePEPortEntry 2 }

ieee8021BridgePEPortType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        pepCascade(1),
                        pepUpstream(2),
                        pepExtended(3)
                    }
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The operational mode of a port participating in
        Port Exension.  The enumerated values are:
        pepCascade - the port is operating as a Cascade port
        pepUpstream - the port is operating as an Upstream port
        pepExtended - the port is operating as an Extended port"
    REFERENCE       "10.2.1" 
    ::= { ieee8021BridgePEPortEntry 3 }

ieee8021BridgePEPortUpstreamCSPAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The MAC address used for communication of the PE CSP
        protocol of the device connected to the upstream port
        of the Port Extender (which may be the Controlling 
        Bridge or an upstream Port Extender).  This provides
        the hierarchal relationship in a cascade of Port
        Extenders"
    REFERENCE       "10.2.1" 
    ::= { ieee8021BridgePEPortEntry 4 }

ieee8021BridgePEPortEcid OBJECT-TYPE
    SYNTAX          IEEE802BridgePEEChannelIDTC
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The default ECID assigend to this port and the port
        on the Port Extender to which this port corresponds."
    REFERENCE       "10.2.1" 
    ::= { ieee8021BridgePEPortEntry 5 }

ieee8021BridgePEPortNumber OBJECT-TYPE
    SYNTAX          IEEE8021BridgePortNumberOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Port number on the of the Port on the Port Extender,
        or zero for the Upstream Port."
    REFERENCE       "10.2.1" 
    ::= { ieee8021BridgePEPortEntry 6 }

ieee8021BridgePECounterDiscontinuityTime OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The value of sysUpTime on the most recent occasion at which
        any one or more of the counters in this conceptaul row
        suffered a discontinuity.  The relevant counters are the
        specific instances associated with this conceptual row of 
        any Counter32 or Counter64 object. If no such discontinuities
        have occurred since the last re-initialization of the local 
        management subsystem, then this object contains a zero value." 
    ::= { ieee8021BridgePEPortEntry 7 }

ieee8021BridgePEPortRxrqErrorsBridge OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of PE CSP flow control overflow errors
        that have occured for requests on the Bridge."
    REFERENCE       "10.2.1" 
    ::= { ieee8021BridgePEPortEntry 8 }

ieee8021BridgePEPortRxrspErrorsBridge OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "octets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of PE CSP flow control overflow errors
        that have occured for responses on the Bridge."
    REFERENCE       "10.2.1" 
    ::= { ieee8021BridgePEPortEntry 9 }

ieee8021BridgePEPortRxrqErrorsPE OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of PE CSP flow control overflow errors
        that have occured for requests on the Port Extender."
    REFERENCE       "10.2.1" 
    ::= { ieee8021BridgePEPortEntry 10 }

ieee8021BridgePEPortRxrspErrorsPE OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "octets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of PE CSP flow control overflow errors
        that have occured for responses on the Port Extender."
    REFERENCE       "10.2.1" 
    ::= { ieee8021BridgePEPortEntry 11 }

ieee8021BridgePEPCP OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates whether the Port Exender supports
        modification of the priority code point
        table (true) or not (false)."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEPortEntry 12 }

ieee8021BridgePEROW OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates whether the Port Extender supports
        rows in the PCP table in addition to the 8P0D
        row (true)or not (false)."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEPortEntry 13 }

ieee8021BridgePEDEI OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates whether the Port Extender supports
        encoding of the Drop Eligible Indicatior (true)
        or not (false)."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEPortEntry 14 }

ieee8021BridgePECN  OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates whether the Port Extender supports
        Congestion Notification (true) or not (false)."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEPortEntry 15 }

ieee8021BridgePEPFC OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates whether the Port Extender supports
        Priority-based flow control(true) or
        not (false)."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEPortEntry 16 }

ieee8021BridgePEExtPortEChannelsSupported OBJECT-TYPE
    SYNTAX	       Unsigned32 (1..1048575)
    UNITS          "E-channels"
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "Indicates the number of Extended Port
        E-channels supported by the Port Extender."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEPortEntry 17 }

ieee8021BridgePERemoteRepEChannelsSupported  OBJECT-TYPE
    SYNTAX	       Unsigned32 (1..3145727)
    UNITS          "E-channels"
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "Indicates the number of Remote Replication
        E-channels supported by the Port Extender."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEPortEntry 18 }

ieee8021BridgePETCsSupported OBJECT-TYPE
    SYNTAX	       Unsigned32 (1..8)
    UNITS          "traffic classes"
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "Indicates the number of traffic clasees
        supported by the Port Extender."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEPortEntry 19 }

ieee8021BridgePEUtVLANsSupported OBJECT-TYPE
    SYNTAX	       Unsigned32 (1..4094)
    UNITS          "VLANs"
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "Indicates the number of untagged VLANs
        supported by the Port Extender."
    REFERENCE       "10.2.1"
    ::= { ieee8021BridgePEPortEntry 20 }

-- PE Remote Replication entry table managed object

ieee8021BridgePERemoteReplicationTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Ieee8021BridgePERemoteReplicationEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table that contains one row for each Remote Replication
        entry in the filtering database."
    REFERENCE       "10.3.1"
    ::= { ieee8021BridgePEObjects 2 }

ieee8021BridgePERemoteReplicationEntry OBJECT-TYPE
    SYNTAX          Ieee8021BridgePERemoteReplicationEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of Remote Replication objects."
    INDEX           {
                        ieee8021BridgePEPortComponentId,
                        ieee8021BridgePERREcid
                    } 
    ::= { ieee8021BridgePERemoteReplicationTable 1 }

Ieee8021BridgePERemoteReplicationEntry ::= SEQUENCE {
        ieee8021BridgePERREcid    IEEE802BridgePEEChannelIDTC,
        ieee8021BridgePERRPortMap PortList
}

ieee8021BridgePERREcid OBJECT-TYPE
    SYNTAX          IEEE802BridgePEEChannelIDTC
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The ECID assigend to this Remote Replication
        filtering entry."
    REFERENCE       "10.3.1" 
    ::= { ieee8021BridgePERemoteReplicationEntry 1 }

ieee8021BridgePERRPortMap OBJECT-TYPE
    SYNTAX          PortList
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The list of ports to which a frame is to be
        replicated."
    REFERENCE       "10.3.1" 
    ::= { ieee8021BridgePERemoteReplicationEntry 2 }

--PE Enhanced Transmission Selection table managed object

ieee8021BridgePEETSTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Ieee8021BridgePEETSEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table that contains per port information
        related to Enhanced Transmission Selection.
        A row is created in this table for any port on a
        Controlling Bridge that corresponds to a Cascade
        Port. These objects refer to the ETS configuration 
        of the attached Upstream Port"
    REFERENCE       "10.2.2"
    ::= { ieee8021BridgePEObjects 3 }

ieee8021BridgePEETSEntry OBJECT-TYPE
    SYNTAX          Ieee8021BridgePEETSEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of per Cascade Port ETS objects."
    INDEX           {
                        ieee8021BridgePEPortComponentId,
                        ieee8021BridgePEPort,
                        ieee8021BridgePEETSTrafficClass
                    } 
    ::= { ieee8021BridgePEETSTable 1 }

Ieee8021BridgePEETSEntry ::= SEQUENCE {
        ieee8021BridgePEETSTrafficClass
            IEEE802BridgePETrafficClassValueTC,
        ieee8021BridgePEETSTrafficSelectionAlgorthm          
            IEEE802BridgePETrafficSelectionAlgorithmTC,
        ieee8021BridgePEETSBandwidth                     
            IEEE802BridgePETrafficClassBandwidthValue 
}

ieee8021BridgePEETSTrafficClass OBJECT-TYPE
    SYNTAX IEEE802BridgePETrafficClassValueTC
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Indicates the traffic class to
        which this bandwidth applies"
    REFERENCE
        "10.2.3"
    ::= { ieee8021BridgePEETSEntry 1 }

ieee8021BridgePEETSTrafficSelectionAlgorthm OBJECT-TYPE
    SYNTAX IEEE802BridgePETrafficSelectionAlgorithmTC
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Inticates the Traffic Selection Algorthm 
        assigned to this traffic class"
    REFERENCE
        "10.2.3"
::= { ieee8021BridgePEETSEntry 2 }

ieee8021BridgePEETSBandwidth OBJECT-TYPE
    SYNTAX IEEE802BridgePETrafficClassBandwidthValue 
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indicates the bandwidth assigned to this traffic class."
    REFERENCE
        "10.2.3"
::= { ieee8021BridgePEETSEntry 3 }

-- =============================================================
-- Conformance Information
-- =============================================================

ieee8021BridgePEGroups  OBJECT IDENTIFIER
    ::= { ieee8021BridgePEConformance 1 }

ieee8021BridgePECompliances  OBJECT IDENTIFIER
    ::= { ieee8021BridgePEConformance 2 }


-- =============================================================
-- Units of conformance
-- =============================================================

ieee8021BridgePEGroup OBJECT-GROUP
    OBJECTS         {
                        ieee8021BridgePEPortUpstreamCSPAddress,
                        ieee8021BridgePEPortEcid,
                        ieee8021BridgePEPortNumber,
                        ieee8021BridgePECounterDiscontinuityTime,
                        ieee8021BridgePEPortRxrqErrorsBridge,
                        ieee8021BridgePEPortRxrspErrorsBridge,
                        ieee8021BridgePEPortRxrqErrorsPE,
                        ieee8021BridgePEPortRxrspErrorsPE,
                        ieee8021BridgePEPCP,
                        ieee8021BridgePEROW,
                        ieee8021BridgePEDEI,
                        ieee8021BridgePECN,
                        ieee8021BridgePEPFC,
                        ieee8021BridgePEExtPortEChannelsSupported,
                        ieee8021BridgePERemoteRepEChannelsSupported,
                        ieee8021BridgePETCsSupported,
                        ieee8021BridgePEUtVLANsSupported,
                        ieee8021BridgePERRPortMap,
                        ieee8021BridgePEETSTrafficSelectionAlgorthm,
                        ieee8021BridgePEETSBandwidth
                    }
    STATUS          current
    DESCRIPTION
        "The collection of objects used to represent
        Port Extension management objects."
    ::= { ieee8021BridgePEGroups 1 }

-- =============================================================
-- compliance statements
-- =============================================================

ieee8021BridgePECompliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for devices supporting PE
        as defined in IEEE 802.1BR."
    MODULE          -- this module
    MANDATORY-GROUPS { ieee8021BridgePEGroup }
    ::= { ieee8021BridgePECompliances 1 }

END