UDP-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Counter32,
    IpAddress, mib-2                   FROM SNMPv2-SMI
    MODULE-COMPLIANCE, OBJECT-GROUP    FROM SNMPv2-CONF;


udpMIB MODULE-IDENTITY
    LAST-UPDATED "9411010000Z"
    ORGANIZATION "IETF SNMPv2 Working Group"
    CONTACT-INFO
            "        Keith McCloghrie

             Postal: Cisco Systems, Inc.
                     170 West Tasman Drive
                     San Jose, CA  95134-1706
                     US

             Phone:  +1 408 526 5260
             Email:  kzm@cisco.com"
    DESCRIPTION
            "The MIB module for managing UDP implementations."
    REVISION      "9103310000Z"
    DESCRIPTION
            "The initial revision of this MIB module was part of MIB-
            II."
    ::= { mib-2 50 }

-- the UDP group

udp      OBJECT IDENTIFIER ::= { mib-2 7 }

udpInDatagrams OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of UDP datagrams delivered to UDP users."
    ::= { udp 1 }

udpNoPorts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of received UDP datagrams for which there
            was no application at the destination port."
    ::= { udp 2 }

udpInErrors OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The number of received UDP datagrams that could not be
            delivered for reasons other than the lack of an application
            at the destination port."
    ::= { udp 3 }

udpOutDatagrams OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of UDP datagrams sent from this entity."
    ::= { udp 4 }

-- the UDP Listener table

-- The UDP listener table contains information about this
-- entity's UDP end-points on which a local application is
-- currently accepting datagrams.

udpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF UdpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A table containing UDP listener information."
    ::= { udp 5 }

udpEntry OBJECT-TYPE
    SYNTAX      UdpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about a particular current UDP listener."
    INDEX   { udpLocalAddress, udpLocalPort }
    ::= { udpTable 1 }

UdpEntry ::= SEQUENCE {
        udpLocalAddress  IpAddress,
        udpLocalPort     INTEGER
    }

udpLocalAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The local IP address for this UDP listener.  In the case of
            a UDP listener which is willing to accept datagrams for any
            IP interface associated with the node, the value 0.0.0.0 is
            used."
    ::= { udpEntry 1 }

udpLocalPort OBJECT-TYPE
    SYNTAX      INTEGER (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The local port number for this UDP listener."
    ::= { udpEntry 2 }

-- conformance information

udpMIBConformance OBJECT IDENTIFIER ::= { udpMIB 2 }

udpMIBCompliances OBJECT IDENTIFIER ::= { udpMIBConformance 1 }
udpMIBGroups      OBJECT IDENTIFIER ::= { udpMIBConformance 2 }

-- compliance statements

udpMIBCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for SNMPv2 entities which
            implement UDP."
    MODULE  -- this module
        MANDATORY-GROUPS { udpGroup
                           }
    ::= { udpMIBCompliances 1 }

-- units of conformance

udpGroup OBJECT-GROUP
    OBJECTS   { udpInDatagrams, udpNoPorts,
                udpInErrors, udpOutDatagrams,
                udpLocalAddress, udpLocalPort }
    STATUS    current
    DESCRIPTION
            "The udp group of objects providing for management of UDP
            entities."
    ::= { udpMIBGroups 1 }

END

