RADLAN-IP DEFINITIONS ::= BEGIN

-- Title:      RADLAN IP Private Extension
-- Version:    7.45.00.00
-- Date:       22 Jun 2006

IMPORTS
    rnd                                                     FROM RADLAN-MIB
    ipAddrEntry                                             FROM IP-MIB
    InterfaceIndexOrZero, InterfaceIndex                    FROM IF-MIB
    rip2IfConfEntry                                         FROM RIPv2-MIB
    ipCidrRouteEntry,ipCidrRouteDest,
    ipCidrRouteMask, ipCidrRouteTos, ipCidrRouteNextHop     FROM IP-FORWARD-MIB
    Unsigned32, Integer32, Counter32, IpAddress,
    MODULE-IDENTITY, OBJECT-TYPE                            FROM SNMPv2-SMI
    TEXTUAL-CONVENTION,
    DisplayString, RowStatus, TruthValue, PhysAddress,
    TimeStamp, RowPointer, TestAndIncr, StorageType         FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP                         FROM SNMPv2-CONF
    InetAddress, InetAddressType,
    InetAddressPrefixLength,
    InetVersion, InetZoneIndex                              FROM INET-ADDRESS-MIB
    InterfaceIndex                                          FROM IF-MIB
    IpAddressOriginTC, IpAddressStatusTC
                                                            FROM IP-MIB;


ipSpec MODULE-IDENTITY
       LAST-UPDATED "200606220000Z"
       ORGANIZATION "Marvell Semiconductor, Inc."
       CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
       DESCRIPTION
            "The private MIB module definition for IP MIB."
       REVISION "200606220000Z"
       DESCRIPTION
            "Initial version of this MIB."
       ::= { rnd 26 }


--
-- The textual conventions we define and use for rlIpAddressTable (in this MIB).
--

RlIpAddressOriginTC ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION
           "The origin of the address.

            following are same as ipAddressOriginTC in standard MIB:

            manual(2) indicates that the address was manually configured
            to a specified address, e.g., by user configuration.

            dhcp(4) indicates an address that was assigned to this
            system by a DHCP server.

            linklayer(5) indicates an address created by IPv6 stateless
            auto-configuration.

            random(6) indicates an address chosen by the system at
            random, e.g., an IPv4 address within 169.254/16, or an RFC
            3041 privacy address.

            following are additional to standard MIB:

            autoConfig(7) indicates that the address was auto configured configured
            to a specified address, e.g., not by user configuration.

            eui64(8) indicates that the address was partially configured configured
            to a specified address, e.g., address suffix is based on MAC address with
            EUI-64 representation.

            tunnelIsatap(9) indicates that the address an ISATATP tunnel representation.

            tunnelIsatap(10) indicates that the address an 6to4 tunnel representation.

            tunnelIsatap(11) indicates that the address was partially configured configured
            to a specified address, e.g., address prefix is preconfigured.
            "
    SYNTAX     INTEGER {
        other(1),
        manual(2),
        dhcp(4),
        linklayer(5),
        random(6),
-- additional to standard MIB
        autoConfig(7),
        eui64(8),
        tunnelIsatap(9),
        tunnel6to4(10),
        generalPrefix(11)
    }



rsIpAddrTable OBJECT-TYPE
    SYNTAX      SEQUENCE  OF RsIpAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This table is parralel to MIB II IpAddrTable, and is used to
        add/delete entries to/from that table. In addition it contains
        private objects."
    ::=  { ipSpec 1 }

rsIpAddrEntry   OBJECT-TYPE
    SYNTAX      RsIpAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The addressing information for one of this
            entity's IP addresses."
    INDEX  {rsIpAdEntAddr}
    ::=  { rsIpAddrTable 1 }

RsIpAddrEntry ::= SEQUENCE {
    rsIpAdEntAddr                IpAddress,
    rsIpAdEntIfIndex             INTEGER,
    rsIpAdEntNetMask             IpAddress,
    rsIpAdEntForwardIpBroadcast  INTEGER,
    rsIpAdEntBackupAddr          IpAddress, -- obsolete
    rsIpAdEntStatus              INTEGER,
    rsIpAdEntBcastAddr           INTEGER,
    rsIpAdEntArpServer           INTEGER,
    rsIpAdEntName                DisplayString,
    rsIpAdEntOwner               INTEGER,
    rsIpAdEntAdminStatus         INTEGER,
    rsIpAdEntOperStatus          INTEGER,
    rsIpAdEntPrecedence          INTEGER,
    rsIpAdEntUniqueStatus        INTEGER,
    rsIpAdEntIcmpRedirectSend    INTEGER
}

rsIpAdEntAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The IP address to which this entry's addressing
            information pertains."
    ::= { rsIpAddrEntry 1 }

rsIpAdEntIfIndex OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The index value which uniquely identifies the
            interface to which this entry is applicable.  The
            interface identified by a particular value of this
            index is the same interface as identified by the
            same value of ifIndex."
    ::= { rsIpAddrEntry 2 }

rsIpAdEntNetMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The subnet mask associated with the IP address of
            this entry.  The value of the mask is an IP
            address with all the network bits set to 1 and all
            the hosts bits set to 0."
    ::= { rsIpAddrEntry 3 }

rsIpAdEntForwardIpBroadcast OBJECT-TYPE
    SYNTAX INTEGER {
       enable(1),
       disable(2)
       }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        " This variable controls forwarding of IP (sub)net-directed
          broadcasts destined for an attached sub(net). "
    DEFVAL  { enable }
    ::=   { rsIpAddrEntry 4 }

rsIpAdEntBackupAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "In case there are two IP routers in the domain,
             the address of the second IP router."
    ::= { rsIpAddrEntry 5 }

rsIpAdEntStatus OBJECT-TYPE
    SYNTAX INTEGER{
       valid(1),
       invalid(2)
       }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        " The validity of this entry. Invalid indicates that this entry is
          invalid in IpAddrTable (MIB II)."
    DEFVAL  { valid }
    ::=   { rsIpAddrEntry 6 }

rsIpAdEntBcastAddr OBJECT-TYPE
    SYNTAX      INTEGER (0..1)
    MAX-ACCESS read-write
    STATUS      current
    DESCRIPTION
        " Indicates how the host part of ip subnet broadcast messages will be
          filled:
           0 - host part will be filled by 0
           1 - host part will be filled by 1."
    ::=   { rsIpAddrEntry 7 }

rsIpAdEntArpServer OBJECT-TYPE
    SYNTAX INTEGER{
       enable(1),
       disable(2)
       }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates whether the router will reply to incoming ARP requests on
         this interface, providing the physical address corresponding to this
         IP interface."
    DEFVAL  { disable }
    ::=   { rsIpAddrEntry 8 }

    rsIpAdEntName OBJECT-TYPE
        SYNTAX      DisplayString (SIZE (0..30))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
           "The IP Interface name"
    ::=   { rsIpAddrEntry 9 }

rsIpAdEntOwner OBJECT-TYPE
        SYNTAX  INTEGER{
               static(1),
               dhcp(2),
               internal(3),
               default(4)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
           "The IP Interface owner. Static if interface defined by user, dhcp
            if received by boot protocol like DHCP and internal
            for internal usage."
    DEFVAL  { static }
    ::=   { rsIpAddrEntry 10 }

rsIpAdEntAdminStatus     OBJECT-TYPE
        SYNTAX  INTEGER{
               up(1),
               down(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
           "The IP Interface admin status."
    DEFVAL  { up }
    ::=   { rsIpAddrEntry 11 }

rsIpAdEntOperStatus   OBJECT-TYPE
            SYNTAX INTEGER {
                       active(1),
                       inactive(2)
            }
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                "If active the interface can be used to send and receive frames."
            ::= { rsIpAddrEntry 12 }

rsIpAdEntPrecedence   OBJECT-TYPE
            SYNTAX INTEGER (1..255)
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
               "The IP preference, to be selected as source IP for rsIpAdEntIfIndex.
                this source IP selection is first by preference value.
                if more than one IP has the same preference the one with the
                lowest IP is selected.
                (higher value -> higher preference)"
            DEFVAL  { 1 }
            ::= { rsIpAddrEntry 13 }

rsIpAdEntUniqueStatus   OBJECT-TYPE
            SYNTAX    INTEGER {
                        valid (1),
                        validDuplicated (2),
                        tentative      (3),
                        duplicated   (4),
                        delayed (5),
                        notReceived (6)
            }
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION       "The IP address unique status defines IP address
                               state in an assignment process and
                               after duplication detection."
            ::= { rsIpAddrEntry 14 }

rsIpAdEntIcmpRedirectSend OBJECT-TYPE
    SYNTAX  INTEGER {
        enable(1),
        disable(2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enables or disables sending of ICMP redirect messages to
         re-send a packet through the same interface on which the packet was
         received."
    DEFVAL { enable }
       ::= { rsIpAddrEntry 15 }

icmpSpec               OBJECT IDENTIFIER ::= { ipSpec 2 }

rsIcmpGenErrMsgEnable   OBJECT-TYPE
    SYNTAX INTEGER {
       enable(1),
       disable(2)
   }
    MAX-ACCESS  read-write
    STATUS  current
        DESCRIPTION
           "This variable controlls the ability to generate ICMP error messages"
    DEFVAL  { enable }
    ::= { icmpSpec 1 }

rsIcmpRdTable OBJECT-TYPE
    SYNTAX      SEQUENCE  OF RsIcmpRdEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This table contains ICMP Router Discovery parameters
        configurated per IP interface."
    ::=  {icmpSpec 2}

rsIcmpRdEntry   OBJECT-TYPE
    SYNTAX      RsIcmpRdEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "The ICMP parameters configurated for IP interface."
    INDEX  {rsIcmpRdIpAddr}
    ::=  {rsIcmpRdTable 1}

RsIcmpRdEntry ::= SEQUENCE {
    rsIcmpRdIpAddr             IpAddress,
    rsIcmpRdIpAdvertAddr       IpAddress,
    rsIcmpRdMaxAdvertInterval  INTEGER,
    rsIcmpRdMinAdvertInterval  INTEGER,
    rsIcmpRdAdvertLifetime     INTEGER,
    rsIcmpRdAdvertise          INTEGER,
    rsIcmpRdPreferenceLevel    INTEGER,
    rsIcmpRdEntStatus          INTEGER
    }

rsIcmpRdIpAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The IP address to which this entry's information pertains."
    ::= {rsIcmpRdEntry 1}

rsIcmpRdIpAdvertAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            " The IP destination address to be used for multicast
              Router Advertisements sent from the interface. The
              only permissible values are the all-systems multicast
              address, 224.0.0.1, or the limited-broadcast address,
              255.255.255.255."
    DEFVAL  {'E0000001'H}
    ::= {rsIcmpRdEntry 2}

rsIcmpRdMaxAdvertInterval OBJECT-TYPE
    SYNTAX      INTEGER (4..1800)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The maximum time allowed between sending multicast
             Router Advertisements from the interface, in seconds.
             Must be no less than 4 seconds and no greater than 1800
             seconds."
    DEFVAL  {600}
    ::= {rsIcmpRdEntry 3}

rsIcmpRdMinAdvertInterval OBJECT-TYPE
    SYNTAX      INTEGER (3..1800)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The minimum time allowed between sending unsolicited
             multicast Router Advertisements from the interface, in
             seconds.  Must be no less than 3 seconds and no greater
             than rsIcmpRdMaxAdvertInterval.
             Default: 0.75 * rsIcmpRdMaxAdvertInterval."
    ::= {rsIcmpRdEntry 4}

rsIcmpRdAdvertLifetime OBJECT-TYPE
    SYNTAX      INTEGER (4..9000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
             "The maximum length of time that the advertised addresses
             are to be considered as valid. Must be no less than
             rsIcmpRdMaxAdvertInterval and no greater than 9000 seconds.
             Default: 3 * rsIcmpRdMaxAdvertInterval."
    ::= {rsIcmpRdEntry 5}

rsIcmpRdAdvertise OBJECT-TYPE
    SYNTAX  INTEGER {
       enable  (1),
       disable (2)
       }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
             "A flag indicating whether or not the address is to be
              advertised."
    DEFVAL  {enable}
    ::= {rsIcmpRdEntry 6}

rsIcmpRdPreferenceLevel OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
             "The preferability of the address as a default router
             address, relative to other router addresses on the same
             subnet."
    DEFVAL  {0}
    ::= {rsIcmpRdEntry 7}

rsIcmpRdEntStatus  OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "Setting of any value to this object set values of
             all fields to the default values."
    ::=   {rsIcmpRdEntry 8}


rip2Spec              OBJECT IDENTIFIER ::= { ipSpec  3 }
-- see rlIpRouters

arpSpec                OBJECT IDENTIFIER ::= { ipSpec 4 }

rsArpDeleteTable OBJECT-TYPE
    SYNTAX  INTEGER {
       noAction(0),  -- for get only
       deleteArpTab(1),
       deleteIpArpDynamicEntries(2),
       deleteIpArpStaticEntries(3),
       deleteIpArpDelDynamicRefreshStatic(4)
     }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
--  old description
--         "Setting this object to any not-null value has the effect of deleting
--          all entries of the ARP table."
-- new description
           "Setting to value deleteArpTab(1): deletes the arp table -
                                              static and dynamic entries
            deleteIpArpDynamicEntries(2):     delete all dynamic entries
            deleteIpArpStaticEntries(3):      delete all static entries
            deleteIpArpDelDynamicRefreshStatic(4) - delete all dynamic -
                                                    refresh static, thus
                                                    refrashing FFT.
            on get returns the last action"
    ::= { arpSpec 1  }

-- range 0 to 40,000,000 to allow system convesion to timer
rsArpInactiveTimeOut OBJECT-TYPE
    SYNTAX      Unsigned32 (0..40000000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "This variable defines the maximum time period (in second) that can
          pass between ARP requests concerning an entry in the ARP table.
          After this time period, the entry is deleted from the table.
          Default value 0 means using value based on IP forwarding mode."
    DEFVAL  { 0 }
    ::= { arpSpec 2  }

rsArpProxy OBJECT-TYPE
    SYNTAX INTEGER {
       enable(1),
       disable(2)
    }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "When ARP Proxy is enabled, the router can respond to
          ARP requests for nodes located on a different sub-net,
          provided they are it its network table. The router responds
          with its own MAC address.
          When ARP Proxy is disabled, the router responds only
          to ARP requests for its own IP addresses."
    DEFVAL  { disable }
    ::= { arpSpec 3  }

rsArpRequestsSent OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "Displays how many ARP requests have been sent out to an ARP server
          for address resolution."
    ::= { arpSpec 4  }

rsArpRepliesSent OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "Displays how many ARP replies have been sent out to an ARP client
          in response to request packets."
    ::= { arpSpec 5  }

rsArpProxyRepliesSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "Displays how many proxy ARP replies have been sent out in response
          to request packets. A proxy router serving as a gateway to a subnet
          would respond with a proxy reply."
    ::= { arpSpec 6  }

rsArpUnresolveTimer OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "Specifies the frequency in seconds in which to send out ARP
          requests to resolve the Next Hop MAC address."
    ::= { arpSpec 7  }

rsArpMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "MIB's version, the current version is 2.
          Version 1:
            rsArpDeleteTable
                Setting this object to any not-null value has the effect
                of deleting all entries of the ARP table.
          Version 2:
            rsArpDeleteTable
                Setting to value deleteArpTab(1): deletes the arp table -
                                                  static and dynamic entries
                deleteIpArpDynamicEntries(2):     delete all dynamic entries
                deleteIpArpStaticEntries(3):      delete all static entries
                deleteIpArpDelDynamicRefreshStatic(4):
                                                    delete all dynamic -
                                                    refresh static, thus
                                                    refrashing FFT.
                on get returns the last action.
            New MIB variables support:
                rsArpRequestsSent
                rsArpRepliesSent
                rsArpProxyRepliesSent
                rsArpUnresolveTimer
                rsArpMibVersion
          Version 3:
            New MIB variables support:
            rsArpStaticTable
            rsArpInterfaceTable"
    ::= { arpSpec 8  }

rsArpStaticTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RsArpStaticEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table used for adding static ARP entries
         without specifying Layer 2 interface."
    ::= { arpSpec 9 }

rsArpStaticEntry OBJECT-TYPE
    SYNTAX  RsArpStaticEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Each entry contains one IpAddress to `physical' address equivalence."
    INDEX   { rsArpStaticIpAddress }
              ::= { rsArpStaticTable 1 }

RsArpStaticEntry ::= SEQUENCE {
        rsArpStaticIpAddress    IpAddress,
        rsArpStaticPhysAddress  PhysAddress,
        rsArpStaticRowStatus    RowStatus
    }

rsArpStaticIpAddress OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The IpAddress corresponding to the media-dependent `physical' address."
    ::= { rsArpStaticEntry 1 }

rsArpStaticPhysAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The media-dependent `physical' address."
    ::= { rsArpStaticEntry 2 }


rsArpStaticRowStatus OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-write
    STATUS current
    DESCRIPTION
        "Entry status."
    ::= { rsArpStaticEntry  3 }


rsArpInterfaceTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RsArpInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "L2 Interface specific configuration for ARP Application.
         Entry in this table will be dynamically created,
         when first IP Address is defined on specific L2 interface,
         and destroyed when the last IP address on this L2 interface is removed"
    ::= { arpSpec 10 }

rsArpInterfaceEntry OBJECT-TYPE
    SYNTAX  RsArpInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Each entry contains L2 Interface specific configuration
         for ARP Application."
    INDEX   { rsArpInterfaceIfIndex }
              ::= { rsArpInterfaceTable 1 }

RsArpInterfaceEntry ::= SEQUENCE {
        rsArpInterfaceIfIndex           InterfaceIndex,
        rsArpInterfaceInactiveTimeOut   Unsigned32,
        rsArpInterfaceArpProxy          INTEGER
    }

rsArpInterfaceIfIndex OBJECT-TYPE
    SYNTAX  InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The index value that uniquely identifies the interface to
         which this entry is applicable.  The interface identified by
         a particular value of this index is the same interface as
         identified by the same value of the IF-MIB's ifIndex."
    ::= { rsArpInterfaceEntry 1 }

rsArpInterfaceInactiveTimeOut OBJECT-TYPE
    SYNTAX      Unsigned32 (0..40000000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "This variable defines the maximum time period (in second) that can
          pass between ARP requests concerning an entry in the ARP table.
          After this time period, the entry is deleted from the table.
          Default value 0 means using value from rsArpInactiveTimeOut"
    DEFVAL  { 0 }
    ::= { rsArpInterfaceEntry 2  }

rsArpInterfaceArpProxy OBJECT-TYPE
    SYNTAX INTEGER {
       enable(1),
       disable(2)
    }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "When ARP Proxy is enabled, the router can respond to
          ARP requests for nodes located on a different sub-net,
          provided they are it its network table. The router responds
          with its own MAC address.
          When ARP Proxy is disabled, the router responds only
          to ARP requests for its own IP addresses."
    DEFVAL  { disable }
    ::= { rsArpInterfaceEntry 3  }

rsArpNumOfEntries OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
         "Displays how many ARP entries stored in ARP Table."
    ::= { arpSpec 11  }


tftp     OBJECT IDENTIFIER ::= { ipSpec 5 }

rsTftpRetryTimeOut OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        " General Retransmission time-out value (seconds) "
    DEFVAL  { 15 }
    ::= { tftp 1 }

rsTftpTotalTimeOut OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        " Total Retransmission time-out value (seconds) "
    DEFVAL  { 60 }
    ::= { tftp 2 }

rsSendConfigFile OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The file name include path where the Router Server will put the full
         configuration. The default destination address will be the sender
         address."
    ::= { tftp 3 }

rsGetConfigFile OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The file name include path where the Router Server will get the full
         configuration from. The default destination address will be the sender
         address."
    ::= { tftp 4 }

rsLoadSoftware OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The file name include path where the Router Server will get the
         software. The default source address will be the sender address."
    ::= { tftp 5 }

rsFileServerAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The IP address of the configuration / sw server."
        ::= { tftp 6 }

rsSoftwareDeviceName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..8))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The Software Device Name specifies a device name, using this Software"
    ::= { tftp 7 }

rsSoftwareFileAction OBJECT-TYPE
   SYNTAX INTEGER {
        download(1),
        upload  (2)
   }
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
    "Holds the current action done on the software file "
   DEFVAL {download }
     ::= {tftp 8 }

ipRedundancy    OBJECT IDENTIFIER ::= { ipSpec 6 }
-- see rlIpRouter.mib

ipRouteLeaking    OBJECT IDENTIFIER ::= { ipSpec 7 }
-- see rlIpRouter.mib

ipRipFilter    OBJECT IDENTIFIER ::= { ipSpec 8 }
-- see rlIpRouter.mib

rsRipEnable OBJECT-TYPE
    SYNTAX  INTEGER {
        enable(1),
        disable(2),
        shutdown(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enables, disables or shutdown (doesn't delete configuration) RIP."
::=  { ipSpec 9 }

rsTelnetPassword OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
           ""
    ::=  { ipSpec 11 }

rlTranslationNameToIpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlTranslationNameToIpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table translates IP interfaces's name to
        IP interface's address"
    ::= { ipSpec 12 }

rlTranslationNameToIpEntry OBJECT-TYPE
    SYNTAX      RlTranslationNameToIpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The row definition for this table."
    INDEX { IMPLIED rlTranslationNameToIpName }
    ::= { rlTranslationNameToIpTable 1 }

RlTranslationNameToIpEntry ::= SEQUENCE {
    rlTranslationNameToIpName   DisplayString,
    rlTranslationNameToIpIpAddr IpAddress
}

rlTranslationNameToIpName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..30))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP Interface name"
    ::=  { rlTranslationNameToIpEntry 1 }

rlTranslationNameToIpIpAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP Interface address"
    ::=  { rlTranslationNameToIpEntry 2 }

-- Mib for Preferance among routing protocols:
-- Range value 0..255 .  O is most preferred, 255 never used for forwarding.
-- only exception is direct which range 0..254 we prevent direct from becoming unreachable
-- (according to RFC1812  section 5.2.4)

rlIpRoutingProtPreference OBJECT IDENTIFIER  ::=  { ipSpec 13 }
-- see rlIpRouter.mib

rlOspf OBJECT IDENTIFIER ::=  { ipSpec 14 }
-- see rlIpRouter.mib

--IP address table mib ver

rlIpAddrTableMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IpAddrTable MIB's version."
    ::= {ipSpec 15 }

rlIpCidrRouteExtTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlIpCidrRouteExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Augmenting ipCidrRouteTable (ip forwarfing information table)
             for added info as read only"
    ::= {ipSpec 16 }

rlIpCidrRouteExtEntry OBJECT-TYPE
    SYNTAX      RlIpCidrRouteExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row of the table ipCidrRouteTable Extended
         by this definition."
    AUGMENTS { ipCidrRouteEntry }
    ::= {rlIpCidrRouteExtTable  1 }

RlIpCidrRouteExtEntry  ::= SEQUENCE {
    rlIpCidrRouteProto      INTEGER
}

rlIpCidrRouteProto OBJECT-TYPE
    SYNTAX   INTEGER {
        local(1),                 -- local interface
        netmgmt(2),               -- static route
        rip(3),                   -- Berkeley RIP or RIP-II
        ospfInternal(4),          -- Open Shortest Path First Internal Route
        ospfExternal(5),          -- Open Shortest Path First External Route
        ospfAggregateNetRange(6), -- Open Shortest Path First
        bgp4Internal(7),          -- Border Gateway Protocol Internal Route
        bgp4External(8),          -- Border Gateway Protocol External Route
        aggregateRoute(9),        --
        other(10)                 -- not specified
    }

    MAX-ACCESS  read-only
    STATUS      current
        DESCRIPTION
       "Added infor for ipCidrRouteTable.
        extends the info of ipCidrRouteProto to show the route inner protocol.
        Allowes the user to see which type of route in the protocol
        e.g. ospf internal, ospf external."
    ::= { rlIpCidrRouteExtEntry  1 }


rlIpStaticRoute OBJECT IDENTIFIER  ::=  { ipSpec 17 }

rlIpStaticRouteTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlIpStaticRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "This entity's    static (user configured) IP Routing table.
       entries are MAX-ACCESSible even if not used for forwarding "
    ::=  { rlIpStaticRoute      1 }

rlIpStaticRouteEntry OBJECT-TYPE
    SYNTAX      RlIpStaticRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A particular Static(user configured) route to  a  particular  destina-
         tion, under a particular policy."
    INDEX { rlIpStaticRouteDest,
            rlIpStaticRouteMask,
            rlIpStaticRouteTos,
            rlIpStaticRouteNextHop }
    ::=  { rlIpStaticRouteTable 1 }


RlIpStaticRouteEntry ::= SEQUENCE {
        rlIpStaticRouteDest                  IpAddress,
        rlIpStaticRouteMask                  IpAddress,
        rlIpStaticRouteTos                   INTEGER,
        rlIpStaticRouteNextHop               IpAddress,
        rlIpStaticRouteMetric                INTEGER,
        rlIpStaticRouteType                  INTEGER,
        rlIpStaticRouteNextHopAS             INTEGER,
        rlIpStaticRouteForwardingStatus      INTEGER,
        rlIpStaticRouteRowStatus             RowStatus,
        rlIpStaticRouteOwner                 INTEGER
      }

rlIpStaticRouteDest OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The destination IP address of this route.
       This object may not take a Multicast (Class  D)
       address value.
       Any assignment (implicit or  otherwise)  of  an
       instance  of  this  object to a value x must be
       rejected if the bitwise logical-AND of  x  with
       the  value of the corresponding instance of the
       rlIpStaticRouteMask object is not equal to x."
    ::= { rlIpStaticRouteEntry 1 }

rlIpStaticRouteMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Indicate the mask to be logical-ANDed with the
       destination address before being compared to
       the value in the rlIpStaticRouteDest  field.   For
       those  systems that do not support arbitrary
       subnet masks, an agent constructs the value  of
       the  rlIpStaticRouteMask  by  reference to the IP Ad-
       dress Class.
       Any assignment (implicit or  otherwise)  of  an
       instance of this object to a value x must be
       rejected if the bitwise logical-AND of  x  with
       the  value of the corresponding instance of the
       rlIpStaticRouteDest object is not equal to ipCidrRoute-
       Dest."
    ::= { rlIpStaticRouteEntry 2 }

rlIpStaticRouteTos OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "See ipCidrRouteTos definition
        For now only value 0 is valid"
    ::= { rlIpStaticRouteEntry 3 }

rlIpStaticRouteNextHop OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "On remote routes, the address of the next sys-
       tem en route; Otherwise, 0.0.0.0."
    ::= { rlIpStaticRouteEntry 4 }

rlIpStaticRouteMetric OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "The routing  metric  for  this  route.
       The semantics of this metric are determined by the user.
       normal semantic will be next hop count or some administarative distance
       to create routing policy."
    ::= { rlIpStaticRouteEntry 5 }

rlIpStaticRouteType OBJECT-TYPE
    SYNTAX   INTEGER {
                reject   (1), -- route which discards traffic
                local    (2), -- local interface
                remote   (3)  -- remote destination
             }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "The type of route.  Note that local(3)  refers
       to  a route for which the next hop is the final
       destination this is the case when user overides the a local interface
       entry to change it parameters;
       remote(4) refers to  a  route  for
       which  the  next  hop is not the final destina-
       tion.
       reject (2) refers to a route which, if matched, discards
       the message as unreachable. This is may be used as a means of
       correctly aggregating routes, When static routes are distributed (leaked)
       to other protocols."
    ::= { rlIpStaticRouteEntry 6 }

rlIpStaticRouteNextHopAS OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "The Autonomous System Number of the Next  Hop.
       The  semantics of this object are determined by
       the routing-protocol specified in  the  route's
       ipCidrRouteProto  value. When  this object is
       unknown or not relevant its value should be set
       to zero."
    DEFVAL { 0 }
    ::= { rlIpStaticRouteEntry 7 }

rlIpStaticRouteForwardingStatus OBJECT-TYPE
    SYNTAX   INTEGER {
                active (1),
                inactive  (2)
             }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "active - An indication that the route has implication on routing
       inactive - the route is a backup route or it is down. It is not used
                  in forwarding decision.
       Down means that the Ip interface on which it is configured is down.
       (Note: ip interface down may be for two reason - its admin status or
       the L2 interface , on which the ip interface is configured, status"
    ::= { rlIpStaticRouteEntry 8 }

rlIpStaticRouteRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlIpStaticRouteEntry 9 }

rlIpStaticRouteOwner OBJECT-TYPE
    SYNTAX   INTEGER {
                static  (1),
                dhcp    (2),
                default (3)
             }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "Static - The route is configured over Static IP.
                 This route is written to configuration files.
        Dhcp -   The route is Configured by DHCP
                 (received as part of DHCP configuration)
                 This route IS NOT written to configuration files
        Dhcp -   The route is Configured default system config
                 exist till any other configuration
                 is applied"
    ::= { rlIpStaticRouteEntry 10 }

rlIpRouter OBJECT IDENTIFIER  ::=  { ipSpec 18 }


rlIpAddressesNumber OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "This variable specifies current number of entries in rsIpAddrTable."
    DEFVAL  { 0 }
    ::=  { ipSpec 23 }

rlIpStaticPrefixesNumber OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "This variable specifies current number of static prefixes in the system."
    DEFVAL  { 0 }
    ::=  { ipSpec 24 }

rlIpTotalPrefixesNumber OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "This variable specifies current total number of prefixes in the system."
    DEFVAL  { 0 }
    ::=  { ipSpec 25 }

--- rlManagementIPv4

rlManagementIpv4 OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The system management IPv4 address which is kept between system modes changes"
    ::= { ipSpec 32 }

rlManagementIpv4Action OBJECT-TYPE
    SYNTAX   INTEGER {
                clear (1)
             }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The system management IPv4 action:
             clear - delete all ipv4 interfaces from startup configuration database except rlManagementIpv4"
    ::= { ipSpec 33 }

rlManagementIpIfindex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The system management IPs addresses ifIndex which is kept between system modes changes"
    ::= { ipSpec 34 }

rlSourceAddressSelectionTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlSourceAddressSelectionEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION        "The table specifies IPv4 and IPv6 source 
                       interfaces per application. Only supported 
                       applications are present in the table."
   ::= { ipSpec 35 }

rlSourceAddressSelectionEntry OBJECT-TYPE
   SYNTAX  RlSourceAddressSelectionEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION        "The row definition for this table."
   INDEX { IMPLIED rlSourceAddressSelectionApp}
   ::= { rlSourceAddressSelectionTable 1 }


RlSourceAddressSelectionEntry ::= SEQUENCE {
   rlSourceAddressSelectionApp                  DisplayString,
   rlSourceAddressSelectionInterfaceIPv4        InterfaceIndexOrZero,
   rlSourceAddressSelectionInterfaceIPv6        InterfaceIndexOrZero
}

rlSourceAddressSelectionApp OBJECT-TYPE
   SYNTAX DisplayString(SIZE(1..160))
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION       "The application which source interfaces are 
                      defined in the entry."
   ::= { rlSourceAddressSelectionEntry 1 }

rlSourceAddressSelectionInterfaceIPv4 OBJECT-TYPE
   SYNTAX InterfaceIndexOrZero
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION       "The ifIndex value of source interface for IPv4 address.
                      Zero means the interface is undefined."
   DEFVAL { 0 }
   ::= { rlSourceAddressSelectionEntry 2 }

rlSourceAddressSelectionInterfaceIPv6 OBJECT-TYPE
   SYNTAX InterfaceIndexOrZero
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION       "The ifIndex value of source interface for IPv6 address.
                      Zero means the interface is undefined."
   DEFVAL { 0 }
   ::= { rlSourceAddressSelectionEntry 3 }



--
-- Internet Address Table (Private/Extension)
--

rlIpAddressTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF RlIpAddressEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
           "This table is parralel to MIB II ipAddressTable, and is used to
            add/delete entries to/from that table.
            The table contains addressing information relevant to the
            entity's interfaces.

            In addition to ipAddressTable defined in standard MIB a represenattion of
            IPv6 addresses based on additionl address origin such as EUI-64, general
            prefix etc.
            In this case the address information is partial address information.
            Together with the address origin and the general prefix (when needed) user can
            construct full address information.

            The index (key) for this table includes this information additionally to the address."
    ::= { ipSpec 36 }

rlIpAddressEntry OBJECT-TYPE
    SYNTAX     RlIpAddressEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
           "An address mapping for a particular interface."
    INDEX { rlIpAddressAddrType,
            rlIpAddressAddr,
            rlIpAddressOrigin,
            rlIpAddressGeneralPrefixName }
    ::= { rlIpAddressTable 1 }

RlIpAddressEntry ::= SEQUENCE {
        rlIpAddressAddrType     InetAddressType,
        rlIpAddressAddr         InetAddress,
        rlIpAddressOrigin       RlIpAddressOriginTC,
        rlIpAddressGeneralPrefixName
                                DisplayString,
        rlIpAddressIfIndex      InterfaceIndex,
        rlIpAddressExtdType     INTEGER,
        rlIpAddressPrefix       RowPointer,
        rlIpAddressStatus       IpAddressStatusTC,
        rlIpAddressCreated      TimeStamp,
        rlIpAddressLastChanged  TimeStamp,
        rlIpAddressRowStatus    RowStatus,
        rlIpAddressStorageType  StorageType,
        rlIpAddressExtdPrefixLength InetAddressPrefixLength,
        rlIpAddressCompleteAddr InetAddress,
        rlIpAddressOperStatus   INTEGER
    }

rlIpAddressAddrType OBJECT-TYPE
    SYNTAX     InetAddressType
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
           "The address type of rlIpAddressAddr."
    ::= { rlIpAddressEntry 1 }

rlIpAddressAddr OBJECT-TYPE
    SYNTAX     InetAddress
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
           "The IP address to which this entry's addressing information
            pertains.  The address type of this object is specified in
            rlIpAddressAddrType.

            In case of auto-configure address such as eui-64, general-prefix and others
            it contains the partial address before appropriate manipulation.

            Implementors need to be aware that if the size of
            rlIpAddressAddr exceeds 116 octets, then OIDS of instances of
            columns in this row will have more than 128 sub-identifiers
            and cannot be accessed using SNMPv1, SNMPv2c, or SNMPv3.

            Note:
            Since interpeak doesnt use origin, 3rd index (key) - rlIpAddressOrigin, as part of the key,
            we assume that no same address can exists from different origins."
    ::= { rlIpAddressEntry 2 }

-- additional to standard MIB (1)

rlIpAddressOrigin OBJECT-TYPE
    SYNTAX     RlIpAddressOriginTC
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
           "The origin of the address."
    ::= { rlIpAddressEntry 3 }

rlIpAddressGeneralPrefixName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name assigned to the prefix."
    ::= { rlIpAddressEntry 4 }

-- (1)

rlIpAddressIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndex
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
           "The index value that uniquely identifies the interface to
            which this entry is applicable.  The interface identified by
            a particular value of this index is the same interface as
            identified by the same value of the IF-MIB's ifIndex."
    ::= { rlIpAddressEntry 5 }

rlIpAddressExtdType OBJECT-TYPE
    SYNTAX     INTEGER {
                 unicast(1),
                 anycast(2),
                 broadcast(3),
                 multicast(4)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
           "Extend standard field ipAddressType to multicast"
    DEFVAL { unicast }
    ::= { rlIpAddressEntry 6 }

rlIpAddressPrefix OBJECT-TYPE
    SYNTAX     RowPointer
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "A pointer to the row in the prefix table to which this
            address belongs.  May be { 0 0 } if there is no such row."
    DEFVAL { zeroDotZero }
    ::= { rlIpAddressEntry 7 }

-- following filed has changed to a key (2)
-- rlIpAddressOrigin OBJECT-TYPE
--     SYNTAX     IpAddressOriginTC
--     MAX-ACCESS read-only
--     STATUS     current
--     DESCRIPTION
--            "The origin of the address."
--     ::= { rlIpAddressEntry 8 }
-- (2)

rlIpAddressStatus OBJECT-TYPE
    SYNTAX     IpAddressStatusTC
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
           "The status of the address, describing if the address can be
            used for communication.

            In the absence of other information, an IPv4 address is
            always preferred(1)."
    DEFVAL { preferred }
    ::= { rlIpAddressEntry 8 }

rlIpAddressCreated OBJECT-TYPE
    SYNTAX     TimeStamp
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The value of sysUpTime at the time this entry was created.
            If this entry was created prior to the last re-
            initialization of the local network management subsystem,
            then this object contains a zero value."
    ::= { rlIpAddressEntry 9 }

rlIpAddressLastChanged OBJECT-TYPE
    SYNTAX     TimeStamp
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The value of sysUpTime at the time this entry was last
            updated.  If this entry was updated prior to the last re-
            initialization of the local network management subsystem,
            then this object contains a zero value."
    ::= { rlIpAddressEntry 10 }

rlIpAddressRowStatus OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
           "The status of this conceptual row.

            The RowStatus TC requires that this DESCRIPTION clause
            states under which circumstances other objects in this row
            can be modified.  The value of this object has no effect on
            whether other objects in this conceptual row can be
            modified.

            A conceptual row can not be made active until the
            rlIpAddressIfIndex has been set to a valid index."
    ::= { rlIpAddressEntry 11 }

rlIpAddressStorageType OBJECT-TYPE
    SYNTAX     StorageType
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
           "The storage type for this conceptual row.  If this object
            has a value of 'permanent', then no other objects are
            required to be able to be modified."
    DEFVAL { volatile }
    ::= { rlIpAddressEntry 12 }


-- additional fields - based on 'ipAddressEntry' augmentation (3)

rlIpAddressExtdPrefixLength OBJECT-TYPE
    SYNTAX     InetAddressPrefixLength
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
           "The prefix length of this address."
    DEFVAL { 64 }
    ::= { rlIpAddressEntry 13 }

rlIpAddressCompleteAddr OBJECT-TYPE
    SYNTAX     InetAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The Complete IP address to which this entry's addressing information
            pertains.

            In case of auto-configure address such as eui-64, general-prefix and others
            it contains the complete address after appropriate manipulation"
    ::= { rlIpAddressEntry 14 }

-- (3)

rlIpAddressOperStatus   OBJECT-TYPE
    SYNTAX INTEGER {
               up(1),
               down(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current operational state of the IP address."
    ::= { rlIpAddressEntry 15 }

rlIpDefaultDSCP OBJECT-TYPE
SYNTAX  INTEGER(0..63)
MAX-ACCESS  read-write
STATUS  current
DESCRIPTION
      "The default value inserted into the DSCP
      field of the IP header of datagrams originated at
      this entity, whenever a DSCP value is not supplied
      by the application."
::= { ipSpec 37 }

rlIpDefaultUP OBJECT-TYPE
SYNTAX  INTEGER(0..7)
MAX-ACCESS  read-write
STATUS  current
DESCRIPTION
      "The default value inserted into the User Priority
      field in the 802.1q VLAN tag of IPv4 frames sent by the
      CPU."
::= { ipSpec 38 }

rlIpv4MtuSize OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
           "Sets the maximum transmission unit (MTU) size in bytes of IPv4 packets (payload)."
    ::= { ipSpec 39 }

rlIcmpCountersClear OBJECT-TYPE
    SYNTAX   INTEGER {
                clear (0)
             }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "clear - delete all icmp counters"
    ::= { ipSpec 40 }

rlIpCountersClear OBJECT-TYPE
    SYNTAX   INTEGER {
                clear (0)
             }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "clear - delete all ip counters"
    ::= { ipSpec 41 }
    
rlManagementIpPortIfindex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The system management port ifIndex"
    ::= { ipSpec 42 }

END


