
RADLAN-ippreflist-MIB DEFINITIONS ::= BEGIN

-- Title:      IP Prefix List
-- Version:    7.50.00.00
-- Date:       22-May-2011
--

IMPORTS
    TruthValue, TEXTUAL-CONVENTION, TimeStamp,
    DisplayString, DateAndTime, RowStatus                FROM SNMPv2-TC
    TimeTicks, IpAddress, NOTIFICATION-TYPE,
    MODULE-IDENTITY, OBJECT-TYPE, Unsigned32             FROM SNMPv2-SMI
    InetAddress, InetAddressType,
    InetAddressPrefixLength,
    InetVersion, InetZoneIndex                           FROM INET-ADDRESS-MIB
    rnd                                                  FROM RADLAN-MIB;



rlIpPrefList  OBJECT IDENTIFIER ::= { rnd 212 }


RlIpPrefListEntryType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "Prefix List entry type defines data type in the entry. Rule (1) means
         the entry inludes classification and action. Description (2) means
         the entry icludes comments only."
    SYNTAX  INTEGER {
        rule(1),
        description(2)
}

RlIpPrefListActionType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "Prefix List action type. Drop action prevents packet forwarding.
         Permit action allows packet forwarding."
    SYNTAX  INTEGER {
        drop(1),
        permit(2)
}

RlIpPrefListType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "Classification type is used to create prefix list rule.
         IPv4 type means match IPv4 packets. IPv6 type means match IPv6 packets."
    SYNTAX  INTEGER {
        ipv4(1),
        ipv6(2)
}


rlIpPrefListTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlIpPrefListEntry
    MAX-ACCESS   not-accessible
    STATUS   current
    DESCRIPTION
       "The IP Prefix List table."
    ::= {  rlIpPrefList 1 }


rlIpPrefListEntry OBJECT-TYPE
    SYNTAX      RlIpPrefListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the rlIpPrefListTable."
    INDEX  { rlIpPrefListType, rlIpPrefListName, rlIpPrefListEntryIndex }
    ::= { rlIpPrefListTable 1 }

RlIpPrefListEntry::= SEQUENCE {

   rlIpPrefListType                                RlIpPrefListType,
   rlIpPrefListName                                DisplayString,
   rlIpPrefListEntryIndex                          Unsigned32,
   rlIpPrefListEntryType                           RlIpPrefListEntryType,
   rlIpPrefListInetAddrType                        InetAddressType,
   rlIpPrefListInetAddr                            InetAddress,
   rlIpPrefListPrefixLength                        INTEGER,
   rlIpPrefListAction                              RlIpPrefListActionType,
   rlIpPrefListGeLength                            INTEGER,
   rlIpPrefListLeLength                            INTEGER,
   rlIpPrefListDescription                         DisplayString,
   rlIpPrefListHitCount                            INTEGER,
   rlIpPrefListRowStatus                           RowStatus

}




rlIpPrefListType OBJECT-TYPE
    SYNTAX      RlIpPrefListType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Prefix List Type."
    ::= { rlIpPrefListEntry 1 }


rlIpPrefListName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(1..64))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Prefix List Name."
    ::= { rlIpPrefListEntry 2 }

rlIpPrefListEntryIndex OBJECT-TYPE
    SYNTAX      Unsigned32(1..4294967294)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry Index for specific prefix list."
    ::= { rlIpPrefListEntry 3 }


rlIpPrefListEntryType OBJECT-TYPE
    SYNTAX     RlIpPrefListEntryType
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "Prefix list entry type."
    ::= { rlIpPrefListEntry 4 }


rlIpPrefListInetAddrType OBJECT-TYPE
    SYNTAX     InetAddressType
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
           "The address type of rlIpPrefListIpAddr."
    ::= { rlIpPrefListEntry 5 }


rlIpPrefListInetAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "IP address."
    ::= { rlIpPrefListEntry 6 }


rlIpPrefListPrefixLength OBJECT-TYPE
    SYNTAX     INTEGER(0..128)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
           "The prefix list can be a number from 0 to 32 for IPv4 address
           and from 0 to 128 for IPv6 address."
    ::= { rlIpPrefListEntry 7 }


rlIpPrefListAction OBJECT-TYPE
    SYNTAX      RlIpPrefListActionType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Drop or permit action for a matching condition."
    ::= { rlIpPrefListEntry 8 }


rlIpPrefListGeLength OBJECT-TYPE
    SYNTAX      INTEGER(0..128)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies the lesser value of a range by applying the ge-length argument
        to the specified range. ge-length repesents the minimum prefix length to be matched."
    DEFVAL{ 0 }
    ::= { rlIpPrefListEntry 9 }

rlIpPrefListLeLength OBJECT-TYPE
    SYNTAX      INTEGER(0..128)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies the greater value of a range by applying the ge-length argument
        to the specified range. le-length repesents the maximum prefix length to be matched."
    DEFVAL{ 0 }
    ::= { rlIpPrefListEntry 10 }


rlIpPrefListDescription OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..80))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Prefix List Name."
    ::= { rlIpPrefListEntry 11 }


rlIpPrefListHitCount OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Match counter."
    ::= { rlIpPrefListEntry 12 }



rlIpPrefListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Row status."
    ::= { rlIpPrefListEntry 13 }




------------------------------------------------------------------



rlIpPrefListInfoTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlIpPrefListInfoEntry
    MAX-ACCESS   not-accessible
    STATUS   current
    DESCRIPTION
       "The IP Prefix List Info table."
    ::= {  rlIpPrefList 2 }


rlIpPrefListInfoEntry OBJECT-TYPE
    SYNTAX      RlIpPrefListInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the rlIpPrefListInfoTable."
    INDEX  { rlIpPrefListInfoType, rlIpPrefListInfoName }
    ::= { rlIpPrefListInfoTable 1 }



RlIpPrefListInfoEntry::= SEQUENCE {
   rlIpPrefListInfoType                                RlIpPrefListType,
   rlIpPrefListInfoName                                DisplayString,
   rlIpPrefListInfoEntriesNumber                       INTEGER,
   rlIpPrefListInfoRangeEntries                        INTEGER,
   rlIpPrefListInfoNextFreeIndex                       INTEGER

}


rlIpPrefListInfoType OBJECT-TYPE
    SYNTAX      RlIpPrefListType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Prefix List Type."
    ::= { rlIpPrefListInfoEntry 1 }


rlIpPrefListInfoName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(1..64))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Prefix List Name."
    ::= { rlIpPrefListInfoEntry 2 }

rlIpPrefListInfoEntriesNumber OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of entries for specific prefix list."
    ::= { rlIpPrefListInfoEntry 3 }


rlIpPrefListInfoRangeEntries OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of entries with range for specific prefix list."
    ::= { rlIpPrefListInfoEntry 4 }


rlIpPrefListInfoNextFreeIndex OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Next free index for specific prefix list."
    ::= { rlIpPrefListInfoEntry 5 }


END

