MARVELL-TIMEBASED-PORT-SHUTDOWN-MIB DEFINITIONS ::= BEGIN

-- Title:      MARVELL TIME-BASED PORT OPERATION  Configuration
-- Version:    7.50.00.00
-- Date:       06-Aug-2011
--

IMPORTS
    TruthValue,TEXTUAL-CONVENTION,DisplayString,
    RowStatus                                            FROM SNMPv2-TC
    MODULE-IDENTITY, OBJECT-TYPE                         FROM SNMPv2-SMI
    ifIndex                                              FROM IF-MIB
    PortList                                             FROM Q-BRIDGE-MIB
    rnd                                                  FROM RADLAN-MIB;



    rlTimeBasedPort MODULE-IDENTITY
       LAST-UPDATED "201108060000Z"
       ORGANIZATION "Marvell Semiconductor, Inc."
       CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
       DESCRIPTION
                "The private MIB module definition for Time Based Port Operation MIB."
       REVISION "201108060000Z"
       DESCRIPTION
                "Initial version of this MIB."
    ::= { rnd 208 }

     rlTimeBasedPortVersion OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
        "This scalar keep current supported version for Time Based Port feature.Initial version value is 1"
    ::=  { rlTimeBasedPort  1 }



    rlTimeBasedPortTable  OBJECT-TYPE
        SYNTAX  SEQUENCE OF RlTimeBasedPortEntry
        MAX-ACCESS   not-accessible
        STATUS   current
        DESCRIPTION
       "The table is used to manage time based port operation schedules."
    ::=  { rlTimeBasedPort  2 }


    rlTimeBasedPortEntry OBJECT-TYPE
    SYNTAX     RlTimeBasedPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlTimeBasedPortEntry."
    INDEX  { ifIndex,rlTimeBasedPortTimeRangeName }
    ::= { rlTimeBasedPortTable 1 }


    RlTimeBasedPortEntry ::= SEQUENCE {
    rlTimeBasedPortTimeRangeName     DisplayString,
    rlTimeBasedPortAction            INTEGER,
    rlTimeBasedPortActive            TruthValue,
    rlTimeBasedPortRowStatus         RowStatus
    }


    rlTimeBasedPortTimeRangeName  OBJECT-TYPE
    SYNTAX     DisplayString(SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Name of time range."
    ::= { rlTimeBasedPortEntry 1 }


    rlTimeBasedPortAction  OBJECT-TYPE
    SYNTAX      INTEGER {
        up   (1),
        down (2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This field constitutes what action must be applyed to port during the time range."
    ::= { rlTimeBasedPortEntry 2 }

    rlTimeBasedPortActive  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This field indicates if the time-range is active or not ."
    ::= { rlTimeBasedPortEntry 3 }


    rlTimeBasedPortRowStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
         "The status of a table entry.
          It is used to delete an entry from this table."
    ::= { rlTimeBasedPortEntry 4 }


END

