MARVELL-UDLD-MIB DEFINITIONS ::= BEGIN

-- Title:                MARVELL UDLD ROS
--                       Private UDLD MIB
-- Version:              7.60
-- Date:                 06 Dec 2012

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Gauge32, Unsigned32,
    NOTIFICATION-TYPE
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue, RowStatus, MacAddress
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    rnd, rndNotifications
        FROM RADLAN-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    InterfaceIndex
        FROM IF-MIB;

UdldString ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
            "The Device-ID TLV should contain the switch base MAC address in ACSII format."
    SYNTAX      SnmpAdminString


UdldPortBidirectionalState ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION    "Port UDLD current status (shutdown, idle, detection, undetermined, bidirectional)."
    SYNTAX INTEGER {
        shutdown(1),
        idle(2),
        detection(3),
        undetermined(4),
        bidirectional(5)
}

UdldNeighborCurrentState ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION    "Port UDLD Neighbor current status (Disabled, Enabled, Undefined, Bidirectional)."
    SYNTAX INTEGER {
        disabled(1),
        enabled(2),
        undefined(3),
        bidirectional(4)
}

UdldGlobalMode  ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION    "Global (fiber) Port UDLD curent status (normal, aggressive, disabled)."
    SYNTAX INTEGER {
        normal(1),
        aggressive(2),
        disabled(3)
}

UdldPortMode  ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION    "Port UDLD curent status (normal, aggressive, disabled, default)."
    SYNTAX INTEGER {
        normal(1),
        aggressive(2),
        disabled(3),
        default(4)
}

rlUdld MODULE-IDENTITY
    LAST-UPDATED "201208010000Z"
    ORGANIZATION "Marvell Semiconductor, Inc."
    CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
    DESCRIPTION
           "This private MIB module for UDLD (Cisco Systems UniDirectional Link Detection Protocol)."
    REVISION "201208010000Z"
    DESCRIPTION
           "Initial revision."
     ::= { rnd 218 }

-----------------------------------
-- UDLD - rlUdldPortTable
------------------------------------

rlUdldPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlUdldPortEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The table holds information for Udld Ethernet ports."
    ::= {rlUdld 1 }

rlUdldPortEntry  OBJECT-TYPE
    SYNTAX      RlUdldPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry in the rlUdldPortTable."
    INDEX    { rlUdldPortIfIndex  }
    ::= {rlUdldPortTable 1 }

RlUdldPortEntry ::= SEQUENCE {
    rlUdldPortIfIndex                   InterfaceIndex,
    rlUdldPortAdminMode                 UdldPortMode,
    rlUdldPortOperMode                  UdldPortMode,
    rlUdldPortDefaultConfiguration      TruthValue,
    rlUdldBidirectionalState            UdldPortBidirectionalState,
    rlUdldNumberOfDetectedNeighbors     INTEGER
}

rlUdldPortIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Interface Index. This variable is the key for udld port table.
         uniquely identifies the udld port information."
    ::= { rlUdldPortEntry 1 }

rlUdldPortAdminMode OBJECT-TYPE
    SYNTAX      UdldPortMode
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies port UDLD admin configured mode (normal, aggressive, disable)."
    ::= { rlUdldPortEntry 2 }

rlUdldPortOperMode OBJECT-TYPE
    SYNTAX      UdldPortMode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable identifies port UDLD operational mode (normal, aggressive, disable).
        for fiber ports it is combination of global mode and port mode"
    ::= { rlUdldPortEntry 3 }

rlUdldPortDefaultConfiguration OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates whether tne user configure the udld port. to present (default) or not in port configuration."
    ::= {  rlUdldPortEntry 4 }

rlUdldBidirectionalState OBJECT-TYPE
    SYNTAX      UdldPortBidirectionalState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable identifies the port UDLD status (shutdown, idle, detection, undetermined, bidirectional)."
    ::= { rlUdldPortEntry 5 }

rlUdldNumberOfDetectedNeighbors OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number Of Detected Neighbors for this port."
    ::= { rlUdldPortEntry 6 }

------------------------------------
-- UDLD - rlUdldNeighborTable
------------------------------------

rlUdldNeighborTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlUdldNeighborEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The table holds information for Udld Neighbor of ethernet ports."
    ::= {rlUdld 2 }

rlUdldNeighborEntry  OBJECT-TYPE
    SYNTAX      RlUdldNeighborEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry in the rlUdldNeighborTable."
    INDEX    { rlUdldNeighborPortIfIndex, rlUdldNeighborDeviceID, rlUdldNeighborPortID }
    ::= {rlUdldNeighborTable  1 }

RlUdldNeighborEntry ::= SEQUENCE {
    rlUdldNeighborPortIfIndex               InterfaceIndex,
    rlUdldNeighborDeviceID                  UdldString,
    rlUdldNeighborPortID                    UdldString,
    rlUdldNeighborDeviceMACAddress          MacAddress,
    rlUdldNeighborDeviceName                UdldString,
    rlUdldNeighborMessageTime               INTEGER,
    rlUdldNeighborLeftLifeTime              INTEGER,
    rlUdldNeighborCurrentState              UdldNeighborCurrentState
}

rlUdldNeighborPortIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Interface Index. This variable is the key for udld port Neighbor table.
         uniquely identifies the udld port index."
    ::= { rlUdldNeighborEntry 1 }

rlUdldNeighborDeviceID  OBJECT-TYPE
    SYNTAX      UdldString
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Neighbor Device-ID TLV should contain the switch base MAC address in ACSII format."
    ::= { rlUdldNeighborEntry 2 }

rlUdldNeighborPortID  OBJECT-TYPE
    SYNTAX      UdldString
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Port-ID TLV should contain the port ACSII name as it is printed in show CLI commands."
    ::= { rlUdldNeighborEntry 3 }

rlUdldNeighborDeviceMACAddress OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "The Neighbor mac address"
    ::= { rlUdldNeighborEntry 4 }

rlUdldNeighborDeviceName  OBJECT-TYPE
    SYNTAX      UdldString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Neighbor NeighborDevice Name TLV should contain sysName in ACSII."
    ::= { rlUdldNeighborEntry 5 }

rlUdldNeighborMessageTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Neighbor Message Time is from Message Interval TLV.
        This time interval value used by a neighbor to send UDLD probes
        after the linkup or detection phases. Its time unit is 1 second."
    ::= { rlUdldNeighborEntry 6 }

rlUdldNeighborLeftLifeTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The remaining holdtime for Neighbor entry in cache in seconds."
    ::= { rlUdldNeighborEntry 7 }

rlUdldNeighborCurrentState OBJECT-TYPE
    SYNTAX      UdldNeighborCurrentState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable identifies the Neighbor port UDLD current status (Disabled, Enabled, Undefined, Bidirectional)."
    ::= { rlUdldNeighborEntry 8 }

------------------------------------
-- UDLD - Global UDLD Mode
------------------------------------

rlUdldGlobalUDLDMode OBJECT-TYPE
    SYNTAX      UdldGlobalMode
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Define Global UDLD Mode (normal, aggressive, disable)"
    ::= { rlUdld 3 }

------------------------------------
-- UDLD - Global Message Time
------------------------------------

rlUdldGlobalMessageTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Define global value of the interval between two sent probe messages, use the udld
        message time command in Global Configuration mode."
    ::= { rlUdld 4 }

END

