ELTEX-ISIS-MIB DEFINITIONS ::= BEGIN

  IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Integer32,
    Counter32,
    Gauge32,
    Unsigned32,
    IpAddress,
    TimeTicks
      FROM SNMPv2-SMI

    TEXTUAL-CONVENTION,
    DisplayString,
    TruthValue,
    RowStatus,
    TimeStamp,
    TimeInterval
      FROM SNMPv2-TC

    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
      FROM SNMPv2-CONF

    InetAddressType,
    InetAddress,
    InetPortNumber,
    InetAddressPrefixLength
      FROM INET-ADDRESS-MIB

    InterfaceIndexOrZero,
    InterfaceIndex
      FROM IF-MIB

    SnmpAdminString
      FROM SNMP-FRAMEWORK-MIB

    eltexLtd
      FROM ELTEX-SMI-ACTUAL;
      

  eltexIsisMIB MODULE-IDENTITY
    LAST-UPDATED "201906060000Z" -- Mon Jun 06 00:00:00 GMT 2019
    ORGANIZATION "Eltex Enterprise Co, Ltd."
    CONTACT-INFO 
        "eltex-co.ru"
    DESCRIPTION  
        "The MIB module for management of the ISIS protocol."

  ::= { eltexLtd 55 }

-------------------------------------------------------------------------------
-- Textual Conventions.

    EltexIsisSystemID ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION "A system ID."
        SYNTAX OCTET STRING (SIZE(6))

    EltexIsisAdminState ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION "Type used in enabling and disabling a row.
                     Values match those in RFC 2863."
        SYNTAX INTEGER
            {
                on(1),
                off(2)
            }

    EltexNETAddress ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION
            "Network Entity Title address"
        SYNTAX OCTET STRING (SIZE(0..20))

    EltexIsisOperStatus ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION
           "The current operational state of ISIS entity."
        SYNTAX INTEGER 
            {
                operStatusUp(1),       -- active
                operStatusDown(2),     -- inactive
                operStatusGoingUp(3),  -- activating
                operStatusGoingDown(4),-- deactivating
                operStatusActFailed(5) -- activation failed
            }

    EltexIsisISLevel ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION "Identifies a level."
        SYNTAX INTEGER
            {
                area(1),        -- L1
                domain(2)       -- L2
            }

    EltexIsisLinkStatePDUID ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION "A Link State PDU Identifier."
        SYNTAX OCTET STRING (SIZE(8))

    EltexIsisISPriority ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION
            "Integer sub-range for IS-IS priority."
        SYNTAX Integer32 (0..127)

    EltexIsisMetricStyle ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION
            "Do we use 1195 style Metrics or wide metrics."
        SYNTAX INTEGER
            {
                narrow(1),
                wide(2),
                both(3)
            }

    EltexIsisWideMetric ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION
            "Wide Metric for IS Neighbors.  ISO 10589 provides a
             6 bit metric.  Traffic Engineering extensions provide
             24 bit metrics."
        SYNTAX Unsigned32 (1..16777215)

    EltexIsisAuthType ::= TEXTUAL-CONVENTION
       STATUS current
       DESCRIPTION
          "The authentication type."
       SYNTAX       INTEGER {
                       none (0),
                       simplePassword (1),
                       hmac-md5 (2)
                    }

    EltexIsisHelloPaddingAction ::= TEXTUAL-CONVENTION
       STATUS current
       DESCRIPTION
          "What to do with padding in hello packets?

           - disabled (0) - Disable padding in all hello packets.
           - enabled  (1) - Add padding in all hello packets.
           - adaptive (2) - Enable padding in hello packets before
                            establishing a connection with a neighbor.
          "
       SYNTAX       INTEGER {
                       disabled (0),
                       enabled  (1),
                       adaptive (2)
                    }

-------------------------------------------------------------------------------

  eltexIsisObjects    OBJECT IDENTIFIER ::= { eltexIsisMIB 1 }

  eltexIsisSystem     OBJECT IDENTIFIER ::= { eltexIsisObjects 1 }
--
-- ISIS System Table.
--

  eltexIsisSysTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisSysEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "The set of instances of the Integrated IS-IS
                   protocol existing on the system."
  ::= { eltexIsisSystem 1 }

  eltexIsisSysEntry OBJECT-TYPE
      SYNTAX EltexIsisSysEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Each row defines information specific to a single
                   instance of the IS-IS protocol existing on the system."
      REFERENCE "{ISIS.poi cLNSISISBasic-P (1)}"
      INDEX { eltexIsisSysInstance }
  ::= { eltexIsisSysTable 1 }
  
  EltexIsisSysEntry ::= SEQUENCE {
          eltexIsisSysInstance
              Integer32,
          eltexIsisSysType
              INTEGER,
          eltexIsisSysID
              EltexIsisSystemID,
          eltexIsisSysAdminState
              EltexIsisAdminState,
          eltexIsisSysOperState
              EltexIsisOperStatus,
          eltexIsisSysRowStatus
              RowStatus,
          eltexIsisSysMaxAge
              Unsigned32,
          eltexIsisSysMaxLSPGenInt
              Unsigned32,
          eltexIsisSysCalcMaxDelay
              Unsigned32,
          eltexIsisSysCalcThrshUpdStart
              Unsigned32,
          eltexIsisSysCalcThrshUpdRestart
              Unsigned32,
          eltexIsisSysCalcThrshRestartLimit
              Unsigned32,
          eltexIsisSysHostNameDynamic
              TruthValue
      }

  eltexIsisSysInstance OBJECT-TYPE
      SYNTAX Integer32 (1..2147483647)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "The unique identifier of the Integrated IS-IS
                   instance to which this row corresponds.
                   This object follows the index behavior."
  ::= { eltexIsisSysEntry 1 }

  eltexIsisSysType OBJECT-TYPE
      SYNTAX INTEGER
          {
              reserved (0),
              level1IS (1),
              level2IS (2),
              level1L2IS (3)
          }
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION "At which levels is the Intermediate System
                   running? This object follows the
                   replaceOnlyWhileDisabled behavior."
      REFERENCE "{ISIS.aoi iSType (2)}"
      DEFVAL { level1L2IS }
  ::= { eltexIsisSysEntry 2 }

  eltexIsisSysID OBJECT-TYPE
      SYNTAX EltexIsisSystemID
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The ID for this instance of the Integrated IS-IS
                   protocol."
      REFERENCE "{ISIS.aoi systemId (119)}"
  ::= { eltexIsisSysEntry 3 }

  eltexIsisSysAdminState OBJECT-TYPE
      SYNTAX EltexIsisAdminState
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION "The administrative state of this instance of the
                   Integrated IS-IS protocol.  Setting this object to the
                   value 'on' when its current value is 'off' enables operation
                   of this instance of the Integrated IS-IS protocol."
      DEFVAL { off }
  ::= { eltexIsisSysEntry 4 }

  eltexIsisSysOperState OBJECT-TYPE
      SYNTAX EltexIsisOperStatus
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The current operational status of this IS-IS instance."
  ::= { eltexIsisSysEntry 5 }

  eltexIsisSysRowStatus OBJECT-TYPE
      SYNTAX RowStatus
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION "The state of the IS-IS router.  Turning this to
                   state 'destroy' forces the router to forget all
                   the current configuration.  Setting the state to
                   'notInService' stops protocol processing, but
                   retains the configuration."
  ::= { eltexIsisSysEntry 6 }

  eltexIsisSysMaxAge OBJECT-TYPE
      SYNTAX Unsigned32 (350..65535)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION "Value to place in RemainingLifeTime field of
                   the LSPs we generate.
                   This should be at least 300 seconds greater than
                   eltexIsisSysMaxLSPGenInt."
      DEFVAL { 1200 }
  ::= { eltexIsisSysEntry 7 }

  eltexIsisSysMaxLSPGenInt OBJECT-TYPE
      SYNTAX Unsigned32 (1..65235)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION 
            "Maximum interval, in seconds, between generated LSPs
             by this instance of the protocol. This object follows
             the resettingTimer behavior.  The value must be
             greater than any value configured for
             eltexIsisSysLevelMinLSPGenInt, and should be at least 300
             seconds less than eltexIsisSysMaxAge.

             Note that this value is specified in seconds whereas
             eltexIsisSysLevelMinLSPGenInt is specified in milliseconds."
      DEFVAL { 900 }
  ::= { eltexIsisSysEntry 8 }

  eltexIsisSysCalcMaxDelay OBJECT-TYPE
      SYNTAX Unsigned32 (0..'FFFFFFFF'H)
      MAX-ACCESS read-write
      STATUS  current
      DESCRIPTION
          "The maximum delay before the Routing Table is
           recalculated following a change to the Link State
           Database.  (Recalculation is delayed to reduce the
           frequency of recalculations of the Routing Table).

           This parameter has units of milliseconds.  A value of
           0 indicates that a routing calculation will
           immediately follow an update to the database."
       DEFVAL { 5000 }
  ::= { eltexIsisSysEntry 9 }

  eltexIsisSysCalcThrshUpdStart OBJECT-TYPE
      SYNTAX Unsigned32 (0..'FFFFFFFF'H)
      MAX-ACCESS read-write
      STATUS  current
      DESCRIPTION
          "This parameter can be used to override the routing
           calculation delay indicated by the eltexIsisSysCalcMaxDelay
           parameter when the number of updates to the Link State
           Database reaches a threshold value.

           This parameter specifies the threshold number of updates
           that can be made to the Link State Database such that any
           subsequent update to the database causes a full routing
           calculation to start immediately.

           - 0 indicates that a routing calculation will immediately
             follow an update to the database.

           - 0xFFFFFFFF indicates that this threshold is infinite, and
             hence the timing of a routing calculation is determined
             solely by the configured calculation delay."
       DEFVAL { 4294967295 }
  ::= { eltexIsisSysEntry 10 }

  eltexIsisSysCalcThrshUpdRestart OBJECT-TYPE
      SYNTAX Unsigned32 (0..'FFFFFFFF'H)
      MAX-ACCESS read-write
      STATUS  current
      DESCRIPTION
          "This parameter can be used to interrupt a full routing
           calculation when the number of pending updates to the Link
           State Database has reached a threshold value.

           This parameter specifies the threshold number of updates
           that can be made to the Link State Database such that any
           subsequent update to the database causes the current
           routing  calculation to be interrupted, and a new
           calculation to start using an up to date Link State
           Database.

           - 0 indicates that an update to the Link State Database
             will cause any current routing calculation to be
             interrupted and a new one to start.

           - 0xFFFFFFFF indicates that this threshold is infinite, and
             hence no number of pending updates to the database will
             cause a routing calculation to be interrupted."
       DEFVAL { 4294967295 }
  ::= { eltexIsisSysEntry 11 }

  eltexIsisSysCalcThrshRestartLimit OBJECT-TYPE
      SYNTAX Unsigned32 (1..'FFFFFFFF'H)
      MAX-ACCESS read-write
      STATUS  current
      DESCRIPTION
          "This parameter limits the number of consecutive times a
           routing calculation can be interrupted by new updates.
           This guarantees that the routing calculation will actually
           complete.

           - 1 indicates that once a calculation has been interrupted
             once, it will not be interrupted again.

           - 0xFFFFFFFF indicates that the calculation can always be
             interrupted."
       DEFVAL { 10 }
  ::= { eltexIsisSysEntry 12 }

    eltexIsisSysHostNameDynamic OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Enable translation from System ID to hostname.

             Advertise hostname to other Intermediate Systems in the
             Dynamic Hostname TLV."
        DEFVAL { true }
    ::= { eltexIsisSysEntry 13 }

--
-- NET Address Table.
--

  eltexIsisNetAddrTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisNetAddrEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "The set of NET addresses configured on this
                   Intermediate System."
      REFERENCE "{ISIS.aoi manualAreaAddresses (10)}"
  ::= { eltexIsisSystem 2 }

  eltexIsisNetAddrEntry OBJECT-TYPE
      SYNTAX EltexIsisNetAddrEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Each entry contains one NET address manually configured
                   on this system"
      INDEX { eltexIsisSysInstance,
              eltexIsisNetAddr }
  ::= { eltexIsisNetAddrTable 1 }

  EltexIsisNetAddrEntry ::=
      SEQUENCE {
          eltexIsisNetAddr
              EltexNETAddress,
          eltexIsisNetAddrRowStatus
              RowStatus
          }

  eltexIsisNetAddr OBJECT-TYPE
      SYNTAX EltexNETAddress
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "A manually configured NET address for this system.  This
                   object follows the index behavior. "

  ::= { eltexIsisNetAddrEntry 1 }

  eltexIsisNetAddrRowStatus OBJECT-TYPE
      SYNTAX RowStatus
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION "The state of the eltexIsisNetAddrEntry."
  ::= { eltexIsisNetAddrEntry 2 }

--
-- The Router Table keeps track of hostnames and system IDs
-- associated with peers in the area and domain.
--

  eltexIsisRouterTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisRouterEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The set of hostnames and system ID."
  ::= { eltexIsisSystem 5 }

  eltexIsisRouterEntry OBJECT-TYPE
      SYNTAX EltexIsisRouterEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "Each entry tracks information about one peer at
           one level."
      INDEX { eltexIsisSysInstance,
              eltexIsisRouterSysID,
              eltexIsisRouterLevel }
  ::= { eltexIsisRouterTable 1 }

  EltexIsisRouterEntry ::=
      SEQUENCE {
          eltexIsisRouterSysID
              EltexIsisSystemID,
          eltexIsisRouterLevel
              EltexIsisISLevel,
          eltexIsisRouterHostName
              SnmpAdminString
      }

  eltexIsisRouterSysID OBJECT-TYPE
      SYNTAX EltexIsisSystemID
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The System ID of the Router Peer."
  ::= { eltexIsisRouterEntry 1 }

  eltexIsisRouterLevel OBJECT-TYPE
      SYNTAX EltexIsisISLevel
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The level of this Intermediate System."
  ::= { eltexIsisRouterEntry 2 }

  eltexIsisRouterHostName OBJECT-TYPE
      SYNTAX SnmpAdminString
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The hostname listed in LSP, or NULL if none."
  ::= { eltexIsisRouterEntry 3 }

--
-- ISIS System Level Table.
--

  eltexIsisSysLevelTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisSysLevelEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Level specific information about an instance of IS-IS."
  ::= { eltexIsisSystem 3 }

  eltexIsisSysLevelEntry OBJECT-TYPE
      SYNTAX EltexIsisSysLevelEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Describe variables defined for Area or Domain."
      INDEX { eltexIsisSysInstance,
              eltexIsisSysLevelIndex }
  ::= { eltexIsisSysLevelTable 1 }
  
  EltexIsisSysLevelEntry ::= SEQUENCE {
          eltexIsisSysLevelIndex
              INTEGER,
          eltexIsisSysLevelMinLSPGenInt
              Unsigned32,
          eltexIsisSysLevelMetricStyle
              EltexIsisMetricStyle,
          eltexIsisSysLevelAuthType
              EltexIsisAuthType,
          eltexIsisSysLevelAuthKey
              OCTET STRING,
          eltexIsisSysLevelAuthKeyChain
              OCTET STRING,
          eltexIsisSysLevelOrigLSPBuffSize
              Unsigned32
      }

  eltexIsisSysLevelIndex OBJECT-TYPE
      SYNTAX INTEGER
          {
              level1IS (1),
              level2IS (2)
          }
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The level that this entry describes."
  ::= { eltexIsisSysLevelEntry 1 }

  eltexIsisSysLevelMinLSPGenInt OBJECT-TYPE
      SYNTAX Unsigned32 (1000..65535000)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
          "Minimum interval, in milliseconds, between successive
           generation of LSPs with the same LSPID at this level
           by this instance of the protocol.  This object
           follows the resettingTimer behavior."
      DEFVAL { 30000 }
  ::= { eltexIsisSysLevelEntry 2 }

  eltexIsisSysLevelMetricStyle OBJECT-TYPE
      SYNTAX EltexIsisMetricStyle
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
          "Which style of Metric do we generate in our LSPs
           at this level?"
      DEFVAL { both }
  ::= { eltexIsisSysLevelEntry 3 }

  eltexIsisSysLevelAuthType OBJECT-TYPE
      SYNTAX      EltexIsisAuthType
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "Authentication type for area/domain level authentication."
  ::= { eltexIsisSysLevelEntry 4 }

  eltexIsisSysLevelAuthKey OBJECT-TYPE
      SYNTAX      OCTET STRING (SIZE (0..20))
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "Authentication key for area/domain level
           authentication. If the field eltexIsisSysLevelAuthKeyChain
           is set and key chain with this name is present in the
           configuration, then this field is ignored."
  ::= { eltexIsisSysLevelEntry 5 }

  eltexIsisSysLevelAuthKeyChain OBJECT-TYPE
      SYNTAX      OCTET STRING (SIZE (0..32))
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "Name of key chain for area/domain level
           authentication."
  ::= { eltexIsisSysLevelEntry 6 }


  eltexIsisSysLevelOrigLSPBuffSize OBJECT-TYPE
      SYNTAX Unsigned32 (512..9000)
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
          "The maximum size of LSPs and SNPs originated by
           this Intermediate System at this level.

           This field can only be changed if the eltexIsisSysAdminState
           field is set to off."
      DEFVAL { 1500 }
  ::= { eltexIsisSysLevelEntry 7 }

  eltexIsisCirc     OBJECT IDENTIFIER ::= { eltexIsisObjects 2 }

--
-- Circuit configuration table.
--

  eltexIsisCircTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisCircEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "The table of circuits used by each instance of
                   Integrated IS-IS on this system."
      REFERENCE "{ISIS.aoi manualAreaAddresses (10)}"
  ::= { eltexIsisCirc 1 }

  eltexIsisCircEntry OBJECT-TYPE
      SYNTAX EltexIsisCircEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Each entry contains configuration of one IS-IS circuit"
      INDEX { eltexIsisSysInstance,
              eltexIsisCircIfindex }
  ::= { eltexIsisCircTable 1 }

  EltexIsisCircEntry ::=
      SEQUENCE {
          eltexIsisCircIfindex
              InterfaceIndex,
          eltexIsisCircRowStatus
              RowStatus,
          eltexIsisCircAdminState
              EltexIsisAdminState,
          eltexIsisCircOperState
              EltexIsisOperStatus,
          eltexIsisCircLevel
              INTEGER,
          eltexIsisCircPassiveCircuit
              TruthValue,
          eltexIsisCircPtToPt
              TruthValue,
          eltexIsisCircHelloPadding
              EltexIsisHelloPaddingAction,
          eltexIsisCircPDUBuffSize
              Unsigned32,
          eltexIsisCircBfdEnable
              TruthValue
          }

  eltexIsisCircIfindex OBJECT-TYPE
      SYNTAX InterfaceIndex
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION "The value of ifIndex for the interface to which this
                   circuit corresponds."
::= { eltexIsisCircEntry 1 }

  eltexIsisCircRowStatus OBJECT-TYPE
      SYNTAX RowStatus
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION "The state of the eltexIsisNetAddrEntry."
  ::= { eltexIsisCircEntry 2 }
  
  eltexIsisCircAdminState OBJECT-TYPE
      SYNTAX EltexIsisAdminState
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION "The administrative state of the circuit."
      DEFVAL { off }
    ::= { eltexIsisCircEntry 3 }
    
  eltexIsisCircOperState OBJECT-TYPE
        SYNTAX EltexIsisOperStatus
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION "The operational state of this circuit."
    ::= { eltexIsisCircEntry 4 }

  eltexIsisCircLevel OBJECT-TYPE
      SYNTAX INTEGER
          {
              reserved (0),
              level1(1),
              level2(2),
              level1L2(3)
          }
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION "Indicates which type of packets will be sent and
                   accepted on this circuit."
      DEFVAL { level1L2 }
  ::= { eltexIsisCircEntry 5 }

  eltexIsisCircPassiveCircuit OBJECT-TYPE
      SYNTAX TruthValue
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION
          "Specify if normal transmission and interpretation of IS-IS
           PDUs are suppressed on this circuit. If set to 'true', 
           the interface is included in LSPs but can't set up 
           adjacency with any neighbor router."
      DEFVAL { false }
  ::= { eltexIsisCircEntry 6 }

  eltexIsisCircPtToPt OBJECT-TYPE
      SYNTAX TruthValue
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
          "Specify interface type like point to point.

           This field can only be changed if the eltexIsisCircAdminState
           field is set to off."
      DEFVAL { false }
  ::= { eltexIsisCircEntry 7 }

  eltexIsisCircHelloPadding OBJECT-TYPE
      SYNTAX EltexIsisHelloPaddingAction
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
          "What to do with padding in hello packets?"
       DEFVAL { enabled }
  ::= { eltexIsisCircEntry 8 }

  eltexIsisCircPDUBuffSize OBJECT-TYPE
      SYNTAX      Unsigned32 (512..9000)
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "Maximum size of PDU that can be sent or received over this
           circuit.

           This field can only be changed if the eltexIsisCircAdminState
           field is set to off."
      DEFVAL { 1500 }
  ::= { eltexIsisCircEntry 9 }

eltexIsisCircBfdEnable OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "Indicates whether Bidirectional Forwarding Detection (BFD)
           is desired on this circuit."
      DEFVAL { false }
  ::= { eltexIsisCircEntry 10 }

--
-- Circuit Level Table.
-- This table captures level-specific information about a circuit
--

  eltexIsisCircLevelTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisCircLevelEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
            "Level specific information about circuits used by IS-IS."
  ::= { eltexIsisCirc 2 }

  eltexIsisCircLevelEntry OBJECT-TYPE
      SYNTAX EltexIsisCircLevelEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Each entry contains configuration of one IS-IS circuit"
      INDEX { eltexIsisSysInstance,
              eltexIsisCircIfindex,
              eltexIsisCircLevelIndex }
  ::= { eltexIsisCircLevelTable 1 }

  EltexIsisCircLevelEntry ::=
      SEQUENCE {
          eltexIsisCircLevelIndex
              INTEGER,
          eltexIsisCircLevelRowStatus
              RowStatus,
          eltexIsisCircLevelMetric
              EltexIsisWideMetric,
          eltexIsisCircLevelAuthType
              EltexIsisAuthType,
          eltexIsisCircLevelAuthKey
              OCTET STRING,
          eltexIsisCircLevelAuthKeyChain
              OCTET STRING
          }

  eltexIsisCircLevelIndex OBJECT-TYPE
      SYNTAX INTEGER
          {
              level1IS (1),
              level2IS (2)
          }
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The level that this entry describes."
  ::= { eltexIsisCircLevelEntry 1 }

  eltexIsisCircLevelRowStatus OBJECT-TYPE
      SYNTAX RowStatus
      MAX-ACCESS read-create
      STATUS current
      DESCRIPTION "The state of the eltexIsisCircLevelEntry."
  ::= { eltexIsisCircLevelEntry 2 }

  eltexIsisCircLevelMetric OBJECT-TYPE
      SYNTAX EltexIsisWideMetric
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
          "The metric value of this circuit for this level.

           This metric should not be configured with a zero value
           unless the circuit is a passive circuit.  If a non-passive
           circuit is configured with a zero metric, it is treated as
           having metric 1 for LSP generation and SPF calculation
           purposes."
      DEFVAL { 10 }
  ::= { eltexIsisCircLevelEntry 3 }

  eltexIsisCircLevelAuthType OBJECT-TYPE
      SYNTAX EltexIsisAuthType
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
           "Authentication type for circuit level authentication."
  ::= { eltexIsisCircLevelEntry 4 }

  eltexIsisCircLevelAuthKey OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (0..20))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
           "Authentication key for circuit level authentication.
            If the field eltexIsisCircLevelAuthKeyChain is set
            and key chain with this name is present in the
            configuration, then this field is ignored."
  ::= { eltexIsisCircLevelEntry 5 }

  eltexIsisCircLevelAuthKeyChain OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (0..32))
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
           "Name of key chain for circuit level authentication."
  ::= { eltexIsisCircLevelEntry 6 }

--
-- Circuit Level Status Table.
-- This table captures the operational values of
-- level-specific circuit.
--

  eltexIsisCircLevelStatusTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisCircLevelStatusEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
            "The operational values of level-specific circuit."
  ::= { eltexIsisCirc 4 }

  eltexIsisCircLevelStatusEntry OBJECT-TYPE
      SYNTAX EltexIsisCircLevelStatusEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Each entry contains operational values of one
                   IS-IS circuit."
      INDEX { eltexIsisSysInstance,
              eltexIsisCircIfindex,
              eltexIsisCircLevelIndex }
  ::= { eltexIsisCircLevelStatusTable 1 }

  EltexIsisCircLevelStatusEntry ::=
      SEQUENCE {
          eltexIsisCircLevelStatusMetric
              Unsigned32
          }

  eltexIsisCircLevelStatusMetric OBJECT-TYPE
      SYNTAX Unsigned32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The metric value of this circuit for this level."
  ::= { eltexIsisCircLevelStatusEntry 1 }


  eltexIsisISAdj     OBJECT IDENTIFIER ::= { eltexIsisObjects 3 }

-- The IS Adjacency Table
--
-- Each adjacency to an IS corresponds to one entry in this
-- table.

  eltexIsisISAdjTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisISAdjEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "The table of adjacencies to Intermediate Systems."
  ::= { eltexIsisISAdj 1 }

  eltexIsisISAdjEntry OBJECT-TYPE
      SYNTAX EltexIsisISAdjEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Each entry corresponds to one adjacency to an
                   Intermediate System on this system."
      INDEX { eltexIsisSysInstance,
              eltexIsisCircIfindex,
              eltexIsisISAdjIndex }
  ::= { eltexIsisISAdjTable 1 }

  EltexIsisISAdjEntry ::=
      SEQUENCE {
          eltexIsisISAdjIndex
              Integer32,
          eltexIsisISAdjState
              INTEGER,
          eltexIsisISAdj3WayState
              INTEGER,
          eltexIsisISAdjNeighSNPAAddress
              EltexNETAddress,
          eltexIsisISAdjNeighSysType
              INTEGER,
          eltexIsisISAdjNeighSysID
              EltexIsisSystemID,
          eltexIsisISAdjNbrExtendedCircID
              Unsigned32,
          eltexIsisISAdjUsage
              INTEGER,
          eltexIsisISAdjHoldTimer
              Unsigned32,
          eltexIsisISAdjNeighPriority
              EltexIsisISPriority,
          eltexIsisISAdjLastUpTime
              TimeTicks,
          eltexIsisISAdjRestartCapable
              TruthValue,
          eltexIsisISAdjPeerRestartState
              INTEGER,
          eltexIsisISAdjSuppressed
              TruthValue,
          eltexIsisISAdjNeighLanID
              OCTET STRING,
          eltexIsisISAdjNeighHostname
              SnmpAdminString,
          eltexIsisISAdjNeighLanIDHostname
              SnmpAdminString
    }

  eltexIsisISAdjIndex OBJECT-TYPE
      SYNTAX Integer32 (1..2000000000)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "A unique value identifying the IS adjacency from all
                   other such adjacencies on this circuit. This value is
                   automatically assigned by the system when the adjacency
                   is created."
  ::= { eltexIsisISAdjEntry 1 }

  eltexIsisISAdjState OBJECT-TYPE
      SYNTAX INTEGER
          {
               down (1),
               initializing (2),
               up (3),
               failed(4)
          }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The state of the adjacency."
      REFERENCE "{ISIS.aoi adjacencyState (78)}"
  ::= { eltexIsisISAdjEntry 2 }

  eltexIsisISAdj3WayState OBJECT-TYPE
      SYNTAX INTEGER
          {
               up (0),
               initializing (1),
               down (2),
               failed (3)
          }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The 3Way state of the adjacency.  These are picked
                   to match the historical on-the-wire representation
                   of the 3Way state, and are not intended to match
                   eltexIsisISAdjState."
      REFERENCE "{ RFC 3373 }"
  ::= { eltexIsisISAdjEntry 3 }

  eltexIsisISAdjNeighSNPAAddress OBJECT-TYPE
      SYNTAX EltexNETAddress
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The SNPA address of the neighboring system."
      REFERENCE "{ISIS.aoi neighbourSNPAAddress (79)}"
  ::= { eltexIsisISAdjEntry 4 }

  eltexIsisISAdjNeighSysType OBJECT-TYPE
      SYNTAX INTEGER
          {
              l1IntermediateSystem(1),
              l2IntermediateSystem(2),
              l1L2IntermediateSystem(3),
              unknown(4)
          }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The type of the neighboring system."
      REFERENCE "{ISIS.aoi neighbourSystemType (80)}"
  ::= { eltexIsisISAdjEntry 5 }

  eltexIsisISAdjNeighSysID OBJECT-TYPE
      SYNTAX EltexIsisSystemID
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The system ID of the neighboring Intermediate
                   System."
      REFERENCE "{ISIS.aoi neighbourSystemIds (83)}"
  ::= { eltexIsisISAdjEntry 6 }

  eltexIsisISAdjNbrExtendedCircID OBJECT-TYPE
      SYNTAX Unsigned32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The 4 byte Extended Circuit ID learned from the
                   Neighbor during 3-way handshake, or 0."
  ::= { eltexIsisISAdjEntry 7 }


  eltexIsisISAdjUsage OBJECT-TYPE
      SYNTAX INTEGER
          {
              reserved (0),
              level1(1),
              level2(2),
              level1and2(3)
          }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "How is the adjacency used?  On a point-to-point link,
                   this might be level1and2, but on a LAN, the usage will
                   be level1 on the adjacency between peers at L1,
                   and level2 for the adjacency between peers at L2."
      REFERENCE "{ISIS.aoi adjacencyUsage (82)}"
  ::= { eltexIsisISAdjEntry 8 }

  eltexIsisISAdjHoldTimer OBJECT-TYPE
      SYNTAX Unsigned32 (1..65535)
      UNITS "seconds"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The holding time in seconds for this adjacency.
                   This value is based on received IIH PDUs and
                   the elapsed time since receipt."
      REFERENCE "{ISIS.aoi holdingTimer (85)}"
  ::= { eltexIsisISAdjEntry 9 }

  eltexIsisISAdjNeighPriority OBJECT-TYPE
      SYNTAX EltexIsisISPriority
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "Priority of the neighboring Intermediate System for
                   becoming the Designated Intermediate System."
      REFERENCE "{ISIS.aoi lANPriority (86)}"
  ::= { eltexIsisISAdjEntry 10 }

  eltexIsisISAdjLastUpTime OBJECT-TYPE
      SYNTAX TimeTicks
      UNITS "seconds"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "If the eltexIsisISAdjState is in state 'up', the value
                   of sysUpTime when the adjacency most recently
                   entered the state 'up',  or 0 if it has never
                   been in state 'up'."
  ::= { eltexIsisISAdjEntry 11 }

  eltexIsisISAdjRestartCapable OBJECT-TYPE
      SYNTAX TruthValue
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "Does the neighbor support restart signalling?

                   This object is set to 'true' if the peer includes the
                   restart TLV in IIH PDUs."
  ::= { eltexIsisISAdjEntry 12 }

  eltexIsisISAdjPeerRestartState OBJECT-TYPE
      SYNTAX INTEGER
          {
              notRestarting(1),
              restartingNoHelp(2),
              helpingRestart(3)
          }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "Is the peer currently restarting?

                   Set to 'notRestarting' if the neighbor is not restarting
                   (is not including a restart TLV in the IIH, or is not setting the
                   RR bit).

                   Set to 'restartingNoHelp' if the neighbor is restarting
                   (is including a restart TLV with the RR bit in IIH PDUs), but
                   the local node is not helping the restart.

                   Set to 'helpingRestart' if the neighbor is restarting and the
                   local node is helping the restart."
  ::= { eltexIsisISAdjEntry 13 }

  eltexIsisISAdjSuppressed OBJECT-TYPE
      SYNTAX TruthValue
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "Has the peer requested that the adjacency be suppressed?
                   If set to 'true', the adjacency will not be added to the
                   local LSP.

                   This object is set to 'true' if the peer sets the SA bit in
                   the restart TLV in IIH PDUs."
  ::= { eltexIsisISAdjEntry 14 }

  eltexIsisISAdjNeighLanID OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE(0..7))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "On a broaeltexast circuit, the LAN ID reported by the
                   neighbor for the Designated Intermediate System on this
                   circuit at this level.  For a non-broadcast circuit, or if,
                   for any reason, the neighbor is not partaking in the
                   relevant Designated Intermediate System election process,
                   then the value returned is the zero length OCTET STRING."
  ::= { eltexIsisISAdjEntry 15 }

  eltexIsisISAdjNeighHostname OBJECT-TYPE
      SYNTAX SnmpAdminString
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The hostname corresponding to eltexIsisISAdjNeighSysID.
                   This is the null string if no hostname is known."
  ::= { eltexIsisISAdjEntry 16 }

  eltexIsisISAdjNeighLanIDHostname OBJECT-TYPE
      SYNTAX SnmpAdminString
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The hostname corresponding to the system ID part of the
                   eltexIsisISAdjNeighLanID object.
                   This is the null string if no hostname is known."
  ::= { eltexIsisISAdjEntry 17 }


-- The IS Adjacency Area Address Table

-- The IS Adjacency Area Address Table contains the set of
-- Area Addresses of neighboring
-- Intermediate Systems as reported in IIH PDUs.

  eltexIsisISAdjAreaAddrTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisISAdjAreaAddrEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "This table contains the set of Area Addresses of
                   neighboring Intermediate Systems as reported in received
                   IIH PDUs."
      REFERENCE "{ISIS.aoi areaAddressesOfNeighbour (84)}"
  ::= { eltexIsisISAdj 2 }

  eltexIsisISAdjAreaAddrEntry OBJECT-TYPE
      SYNTAX EltexIsisISAdjAreaAddrEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Each entry contains one Area Address reported by a
                   neighboring Intermediate System in its IIH PDUs."
      INDEX { eltexIsisSysInstance,
              eltexIsisCircIfindex,
              eltexIsisISAdjIndex,
              eltexIsisISAdjAreaAddrIndex }
  ::= { eltexIsisISAdjAreaAddrTable 1 }

  EltexIsisISAdjAreaAddrEntry ::=
      SEQUENCE {
          eltexIsisISAdjAreaAddrIndex
              Integer32,
          eltexIsisISAdjAreaAddress
              EltexNETAddress
          }

  eltexIsisISAdjAreaAddrIndex OBJECT-TYPE
      SYNTAX Integer32 (1..2000000000)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "An index for the areas associated with one neighbor.
                   This provides a simple way to walk the table."
  ::= { eltexIsisISAdjAreaAddrEntry 1 }

  eltexIsisISAdjAreaAddress OBJECT-TYPE
      SYNTAX EltexNETAddress
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "One Area Address as reported in IIH PDUs received from
                   the neighbor."
  ::= { eltexIsisISAdjAreaAddrEntry 2 }

-- The IS Adjacency IP Address Table

-- The IS Adjacency IP Address Table contains the
-- set of IP Addresses of neighboring Intermediate Systems
-- as reported in received IIH PDUs.

  eltexIsisISAdjIPAddrTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisISAdjIPAddrEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "This table contains the set of IP Addresses of
                   neighboring Intermediate Systems as reported in received
                   IIH PDUs."
  ::= { eltexIsisISAdj 3 }

  eltexIsisISAdjIPAddrEntry OBJECT-TYPE
      SYNTAX EltexIsisISAdjIPAddrEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Each entry contains one IP Address reported by a
                   neighboring Intermediate System in its IIH PDUs."
      INDEX { eltexIsisSysInstance,
              eltexIsisCircIfindex,
              eltexIsisISAdjIndex,
              eltexIsisISAdjIPAddrIndex
              }
  ::= { eltexIsisISAdjIPAddrTable 1 }

  EltexIsisISAdjIPAddrEntry ::=
      SEQUENCE {
          eltexIsisISAdjIPAddrIndex
              Integer32,
          eltexIsisISAdjIPAddrType
               InetAddressType,
          eltexIsisISAdjIPAddrAddress
              InetAddress
      }

  eltexIsisISAdjIPAddrIndex OBJECT-TYPE
      SYNTAX Integer32 (1..2000000000)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "An index to this table which identifies the IP addresss
                   to which this entry belongs."
  ::= { eltexIsisISAdjIPAddrEntry 1 }

  eltexIsisISAdjIPAddrType OBJECT-TYPE
      SYNTAX InetAddressType
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The type of one IP Address as reported in IIH PDUs
                   received from the neighbor."
  ::= { eltexIsisISAdjIPAddrEntry 2 }

  eltexIsisISAdjIPAddrAddress OBJECT-TYPE
      SYNTAX InetAddress (SIZE(4|16))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "One IP Address as reported in IIH PDUs received from the
                   neighbor."
  ::= { eltexIsisISAdjIPAddrEntry 3 }

eltexIsisLSPDataBase     OBJECT IDENTIFIER ::= { eltexIsisObjects 5 }

-- The LSP Database Table
--
-- The table provides Summary Information about LSPs

  eltexIsisLSPSummaryTable OBJECT-TYPE
      SYNTAX SEQUENCE OF EltexIsisLSPSummaryEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "The table of LSP Headers."
  ::= { eltexIsisLSPDataBase 1 }

  eltexIsisLSPSummaryEntry OBJECT-TYPE
      SYNTAX EltexIsisLSPSummaryEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "Each entry provides a summary describing an
                   LSP currently stored in the system."
      INDEX {  eltexIsisSysInstance,
               eltexIsisLSPLevel,
               eltexIsisLSPID }
  ::= { eltexIsisLSPSummaryTable 1 }

  EltexIsisLSPSummaryEntry ::=
      SEQUENCE {
          eltexIsisLSPLevel
              EltexIsisISLevel,
          eltexIsisLSPID
              EltexIsisLinkStatePDUID,
          eltexIsisLSPSeq
              Unsigned32,
          eltexIsisLSPZeroLife
              TruthValue,
          eltexIsisLSPChecksum
              Unsigned32,
          eltexIsisLSPLifetimeRemain
              Unsigned32,
          eltexIsisLSPPDULength
              Unsigned32,
          eltexIsisLSPAttributes
              Unsigned32,
          eltexIsisLSPIDHostname
              SnmpAdminString
      }

  eltexIsisLSPLevel OBJECT-TYPE
      SYNTAX EltexIsisISLevel
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "At which level does this LSP appear?"
  ::= { eltexIsisLSPSummaryEntry 1 }

  eltexIsisLSPID OBJECT-TYPE
      SYNTAX EltexIsisLinkStatePDUID
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION "The 8 byte LSP ID, consisting of the SystemID,
                   Circuit ID, and Fragment Number."
  ::= { eltexIsisLSPSummaryEntry 2 }

  eltexIsisLSPSeq OBJECT-TYPE
      SYNTAX Unsigned32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The sequence number for this LSP."
  ::= { eltexIsisLSPSummaryEntry 3 }

  eltexIsisLSPZeroLife OBJECT-TYPE
      SYNTAX TruthValue
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "Is this LSP being purged by this System?"
  ::= { eltexIsisLSPSummaryEntry 4 }

  eltexIsisLSPChecksum OBJECT-TYPE
      SYNTAX Unsigned32 (0..65535)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The 16 bit Fletcher Checksum."
  ::= { eltexIsisLSPSummaryEntry 5 }

  eltexIsisLSPLifetimeRemain OBJECT-TYPE
      SYNTAX Unsigned32 (0..65535)
      UNITS "seconds"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The remaining lifetime in seconds for this LSP.

                   For a current LSP (eltexIsisLSPZeroLife is 'false'), this
                   indicates the time remaining before the LSP will expire.
                   For an LSP being purged from the system (eltexIsisLSPZeroLife
                   is 'true'), the LSP remains in the database for
                   ZeroAgeLifetime, and this will indicate the time remaining
                   before final deletion of the LSP."
  ::= { eltexIsisLSPSummaryEntry 6 }

  eltexIsisLSPPDULength OBJECT-TYPE
      SYNTAX Unsigned32 (0..65535)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The length of this LSP."
  ::= { eltexIsisLSPSummaryEntry 7 }

  eltexIsisLSPAttributes OBJECT-TYPE
      SYNTAX Unsigned32 (0..255)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "Flags carried by the LSP."
  ::= { eltexIsisLSPSummaryEntry 8 }

  eltexIsisLSPIDHostname OBJECT-TYPE
      SYNTAX SnmpAdminString
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION "The hostname corresponding to the system ID part of the
                   eltexIsisLSPID object.

                   This is the null string if no hostname is known."
  ::= { eltexIsisLSPSummaryEntry 9 }

-- LSP Table
--
-- The full LSP as a sequence of {Type, Len, Value} tuples
-- Since the underlying LSP may have changed while downloading
-- TLVs, we provide the Sequence number and Checksum for each
-- LSP TLV, so the network manager may verify that they are
-- still working on the same version of the LSP.

    eltexIsisLSPTLVTable OBJECT-TYPE
     -- FAMILY-SHORT-NAME eltexIsis_lsp_tlv
        SYNTAX SEQUENCE OF EltexIsisLSPTLVEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The contents of each LSP."
    ::= { eltexIsisLSPDataBase 2 }

    eltexIsisLSPTLVEntry OBJECT-TYPE
        SYNTAX EltexIsisLSPTLVEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Each entry describes an LSP current stored in the
             system."
        INDEX {  eltexIsisSysInstance,
                 eltexIsisLSPLevel,
                 eltexIsisLSPID,
                 eltexIsisLSPTLVIndex }
    ::= { eltexIsisLSPTLVTable 1 }

    EltexIsisLSPTLVEntry ::=
        SEQUENCE {
            eltexIsisLSPTLVIndex
                Unsigned32,
            eltexIsisLSPTLVSeq
                Unsigned32,
            eltexIsisLSPTLVChecksum
                Unsigned32,
            eltexIsisLSPTLVType
                Unsigned32,
            eltexIsisLSPTLVLen
                Unsigned32,
            eltexIsisLSPTLVValue
                OCTET STRING,
            eltexIsisLSPTLVHostname
                SnmpAdminString
        }

    eltexIsisLSPTLVIndex OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The index of this TLV in the LSP.  The first TLV has index 1
             and the Nth TLV has an index of N."
    ::= { eltexIsisLSPTLVEntry 1 }

    eltexIsisLSPTLVSeq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The sequence number for this LSP."
    ::= { eltexIsisLSPTLVEntry 2 }

    eltexIsisLSPTLVChecksum OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The 16 bit Fletcher Checksum."
    ::= { eltexIsisLSPTLVEntry 3 }

    eltexIsisLSPTLVType OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The type of this TLV."
    ::= { eltexIsisLSPTLVEntry 4 }

    eltexIsisLSPTLVLen OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The length of this TLV."
    ::= { eltexIsisLSPTLVEntry 5 }

    eltexIsisLSPTLVValue OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE(0..255))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The value of this TLV."
    ::= { eltexIsisLSPTLVEntry 6 }

    eltexIsisLSPTLVHostname OBJECT-TYPE
        SYNTAX SnmpAdminString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
             "The hostname corresponding to the system ID part of the
              eltexIsisLSPID object.

              This is the null string if no hostname is known."
    ::= { eltexIsisLSPTLVEntry 7 }

END
