RADLAN-TCPSESSIONS DEFINITIONS ::= BEGIN

-- Title:      RADLAN UDP Private Extension
-- Version:    7.37.00.00
-- Date:       17 May 2004

IMPORTS
    Unsigned32, Integer32,
    MODULE-IDENTITY, OBJECT-TYPE, mib-2                     FROM SNMPv2-SMI
    DisplayString,
    TEXTUAL-CONVENTION                                      FROM SNMPv2-TC
    InetAddress,InetAddressType                             FROM INET-ADDRESS-MIB;

tcp      OBJECT IDENTIFIER ::= { mib-2 6 }

rlTcpSessionTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlTcpSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A table containing TCP sessions information."
    ::= { tcp 16 }


rlTcpSessionEntry OBJECT-TYPE
    SYNTAX      RlTcpSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            ""
    INDEX   { rlTcpSessionLocalAddrType,
              rlTcpSessionLocalAddress,
              rlTcpSessionLocalPort,
              rlTcpSessionRemAddrType,
              rlTcpSessionRemAddress,
              rlTcpSessionRemPort }
    ::= { rlTcpSessionTable 1 }

RlTcpSessionEntry ::= SEQUENCE {
        rlTcpSessionLocalAddrType  InetAddressType,
        rlTcpSessionLocalAddress   InetAddress,
        rlTcpSessionLocalPort      INTEGER,
        rlTcpSessionRemAddrType    InetAddressType,
        rlTcpSessionRemAddress     InetAddress,
        rlTcpSessionRemPort        INTEGER,
        rlTcpSessionState          INTEGER,
        rlTcpSessionAppName        DisplayString
    }

rlTcpSessionLocalAddrType  OBJECT-TYPE
    SYNTAX     InetAddressType
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The type of the rlTcpSessionLocalAddress address"
    ::= { rlTcpSessionEntry 1 }

rlTcpSessionLocalAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The local IP address for this TCP connection.  In the case
         of a connection in the listen state which is willing to
         accept connections for any IP interface associated with the
         node, the value 0.0.0.0 is used."
    ::= { rlTcpSessionEntry 2 }

rlTcpSessionLocalPort OBJECT-TYPE
    SYNTAX      INTEGER (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The local port number for this TCP connection."
    ::= { rlTcpSessionEntry 3 }

rlTcpSessionRemAddrType  OBJECT-TYPE
    SYNTAX     InetAddressType
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The type of the rlTcpSessionRemAddress address"
::= { rlTcpSessionEntry 4 }

rlTcpSessionRemAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The remote IP address for this TCP connection."
    ::= { rlTcpSessionEntry 5 }


rlTcpSessionRemPort OBJECT-TYPE
    SYNTAX      INTEGER (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The remote port number for this TCP connection."
    ::= { rlTcpSessionEntry 6 }

rlTcpSessionState OBJECT-TYPE
    SYNTAX      INTEGER {
                    closed(1),
                    listen(2),
                    synSent(3),
                    synReceived(4),
                    established(5),
                    finWait1(6),
                    finWait2(7),
                    closeWait(8),
                    lastAck(9),
                    closing(10),
                    timeWait(11),
                    deleteTCB(12)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The state of this TCP connection.

            The only value which may be set by a management station is
            deleteTCB(12).  Accordingly, it is appropriate for an agent
            to return a `badValue' response if a management station
            attempts to set this object to any other value.

            If a management station sets this object to the value
            deleteTCB(12), then this has the effect of deleting the TCB
            (as defined in RFC 793) of the corresponding connection on
            the managed node, resulting in immediate termination of the
            connection.

            As an implementation-specific option, a RST segment may be
            sent from the managed node to the other TCP endpoint (note
            however that RST segments are not sent reliably)."
    ::= { rlTcpSessionEntry 7 }

rlTcpSessionAppName OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(0..12))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The name of the application for this TCP connection."
    ::= {rlTcpSessionEntry 8}

END
