MARVELL-SCT-MIB DEFINITIONS ::= BEGIN

-- Title:      Marvell Switch Interfaces Private
-- Version:    7.50
-- Date:       16 Aug 2010

IMPORTS
    OBJECT-TYPE, Counter32                         FROM SNMPv2-SMI
    TruthValue                                      FROM SNMPv2-TC
    rnd                                             FROM RADLAN-MIB;

rlSctMib MODULE-IDENTITY
        LAST-UPDATED "201008161234Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
            "The private MIB module definition for SCT MIB."
        ::= { rnd 203 }

--rlSctCpuRateEnabled
rlSctCpuRateEnabled OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indication whether the counter CPU rate is enabled"
    ::= { rlSctMib 1 }

--rlSctCpuRate
rlSctCpuRate OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "the amount of packets per second the CPU is handling."
    ::= { rlSctMib 2 }

END

