RADLAN-TIMESYNCHRONIZATION-MIB DEFINITIONS ::= BEGIN

IMPORTS
    rnd                                         FROM RADLAN-MIB
    Unsigned32, Integer32, IpAddress,
    MODULE-IDENTITY, OBJECT-TYPE                FROM SNMPv2-SMI
    InetAddressType, InetAddress                FROM INET-ADDRESS-MIB
    DisplayString, TEXTUAL-CONVENTION   ,
    RowStatus, TruthValue                       FROM SNMPv2-TC
    InterfaceIndex                              FROM IF-MIB;

rlTimeSynchronization MODULE-IDENTITY
      LAST-UPDATED "200408030024Z"
      ORGANIZATION "Marvell Semiconductor, Inc."
      CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
      DESCRIPTION
              "The MIB module describes the private MIB for SNTP & TIME definitions."
      REVISION     "200906180024Z"
      DESCRIPTION
              "Added support in DHCP timezone option."
      REVISION     "200709060024Z"
      DESCRIPTION
              "Added rlClockStatus"
      REVISION     "200311230024Z"
      DESCRIPTION
              "Initial revision"
      ::= { rnd 92 }

rlTimeSyncMethodMode OBJECT IDENTIFIER ::= { rlTimeSynchronization 1 }
rlSntpNtpClient  OBJECT IDENTIFIER ::= { rlTimeSynchronization 2 }

rlSntpNtpConfig  OBJECT IDENTIFIER ::= { rlSntpNtpClient 1 }
rlSntpConfig  OBJECT IDENTIFIER ::= { rlSntpNtpClient 2 }
rlNtpConfig  OBJECT IDENTIFIER ::= { rlSntpNtpClient 3 }

--
-- Textual Conventions
--

NTPTimeStamp ::= TEXTUAL-CONVENTION
        DISPLAY-HINT "4d.4d"
        STATUS       current
        DESCRIPTION  "NTP timestamps are represented as a 64-bit
                      unsigned fixed-point number, in seconds relative to
                      00:00 on 1 January 1900.  The integer part is in the
                      first 32 bits and the fraction part is in the last
                      32 bits."
        REFERENCE    "D.L. Mills, 'Network Time Protocol (Version 3)',
                      RFC-1305, March 1992, Section 3.1"
        SYNTAX       OCTET STRING (SIZE (8))

NTPSignedTimeValue ::= TEXTUAL-CONVENTION
        DISPLAY-HINT "2d.2d"
        STATUS       current
        DESCRIPTION  "The time in seconds that could represent signed
                      quantities like time delay with respect to some
                      source.  This textual-convention is specific to RADLAN
                      implementation of NTP where 32-bit integers are used
                      for such quantities.  The signed integer part is in
                      the first 16 bits and the fraction part is in the
                      last 16 bits."
        SYNTAX       OCTET STRING (SIZE (4))

NTPStratum ::= TEXTUAL-CONVENTION
        STATUS       current
        DESCRIPTION  "Indicates the stratum of the clock.  The stratum
                      defines the accuracy of a time server.  Higher the
                      stratum, lower the accuracy.
                      0, unspecified
                      1, primary reference (e.g., calibrated atomic clock,
                         radio clock)
                      2-255, secondary reference (via NTP)"
        REFERENCE    "D.L. Mills, 'Network Time Protocol (Version 3)',
                      RFC-1305, March 1992, Section 2.2"
        SYNTAX       Integer32 (0..255)

-- ----------------------------------------------------------------------
-- Global TimeSyncMethod
-- ----------------------------------------------------------------------

RlTimeSyncMethod  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "Method to be used for time synchronization in the device."
   SYNTAX INTEGER { none(1),
                    sntp(2),
                    ntp(3)
                  }

RlDaylightSavingTimeMode  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "Daylight Saving Time - Recurring/Date/None."
   SYNTAX INTEGER {
                    recurring(1),
                    date(2),
                    none(3)
                  }

rlTimeSyncMibVersion OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "TimeSync Mib Version."
        ::= { rlTimeSyncMethodMode 1 }

rndTimeSyncManagedTime  OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(6))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The time will be sent in the format hhmmss"
        ::= { rlTimeSyncMethodMode 2 }

rndTimeSyncManagedDate  OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(6))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The date will be sent in the format ddmmyy"
         ::= { rlTimeSyncMethodMode 3 }

rndTimeSyncManagedDateTime  OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(12))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The date and time will be sent in the format ddmmyyhhmmss"
        ::= { rlTimeSyncMethodMode 4 }

rlTimeSyncMethod OBJECT-TYPE
        SYNTAX      RlTimeSyncMethod
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Method to be used for time synchronization in the device."
        DEFVAL      { none }
        ::= { rlTimeSyncMethodMode 5 }

rlTimeZone OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(1..6))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Offset from Greenwich time (format [+/-]hh:mm)."
        ::=  {rlTimeSyncMethodMode 6 }

rlTimeZoneCode OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..16))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Code definition for current TimeZone."
        ::=  {rlTimeSyncMethodMode 7 }

rlDaylightSavingTimeMode OBJECT-TYPE
        SYNTAX      RlDaylightSavingTimeMode
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Daylight Saving Time - Recurring/Date/None."
        DEFVAL      { none }
        ::= { rlTimeSyncMethodMode 8 }

rlDaylightSavingTimeStart OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE(14))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Daylight Saving Time start date.
                 In recurring mode (format 1): week wday month hh:mm
                 In recurring mode (format 2): RJul n hh:mm
                 In date mode:      month day year hh:mm
                 week:  0-6  (0=First, 6=Last)
                 wday:  1-7  (Sunday-Saturday)
                 month: 1-12 (January-December)
                 day:   1-31
                 year:  0-99 (2000-2099)
                 hh:    0-23 (hours)
                 mm:    0-59 (minutes)
                 n:     0-365 (zero-based Julian day of the year. Leap days shall be
                               counted, and it is possible to refer to February 29).
                 Format 2 for recurring mode is used only in the dynamic entry and
                 should not be used in the static entry (with index 1)."
        ::= { rlTimeSyncMethodMode 9 }

rlDaylightSavingTimeEnd OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE(14))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Daylight Saving Time start date.
                 In recurring mode (format 1): week wday month hh:mm
                 In recurring mode (format 2): RJul n hh:mm
                 In date mode:      month day year hh:mm
                 week:  0-6  (0=First, 6=Last)
                 wday:  1-7  (Sunday-Saturday)
                 month: 1-12 (January-December)
                 day:   1-31
                 year:  0-99 (2000-2099)
                 hh:    0-23 (hours)
                 mm:    0-59 (minutes)
                 n:     0-365 (zero-based Julian day of the year. Leap days shall be
                               counted, and it is possible to refer to February 29).
                 Format 2 for recurring mode is used only in the dynamic entry and
                 should not be used in the static entry (with index 1)."
        ::= { rlTimeSyncMethodMode 10 }

rlDaylightSavingTimeOffset OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Daylight Saving Time - The number of minutes to add to
                     the clock during summer time."
        DEFVAL      { 60 }
        ::= { rlTimeSyncMethodMode 11 }

rlDaylightSavingTimeCode OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..16))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Code definition for current Daylight Saving Time."
        ::=  {rlTimeSyncMethodMode 12 }

rlTZDSTOffset OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Local Time Zone and Daylight Saving Time offset
                     in seconds."
        ::= { rlTimeSyncMethodMode 13 }

rlTimeZoneName OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..16))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Human readable string describing Local Time Zone and Daylight Saving Time."
        ::=  {rlTimeSyncMethodMode 14 }



--
-- TimeZone table
--

-- TimeZone table aimed to replace next mibs:
--    rlTimeSyncMethod
--    rlTimeZone
--    rlTimeZoneCode
--    rlDaylightSavingTimeMode
--    rlDaylightSavingTimeStart
--    rlDaylightSavingTimeEnd
--    rlDaylightSavingTimeOffset
--    rlDaylightSavingTimeCode
--    rlTZDSTOffset
--    rlTimeZoneName
-- Table consist of one entry (with index = 1) and each field corresponding
-- to one of this MIB scalars, holding Timezone and Summertime static information.
-- In case DHCP timezone option is supported, the table will contain another row,
-- with index = 2, that will contain dynamic values for Timezone and Summertime
-- received through DHCP.

rlTimeZoneTable  OBJECT-TYPE
  SYNTAX  SEQUENCE OF RlTimeZoneEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION   "TimeZone information."
  ::= { rlTimeSyncMethodMode 15 }

rlTimeZoneEntry OBJECT-TYPE
   SYNTAX      RlTimeZoneEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION        "The row definition for this table."
   INDEX { rlTimeZoneIndex }
::= { rlTimeZoneTable 1 }

RlTimeZoneEntry ::= SEQUENCE {
    rlTimeZoneIndex                     INTEGER,
    rlTimeZoneTimeSyncMethod            RlTimeSyncMethod,
    rlTimeZoneTimeZoneOffset            DisplayString (SIZE(1..6)),
    rlTimeZoneTimeZoneCode              DisplayString (SIZE(0..16)),
    rlTimeZoneDaylightSavingTimeMode    RlDaylightSavingTimeMode,
    rlTimeZoneDaylightSavingTimeStart   OCTET STRING (SIZE(14)),
    rlTimeZoneDaylightSavingTimeEnd     OCTET STRING (SIZE(14)),
    rlTimeZoneDaylightSavingTimeOffset  Integer32,
    rlTimeZoneDaylightSavingTimeCode    DisplayString (SIZE(0..16)),
    rlTimeZoneTZDSTOffset               INTEGER,
    rlTimeZoneTimeZoneName              DisplayString (SIZE(0..16)),
    rlTimeZoneDataType                  INTEGER,
    rlTimeZoneDataSourceIfIndex         INTEGER,
    rlTimeZoneDataDynamicConfSource     INTEGER
}

rlTimeZoneIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..2)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Entry index. A row with index 2 will be existing in case the DHCP
                 timezone is supported, and will contain Timezone and Summertime dynamic
                 values.
                 Using index 2 in SET operations is allowed only for SNMP
                 inner clients (SNMPServ users), on condition that DHCP timezone option
                 is supported."
    ::= { rlTimeZoneEntry 1 }

rlTimeZoneTimeSyncMethod OBJECT-TYPE
    SYNTAX      RlTimeSyncMethod
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Method to be used for time synchronization in the device."
    DEFVAL      { none }
    ::= { rlTimeZoneEntry 2 }

rlTimeZoneTimeZoneOffset OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..6))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Offset from Greenwich time (format [+/-]hh:mm)."
    ::= { rlTimeZoneEntry 3 }

rlTimeZoneTimeZoneCode OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..16))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Code definition for current TimeZone."
   ::= { rlTimeZoneEntry 4 }

rlTimeZoneDaylightSavingTimeMode OBJECT-TYPE
    SYNTAX      RlDaylightSavingTimeMode
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Daylight Saving Time - Recurring/Date/None."
    DEFVAL      { none }
   ::= { rlTimeZoneEntry 5 }

rlTimeZoneDaylightSavingTimeStart OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(14))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Daylight Saving Time start date.
                 In recurring mode (format 1): week wday month hh:mm
                 In recurring mode (format 2): RJul n hh:mm
                 In date mode:      month day year hh:mm
                 week:  0-6  (0=First, 6=Last)
                 wday:  1-7  (Sunday-Saturday)
                 month: 1-12 (January-December)
                 day:   1-31
                 year:  0-99 (2000-2099)
                 hh:    0-23 (hours)
                 mm:    0-59 (minutes)
                 n:     0-365 (zero-based Julian day of the year. Leap days shall be
                               counted, and it is possible to refer to February 29).
                 Format 2 for recurring mode is used only in the dynamic entry and
                 should not be used in the static entry (with index 1)."
   ::= { rlTimeZoneEntry 6 }

rlTimeZoneDaylightSavingTimeEnd OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(14))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Daylight Saving Time start date.
                 In recurring mode (format 1): week wday month hh:mm
                 In recurring mode (format 2): RJul n hh:mm
                 In date mode:      month day year hh:mm
                 week:  0-6  (0=First, 6=Last)
                 wday:  1-7  (Sunday-Saturday)
                 month: 1-12 (January-December)
                 day:   1-31
                 year:  0-99 (2000-2099)
                 hh:    0-23 (hours)
                 mm:    0-59 (minutes)
                 n:     0-365 (zero-based Julian day of the year. Leap days shall be
                               counted, and it is possible to refer to February 29).
                 Format 2 for recurring mode is used only in the dynamic entry and
                 should not be used in the static entry (with index 1)."
   ::= { rlTimeZoneEntry 7 }

rlTimeZoneDaylightSavingTimeOffset OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Daylight Saving Time - The number of minutes to add to
                 the clock during summer time."
    DEFVAL      { 60 }
    ::= { rlTimeZoneEntry 8 }

rlTimeZoneDaylightSavingTimeCode OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..16))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Code definition for current Daylight Saving Time."
   ::= { rlTimeZoneEntry 9 }

rlTimeZoneTZDSTOffset OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Local Time Zone and Daylight Saving Time offset in seconds."
   ::= { rlTimeZoneEntry 10 }

rlTimeZoneTimeZoneName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..16))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Human readable string describing Local Time Zone and Daylight Saving Time."
    ::= { rlTimeZoneEntry 11 }

rlTimeZoneDataType OBJECT-TYPE
    SYNTAX      INTEGER {
                    static(1),
                    dynamic(2)
                    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The type of data in this entry: static or dynamic."
    DEFVAL      { static }
        ::= { rlTimeZoneEntry 12 }

rlTimeZoneDataSourceIfIndex OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "IfIndex of the interface through which the dynamic data of this row has been learned.
                     The value of this field will be 0 if rlTimeZoneTimeDataType is static (since it is
                     relevant only for dynamic entry), and this is the only value allowed for SET in this case."
        DEFVAL      { 0 }
        ::= { rlTimeZoneEntry 13 }

rlTimeZoneDataDynamicConfSource OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(1),
                    dhcpv4(2),
                    dhcpv6(3)
                    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The source of dynamic data in this entry, for example: dhcpv4.
                 Values other than 'none' are relevant only for dynamic entry."
    DEFVAL      { none }
        ::= { rlTimeZoneEntry 14 }


rlClockStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                       invalid(1),
                       manuallySet(2),
                       synchronizedBySntp(3),
                       synchronizedByNtp(101)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Current status of the clock. The value 'invalid' means time is meaninglesss,
                     since it has neither been manually configured nor achieved as a result
                     of SNTP or NTP synchronization."
        ::=  {rlTimeSyncMethodMode 16 }

rlDhcpTimezoneOptionEnabled OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Specifies whether the DHCP Timezone option (DHCPv4 option 100) is supported in the system.
                     Setting this value to FALSE, will clear Timezone and Summertime dynamic configuration,
                     so that:
                     1) rlTimeZoneTimeZoneCode and rlTimeZoneDaylightSavingTimeCode length will
                        be 0 for rlTimeZoneEntry whose index = 2 (dynamic entry).
                     2) the operative values of Timezone and Summertime will be those
                        statically configured. Thus, GET operations on the following
                        MIB scalars will result is static values:
                        rlTimeZone, rlTimeZoneCode, rlDaylightSavingTimeMode,
                        rlDaylightSavingTimeStart, rlDaylightSavingTimeEnd, rlDaylightSavingTimeOffset,
                        rlDaylightSavingTimeCode, rlTZDSTOffset."
        ::=  {rlTimeSyncMethodMode 17 }

rlAutomaticClockSetFromPCEnabled OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Specifies whether automatic set of time and date is permitted from
                     connected host PC.
                     The feature is meant to be used in order to initialize the clock
                     after reboot (if SNTP is not in use), since the device does not have
                     a realtime clock."
        DEFVAL      { false }
        ::=  {rlTimeSyncMethodMode 18 }

rlTimeAndDateHaveBeenSet OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates whether the time and date have been set in the
                     device, manually or through SNTP synchronization.
                     If only time has been set, the value of this MIB will
                     be FALSE. If only date has been set, the value of this MIB
                     will be FALSE."
        ::=  {rlTimeSyncMethodMode 19 }



-- ----------------------------------------------------------------------
-- SNTP/NTP client configuration parameters
-- ----------------------------------------------------------------------

RlSntpNtpSyncType   ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION     "Method to be used for time synchronization in the device."
    SYNTAX          INTEGER {
                        none(1),
                        unicast(2),
                        anycast(3),
                        broadcast(4)
                    }

RlSntpNtpSyncEntryType  ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION     "Entry in rlSntpNtpConfigSrvTable."
    SYNTAX          INTEGER {
                        primaryPollSrv(1),
                        syncSrv(2)
                    }

rlSntpNtpMibVersion OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SntpNtp Mib Version."
        ::= { rlSntpNtpConfig 1 }

rlSntpNtpConfigMode OBJECT-TYPE
        SYNTAX      INTEGER {
                       none(1),
                       unicast(2),
                       anycast(3),
                       multicast(4),
                       unicastAnycast(5),
                       unicastMulticast(6),
                       anycastMulticast(7),
                       unicastAnycastMulticast(8)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Current configuration operational mode of SNTP/NTP client."
        DEFVAL      { none }
        ::= { rlSntpNtpConfig 2 }

rlSntpNtpConfigSysStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of the local clock. If the value is set
                     to 1, i.e., this is a primary reference, then the
                     Primary-Clock procedure described in Section 3.4.6,
                     in RFC-1305 is invoked."
        ::= { rlSntpNtpConfig 3 }

rlSntpNtpConfigPollInterval OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Period of time (in seconds) between succesive attempts to
                     perform an update via SNTP."
        DEFVAL      { 1024 }
        ::= { rlSntpNtpConfig 4 }

rlSntpNtpConfigPrimaryPollSrvAddr OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Ip Address of a trusted SNTP server for polling."
        ::= { rlSntpNtpConfig 5 }

rlSntpNtpConfigPrimaryPollSrvMrid OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The mrid of the primary server."
        ::= { rlSntpNtpConfig 6 }

rlSntpNtpConfigPrimaryPollSrvIfIndex OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The interface addressed of the primary server."
        ::= { rlSntpNtpConfig 7 }

rlSntpNtpConfigPrimaryPollSrvStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of the primary polling server."
        ::= { rlSntpNtpConfig 8 }

rlSntpNtpConfigSyncSrvAddr OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Ip Address of the synced server."
        ::= { rlSntpNtpConfig 9 }

rlSntpNtpConfigSyncSrvMrid OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The mrid of the synced server."
        ::= { rlSntpNtpConfig 10 }

rlSntpNtpConfigSyncSrvIfIndex OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The interface addressed of the synced server."
        ::= { rlSntpNtpConfig 11 }

rlSntpNtpConfigSyncSrvType OBJECT-TYPE
        SYNTAX      RlSntpNtpSyncType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Synced server type."
        DEFVAL      { none }
        ::= { rlSntpNtpConfig 12 }


rlSntpNtpConfigSyncSrvStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of the synced server."
        ::= { rlSntpNtpConfig 13 }

rlSntpNtpConfigRetryTimeout OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP/NTP requests Retry Interval."
        ::= { rlSntpNtpConfig 14 }

rlSntpNtpConfigRetryCnt OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP/NTP requests Retry Count."
        ::= { rlSntpNtpConfig 15 }

-- ----------------------------------------------------------------------
-- SNTP Config Servers
-- ----------------------------------------------------------------------

-- Will replace next MIBs:

--  rlSntpNtpConfigPrimaryPollSrvAddr
--  rlSntpNtpConfigPrimaryPollSrvMrid
--  rlSntpNtpConfigPrimaryPollSrvIfIndex
--  rlSntpNtpConfigPrimaryPollSrvStratum

--  rlSntpNtpConfigSyncSrvAddr
--  rlSntpNtpConfigSyncSrvMrid
--  rlSntpNtpConfigSyncSrvIfIndex
--  rlSntpNtpConfigSyncSrvType
--  rlSntpNtpConfigSyncSrvStratum

rlSntpNtpConfigSrvTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RlSntpNtpConfigSrvEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing information about config servers."
        ::= { rlSntpNtpConfig 16 }

rlSntpNtpConfigSrvEntry OBJECT-TYPE
        SYNTAX      RlSntpNtpConfigSrvEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Entry in rlSntpNtpConfigSrvTable."
        INDEX       { rlSntpNtpConfigSrvEntryType }
        ::= { rlSntpNtpConfigSrvTable 1 }

RlSntpNtpConfigSrvEntry ::=
        SEQUENCE {
            rlSntpNtpConfigSrvEntryType         RlSntpNtpSyncEntryType,
            rlSntpNtpConfigSrvInetAddressType   InetAddressType,
            rlSntpNtpConfigSrvInetAddress       InetAddress,
            rlSntpNtpConfigSrvMrid              INTEGER,
            rlSntpNtpConfigSrvIfIndex           INTEGER,
            rlSntpNtpConfigSrvSyncType          RlSntpNtpSyncType,
            rlSntpNtpConfigSrvStratum           NTPStratum
        }

rlSntpNtpConfigSrvEntryType OBJECT-TYPE
        SYNTAX      RlSntpNtpSyncEntryType
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Server type: Synchronize Server or Primary Poll Server."
        ::= { rlSntpNtpConfigSrvEntry 1 }

rlSntpNtpConfigSrvInetAddressType OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Server inet address type."
        ::= { rlSntpNtpConfigSrvEntry 2 }

rlSntpNtpConfigSrvInetAddress OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Server inet address."
        ::= { rlSntpNtpConfigSrvEntry 3 }

rlSntpNtpConfigSrvMrid OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The mrid of the server."
        ::= { rlSntpNtpConfigSrvEntry 4 }

rlSntpNtpConfigSrvIfIndex OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The interface addressed of the server."
        ::= { rlSntpNtpConfigSrvEntry 5 }

rlSntpNtpConfigSrvSyncType OBJECT-TYPE
        SYNTAX      RlSntpNtpSyncType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The type of synchronization."
        ::= { rlSntpNtpConfigSrvEntry 6 }

rlSntpNtpConfigSrvStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of the synced server."
        ::= { rlSntpNtpConfigSrvEntry 7 }

-- ----------------------------------------------------------------------
-- SNTP client configuration parameters
-- ----------------------------------------------------------------------

rlSntpClientMode OBJECT-TYPE
        SYNTAX      INTEGER {
                       none(1),
                       active(2),
                       passive(3)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Current operational mode of SNTP client."
        DEFVAL      { none }
        ::= { rlSntpConfig 1 }

rlSntpUnicastAdminState OBJECT-TYPE
        SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP Unicast Administrative state - Enable/Disable SNTP.
                     In case of reinitializing polling or time
                     synchronization this MIB is modified. The MIB can
                     be enabled even thought it is already enabled."
        DEFVAL      { disabled }
        ::= { rlSntpConfig 2 }

rlSntpBroadcastAdminState OBJECT-TYPE
        SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2),
                       ipv4OnlyEnabled(3),
                       ipv6OnlyEnabled(4)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP Broadcast Administrative state - Enable/Disable SNTP.
                     In case of reinitializing polling or time
                     synchronization this MIB is modified. The MIB can
                     be enabled even thought it is already enabled."
        DEFVAL      { disabled }
        ::= { rlSntpConfig 3 }

rlSntpAnycastAdminState OBJECT-TYPE
        SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2),
                       ipv4OnlyEnabled(3),
                       ipv6OnlyEnabled(4)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP Anycast Administrative state - Enable/Disable SNTP.
                     In case of reinitializing polling or time
                     synchronization this MIB is modified. The MIB can
                     be enabled even thought it is already enabled."
        DEFVAL      { disabled }
        ::= { rlSntpConfig 4 }

rlSntpUnicastPollState OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP Unicast poll state - TRUE for polled."
        DEFVAL      { false }
        ::= { rlSntpConfig 5 }

rlSntpBroadcastPollState OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP Broadcast poll state - TRUE for polled."
        DEFVAL      { false }
        ::= { rlSntpConfig 6 }

rlSntpAnycastPollState OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP Anycast poll state - TRUE for polled."
        DEFVAL      { false }
        ::= { rlSntpConfig 7 }

rlSntpAuthenticationState OBJECT-TYPE
        SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP authentication state- Enable/Disable SNTP."
        DEFVAL      { disabled }
        ::= { rlSntpConfig 8 }

rlTimeValidFlag OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Is time valid."
        DEFVAL      { false }
        ::= { rlSntpConfig 9 }

-- ----------------------------------------------------------------------
-- Table for configuring Interfaces (Broadcast)
-- ----------------------------------------------------------------------

rlSntpConfigBroadcastTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RlSntpBroadcastEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing broadcast mode information per
                     interface."
        ::= { rlSntpConfig 10 }

rlSntpBroadcastEntry OBJECT-TYPE
        SYNTAX      RlSntpBroadcastEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Private paramters for interface:
                     sntp status, broadcast mode."
        INDEX       { rlSntpBroadcastIfIndex }
        ::= { rlSntpConfigBroadcastTable 1 }

RlSntpBroadcastEntry ::=
        SEQUENCE {
           rlSntpBroadcastIfIndex        INTEGER,
           rlSntpBroadcastIfAdminState   INTEGER,
           rlSntpBroadcastMode           INTEGER,
           rlSntpBroadcastPolled         TruthValue,
           rlSntpBroadcastAddress        IpAddress,
           rlSntpBroadcastStratum        NTPStratum,
           rlSntpBroadcastLastResp       NTPTimeStamp,
           rlSntpBroadcastStatus         INTEGER,
           rlSntpBroadcastOffset         NTPTimeStamp,
           rlSntpBroadcastDelay          NTPSignedTimeValue,
           rlSntpBroadcastRowStatus      RowStatus
        }

rlSntpBroadcastIfIndex OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The interface addressed by this entry."
        ::=  {rlSntpBroadcastEntry 1}

rlSntpBroadcastIfAdminState OBJECT-TYPE
        SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP interface Adminstrative state- Enable/Disable SNTP.
                     In case of reinitializing polling or time
                     synchronization this MIB is modified. The MIB can
                     be enabled even thought it is already enabled."
        DEFVAL      { disabled }
        ::= { rlSntpBroadcastEntry 2 }

rlSntpBroadcastMode OBJECT-TYPE
        SYNTAX      INTEGER {
                       none(1),
                       receive(2),
                       send(3),
                       receiveSend(4)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP/NTP Broadcast Mode.
                     none        - no broadcast SNTP packets are received or sent.
                     Receive     - host only receive SNTP packets that were sent
                                   to broadcast address (were not directed to
                                   the host). This is multicast mode in the RFC.
                     Send        - host only send SNTP packets and wait for replies
                                   directed to the host. This is anycast mode in
                                   the RFC.
                     ReceiveSend - host receive broadcast messages (destination
                                   is broadcast address in the received messages)
                                   and send SNTP packets to wait for replies
                                   directed to the host (destination address
                                   of the reply is the host address). This mode
                                   combines anycast and multicast modes in the
                                   RFC."
        DEFVAL      { receiveSend }
        ::= { rlSntpBroadcastEntry 3 }

rlSntpBroadcastPolled OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "TRUE if participating in polling cycle, else FALSE."
        DEFVAL { false }
        ::= {  rlSntpBroadcastEntry 4 }

rlSntpBroadcastAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Ip Address of a trusted SNTP server."
        ::= { rlSntpBroadcastEntry 5 }

rlSntpBroadcastStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of this server."
        ::= { rlSntpBroadcastEntry 6 }

rlSntpBroadcastLastResp OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Broadcast Last Response Time"
        ::= { rlSntpBroadcastEntry 7 }

rlSntpBroadcastStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                       unknown(1),
                       inProcess(2),
                       up(3),
                       down(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The Operational State of the remote IP Address of
                     the SNTP Broadcast.
                     unknown     - requests were not sent yet.
                     inProcess   - replies were not received yet.
                     up          - server sent SNTP packets.
                     down        - server stopped sending SNTP packets."
        DEFVAL      { unknown }
        ::= { rlSntpBroadcastEntry 8 }

rlSntpBroadcastOffset OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated offset of the server's clock relative to
                 the local clock, in seconds.  The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpBroadcastEntry 9 }

rlSntpBroadcastDelay OBJECT-TYPE
        SYNTAX      NTPSignedTimeValue
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated round-trip delay of the server's clock
                 relative to the local clock over the network path
                 between them, in seconds. The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpBroadcastEntry 10 }

rlSntpBroadcastRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The Status of this SNTP broadcast interface
                     information."
        ::= { rlSntpBroadcastEntry 11 }



-- ----------------------------------------------------------------------
-- Table for configuring Interfaces (Anycast)
-- ----------------------------------------------------------------------

rlSntpConfigAnycastTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RlSntpAnycastEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing anycast information per
                     interface."
        ::= { rlSntpConfig 11 }

rlSntpAnycastEntry OBJECT-TYPE
        SYNTAX      RlSntpAnycastEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Private paramters for interface:
                     server info."
        INDEX       { rlSntpAnycastIfIndex }
        ::= { rlSntpConfigAnycastTable 1 }

RlSntpAnycastEntry ::=
        SEQUENCE {
           rlSntpAnycastIfIndex          INTEGER,
           rlSntpAnycastAddress          IpAddress,
           rlSntpAnycastStratum          NTPStratum,
           rlSntpAnycastLastResp         NTPTimeStamp,
           rlSntpAnycastStatus           INTEGER,
           rlSntpAnycastOffset           NTPTimeStamp,
           rlSntpAnycastDelay            NTPSignedTimeValue,
           rlSntpAnycastRowStatus        RowStatus
        }

rlSntpAnycastIfIndex OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The interface addressed by this entry."
        ::=  {rlSntpAnycastEntry 1}

rlSntpAnycastAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Ip Address of a trusted SNTP server."
        ::= { rlSntpAnycastEntry 2 }

rlSntpAnycastStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of this server."
        ::= { rlSntpAnycastEntry 3 }

rlSntpAnycastLastResp OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Anycast Last Response Time"
        ::= { rlSntpAnycastEntry 4 }

rlSntpAnycastStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                       unknown(1),
                       inProcess(2),
                       up(3),
                       down(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The Operational State of the remote IP Address of
                     the SNTP Anycast.
                     unknown     - requests were not sent yet.
                     inProcess   - replies were not received yet.
                     up          - server sent SNTP packets.
                     down        - server stopped sending SNTP packets."
        DEFVAL      { unknown }
        ::= { rlSntpAnycastEntry 5 }

rlSntpAnycastOffset OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated offset of the server's clock relative to
                 the local clock, in seconds.  The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpAnycastEntry 6 }

rlSntpAnycastDelay OBJECT-TYPE
        SYNTAX      NTPSignedTimeValue
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated round-trip delay of the server's clock
                 relative to the local clock over the network path
                 between them, in seconds. The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpAnycastEntry 7 }

rlSntpAnycastRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The Status of this SNTP anycast interface
                     information."
        ::= { rlSntpAnycastEntry 8 }

-- ----------------------------------------------------------------------
-- Table for configuring Servers (Unicast)
-- ----------------------------------------------------------------------

rlSntpConfigServerTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RlSntpServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing trusted SNTP servers to be queried in
                     unicast or broadcast mode."
        ::= { rlSntpConfig 12 }

rlSntpServerEntry OBJECT-TYPE
        SYNTAX      RlSntpServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A trusted server."
        INDEX       { rlSntpServerAddress }
        ::= { rlSntpConfigServerTable 1 }

RlSntpServerEntry ::=
        SEQUENCE {
           rlSntpServerAddress           IpAddress,
           rlSntpServerPolled            TruthValue,
           rlSntpServerStratum           NTPStratum,
           rlSntpServerLastResp          NTPTimeStamp,
           rlSntpServerStatus            INTEGER,
           rlSntpServersOffset           NTPTimeStamp,
           rlSntpServersDelay            NTPSignedTimeValue,
           rlSntpServersKeyIdentifier    Unsigned32,
           rlSntpServerRowStatus         RowStatus
        }

rlSntpServerAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Ip Address of a trusted SNTP server."
        ::= { rlSntpServerEntry 1 }

rlSntpServerPolled OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "TRUE if participating in polling cycle, else FALSE."
        DEFVAL { false }
        ::= {  rlSntpServerEntry 2 }

rlSntpServerStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of this server."
        ::= { rlSntpServerEntry 3 }

rlSntpServerLastResp OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Server Last Response Time"
        ::= { rlSntpServerEntry 4 }

rlSntpServerStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                       unknown(1),
                       inProcess(2),
                       up(3),
                       down(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The Operational State of the remote IP Address of
                     the SNTP Server.
                     unknown     - requests were not sent yet.
                     inProcess   - replies were not received yet.
                     up          - server sent SNTP packets.
                     down        - server stopped sending SNTP packets."
        DEFVAL      { unknown }
        ::= { rlSntpServerEntry 5 }

rlSntpServersOffset OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated offset of the server's clock relative to
                 the local clock, in seconds.  The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpServerEntry 6 }

rlSntpServersDelay OBJECT-TYPE
        SYNTAX      NTPSignedTimeValue
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated round-trip delay of the server's clock
                 relative to the local clock over the network path
                 between them, in seconds. The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpServerEntry 7 }

rlSntpServersKeyIdentifier OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Authentication key identifier. The valid range is
                     1-4294967295.
                     Value zero, means no authentication is being done."
        ::= { rlSntpServerEntry 8 }

rlSntpServerRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The Status of this SNTP server information."
        ::= { rlSntpServerEntry 9 }

-- ----------------------------------------------------------------------
-- Table for configuring authentication keys
-- ----------------------------------------------------------------------

rlSntpConfigAuthenticationTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RlSntpAuthenticationEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table authentication keys."
        ::= { rlSntpConfig 13 }

rlSntpAuthenticationEntry OBJECT-TYPE
        SYNTAX      RlSntpAuthenticationEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Keys information for authenticationof NTP packets."
        INDEX       { rlSntpAuthenticationKeyID }
        ::= { rlSntpConfigAuthenticationTable 1 }

RlSntpAuthenticationEntry ::=
        SEQUENCE {
           rlSntpAuthenticationKeyID        Unsigned32 (1..4294967295),
           rlSntpAuthenticationKeyValue     DisplayString,
           rlSntpAuthenticationKeyState     INTEGER,
           rlSntpAuthenticationRowStatus    RowStatus
        }

rlSntpAuthenticationKeyID OBJECT-TYPE
        SYNTAX      Unsigned32 (1..4294967295)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The key identifier. Valid rabge for key identifier
                     is 1-4294967295."
        ::=  {rlSntpAuthenticationEntry 1}

rlSntpAuthenticationKeyValue OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(1..32))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Key value."
        ::= { rlSntpAuthenticationEntry 2 }

rlSntpAuthenticationKeyState OBJECT-TYPE
        SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Authentication key state - Enable/Disable key."
        DEFVAL      { disabled }
        ::= { rlSntpAuthenticationEntry 3 }

rlSntpAuthenticationRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The Status of this Authentication key information."
        ::= { rlSntpAuthenticationEntry 4 }

rlSntpPort OBJECT-TYPE
        SYNTAX      INTEGER (1.. 65535)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "User defined SNTP port."
        DEFVAL      { 123 }
        ::= { rlSntpConfig 14 }


-- ----------------------------------------------------------------------
-- IPv6 Support
-- ----------------------------------------------------------------------

-- ----------------------------------------------------------------------
-- IPv6: Table for configuring Interfaces (Broadcast)
-- ----------------------------------------------------------------------

rlSntpConfigBroadcastInetTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RlSntpBroadcastInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing broadcast mode information per
                     interface."
        ::= { rlSntpConfig 15 }

rlSntpBroadcastInetEntry OBJECT-TYPE
        SYNTAX      RlSntpBroadcastInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Private paramters for interface:
                     sntp status, broadcast mode."
        INDEX       { rlSntpBroadcastInetIfIndex }
        ::= { rlSntpConfigBroadcastInetTable 1 }

RlSntpBroadcastInetEntry ::=
        SEQUENCE {
           rlSntpBroadcastInetIfIndex       INTEGER,
           rlSntpBroadcastInetIfAdminState  INTEGER,
           rlSntpBroadcastInetMode          INTEGER,
           rlSntpBroadcastInetPolled        TruthValue,
           rlSntpBroadcastInetAddressType   InetAddressType,
           rlSntpBroadcastInetAddress       InetAddress,
           rlSntpBroadcastInetStratum       NTPStratum,
           rlSntpBroadcastInetLastResp      NTPTimeStamp,
           rlSntpBroadcastInetStatus        INTEGER,
           rlSntpBroadcastInetOffset        NTPTimeStamp,
           rlSntpBroadcastInetDelay         NTPSignedTimeValue,
           rlSntpBroadcastInetRowStatus     RowStatus,
           rlSntpBroadcastInetLastReq       NTPTimeStamp
        }

rlSntpBroadcastInetIfIndex OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The interface addressed by this entry."
        ::=  {rlSntpBroadcastInetEntry 1}

rlSntpBroadcastInetIfAdminState OBJECT-TYPE
        SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP interface Adminstrative state- Enable/Disable SNTP.
                     In case of reinitializing polling or time
                     synchronization this MIB is modified. The MIB can
                     be enabled even thought it is already enabled."
        DEFVAL      { disabled }
        ::= { rlSntpBroadcastInetEntry 2 }

rlSntpBroadcastInetMode OBJECT-TYPE
        SYNTAX      INTEGER {
                       none(1),
                       receive(2),
                       send(3),
                       receiveSend(4)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "SNTP/NTP Broadcast Mode.
                     none        - no broadcast SNTP packets are received or sent.
                     Receive     - host only receive SNTP packets that were sent
                                   to broadcast address (were not directed to
                                   the host). This is multicast mode in the RFC.
                     Send        - host only send SNTP packets and wait for replies
                                   directed to the host. This is anycast mode in
                                   the RFC.
                     ReceiveSend - host receive broadcast messages (destination
                                   is broadcast address in the received messages)
                                   and send SNTP packets to wait for replies
                                   directed to the host (destination address
                                   of the reply is the host address). This mode
                                   combines anycast and multicast modes in the
                                   RFC."
        DEFVAL      { receiveSend }
        ::= { rlSntpBroadcastInetEntry 3 }

rlSntpBroadcastInetPolled OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "TRUE if participating in polling cycle, else FALSE."
        DEFVAL { false }
        ::= {  rlSntpBroadcastInetEntry 4 }

rlSntpBroadcastInetAddressType OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Inet Address Type of a trusted SNTP server."
        ::= { rlSntpBroadcastInetEntry 5 }

rlSntpBroadcastInetAddress OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Inet Address of a trusted SNTP server."
        ::= { rlSntpBroadcastInetEntry 6 }

rlSntpBroadcastInetStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of this server."
        ::= { rlSntpBroadcastInetEntry 7 }

rlSntpBroadcastInetLastResp OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Broadcast Last Response Time"
        ::= { rlSntpBroadcastInetEntry 8 }

rlSntpBroadcastInetStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                       unknown(1),
                       inProcess(2),
                       up(3),
                       down(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The Operational State of the remote IP Address of
                     the SNTP Broadcast.
                     unknown     - requests were not sent yet.
                     inProcess   - replies were not received yet.
                     up          - server sent SNTP packets.
                     down        - server stopped sending SNTP packets."
        DEFVAL      { unknown }
        ::= { rlSntpBroadcastInetEntry 9 }

rlSntpBroadcastInetOffset OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated offset of the server's clock relative to
                 the local clock, in seconds.  The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpBroadcastInetEntry 10 }

rlSntpBroadcastInetDelay OBJECT-TYPE
        SYNTAX      NTPSignedTimeValue
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated round-trip delay of the server's clock
                 relative to the local clock over the network path
                 between them, in seconds. The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpBroadcastInetEntry 11 }

rlSntpBroadcastInetRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The Status of this SNTP broadcast interface
                     information."
        ::= { rlSntpBroadcastInetEntry 12 }

rlSntpBroadcastInetLastReq OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Broadcast Last Request Time"
        ::= { rlSntpBroadcastInetEntry 13 }

-- ----------------------------------------------------------------------
-- IPv6: Table for configuring Interfaces (Anycast)
-- ----------------------------------------------------------------------

rlSntpConfigAnycastInetTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RlSntpAnycastInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing anycast information per
                     interface."
        ::= { rlSntpConfig 16 }

rlSntpAnycastInetEntry OBJECT-TYPE
        SYNTAX      RlSntpAnycastInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Private paramters for interface:
                     server info."
        INDEX       { rlSntpAnycastInetIfIndex }
        ::= { rlSntpConfigAnycastInetTable 1 }

RlSntpAnycastInetEntry ::=
        SEQUENCE {
           rlSntpAnycastInetIfIndex          INTEGER,
           rlSntpAnycastInetAddressType      InetAddressType,
           rlSntpAnycastInetAddress          InetAddress,
           rlSntpAnycastInetStratum          NTPStratum,
           rlSntpAnycastInetLastResp         NTPTimeStamp,
           rlSntpAnycastInetStatus           INTEGER,
           rlSntpAnycastInetOffset           NTPTimeStamp,
           rlSntpAnycastInetDelay            NTPSignedTimeValue,
           rlSntpAnycastInetRowStatus        RowStatus,
           rlSntpAnycastInetLastReq          NTPTimeStamp
        }

rlSntpAnycastInetIfIndex OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The interface addressed by this entry."
        ::=  {rlSntpAnycastInetEntry 1}

rlSntpAnycastInetAddressType OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Inet Address Type of a trusted SNTP server."
        ::= { rlSntpAnycastInetEntry 2 }

rlSntpAnycastInetAddress OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Inet Address of a trusted SNTP server."
        ::= { rlSntpAnycastInetEntry 3 }

rlSntpAnycastInetStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of this server."
        ::= { rlSntpAnycastInetEntry 4 }

rlSntpAnycastInetLastResp OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Anycast Last Response Time"
        ::= { rlSntpAnycastInetEntry 5 }

rlSntpAnycastInetStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                       unknown(1),
                       inProcess(2),
                       up(3),
                       down(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The Operational State of the remote IP Address of
                     the SNTP Anycast.
                     unknown     - requests were not sent yet.
                     inProcess   - replies were not received yet.
                     up          - server sent SNTP packets.
                     down        - server stopped sending SNTP packets."
        DEFVAL      { unknown }
        ::= { rlSntpAnycastInetEntry 6 }

rlSntpAnycastInetOffset OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated offset of the server's clock relative to
                 the local clock, in seconds.  The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpAnycastInetEntry 7 }

rlSntpAnycastInetDelay OBJECT-TYPE
        SYNTAX      NTPSignedTimeValue
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated round-trip delay of the server's clock
                 relative to the local clock over the network path
                 between them, in seconds. The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpAnycastInetEntry 8 }

rlSntpAnycastInetRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The Status of this SNTP anycast interface
                     information."
        ::= { rlSntpAnycastInetEntry 9 }

rlSntpAnycastInetLastReq OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Anycast Last Request Time"
        ::= { rlSntpAnycastInetEntry 10 }

-- ----------------------------------------------------------------------
-- IPv6: Table for configuring Servers (Unicast)
-- ----------------------------------------------------------------------

rlSntpConfigServerInetTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RlSntpServerInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing trusted SNTP servers to be queried in
                     unicast or broadcast mode."
        ::= { rlSntpConfig 17 }

rlSntpServerInetEntry OBJECT-TYPE
        SYNTAX      RlSntpServerInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A trusted server."
        INDEX       {   rlSntpServerInetAddressType,
                        rlSntpServerInetAddress }
        ::= { rlSntpConfigServerInetTable 1 }

RlSntpServerInetEntry ::=
        SEQUENCE {
           rlSntpServerInetAddressType      InetAddressType,
           rlSntpServerInetAddress          InetAddress,
           rlSntpServerInetPolled           TruthValue,
           rlSntpServerInetStratum          NTPStratum,
           rlSntpServerInetLastResp         NTPTimeStamp,
           rlSntpServerInetStatus           INTEGER,
           rlSntpServerInetOffset           NTPTimeStamp,
           rlSntpServerInetDelay            NTPSignedTimeValue,
           rlSntpServerInetKeyIdentifier    Unsigned32,
           rlSntpServerInetRowStatus        RowStatus,
           rlSntpServerInetLastReq          NTPTimeStamp
        }

rlSntpServerInetAddressType OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Inet Address Type of a trusted SNTP server."
        ::= { rlSntpServerInetEntry 1 }

rlSntpServerInetAddress OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Inet Address of a trusted SNTP server."
        ::= { rlSntpServerInetEntry 2 }

rlSntpServerInetPolled OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "TRUE if participating in polling cycle, else FALSE."
        DEFVAL { false }
        ::= {  rlSntpServerInetEntry 3 }

rlSntpServerInetStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of this server."
        ::= { rlSntpServerInetEntry 4 }

rlSntpServerInetLastResp OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Server Last Response Time"
        ::= { rlSntpServerInetEntry 5 }

rlSntpServerInetStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                       unknown(1),
                       inProcess(2),
                       up(3),
                       down(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The Operational State of the remote IP Address of
                     the SNTP Server.
                     unknown     - requests were not sent yet.
                     inProcess   - replies were not received yet.
                     up          - server sent SNTP packets.
                     down        - server stopped sending SNTP packets."
        DEFVAL      { unknown }
        ::= { rlSntpServerInetEntry 6 }

rlSntpServerInetOffset OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated offset of the server's clock relative to
                 the local clock, in seconds.  The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpServerInetEntry 7 }

rlSntpServerInetDelay OBJECT-TYPE
        SYNTAX      NTPSignedTimeValue
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated round-trip delay of the server's clock
                 relative to the local clock over the network path
                 between them, in seconds. The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpServerInetEntry 8 }

rlSntpServerInetKeyIdentifier OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Authentication key identifier. The valid range is
                     1-4294967295.
                     Value zero, means no authentication is being done."
        ::= { rlSntpServerInetEntry 9 }

rlSntpServerInetRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The Status of this SNTP server information."
        ::= { rlSntpServerInetEntry 10 }

rlSntpServerInetLastReq OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Server Last Request Time"
        ::= { rlSntpServerInetEntry 11 }


rlSntpAllServerInetTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RlSntpAllServerInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table containing all SNTP servers (for example: statically
                     configured, dynamically configured) to be queried in unicast
                     or broadcast mode."
        ::= { rlSntpConfig 18 }

rlSntpAllServerInetEntry OBJECT-TYPE
        SYNTAX      RlSntpAllServerInetEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A server entry."

        INDEX       {   rlSntpAllServerSource,
                        rlSntpAllServerIfIndex,
                        rlSntpAllServerPreference,
                        rlSntpAllServerInetAddressType,
                        rlSntpAllServerInetAddress
                    }
        ::= { rlSntpAllServerInetTable 1 }

RlSntpAllServerInetEntry ::=
        SEQUENCE {
           rlSntpAllServerSource              INTEGER,
           rlSntpAllServerIfIndex             InterfaceIndex,
           rlSntpAllServerPreference          INTEGER,
           rlSntpAllServerInetAddressType     InetAddressType,
           rlSntpAllServerInetAddress         InetAddress,
           rlSntpAllServerInetPolled          TruthValue,
           rlSntpAllServerInetStratum         NTPStratum,
           rlSntpAllServerInetLastResp        NTPTimeStamp,
           rlSntpAllServerInetStatus          INTEGER,
           rlSntpAllServerInetOffset          NTPTimeStamp,
           rlSntpAllServerInetDelay           NTPSignedTimeValue,
           rlSntpAllServerInetKeyIdentifier   Unsigned32,
           rlSntpAllServerInetLastReq         NTPTimeStamp
        }

rlSntpAllServerSource OBJECT-TYPE
        SYNTAX INTEGER {
         static(1),
         dhcpv6(2),
		 dhcpv4(3)
        }
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The SNTP server source: static means manually defined,
                     dhcpv6 means learnt from DHCP. Only static entries are
                     stored in CDB."
        ::= { rlSntpAllServerInetEntry 1 }

rlSntpAllServerIfIndex OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The ifIndex from which the SNTP server configuration was
                     received (for dhcpv6 configurations). For static entries
                     the value of this field will always be 1. "
        ::= { rlSntpAllServerInetEntry 2 }

rlSntpAllServerPreference OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The preference of SNTP server (for dhcpv6 configurations).
                     For static entries the value of this field will always be 0. "
        ::= { rlSntpAllServerInetEntry 3 }

rlSntpAllServerInetAddressType OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "SNTP server inet address type."
        ::= { rlSntpAllServerInetEntry 4 }

rlSntpAllServerInetAddress OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "SNTP server inet address."
        ::= { rlSntpAllServerInetEntry 5 }

rlSntpAllServerInetPolled OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "TRUE if participating in polling cycle, else FALSE."
        DEFVAL { false }
        ::= {  rlSntpAllServerInetEntry 6 }

rlSntpAllServerInetStratum OBJECT-TYPE
        SYNTAX      NTPStratum
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The stratum of this server."
        ::= { rlSntpAllServerInetEntry 7 }

rlSntpAllServerInetLastResp OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Server Last Response Time"
        ::= { rlSntpAllServerInetEntry 8 }

rlSntpAllServerInetStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                       unknown(1),
                       inProcess(2),
                       up(3),
                       down(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The Operational State of the remote IP Address of
                     the SNTP Server.
                     unknown     - requests were not sent yet.
                     inProcess   - replies were not received yet.
                     up          - server sent SNTP packets.
                     down        - server stopped sending SNTP packets."
        DEFVAL      { unknown }
        ::= { rlSntpAllServerInetEntry 9 }

rlSntpAllServerInetOffset OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated offset of the server's clock relative to
                 the local clock, in seconds.  The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpAllServerInetEntry 10 }

rlSntpAllServerInetDelay OBJECT-TYPE
        SYNTAX      NTPSignedTimeValue
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The estimated round-trip delay of the server's clock
                 relative to the local clock over the network path
                 between them, in seconds. The host determines the
                 value of this object using the algorithm described in
                 RFC 2030."
        ::= { rlSntpAllServerInetEntry 11 }

rlSntpAllServerInetKeyIdentifier OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Authentication key identifier. The valid range is
                     1-4294967295.
                     Value zero, means no authentication is being done."
        ::= { rlSntpAllServerInetEntry 12 }

rlSntpAllServerInetLastReq OBJECT-TYPE
        SYNTAX      NTPTimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "SNTP Server Last Request Time"
        ::= { rlSntpAllServerInetEntry 13 }

rlSntpRestoreDefaultServers OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this scalar to true restores sntp default unicast servers.
                     Meaning: all manually configured servers are deleted, and the
                     default SNTP servers are recreated with their default values.
                     This is an 'action' scalar."
        ::= { rlSntpConfig 19 }

END
