RADLAN-PHY-MIB DEFINITIONS ::= BEGIN

-- Title:      RADLAN PHY MIB
-- Version:    7.38
-- Date:       10 Sep 2004
--
IMPORTS
    OBJECT-TYPE, MODULE-IDENTITY                FROM SNMPv2-SMI
    ifIndex                                     FROM IF-MIB
    TimeStamp, DisplayString                    FROM SNMPv2-TC
    TruthValue, TEXTUAL-CONVENTION              FROM SNMPv2-TC
    rnd                                         FROM RADLAN-MIB;

   rlPhy MODULE-IDENTITY
      LAST-UPDATED "200209300024Z"  -- September 30, 2002
      ORGANIZATION "Marvell Semiconductor, Inc."
      CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
      DESCRIPTION
              "The MIB module describes the private MIB for testing Layer1 interfaces supported
               by Radlan's software and products."
      REVISION     "200209300024Z"  -- September 30, 2002
      DESCRIPTION
              "Initial revision"
      REVISION     "200309210024Z"  -- September 21, 2003
      DESCRIPTION
              "Added MODULE-IDENTITY and TEXTUAL-CONVENTION IMPORTS."
      ::= { rnd 90  }


RlPhyTestType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "A value indicating the test to perform."
   SYNTAX  INTEGER {
        rlPhyTestTableNoTest(1),
        rlPhyTestTableCableStatus(2),
        rlPhyTestTableCableFault(3),
        rlPhyTestTableCableLength(4),
        rlPhyTestTableTransceiverTemp(5),
        rlPhyTestTableTransceiverSupply(6),
        rlPhyTestTableTxBias(7),
        rlPhyTestTableTxOutput(8),
        rlPhyTestTableRxOpticalPower(9),
        rlPhyTestTableDataReady(10),
        rlPhyTestTableLOS(11),
        rlPhyTestTableTxFault(12),
        rlPhyTestTableCableChannel1(13),
        rlPhyTestTableCableChannel2(14),
        rlPhyTestTableCableChannel3(15),
        rlPhyTestTableCableChannel4(16),
        rlPhyTestTableCablePolarity1(17),
        rlPhyTestTableCablePolarity2(18),
        rlPhyTestTableCablePolarity3(19),
        rlPhyTestTableCablePolarity4(20),
        rlPhyTestTableCablePairSkew1(21),
        rlPhyTestTableCablePairSkew2(22),
        rlPhyTestTableCablePairSkew3(23),
        rlPhyTestTableCablePairSkew4(24),
        rlPhyTestTableSFPEepromQualified(25),
        rlPhyTestTableRxOpticalPower1(27),
        rlPhyTestTableRxOpticalPower2(28),
        rlPhyTestTableRxOpticalPower3(29),
        rlPhyTestTableTxBias1(30),
        rlPhyTestTableTxBias2(31),
        rlPhyTestTableTxBias3(32),
        rlPhyTestTableLOS1(33),
        rlPhyTestTableLOS2(34),
        rlPhyTestTableLOS3(35),
        rlPhyTestTableTxOutput1(36),
        rlPhyTestTableTxOutput2(37),
        rlPhyTestTableTxOutput3(38),
        rlPhyTestTableRxOpticalPower4(39),
        rlPhyTestTableRxOpticalPower5(40),
        rlPhyTestTableRxOpticalPower6(41),
        rlPhyTestTableRxOpticalPower7(42),
        rlPhyTestTableTxBias4(43),
        rlPhyTestTableTxBias5(44),
        rlPhyTestTableTxBias6(45),
        rlPhyTestTableTxBias7(46),
        rlPhyTestTableLOS4(47),
        rlPhyTestTableLOS5(48),
        rlPhyTestTableLOS6(49),
        rlPhyTestTableLOS7(50),
        rlPhyTestTableTxOutput4(51),
        rlPhyTestTableTxOutput5(52),
        rlPhyTestTableTxOutput6(53),
        rlPhyTestTableTxOutput7(54)
    }

rlPhyTest OBJECT IDENTIFIER ::= { rlPhy 1 }

rlPhyTestSetTable   OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPhyTestSetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION ""
    ::= { rlPhyTest 1}

rlPhyTestSetEntry OBJECT-TYPE
    SYNTAX       RlPhyTestSetEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
            "An entry containing objects for invoking tests on an interface."
    INDEX {ifIndex }
    ::= { rlPhyTestSetTable 1 }

RlPhyTestSetEntry ::=
    SEQUENCE {
        rlPhyTestSetType        RlPhyTestType
    }

rlPhyTestSetType       OBJECT-TYPE
    SYNTAX  RlPhyTestType
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
            "A control variable used to start operator initiated interface
             tests.1 indicates that no test has been initiated. Only
             operator initiated interface tests can be set to this variable."
              ::= { rlPhyTestSetEntry 1 }

rlPhyTestGetTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlPhyTestGetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION ""
    ::= { rlPhyTest 2 }

rlPhyTestGetEntry OBJECT-TYPE
    SYNTAX       RlPhyTestGetEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
            "An entry containing results of tests on an interface."
    INDEX {ifIndex, rlPhyTestGetType}
    ::= { rlPhyTestGetTable 1 }

RlPhyTestGetEntry ::=
    SEQUENCE {
        rlPhyTestGetType        RlPhyTestType,
        rlPhyTestGetStatus      INTEGER,
        rlPhyTestGetResult      INTEGER,
        rlPhyTestGetUnits       INTEGER,
        rlPhyTestGetAlarm       INTEGER,
        rlPhyTestGetTimeStamp   DisplayString
    }

rlPhyTestGetType       OBJECT-TYPE
    SYNTAX     RlPhyTestType
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "A control variable used to, 1 to indicate that this test can be
            done on the specified port, 2 to initiate the test whenever the
            user wishes"
              ::= { rlPhyTestGetEntry 1 }

rlPhyTestGetStatus  OBJECT-TYPE
    SYNTAX       INTEGER {
        none(1),          -- no test yet requested
        success(2),
        inProgress(3),
        notSupported(4),
        unAbleToRun(5),   -- due to state of system
        aborted(6),
        failed(7)
                 }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "This object contains the status of the most recently
        requested test for operator initiated tests or the value
        none(1) if no tests have been requested since the last
        reset. For non operator initiated tests the value is always
        none(1).
        Note that this facility provides no provision for saving
        the results of one test when starting another, as could
        be required if used by multiple managers concurrently."
    ::= { rlPhyTestGetEntry 2 }

rlPhyTestGetResult  OBJECT-TYPE
    SYNTAX       INTEGER
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "This object holds the test result"
    ::= { rlPhyTestGetEntry 3 }

rlPhyTestGetUnits   OBJECT-TYPE
   SYNTAX  INTEGER {
        integer(1),
        boolean(2),
        downUP(3),
        reverseNormal(4),
        mdiMdix(5),
        meter(6),
        degree(7),  -- Celsius
        microVolt(8),
        microOham(9),
        microAmper(10),
        microWatt(11),
        millisecond(12),
        alaskaPhyLength(13),
        alaskaPhyStatus(14),
        dbm(15),
        decidbm(16),
        milidbm(17),
        abcd(18),
        nanosecond(19)
            }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The test result unit of measure. The units can be standard unit or special units
         that are designed for special test.

         The alaskaPhyLength unit is design for the VCT diagnostic and its values are:
         less_than_50M(1), 50-80M(2), 80-110M(3), 110-140M(4), more_than_140M(5).

         The alaskaPhyStatus unit is design for the VCT diagnostic and its values are:
         4_pair_cable(1), 2_pair_cable(2), no_cable(3), open_cable(4), short_cable(5), bad_cable(6), impedance_mismatch(7)."
   ::= { rlPhyTestGetEntry 4 }

rlPhyTestGetAlarm   OBJECT-TYPE
   SYNTAX  INTEGER {
        notRelevant(1),
        noAlarmSet(2),
        lowWarning(3),
        highWarning(4),
        lowAlarm(5),
        highAlarm(6)
   }
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION
        "This object hold the Alarm for this Entry. only Test that have can have alarms
          use this field, other holds the Value notRelevant(1) "
   ::= { rlPhyTestGetEntry 5 }

rlPhyTestGetTimeStamp   OBJECT-TYPE
   SYNTAX  DisplayString (SIZE(1..32))
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION
        "The time in string (formated DD-MMM-YYYY HH:MM:SS e.g
         14-Apr-2002 10:33:31)"
    ::= { rlPhyTestGetEntry 6 }

END
