RADLAN-BRIDGEMIBOBJECTS-MIB DEFINITIONS ::= BEGIN

-- Title:                RADLAN ROS
--                       Private BRIDGE MIB OBJECTS MIB
-- Version:              7.46
-- Date:                 15-Jan-2007

IMPORTS
    rnd                                                              FROM RADLAN-MIB
    OBJECT-TYPE, MODULE-IDENTITY, TimeTicks, Counter32               FROM SNMPv2-SMI
    TruthValue, DisplayString, RowStatus                             FROM SNMPv2-TC
    Counter                                                          FROM RFC1155-SMI
    BridgeId, Timeout, dot1dBasePort, dot1dStpPort, MacAddress       FROM BRIDGE-MIB
    InterfaceIndex, ifIndex, InterfaceIndexOrZero                    FROM IF-MIB
    PortList                                                         FROM Q-BRIDGE-MIB
    SnmpAdminString                                                  FROM SNMP-FRAMEWORK-MIB;

-- -------------------------------------------------------------
-- Textual Conventions
-- -------------------------------------------------------------

VlanList1 ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Each octet within this value specifies a set of eight
        vlans, with the first octet specifying vlan 1 through
        8, the second octet specifying vlan 9 through 16, etc.
        Within each octet, the most significant bit represents
        the lowest numbered vlan, and the least significant bit
        represents the highest numbered vlan.  Thus, each vlan
        of the bridge is represented by a single bit within the
        value of this object.  If that bit has a value of '1'
        then that vlan is included in the set of vlans; the vlan
        is not included if its bit has a value of '0'.
        VlanList1 represent vlans 1-1024"
    SYNTAX OCTET STRING (SIZE(0..128))

VlanList2 ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "As VlanList1 but represent vlans 1025-2048"
    SYNTAX OCTET STRING (SIZE(0..128))

VlanList3 ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "As VlanList1 but represent vlans 2049-3072"
    SYNTAX OCTET STRING (SIZE(0..128))

VlanList4 ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "As VlanList1 but represent vlans 3073-4094"
    SYNTAX OCTET STRING (SIZE(0..128))



rlpBridgeMIBObjects MODULE-IDENTITY
                LAST-UPDATED "200701020000Z"
                ORGANIZATION "Marvell Semiconductor, Inc."
                CONTACT-INFO
                                        "5488 Marvell Lane
                                        Santa Clara, CA 95054
                                        USA

                                        Website:  www.marvell.com"
                DESCRIPTION
                      "This private MIB module defines bridge MIB objects private MIBs."
                REVISION "200701020000Z"
                DESCRIPTION
                      "Initial revision."
        ::= { rnd 57 }

rldot1dPriority  OBJECT IDENTIFIER ::= { rlpBridgeMIBObjects 1 }

rldot1dPriorityMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "MIB's version, the current version is 1."
    ::= { rldot1dPriority 1 }

--
-- rldot1dPriorityPortGroupTable
--

rldot1dPriorityPortGroupTable  OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1dPriorityPortGroupEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of PortGroupNumber for each port."
    ::= { rldot1dPriority 2 }

rldot1dPriorityPortGroupEntry OBJECT-TYPE
    SYNTAX  Rldot1dPriorityPortGroupEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "All ports belonging to a same group have
         the same User Priority to Traffic Class mapping."
   INDEX   { dot1dBasePort }
    ::= { rldot1dPriorityPortGroupTable 1 }

Rldot1dPriorityPortGroupEntry ::= SEQUENCE {
    rldot1dPriorityPortGroupNumber       INTEGER
}

rldot1dPriorityPortGroupNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A group, that port belongs to. All ports belonging
         to a same group have the same User Priority to
         Traffic Class mapping."
    ::= { rldot1dPriorityPortGroupEntry 1 }


rldot1dStp  OBJECT IDENTIFIER ::= { rlpBridgeMIBObjects 2 }

--
-- Scalars
--
rldot1dStpMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "MIB's version, the current version is 2."
    ::= { rldot1dStp 1 }

rldot1dStpType OBJECT-TYPE
    SYNTAX  INTEGER {
        perDevice  (1),
        mstp       (4)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies whether the device supports Spanning Tree per device,
         or per group."
    ::= { rldot1dStp 2 }

rldot1dStpEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable / Disable spanning tree. When working in per vlan mode
         enable / disable STP per all vlans."
    DEFVAL { true }
    ::= { rldot1dStp 3 }

rldot1dStpPortMustBelongToVlan OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies whether a port must belong to a VLAN in order
         to participate in the STP."
    DEFVAL { true }
    ::= { rldot1dStp 4 }

rldot1dStpExtendedPortNumberFormat OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies whether the STP uses the extended port fnumber format."
    DEFVAL { false }
    ::= { rldot1dStp 5 }

--
--   The Spanning Tree Vlan Table
--
rldot1dStpVlanTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1dStpVlanEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
            "A table that contains vlan-specific information
            for the Spanning Tree Protocol."
    ::= { rldot1dStp 6 }

rldot1dStpVlanEntry OBJECT-TYPE
    SYNTAX  Rldot1dStpVlanEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every Vlan
         about the Spanning Tree Protocol state for that
         Vlan."
    INDEX   { rldot1dStpVlan }
    ::= { rldot1dStpVlanTable 1 }

Rldot1dStpVlanEntry ::= SEQUENCE {
    rldot1dStpVlan                      INTEGER,
    rldot1dStpVlanEnable                TruthValue,
    rldot1dStpTimeSinceTopologyChange   TimeTicks,
    rldot1dStpTopChanges                Counter,
    rldot1dStpDesignatedRoot            BridgeId,
    rldot1dStpRootCost                  INTEGER,
    rldot1dStpRootPort                  INTEGER,
    rldot1dStpMaxAge                    Timeout,
    rldot1dStpHelloTime                 Timeout,
    rldot1dStpHoldTime                  INTEGER,
    rldot1dStpForwardDelay              Timeout
}

rldot1dStpVlan OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan index."
    ::= { rldot1dStpVlanEntry 1 }

rldot1dStpVlanEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies whether this vlan is STP enable or disable"
    REFERENCE
        " ??  "
    DEFVAL { true }
    ::= { rldot1dStpVlanEntry 2 }

rldot1dStpTimeSinceTopologyChange OBJECT-TYPE
    SYNTAX  TimeTicks
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time (in hundredths of a second) since the
         last time a topology change was detected by the
         bridge entity."
    REFERENCE
        "IEEE 802.1D-1990: Section 6.8.1.1.3"
    ::= { rldot1dStpVlanEntry 3 }

rldot1dStpTopChanges OBJECT-TYPE
    SYNTAX  Counter
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of topology changes detected by
         this bridge since the management entity was last
         reset or initialized."
    REFERENCE
        "IEEE 802.1D-1990: Section 6.8.1.1.3"
    ::= { rldot1dStpVlanEntry 4 }

rldot1dStpDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the root of the spanning
         tree as determined by the Spanning Tree Protocol
         as executed by this node.  This value is used as
         the Root Identifier parameter in all Configuration
         Bridge PDUs originated by this node."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.1"
    ::= { rldot1dStpVlanEntry 5 }

rldot1dStpRootCost OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The cost of the path to the root as seen from
         this bridge."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.2"
    ::= { rldot1dStpVlanEntry 6 }

rldot1dStpRootPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port which offers the
         lowest cost path from this bridge to the root
         bridge."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.3"
    ::= { rldot1dStpVlanEntry 7 }

rldot1dStpMaxAge OBJECT-TYPE
    SYNTAX  Timeout
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum age of Spanning Tree Protocol
         information learned from the network on any port
         before it is discarded, in units of hundredths of
         a second.  This is the actual value that this
         bridge is currently using."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.4"
    ::= { rldot1dStpVlanEntry 8 }

rldot1dStpHelloTime OBJECT-TYPE
    SYNTAX  Timeout
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of
         Configuration bridge PDUs by this node on any port
         when it is the root of the spanning tree or trying
         to become so, in units of hundredths of a second.
         This is the actual value that this bridge is
         currently using."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.5"
    ::= { rldot1dStpVlanEntry 9 }

rldot1dStpHoldTime OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This time value determines the interval length
         during which no more than two Configuration bridge
         PDUs shall be transmitted by this node, in units
         of hundredths of a second."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.14"
    ::= { rldot1dStpVlanEntry 10 }

rldot1dStpForwardDelay OBJECT-TYPE
    SYNTAX  Timeout
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This time value, measured in units of hundredths
         of a second, controls how fast a port changes its
         spanning state when moving towards the Forwarding
         state.  The value determines how long the port
         stays in each of the Listening and Learning
         states, which precede the Forwarding state.  This
         value is also used, when a topology change has
         been detected and is underway, to age all dynamic
         entries in the Forwarding Database.  [Note that
         this value is the one that this bridge is
         currently using, in contrast to
         dot1dStpBridgeForwardDelay which is the value that
         this bridge and all others would start using
         if/when this bridge were to become the root.]"
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.6"
    ::= { rldot1dStpVlanEntry 11 }

--
-- rldot1dStpVlanPortTable
--
rldot1dStpVlanPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1dStpVlanPortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table that contains pair <vlan, port> specific information
         for the Spanning Tree Protocol."
    ::= { rldot1dStp 7 }

rldot1dStpVlanPortEntry OBJECT-TYPE
    SYNTAX  Rldot1dStpVlanPortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every pair <vlan, port>
         about the Spanning Tree Protocol state for that pair."
    INDEX   { rldot1dStpVlanPortVlan, rldot1dStpVlanPortPort }
    ::= { rldot1dStpVlanPortTable 1 }

Rldot1dStpVlanPortEntry ::= SEQUENCE {
    rldot1dStpVlanPortVlan                  INTEGER,
    rldot1dStpVlanPortPort                  INTEGER,
    rldot1dStpVlanPortPriority              INTEGER,
    rldot1dStpVlanPortState                 INTEGER,
    rldot1dStpVlanPortEnable                INTEGER,
    rldot1dStpVlanPortPathCost              INTEGER,
    rldot1dStpVlanPortDesignatedRoot        BridgeId,
    rldot1dStpVlanPortDesignatedCost        INTEGER,
    rldot1dStpVlanPortDesignatedBridge      BridgeId,
    rldot1dStpVlanPortDesignatedPort        OCTET STRING,
    rldot1dStpVlanPortForwardTransitions    Counter
}

rldot1dStpVlanPortVlan OBJECT-TYPE
    SYNTAX  INTEGER (1..4095)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan number that the port belongs to, and for which this entry
         contains Spanning Tree Protocol management
         information."
    REFERENCE
         "IEEE 802.1s/D2-1999 "
    ::= { rldot1dStpVlanPortEntry 1 }

rldot1dStpVlanPortPort OBJECT-TYPE
    SYNTAX  INTEGER (1..4096)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port for which this entry
         contains Spanning Tree Protocol management
         information."
    REFERENCE
         "IEEE 802.1t/D2-1999: Section 9.2.6"
    ::= { rldot1dStpVlanPortEntry 2 }

rldot1dStpVlanPortPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..255)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value of the priority field which is
         contained in the more significant  4 bits of the most
         significant octet of the (2 octet long) Port ID.
         The other octet of the Port ID is given by the value
         of rldot1dStpVlanPort."
    REFERENCE
        "IEEE 802.1t/D2-1999: Section 9.2.6"
    ::= { rldot1dStpVlanPortEntry 3 }

rldot1dStpVlanPortState OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(1),
        blocking(2),
        listening(3),
        learning(4),
        forwarding(5),
        broken(6)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port's current state as defined by application of
         the Spanning Tree Protocol. This state controls what
         action a port takes on reception of a frame.
         If the bridge has detected a port that is malfunctioning
         it will place that port into the broken(6) state.  For ports
         which are disabled (see dot1dStpVlanPortEnable), this object
         will have a value of disabled(1)."
    REFERENCE
            "IEEE 802.1D-1990: Section 4.5.5.2"
    ::= { rldot1dStpVlanPortEntry 4 }

rldot1dStpVlanPortEnable OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The enabled/disabled status of the port."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.2"
    ::= { rldot1dStpVlanPortEntry 5 }

rldot1dStpVlanPortPathCost OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The contribution of this port to the path cost of
         paths towards the spanning tree root which include
         this port.  802.1D-1990 recommends that the
         default value of this parameter be in inverse
         proportion to the speed of the attached LAN."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.3"
    ::= { rldot1dStpVlanPortEntry 6 }

rldot1dStpVlanPortDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The unique Bridge Identifier of the Bridge
         recorded as the Root in the Configuration BPDUs
         transmitted by the Designated Bridge for the
         segment to which the port is attached."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.4"
    ::= { rldot1dStpVlanPortEntry 7 }

rldot1dStpVlanPortDesignatedCost OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The path cost of the Designated Port of the
         segment connected to this port.  This value is
         compared to the Root Path Cost field in received
         bridge PDUs."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.5"
    ::= { rldot1dStpVlanPortEntry 8 }

rldot1dStpVlanPortDesignatedBridge OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Bridge Identifier of the bridge which this
         port considers to be the Designated Bridge for
         this port's segment."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.6"
    ::= { rldot1dStpVlanPortEntry 9 }

rldot1dStpVlanPortDesignatedPort OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Port Identifier of the port on the Designated
         Bridge for this port's segment."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.7"
    ::= { rldot1dStpVlanPortEntry 10 }

rldot1dStpVlanPortForwardTransitions OBJECT-TYPE
    SYNTAX  Counter
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of times this port has transitioned
         from the Learning state to the Forwarding state."
    ::= { rldot1dStpVlanPortEntry 11 }

--
-- STP Private TRAP variables
--
rldot1dStpTrapVariable  OBJECT IDENTIFIER ::= { rldot1dStp 8 }

rldot1dStpTrapVrblifIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "The ifIndex of port which STP status was changed"
    ::= { rldot1dStpTrapVariable 1  }

rldot1dStpTrapVrblVID OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "The VID of VLAN to which the port belongs which STP status was changed"
    ::= { rldot1dStpTrapVariable 2  }

rldot1dStpTypeAfterReset OBJECT-TYPE
    SYNTAX  INTEGER {
        perDevice(1),
        mstp(4)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "New mode of spaning tree supported by the device after the next reset."
    DEFVAL { perDevice }
    ::= { rldot1dStp 9 }

rldot1dStpMonitorTime OBJECT-TYPE
    SYNTAX  INTEGER (1..20)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Factor of hello-time during which a port is monotored to determine if it is stable."
    DEFVAL { 10 }
    ::= { rldot1dStp 10 }

rldot1dStpBpduCount OBJECT-TYPE
    SYNTAX  INTEGER (1..60)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The number of bpdu that need to received for the link to be considered stable."
    DEFVAL { 10 }
    ::= { rldot1dStp 11 }

rldot1dStpLastChanged  OBJECT-TYPE
    SYNTAX  TimeTicks
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
         "The last time any object in this table was changed
          by SNMP or other local management means."
    REFERENCE
        ""
    ::= { rldot1dStp 12 }

--
-- rldot1dStpPortTable
--
rldot1dStpPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1dStpPortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table that contains extended pair port specific information."
    ::= { rldot1dStp 13 }

rldot1dStpPortEntry OBJECT-TYPE
    SYNTAX  Rldot1dStpPortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every port
         about the Spanning Tree Protocol state for that port."
    INDEX   { rldot1dStpPortPort }
    ::= { rldot1dStpPortTable 1 }

Rldot1dStpPortEntry ::= SEQUENCE {
    rldot1dStpPortPort                  INTEGER,
    rldot1dStpPortDampEnable            TruthValue,
    rldot1dStpPortDampStable            TruthValue,
    rldot1dStpPortFilterBpdu            INTEGER,
    rldot1dStpPortBpduSent              Counter32,
    rldot1dStpPortBpduReceived          Counter32,
    rldot1dStpPortRole                  INTEGER,
    rldot1dStpBpduType                  INTEGER,
    rldot1dStpPortRestrictedRole        TruthValue,
    rldot1dStpPortAutoEdgePort          TruthValue,
    rldot1dStpPortLoopback              TruthValue,
    rldot1dStpPortBpduOperStatus        INTEGER,
    rldot1dStpPortTcnGuardEnable        TruthValue
}

rldot1dStpPortPort OBJECT-TYPE
    SYNTAX  INTEGER (1..4096)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port for which this entry
         contains Spanning Tree Protocol management
         information."
    REFERENCE
         "IEEE 802.1t/D2-1999: Section 9.2.6"
    ::= { rldot1dStpPortEntry 1 }

rldot1dStpPortDampEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specified if dampening is enabled on this port."
    REFERENCE
        ""
    DEFVAL { false }
    ::= { rldot1dStpPortEntry 2 }

rldot1dStpPortDampStable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified if the port is stable."
    REFERENCE
        ""
    DEFVAL { true }
    ::= { rldot1dStpPortEntry 3 }

rldot1dStpPortFilterBpdu OBJECT-TYPE
    SYNTAX  INTEGER {
        false(0),
        true(1),
        none(2)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specified if this port should filter bpdus when stp is disabled."
    REFERENCE
        ""
    DEFVAL { none }
    ::= { rldot1dStpPortEntry 4 }

rldot1dStpPortBpduSent OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified the number of bpdu sent from this port."
    REFERENCE
        ""
    ::= { rldot1dStpPortEntry 5 }

rldot1dStpPortBpduReceived OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified the number of bpdu received in this port."
    REFERENCE
        ""
    ::= { rldot1dStpPortEntry 6 }

rldot1dStpPortRole OBJECT-TYPE
    SYNTAX  INTEGER {
                    unknown(0),
                    disabled(1),
                    alternate(2),
                    backup(3),
                    root(4),
                    designated(5)
                }

    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified the role of this this port."
    REFERENCE
        ""
    ::= { rldot1dStpPortEntry 7 }

rldot1dStpBpduType OBJECT-TYPE
    SYNTAX  INTEGER {
        stp(0),
        rstp(1)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified the type of BPDU transmitted by this port."
    ::= { rldot1dStpPortEntry 8 }

rldot1dStpPortRestrictedRole OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If TRUE causes the Port not to be selected as Root Port for the CIST or
         any MSTI, even if it has the best spanning tree priority vector.
         Such a Port will be selected as an Alternate Port after the Root Port
         has been selected."
    REFERENCE
        "IEEE 802.1ad-D3-1: Section 13.24.29"
    DEFVAL { false }
    ::= { rldot1dStpPortEntry 9 }

rldot1dStpPortAutoEdgePort OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If TRUE causes the Port when become up, to enter the blocking state,
         and if during 3 seconds it doesn't receive a BPDU, it will enter
         the forwarding state."
    REFERENCE
        "IEEE 802.1D-2004: Section 17.13.3"
    DEFVAL { true }
    ::= { rldot1dStpPortEntry 10 }

rldot1dStpPortLoopback OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified loopback was detected on port.
         Usable for only a short period of time if stp loopback guard is enabled
         (since port enters into shutdown state)."
    REFERENCE
        ""
    ::= { rldot1dStpPortEntry 11 }

rldot1dStpPortBpduOperStatus OBJECT-TYPE
    SYNTAX  INTEGER {
        filter(0),
        flood(1),
        bridge(2),
        stp(3)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified BPDU handling operative status for port."
    REFERENCE
        ""
    ::= { rldot1dStpPortEntry 12 }

rldot1dStpPortTcnGuardEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
    "Enable / Disable TCN guard on port. TCN guard prevents receiving topology change notifications."
    ::= { rldot1dStpPortEntry 13 }

rldot1dStpPortsEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable / Disable spanning tree on ports by default ."
    DEFVAL { true }
    ::= { rldot1dStp 14 }

rldot1dStpTaggedFlooding OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "flooding can be done in tagged bpdu ."
    ::= { rldot1dStp 15 }

rldot1dStpPortBelongToVlanDefault OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The default value of rldot1dStpPortMustBelongToVlan ."
    ::= { rldot1dStp 16 }

rldot1dStpEnableByDefault OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The default value of rldot1dStpEnable ."
    ::= { rldot1dStp 17 }

rldot1dStpPortToDefault OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "To order port/s to revert to default setings ."
    ::= { rldot1dStp 18 }

rldot1dStpSupportedType OBJECT-TYPE
    SYNTAX  INTEGER {
        perDevice(1),
        perVlan(2),
        mstp(3)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The type of stp supported by the device."
    ::= { rldot1dStp 19 }

rldot1dStpEdgeportSupportInStp OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "If EdgePort is supported in stpCompatible mode ."
    ::= { rldot1dStp 20 }

rldot1dStpFilterBpdu OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specified if the device should filter BPDUs when STP is disabled."
    ::= { rldot1dStp 21 }

rldot1dStpFloodBpduMethod OBJECT-TYPE
    SYNTAX  INTEGER {
        classic(0),
        bridging(1)  }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specified flooding method:
        1 - classic - untagged to all stp disabled ports
        2 - bridging -normal bridging."
    ::= { rldot1dStp 22 }

rldot1dStpSeparatedBridges OBJECT IDENTIFIER ::= { rldot1dStp 23 }

--
-- rldot1dStpPortBpduGuardTable
--
rldot1dStpPortBpduGuardTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1dStpPortBpduGuardEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table that contains for each port whether it is bpdu guard ."
    ::= { rldot1dStp 24 }

rldot1dStpPortBpduGuardEntry OBJECT-TYPE
    SYNTAX  Rldot1dStpPortBpduGuardEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every port
         whether it is bpdu guard."
    INDEX   { dot1dBasePort }
    ::= { rldot1dStpPortBpduGuardTable 1 }

Rldot1dStpPortBpduGuardEntry ::= SEQUENCE {
    rldot1dStpPortBpduGuardEnable       TruthValue
}


rldot1dStpPortBpduGuardEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specified if bpdu guard is enabled on this port."
    REFERENCE
        ""
    DEFVAL { false }
    ::= { rldot1dStpPortBpduGuardEntry 1 }

rldot1dStpLoopbackGuardEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Define if STP loopback guard feature is globally enabled."
    DEFVAL { false }
    ::= { rldot1dStp 25 }

rldot1dStpSeparatedBridgesTable    OBJECT-TYPE
    SYNTAX  SEQUENCE  OF Rldot1dStpSeparatedBridgesEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
      "Define if separated bridges feature is enabled  for each interface."
    ::=  { rldot1dStpSeparatedBridges 1 }

rldot1dStpSeparatedBridgesEntry OBJECT-TYPE
    SYNTAX  Rldot1dStpSeparatedBridgesEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
      "Defines the contents of each line in the rlSeparatedBridgesTable table."
    INDEX  { ifIndex }
    ::=  { rldot1dStpSeparatedBridgesTable 1 }

Rldot1dStpSeparatedBridgesEntry ::= SEQUENCE {
    rldot1dStpSeparatedBridgesPortEnable             TruthValue
}

rldot1dStpSeparatedBridgesPortEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
      "This variable indicates whether the separated bridge feature is enabled on a specified ifIndex."
    DEFVAL { false }
    ::= {  rldot1dStpSeparatedBridgesEntry  1 }

rldot1dStpSeparatedBridgesEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable / Disable Separated Bridges Feature."
    DEFVAL { false }
    ::= { rldot1dStpSeparatedBridges 2 }

rldot1dStpSeparatedBridgesAutoConfig OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable / Disable Separated Bridges Automatic Configuration."
    DEFVAL { false }
    ::= { rldot1dStpSeparatedBridges 3 }


rldot1dStpDisabledPortStateTable OBJECT-TYPE
    SYNTAX  SEQUENCE  OF Rldot1dStpDisabledPortStateEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
      "Define stp port state for each stp disabled interface.
      This is auxiliary MIB emulates stp enabled port behaviour in ASIC for stp disabled port.
      The MIB contains only stp disabled ports entries "
    ::=  { rldot1dStp 26 }

rldot1dStpDisabledPortStateEntry OBJECT-TYPE
    SYNTAX  Rldot1dStpDisabledPortStateEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
      "Defines the contents of each line in the rldot1dStpDisabledPortStateTable table."
    INDEX  { dot1dStpPort }
    ::=  { rldot1dStpDisabledPortStateTable 1 }

Rldot1dStpDisabledPortStateEntry ::= SEQUENCE {
    rldot1dStpDisabledPortState        INTEGER

}


rldot1dStpDisabledPortState OBJECT-TYPE
    SYNTAX  INTEGER {
                blocking(2),
                listening(3),
                learning(4),
                forwarding(5)

            }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "The port's stp state as defined by  external
            application .  This state controls what action a port takes on
            reception of a frame."

    DEFVAL {forwarding}
    ::= { rldot1dStpDisabledPortStateEntry 1 }


rldot1dExtBase  OBJECT IDENTIFIER ::= { rlpBridgeMIBObjects 3 }

rldot1dExtBaseMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "MIB's version, the current version is 1."
    ::= { rldot1dExtBase 1 }

rldot1dDeviceCapabilities OBJECT-TYPE
--    SYNTAX      BITS {
--        rldot1dIGMPSnoopingFilteringServices(0)
--                              ## can perform filtering of
--                              ## individual multicast addresses
--                              ## controlled by IGMP snooping.
--        rldot1dDefaultFilteringAllServices(1)
--                              ## can perform default filtering
--                              ## behavior for All multicast addresses.
--                              ## controlled by Multicast DB.
--        rldot1dDefaultFilteringUnregServices(2)
--                              ## can perform default filtering
--                              ## behavior for Unregistered
--                              ## multicast addresses.
--                              ## controlled by Multicast DB.
--    }
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates the optional parts of private extension of
         IEEE 802.1D and 802.1Q that are implemented by this
         device and are manageable through this MIB.
         Capabilities that are allowed on a per-port basis are
         indicated in dot1dPortCapabilities."
    ::= { rldot1dExtBase 2 }


rldot1dStpClearPortCounters  OBJECT-TYPE
    SYNTAX  InterfaceIndexOrZero
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Clear the number of bpdu sent and recieved on specific port,
         if Value of 0 is specified then clear counters action is applied to all ports,
         this object behaviors is write-only, when reading this object 
         it will always return 0."
    ::= { rldot1dStp 27 }

rldot1wRStp  OBJECT IDENTIFIER ::= { rlpBridgeMIBObjects 4 }

--
-- rldot1wStpVlanEdgePortTable
--
rldot1wRStpVlanEdgePortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1wRStpVlanEdgePortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table that contains pair <vlan, port> specific information
         for the Rapid Spanning Tree Protocol."
    ::= { rldot1wRStp 1 }

rldot1wRStpVlanEdgePortEntry OBJECT-TYPE
    SYNTAX  Rldot1wRStpVlanEdgePortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every pair <vlan, port>
         about the RAPID Spanning Tree Protocol state for that pair."
    INDEX   { rldot1wRStpVlanEdgePortVlan, rldot1wRStpVlanEdgePortPort }
    ::= { rldot1wRStpVlanEdgePortTable 1 }

Rldot1wRStpVlanEdgePortEntry ::= SEQUENCE {
    rldot1wRStpVlanEdgePortVlan         INTEGER,
    rldot1wRStpVlanEdgePortPort         INTEGER,
    rldot1wRStpEdgePortStatus           TruthValue
}

rldot1wRStpVlanEdgePortVlan OBJECT-TYPE
    SYNTAX  INTEGER (1..4095)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan number that the port belongs to, and for which this entry
         contains Spanning Tree Protocol management information,
         If STP per device then only one value of 1 is allowed.
         If STP per a VLAN then all value of 1..4095 are allowed."
    ::= { rldot1wRStpVlanEdgePortEntry 1 }

rldot1wRStpVlanEdgePortPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port for which this entry
         contains Spanning Tree Protocol management information."
    ::= { rldot1wRStpVlanEdgePortEntry 2 }

rldot1wRStpEdgePortStatus OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies whether this port is an Edge Port or not"
    REFERENCE
        "IEEE 802.1wd6-2000: Section 17.13.3.1 "
    DEFVAL { false }
    ::= { rldot1wRStpVlanEdgePortEntry 3 }

--
-- rldot1wStpForceVersionTable
--
rldot1wRStpForceVersionTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1wRStpForceVersionEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table that contains  <vlan> specific information
         for the Rapid Spanning Tree Protocol."
    ::= { rldot1wRStp 2 }

rldot1wRStpForceVersionEntry OBJECT-TYPE
    SYNTAX  Rldot1wRStpForceVersionEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every  <vlan>
         about the RAPID Spanning Tree Protocol state for that pair."
    INDEX   { rldot1wRStpForceVersionVlan }
    ::= { rldot1wRStpForceVersionTable 1 }

Rldot1wRStpForceVersionEntry ::= SEQUENCE {
    rldot1wRStpForceVersionVlan         INTEGER,
    rldot1wRStpForceVersionState        INTEGER
}

rldot1wRStpForceVersionVlan OBJECT-TYPE
    SYNTAX  INTEGER (1..4095)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan number that the port belongs to, and for which this entry
         contains Spanning Tree Protocol management information,
         If STP per device then only one value of 1 is allowed.
         If STP per a VLAN then all value of 1..4095 are allowed."
    ::= { rldot1wRStpForceVersionEntry 1 }

rldot1wRStpForceVersionState OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies whether this Bridge uses the normal RSTP algorithm,
         or STP Compatibility algorythm:
         0 - STP Compatibility
         2 - Normal RSTP"
    REFERENCE
        "IEEE 802.1wd9-2000: Section 17.16.1 "
    DEFVAL { 2 }
    ::= { rldot1wRStpForceVersionEntry 2 }

rldot1pPriorityMap  OBJECT IDENTIFIER ::= { rlpBridgeMIBObjects 5 }

rldot1pPriorityMapState OBJECT-TYPE
   SYNTAX  INTEGER {
        enable (1),
        disable (2)
   }
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
       "enable / disable"
   ::= { rldot1pPriorityMap 1 }

rldot1pPriorityMapTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1pPriorityMapEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This table hold information the priority maps"
    ::= { rldot1pPriorityMap 2 }

rldot1pPriorityMapEntry OBJECT-TYPE
    SYNTAX  Rldot1pPriorityMapEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The row definition for this table."
    INDEX { rldot1pPriorityMapName }
    ::= { rldot1pPriorityMapTable 1 }

Rldot1pPriorityMapEntry ::= SEQUENCE {
    rldot1pPriorityMapName     DisplayString,
    rldot1pPriorityMapPriority OCTET STRING,
    rldot1pPriorityMapPort     PortList,
    rldot1pPriorityMapPortList PortList,
    rldot1pPriorityMapStatus   RowStatus
}

rldot1pPriorityMapName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (1..25))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The map name"
    ::=  { rldot1pPriorityMapEntry 1 }

rldot1pPriorityMapPriority OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (8))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The map holding the queue"
    ::=  { rldot1pPriorityMapEntry 2 }

rldot1pPriorityMapPort OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS      read-create
    STATUS      current
    DESCRIPTION
        "the port that the map, is applied on in config"
    ::= { rldot1pPriorityMapEntry 3 }

rldot1pPriorityMapPortList OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS      read-only
    STATUS      current
    DESCRIPTION
        "the ports that the map, is applied on in actual"
    ::= { rldot1pPriorityMapEntry 4 }

rldot1pPriorityMapStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The status of the  table entry. It's used to delete an entry"
    ::= { rldot1pPriorityMapEntry 5 }





rldot1sMstp  OBJECT IDENTIFIER ::= { rlpBridgeMIBObjects 6 }

--
--   The Multiple Spanning Tree Instance Table
--
rldot1sMstpInstanceTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1sMstpInstanceEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
            "A table that contains Mstp instance specific information
            for the Multiple Spanning Tree Protocol."
    ::= { rldot1sMstp 1 }

rldot1sMstpInstanceEntry OBJECT-TYPE
    SYNTAX  Rldot1sMstpInstanceEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every instance
         about the multiple Spanning Tree Protocol state for
         that instance."
    INDEX   { rldot1sMstpInstanceId }
    ::= { rldot1sMstpInstanceTable 1 }

Rldot1sMstpInstanceEntry ::= SEQUENCE {
    rldot1sMstpInstanceId                        INTEGER,
    rldot1sMstpInstanceEnable                    TruthValue,
    rldot1sMstpInstanceTimeSinceTopologyChange   TimeTicks,
    rldot1sMstpInstanceTopChanges                Counter,
    rldot1sMstpInstanceDesignatedRoot            BridgeId,
    rldot1sMstpInstanceRootCost                  INTEGER,
    rldot1sMstpInstanceRootPort                  INTEGER,
    rldot1sMstpInstanceMaxAge                    Timeout,
    rldot1sMstpInstanceHelloTime                 Timeout,
    rldot1sMstpInstanceHoldTime                  INTEGER,
    rldot1sMstpInstanceForwardDelay              Timeout,
    rldot1sMstpInstancePriority                  INTEGER,
    rldot1sMstpInstanceRemainingHopes            INTEGER,
    rldot1sMstpInstanceSwId                      INTEGER
}

rldot1sMstpInstanceId OBJECT-TYPE
    SYNTAX  INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Instance index."
    ::= { rldot1sMstpInstanceEntry 1 }

rldot1sMstpInstanceEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies whether this Instance is STP enable or disable"
    REFERENCE
        " ??  "
    ::= { rldot1sMstpInstanceEntry 2 }

rldot1sMstpInstanceTimeSinceTopologyChange OBJECT-TYPE
    SYNTAX  TimeTicks
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time (in hundredths of a second) since the
         last time a topology change was detected by the
         Mstp Instance ."
    REFERENCE
        "IEEE 802.1D-1990: Section 6.8.1.1.3"
    ::= { rldot1sMstpInstanceEntry 3 }

rldot1sMstpInstanceTopChanges OBJECT-TYPE
    SYNTAX  Counter
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of topology changes detected by
         this Instance since the management entity was last
         reset or initialized."
    REFERENCE
        "IEEE 802.1D-1990: Section 6.8.1.1.3"
    ::= { rldot1sMstpInstanceEntry 4 }

rldot1sMstpInstanceDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the root of the spanning
         tree as determined by the Muliple Spanning Tree Protocol
         as executed by this node.  This value is used as
         the Root Identifier parameter in all Configuration
         Bridge PDUs originated by this node."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.1"
    ::= { rldot1sMstpInstanceEntry 5 }

rldot1sMstpInstanceRootCost OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The cost of the path to the root as seen from
         this bridge."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.2"
    ::= { rldot1sMstpInstanceEntry 6 }

rldot1sMstpInstanceRootPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port which offers the
         lowest cost path from this bridge to the root
         bridge."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.3"
    ::= { rldot1sMstpInstanceEntry 7 }

rldot1sMstpInstanceMaxAge OBJECT-TYPE
    SYNTAX  Timeout
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum age of Spanning Tree Protocol
         information learned from the network on any port
         before it is discarded, in units of hundredths of
         a second.  This is the actual value that this
         bridge is currently using."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.4"
    ::= { rldot1sMstpInstanceEntry 8 }

rldot1sMstpInstanceHelloTime OBJECT-TYPE
    SYNTAX  Timeout
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of
         Configuration bridge PDUs by this node on any port
         when it is the root of the spanning tree or trying
         to become so, in units of hundredths of a second.
         This is the actual value that this bridge is
         currently using."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.5"
    ::= { rldot1sMstpInstanceEntry 9 }

rldot1sMstpInstanceHoldTime OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This time value determines the interval length
         during which no more than two Configuration bridge
         PDUs shall be transmitted by this node, in units
         of hundredths of a second."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.14"
    ::= { rldot1sMstpInstanceEntry 10 }

rldot1sMstpInstanceForwardDelay OBJECT-TYPE
    SYNTAX  Timeout
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This time value, measured in units of hundredths
         of a second, controls how fast a port changes its
         spanning state when moving towards the Forwarding
         state.  The value determines how long the port
         stays in each of the Listening and Learning
         states, which precede the Forwarding state.  This
         value is also used, when a topology change has
         been detected and is underway, to age all dynamic
         entries in the Forwarding Database.  [Note that
         this value is the one that this bridge is
         currently using, in contrast to
         dot1dStpBridgeForwardDelay which is the value that
         this bridge and all others would start using
         if/when this bridge were to become the root.]"
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.6"
    ::= { rldot1sMstpInstanceEntry 11 }

rldot1sMstpInstancePriority OBJECT-TYPE
    SYNTAX  INTEGER (0..61440)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "The value of the write-able portion of the Bridge
            ID, i.e., the first four bits of the first octet
            of the (8 octet long) Bridge ID.The value is a product
            of 4096. The next 12 bit are the msti id .
            The other (last) 6 octets of the Bridge ID are given
            by the value of dot1dBaseBridgeAddress."
    REFERENCE
            "IEEE 802.1S-2001: Section 13.24.2"
    ::= {rldot1sMstpInstanceEntry 12 }

rldot1sMstpInstanceRemainingHopes OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This count value determines the amount of hopes
         the information transmited by this bridge on this
         instance can travel."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.3.14"
    ::= { rldot1sMstpInstanceEntry 13 }

rldot1sMstpInstanceSwId OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The logical Instance Id which is binded for this entry from rldot1sMstpSwInstanceTable."
    ::= { rldot1sMstpInstanceEntry 14 }

--
-- rldot1sMstpInstancePortTable
--
rldot1sMstpInstancePortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1sMstpInstancePortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table that contains pair <msti, port> specific information
         for the Spanning Tree Protocol."
    ::= { rldot1sMstp 2 }

rldot1sMstpInstancePortEntry OBJECT-TYPE
    SYNTAX  Rldot1sMstpInstancePortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every pair <msti, port>
         about the Spanning Tree Protocol state for that pair."
    INDEX   { rldot1sMstpInstancePortMstiId, rldot1sMstpInstancePortPort }
    ::= { rldot1sMstpInstancePortTable 1 }

Rldot1sMstpInstancePortEntry ::= SEQUENCE {
    rldot1sMstpInstancePortMstiId                INTEGER,
    rldot1sMstpInstancePortPort                  INTEGER,
    rldot1sMstpInstancePortPriority              INTEGER,
    rldot1sMstpInstancePortState                 INTEGER,
    rldot1sMstpInstancePortEnable                INTEGER,
    rldot1sMstpInstancePortPathCost              INTEGER,
    rldot1sMstpInstancePortDesignatedRoot        BridgeId,
    rldot1sMstpInstancePortDesignatedCost        INTEGER,
    rldot1sMstpInstancePortDesignatedBridge      BridgeId,
    rldot1sMstpInstancePortDesignatedPort        OCTET STRING,
    rldot1sMstpInstancePortForwardTransitions    Counter,
    rldot1sMStpInstancePortAdminPathCost         INTEGER,
    rldot1sMStpInstancePortRole                  INTEGER

}

rldot1sMstpInstancePortMstiId OBJECT-TYPE
    SYNTAX  INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan group number that the port belongs to, and for which this entry
         contains Spanning Tree Protocol management
         information."
    REFERENCE
         "IEEE 802.1s/D11-2001 "
    ::= { rldot1sMstpInstancePortEntry 1 }

rldot1sMstpInstancePortPort OBJECT-TYPE
    SYNTAX  INTEGER (1..4096)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port for which this entry
         contains Spanning Tree Protocol management
         information."
    REFERENCE
         "IEEE 802.1t/D2-1999: Section 9.2.6"
    ::= { rldot1sMstpInstancePortEntry 2 }

rldot1sMstpInstancePortPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..240)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value of the priority field which is
         contained in the more significant  4 bits of the most
         significant octet of the (2 octet long) Port ID.
         The value is a product of 16.
         The other octet of the Port ID is given by the value
         of rldot1dStpVlanGroupPort."
    REFERENCE
        "IEEE 802.1t/D2-1999: Section 9.2.6"
    ::= { rldot1sMstpInstancePortEntry 3 }

rldot1sMstpInstancePortState OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(1),
        blocking(2),
        listening(3),
        learning(4),
        forwarding(5),
        broken(6)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port's current state as defined by application of
         the Spanning Tree Protocol. This state controls what
         action a port takes on reception of a frame.
         If the bridge has detected a port that is malfunctioning
         it will place that port into the broken(6) state.  For ports
         which are disabled (see dot1dStpVlanPortEnable), this object
         will have a value of disabled(1)."
    REFERENCE
            "IEEE 802.1D-1990: Section 4.5.5.2"
    ::= { rldot1sMstpInstancePortEntry 4 }

rldot1sMstpInstancePortEnable OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The enabled/disabled status of the port."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.2"
    ::= { rldot1sMstpInstancePortEntry 5 }

rldot1sMstpInstancePortPathCost OBJECT-TYPE
    SYNTAX  INTEGER (1..200000000)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The contribution of this port to the path cost of
         paths towards the spanning tree root which include
         this port.  802.1D-1990 recommends that the
         default value of this parameter be in inverse
         proportion to the speed of the attached LAN."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.3"
    ::= { rldot1sMstpInstancePortEntry 6 }

rldot1sMstpInstancePortDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The unique Bridge Identifier of the Bridge
         recorded as the Root in the Configuration BPDUs
         transmitted by the Designated Bridge for the
         segment to which the port is attached."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.4"
    ::= { rldot1sMstpInstancePortEntry 7 }

rldot1sMstpInstancePortDesignatedCost OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The path cost of the Designated Port of the
         segment connected to this port.  This value is
         compared to the Root Path Cost field in received
         bridge PDUs."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.5"
    ::= { rldot1sMstpInstancePortEntry 8 }

rldot1sMstpInstancePortDesignatedBridge OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Bridge Identifier of the bridge which this
         port considers to be the Designated Bridge for
         this port's segment."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.6"
    ::= { rldot1sMstpInstancePortEntry 9 }

rldot1sMstpInstancePortDesignatedPort OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Port Identifier of the port on the Designated
         Bridge for this port's segment."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.7"
    ::= { rldot1sMstpInstancePortEntry 10 }

rldot1sMstpInstancePortForwardTransitions OBJECT-TYPE
    SYNTAX  Counter
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of times this port has transitioned
         from the Learning state to the Forwarding state."
    ::= { rldot1sMstpInstancePortEntry 11 }

rldot1sMStpInstancePortAdminPathCost OBJECT-TYPE
    SYNTAX      INTEGER (0..200000000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The administratively assigned value for the contribution
         of this port to the path cost of paths towards the spanning
         tree root.

         Writing a value of '0' assigns the automatically calculated
         default Path Cost value to the port.  If the default Path
         Cost is being used, this object returns '0' when read.

         This complements the object dot1dStpPortPathCost, which
         returns the operational value of the path cost."
    REFERENCE
        "IEEE 802.1D-1998: Section 8.5.5.3"
    ::= { rldot1sMstpInstancePortEntry 12 }

rldot1sMStpInstancePortRole OBJECT-TYPE
    SYNTAX  INTEGER {
                    unknown(0),
                    disabled(1),
                    alternate(2),
                    backup(3),
                    root(4),
                    designated(5),
                    master(6)
                }

    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specify the role of this this port."
    REFERENCE
        ""
    ::= { rldot1sMstpInstancePortEntry 13 }

rldot1sMstpMaxHopes OBJECT-TYPE
    SYNTAX  INTEGER (1..40)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Max number of hopes that an MST BPDU will travel inside a region."
    DEFVAL { 20 }
    ::= { rldot1sMstp 3 }

rldot1sMstpConfigurationName OBJECT-TYPE
    SYNTAX  SnmpAdminString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The active configuration name as will be caried in MST BPDU's."
    ::= { rldot1sMstp 4 }

rldot1sMstpRevisionLevel OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The active revision level."
    DEFVAL { 0 }
    ::= { rldot1sMstp 5 }

--
-- rldot1sMstpVlanTable
--
rldot1sMstpVlanTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1sMstpVlanEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table that contains information about the alocation of vlans to groups."
    ::= { rldot1sMstp 6 }

rldot1sMstpVlanEntry OBJECT-TYPE
    SYNTAX  Rldot1sMstpVlanEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every vlan
         about the group it belongs to."
    INDEX   { rldot1sMstpVlan }
    ::= { rldot1sMstpVlanTable 1 }

Rldot1sMstpVlanEntry ::= SEQUENCE {
      rldot1sMstpVlan              INTEGER,
      rldot1sMstpGroup             INTEGER,
      rldot1sMstpPendingGroup      INTEGER
}

rldot1sMstpVlan OBJECT-TYPE
    SYNTAX  INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The vlan number of the vlan for which this entry
         contains Spanning Tree Protocol management
         information."
    REFERENCE
         "IEEE 802.1s/D11-2001: Section 13.7"
    ::= { rldot1sMstpVlanEntry 1 }

rldot1sMstpGroup OBJECT-TYPE
    SYNTAX  INTEGER (0..4094)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifid the active group number this vlan belonges to."
    REFERENCE
        ""
    DEFVAL { 0 }
    ::= { rldot1sMstpVlanEntry 2 }

rldot1sMstpPendingGroup OBJECT-TYPE
    SYNTAX  INTEGER (0..4094)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifid the pending group number this vlan belonges to."
    REFERENCE
        ""
    DEFVAL { 0 }
    ::= { rldot1sMstpVlanEntry 3 }

--
-- rldot1sMstpExtPortTable
--
rldot1sMstpExtPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Rldot1sMstpExtPortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table that contains MSTP information about ports of the CIST."
    ::= { rldot1sMstp 7 }

rldot1sMstpExtPortEntry OBJECT-TYPE
SYNTAX  Rldot1sMstpExtPortEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of information maintained by every port
         of the CIST."
    INDEX   { rldot1sMstpExtPortPort }
    ::= { rldot1sMstpExtPortTable 1 }

Rldot1sMstpExtPortEntry ::= SEQUENCE {
      rldot1sMstpExtPortPort                   INTEGER,
      rldot1sMstpExtPortInternalOperPathCost   INTEGER,
      rldot1sMstpExtPortDesignatedRegionalRoot BridgeId,
      rldot1sMstpExtPortDesignatedRegionalCost INTEGER,
      rldot1sMstpExtPortBoundary               TruthValue,
      rldot1sMstpExtPortInternalAdminPathCost  INTEGER

}
rldot1sMstpExtPortPort OBJECT-TYPE
    SYNTAX  INTEGER (1..4096)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port for which this entry
         contains Spanning Tree Protocol management
         information."
    REFERENCE
         "IEEE 802.1t/D2-1999: Section 9.2.6"
    ::= { rldot1sMstpExtPortEntry 1 }

rldot1sMstpExtPortInternalOperPathCost OBJECT-TYPE
    SYNTAX  INTEGER (1..200000000)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The contribution of this port to the path cost of
         paths towards the spanning tree regional root which
         include this port.  802.1S-2002 recommends that the
         default value of this parameter be in inverse
         proportion to the speed of the attached LAN."
    ::= { rldot1sMstpExtPortEntry 2 }

rldot1sMstpExtPortDesignatedRegionalRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The unique Bridge Identifier of the Bridge
         recorded as the Root in the Configuration BPDUs
         transmitted by the Designated Bridge for the
         segment to which the port is attached."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.4"
    ::= { rldot1sMstpExtPortEntry 3 }

rldot1sMstpExtPortDesignatedRegionalCost OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The regional path cost of the Designated Port of the
         segment connected to this port.  This value is
         compared to the Root Path Cost field in received
         bridge PDUs."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.5"
    ::= { rldot1sMstpExtPortEntry 4 }

rldot1sMstpExtPortBoundary OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indication if the port is conented to to a lan segment
         outside or inside the region."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.5"
    ::= { rldot1sMstpExtPortEntry 5 }

rldot1sMstpExtPortInternalAdminPathCost OBJECT-TYPE
    SYNTAX  INTEGER (0..200000000)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The administratively assigned value for the contribution
         of this port to the path cost of paths towards the spanning
         tree root.

         Writing a value of '0' assigns the automatically calculated
         default Path Cost value to the port.  If the default Path
         Cost is being used, this object returns '0' when read.

         This complements the object dot1dStpPortPathCost, which
         returns the operational value of the path cost."

    ::= { rldot1sMstpExtPortEntry 6 }

rldot1sMstpDesignatedMaxHopes OBJECT-TYPE
    SYNTAX  INTEGER (1..40)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Max number of hopes that an MST BPDU will travel inside a region."
    ::= { rldot1sMstp 8 }

rldot1sMstpRegionalRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
            "CIST Regional Root Identifier (13.16.4).
            The Bridge Identifier of the current CIST Regional Root."
    REFERENCE
            "IEEE 802.1S-2002: Section 13.16.4"
    ::= { rldot1sMstp 9 }

rldot1sMstpRegionalRootCost OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
            "The CIST path cost from the transmitting Bridge to the
            CIST Regional Root."
    REFERENCE
            "IEEE 802.1S-2002: Section 12.8.1.1.3"
    ::= { rldot1sMstp 10 }

rldot1sMstpPendingConfigurationName OBJECT-TYPE
    SYNTAX  SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The pending configuration name."
    ::= { rldot1sMstp 11 }

rldot1sMstpPendingRevisionLevel OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The pending revision level."
    DEFVAL { 0 }
    ::= { rldot1sMstp 12 }

rldot1sMstpPendingAction OBJECT-TYPE
    SYNTAX  INTEGER {
        copyPendingActive(1),
        copyActivePending(2)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The action to be done with the pending configuration.
         copyPendingActive - to copy the pending mst configuration to the active one.
         copyActivePending - to copy the active mst configuration to the pending one. "
    ::= { rldot1sMstp 13 }

rldot1sMstpRemainingHops OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This count value determines the amount of hops
         the information transmitted by this bridge can travel."
    ::= { rldot1sMstp 14 }

--
-- rldot1sMstpInstanceVlanTable
--
rldot1sMstpInstanceVlanTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Rldot1sMstpInstanceVlanEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table contains vlan lists per MSTP instances."
    ::= { rldot1sMstp 15 }

rldot1sMstpInstanceVlanEntry OBJECT-TYPE
    SYNTAX Rldot1sMstpInstanceVlanEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        " The entry contains vlan lists per specific MSTP instance."
    INDEX { rldot1sMstpInstanceVlanId, rldot1sMstpInstanceVlanDbType }
    ::= { rldot1sMstpInstanceVlanTable 1 }

Rldot1sMstpInstanceVlanEntry::= SEQUENCE {
        rldot1sMstpInstanceVlanId             INTEGER,
        rldot1sMstpInstanceVlanDbType         INTEGER,
        rldot1sMstpInstanceVlanId1To1024      VlanList1,
        rldot1sMstpInstanceVlanId1025To2048   VlanList2,
        rldot1sMstpInstanceVlanId2049To3072   VlanList3,
        rldot1sMstpInstanceVlanId3073To4094   VlanList4
    }

rldot1sMstpInstanceVlanId OBJECT-TYPE
    SYNTAX  INTEGER (0..4094)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifiy the instance number."
    ::= { rldot1sMstpInstanceVlanEntry 1 }

rldot1sMstpInstanceVlanDbType OBJECT-TYPE
    SYNTAX  INTEGER {
        active(1),
        pending(2)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifiy which data-base to access: active or pending."
    ::= { rldot1sMstpInstanceVlanEntry 2 }

rldot1sMstpInstanceVlanId1To1024 OBJECT-TYPE
    SYNTAX  VlanList1
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "first VlanId List of specific MSTP instance."
    ::= { rldot1sMstpInstanceVlanEntry 3 }

rldot1sMstpInstanceVlanId1025To2048 OBJECT-TYPE
    SYNTAX  VlanList2
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "second VlanId List of specific MSTP instance."
    ::= { rldot1sMstpInstanceVlanEntry 4 }

rldot1sMstpInstanceVlanId2049To3072 OBJECT-TYPE
    SYNTAX  VlanList3
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "third VlanId List of specific MSTP instance."
    ::= { rldot1sMstpInstanceVlanEntry 5 }

rldot1sMstpInstanceVlanId3073To4094 OBJECT-TYPE
    SYNTAX  VlanList4
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "fourth VlanId List of specific MSTP instance."
    ::= { rldot1sMstpInstanceVlanEntry 6 }


--
-- rldot1sMstpSwInstanceTable
--


rldot1sMstpSwInstanceTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Rldot1sMstpSwInstanceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table contains logical instance to rldot1sMstpInstanceId mapping."
    ::= { rldot1sMstp 18 }

rldot1sMstpSwInstanceEntry OBJECT-TYPE
    SYNTAX Rldot1sMstpSwInstanceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The entry contains logical instance information."
    INDEX { rldot1sMstpSwInstanceSwId}
    ::= { rldot1sMstpSwInstanceTable 1 }

Rldot1sMstpSwInstanceEntry::= SEQUENCE {
        rldot1sMstpSwInstanceSwId           INTEGER,
        rldot1sMstpSwInstanceId             INTEGER,
        rldot1sMstpSwInstanceStatus         RowStatus
    }

rldot1sMstpSwInstanceSwId OBJECT-TYPE
    SYNTAX  INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The STP Instance logical index."
    ::= { rldot1sMstpSwInstanceEntry 1 }

rldot1sMstpSwInstanceId OBJECT-TYPE
    SYNTAX  INTEGER (1..64)
    MAX-ACCESS read-only
    STATUS  current
    DESCRIPTION
        "The STP Instance index rldot1sMstpInstanceId which exist at rldot1sMstpInstanceTable."
    ::= { rldot1sMstpSwInstanceEntry 2 }


rldot1sMstpSwInstanceStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The status of the entry, used to add, delete or update an entry"
   ::= { rldot1sMstpSwInstanceEntry 3 }



--
-- rldot1sMstpPendingInstanceVlanTable
--

--rldot1sMstpPendingInstanceVlanTable OBJECT-TYPE
--     SYNTAX SEQUENCE OF Rldot1sMstpPendingInstanceVlanEntry
--    MAX-ACCESS not-accessible
--    STATUS current
--     DESCRIPTION
--        "This table contains vlan lists per MSTP instances."
--    ::= { rldot1sMstp 16 }
--
--rldot1sMstpPendingInstanceVlanEntry OBJECT-TYPE
--    SYNTAX Rldot1sMstpPendingInstanceVlanEntry
--    MAX-ACCESS not-accessible
--    STATUS current
--    DESCRIPTION
--        "The entry contains vlan lists per specific MSTP instance."
--    INDEX { rldot1sMstpPendingInstanceVlanId }
--    ::= { rldot1sMstpPendingInstanceVlanTable 1 }
--
--Rldot1sMstpPendingInstanceVlanEntry::= SEQUENCE {
--        rldot1sMstpPendingInstanceVlanId             INTEGER,
--        rldot1sMstpPendingInstanceVlanId1To1024      VlanList1,
--        rldot1sMstpPendingInstanceVlanId1025To2048   VlanList2,
--        rldot1sMstpPendingInstanceVlanId2049To3072   VlanList3,
--        rldot1sMstpPendingInstanceVlanId3073To4094   VlanList4,
--            rldot1sMstpPendingInstanceVlanStatus         RowStatus
--    }
--
--rldot1sMstpPendingInstanceVlanId OBJECT-TYPE
--    SYNTAX  INTEGER (0..4094)
--    MAX-ACCESS  read-only
--    STATUS  current
--    DESCRIPTION
--        "Specifiy the instance number."
--    ::= { rldot1sMstpPendingInstanceVlanEntry 1 }
--
--rldot1sMstpPendingInstanceVlanId1To1024 OBJECT-TYPE
--    SYNTAX  VlanList1
--    MAX-ACCESS  read-write
--    STATUS  current
--    DESCRIPTION
--        "first VlanId List of specific MSTP instance."
--    ::= { rldot1sMstpPendingInstanceVlanEntry 2 }
--
--rldot1sMstpPendingInstanceVlanId1025To2048 OBJECT-TYPE
--    SYNTAX  VlanList2
--    MAX-ACCESS  read-write
--    STATUS  current
--    DESCRIPTION
--        "second VlanId List of specific MSTP instance."
--    ::= { rldot1sMstpPendingInstanceVlanEntry 3 }
--
--rldot1sMstpPendingInstanceVlanId2049To3072 OBJECT-TYPE
--    SYNTAX  VlanList3
--    MAX-ACCESS  read-write
--    STATUS  current
--    DESCRIPTION
--        "third VlanId List of specific MSTP instance."
--    ::= { rldot1sMstpPendingInstanceVlanEntry 4 }
--
--rldot1sMstpPendingInstanceVlanId3073To4094 OBJECT-TYPE
--    SYNTAX  VlanList4
--    MAX-ACCESS  read-write
--    STATUS  current
--    DESCRIPTION
--        "fourth VlanId List of specific MSTP instance."
--    ::= { rldot1sMstpPendingInstanceVlanEntry 5 }
--
--
--rldot1sMstpPendingInstanceVlanStatus OBJECT-TYPE
--    SYNTAX  RowStatus
--    MAX-ACCESS  read-create
--    STATUS  current
--    DESCRIPTION
--        "The status of the table entry, used to add, delete or update an entry, when logical mstp IDs are supported,
--                 Otherwise field value must be Active"
--        DEFVAL {active }
--   ::= { rldot1sMstpPendingInstanceVlanEntry 6 }

rldot1dTpAgingTime  OBJECT IDENTIFIER ::= { rlpBridgeMIBObjects 7 }

rldot1dTpAgingTimeMin OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The min timeout period in seconds for aging out
         dynamically learned forwarding information."
    REFERENCE
        "P802.1d/D9, July 14, 1989: Section 6.7.1.1.3"
    ::= { rldot1dTpAgingTime 1 }

rldot1dTpAgingTimeMax OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The max timeout period in seconds for aging out
         dynamically learned forwarding information."
    REFERENCE
        "P802.1d/D9, July 14, 1989: Section 6.7.1.1.3"
    ::= { rldot1dTpAgingTime 2 }

rldot1sMstpConfigurationDigest OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(16))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The active configuration digest."
    ::= { rldot1sMstp 16 }

rldot1sMstpPendingConfigurationDigest OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(16))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The pending configuration digest."
    ::= { rldot1sMstp 17 }

--
-- PerVlan SpaningTree MIBs
--
-- rlBrgPvst
-- rlBrgPvstVlanTable, rlBrgPvstPortTable
--

rlBrgPvst  OBJECT IDENTIFIER ::= { rlpBridgeMIBObjects 9 }

-- rlBrgPvstVlanTable

rlBrgPvstVlanTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlBrgPvstVlanEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table contains Per Vlan Spanning-Tree vlan configuration."
    ::= { rlBrgPvst 1 }

rlBrgPvstVlanEntry OBJECT-TYPE
    SYNTAX RlBrgPvstVlanEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The entry contains PVST configuration per specific Vlan."
    INDEX { rlBrgPvstVlanId }
    ::= { rlBrgPvstVlanTable 1 }

RlBrgPvstVlanEntry ::= SEQUENCE {
        rlBrgPvstVlanId                INTEGER,
        rlBrgPvstVlanHelloTime         INTEGER,
        rlBrgPvstVlanForwardDelay      INTEGER,
        rlBrgPvstVlanMaxAge            INTEGER,
        rlBrgPvstVlanPriority          INTEGER,
        rlBrgPvstVlanStatus            RowStatus
    }

rlBrgPvstVlanId OBJECT-TYPE
    SYNTAX  INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan number for this entry which contains PVST configuration."
    ::= { rlBrgPvstVlanEntry 1 }

rlBrgPvstVlanHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
         "The time intervals in seconds for the transmission of
          Configuration PVST bridge PDUs by this node on any port
          when it is the root of the spanning tree or trying
          to become so.
          When configuring the Hello time, the following relationship
          should be maintained:
            Max-Age >= 2*(Hello-Time + 1)."
    DEFVAL { 2 }
    ::= { rlBrgPvstVlanEntry 2 }

rlBrgPvstVlanForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER (4..30)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The time interval in seconds, controls how fast a port changes its
         spanning state when moving towards the Forwarding
         state.  The value determines how long the port
         stays in each of the Listening and Learning
         states, which precede the Forwarding state.
         When configuring the forwarding time, the following relationship
         should be maintained:
            2*(Forward-Time - 1) >= Max-Age."
    DEFVAL { 4 }
    ::= { rlBrgPvstVlanEntry 3 }

rlBrgPvstVlanMaxAge OBJECT-TYPE
    SYNTAX  INTEGER (6..40)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
         "The maximum age time in seconds of PVST Protocol information learned
         from the network on any port before it is discarded.
         When configuring the maximum age, the following relationships
         should be maintained:
            2*(Forward-Time - 1) >= Max-Age
            Max-Age >= 2*(Hello-Time + 1)."
    DEFVAL { 15 }
    ::= { rlBrgPvstVlanEntry 4 }

rlBrgPvstVlanPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..61440)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
         "The value of the write-able portion of the Bridge
            ID, i.e., the first four bits of the first octet
            of the (8 octet long) Bridge ID. The value is a product of 4096."
    DEFVAL { 32768 }
    ::= { rlBrgPvstVlanEntry 5 }

rlBrgPvstVlanStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The status of the  table entry, used to add, delete or update an entry"
    ::= { rlBrgPvstVlanEntry 6 }


-- rlBrgPvstOperVlanTable

rlBrgPvstOperVlanTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlBrgPvstOperVlanEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table contains Per Vlan Spanning-Tree active vlan configuration."
    ::= { rlBrgPvst 2 }

rlBrgPvstOperVlanEntry OBJECT-TYPE
    SYNTAX RlBrgPvstOperVlanEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The entry contains PVST active configuration per specific Vlan."
    INDEX { rlBrgPvstOperVlanId }
    ::= { rlBrgPvstOperVlanTable 1 }

RlBrgPvstOperVlanEntry ::= SEQUENCE {
        rlBrgPvstOperVlanId                         INTEGER,
        rlBrgPvstOperVlanEnable                     TruthValue,
        rlBrgPvstOperVlanTimeSinceTopologyChange    TimeTicks,
        rlBrgPvstOperVlanTopChanges                 Counter,
        rlBrgPvstOperVlanDesignatedRoot             BridgeId,
        rlBrgPvstOperVlanRootCost                   INTEGER,
        rlBrgPvstOperVlanRootPort                   INTEGER,
        rlBrgPvstOperVlanRootMaxAge                 INTEGER,
        rlBrgPvstOperVlanRootHelloTime              INTEGER,
        rlBrgPvstOperVlanRootForwardDelay           INTEGER,
        rlBrgPvstOperVlanMaxAge                     INTEGER,
        rlBrgPvstOperVlanHelloTime                  INTEGER,
        rlBrgPvstOperVlanForwardDelay               INTEGER,
--      rlBrgPvstOperVlanHoldTime                   INTEGER,
        rlBrgPvstOperVlanPriority                   INTEGER
    }

rlBrgPvstOperVlanId OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan number for this entry which contains PVST active configuration."
    ::= { rlBrgPvstOperVlanEntry 1 }

rlBrgPvstOperVlanEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates whether this Vlan is enabled for PVST / RPVST."
    ::= { rlBrgPvstOperVlanEntry 2 }

rlBrgPvstOperVlanTimeSinceTopologyChange OBJECT-TYPE
    SYNTAX  TimeTicks
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time (in miliseconds) since the
         last time a topology change was detected on current PVST Instance."
    ::= { rlBrgPvstOperVlanEntry 3 }

rlBrgPvstOperVlanTopChanges OBJECT-TYPE
    SYNTAX  Counter
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of topology changes detected by
         this on current PVST Instance since the management entity was last
         reset or initialized."
    ::= { rlBrgPvstOperVlanEntry 4 }

rlBrgPvstOperVlanDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the root of the spanning
         tree as determined by the PVST Spanning Tree Protocol
         as executed by this node. This value is used as
         the Root Identifier parameter in all Configuration
         Bridge PDUs originated by this node."
    ::= { rlBrgPvstOperVlanEntry 5 }

rlBrgPvstOperVlanRootCost OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The cost of the path to the root as seen from
         current bridge on current vlan."
    ::= { rlBrgPvstOperVlanEntry 6 }

rlBrgPvstOperVlanRootPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port which offers the
         lowest cost path from this bridge to the root bridge."
    ::= { rlBrgPvstOperVlanEntry 7 }

rlBrgPvstOperVlanRootMaxAge OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
         "The rlBrgPvstVlanMaxAge which recieved from the root of current
          PVST instance."
    ::= { rlBrgPvstOperVlanEntry 8 }

rlBrgPvstOperVlanRootHelloTime OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
         "The rlBrgPvstVlanHelloTime which recieved from the root of current
          PVST instance."
    ::= { rlBrgPvstOperVlanEntry 9 }

rlBrgPvstOperVlanRootForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
         "The rlBrgPvstVlanForwardDelay which recieved from the root of current
          PVST instance."
    ::= { rlBrgPvstOperVlanEntry 10 }

rlBrgPvstOperVlanMaxAge OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
         "The operational maximum age time in seconds of PVST Protocol information learned
         from the network on any port before it is discarded.
         When configuring the maximum age, the following relationships
         should be maintained:
            2*(Forward-Time - 1) >= Max-Age
            Max-Age >= 2*(Hello-Time + 1)."
    ::= { rlBrgPvstOperVlanEntry 11 }

rlBrgPvstOperVlanHelloTime OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
         "The operational time intervals in seconds for the transmission of
          Configuration PVST bridge PDUs by this node on any port
          when it is the root of the spanning tree or trying
          to become so.
          When configuring the Hello time, the following relationship
          should be maintained:
            Max-Age >= 2*(Hello-Time + 1)."
    ::= { rlBrgPvstOperVlanEntry 12 }

rlBrgPvstOperVlanForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The operational time interval in seconds, controls how fast a port changes its
         spanning state when moving towards the Forwarding
         state.  The value determines how long the port
         stays in each of the Listening and Learning
         states, which precede the Forwarding state.
         When configuring the forwarding time, the following relationship
         should be maintained:
            2*(Forward-Time - 1) >= Max-Age."
    ::= { rlBrgPvstOperVlanEntry 13 }

rlBrgPvstOperVlanPriority OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
         "The value of the write-able portion of the Bridge
          ID, i.e., the first four bits of the first octet
          of the (8 octet long) Bridge ID. The value is a product of 4096."
    ::= { rlBrgPvstOperVlanEntry 14 }

-- rlBrgPvstPortTable

rlBrgPvstPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlBrgPvstPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table contains Per Vlan Spanning-Tree Port configuration."
    ::= { rlBrgPvst 3 }

rlBrgPvstPortEntry OBJECT-TYPE
    SYNTAX RlBrgPvstPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The entry contains PVST configuration per specific Vlan and Port."
    INDEX { rlBrgPvstPortVlanId, rlBrgPvstPortPort }
    ::= { rlBrgPvstPortTable 1 }

RlBrgPvstPortEntry ::= SEQUENCE {
        rlBrgPvstPortVlanId            INTEGER,
        rlBrgPvstPortPort              INTEGER,
        rlBrgPvstPortPathCost          INTEGER,
        rlBrgPvstPortPriority          INTEGER,
        rlBrgPvstPortStatus            RowStatus
    }

rlBrgPvstPortVlanId OBJECT-TYPE
    SYNTAX  INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan number for this entry which contains PVST configuration."
    ::= { rlBrgPvstPortEntry 1 }

rlBrgPvstPortPort OBJECT-TYPE
    SYNTAX  INTEGER (1..4096)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port for which this entry
         contains Per Vlan Spanning Tree Protocol management
         information."
    ::= { rlBrgPvstPortEntry 2 }

rlBrgPvstPortPathCost OBJECT-TYPE
    SYNTAX  INTEGER (0..200000000)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The contribution of this port to the path cost of
         paths towards the spanning tree root which include
         this port.
         Writing a value of '0' assigns the automatically calculated
         default Path Cost value to the port.  If the default Path
         Cost is being used, this object returns '0' when read.
         Default path cost is determined by port speed and path cost method (long or short)."
    ::= { rlBrgPvstPortEntry 3 }

rlBrgPvstPortPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..240)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The Admin value of the priority field which is
         contained in the more significant 4 bits of the most
         significant octet of the (2 octet long) Port ID.
         The other octet of the Port ID is given by the value
         of rlBrgPvstPortPort.
         The priority value must be a multiple of 16."
    DEFVAL { 128 }
    ::= { rlBrgPvstPortEntry 4 }

rlBrgPvstPortStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The status of the  table entry, used to add, delete or update an entry"
    ::= { rlBrgPvstPortEntry 5 }

-- rlBrgPvstOperPortTable

rlBrgPvstOperPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlBrgPvstOperPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table contains Per Vlan Spanning-Tree active Port configuration."
    ::= { rlBrgPvst 4 }

rlBrgPvstOperPortEntry OBJECT-TYPE
    SYNTAX RlBrgPvstOperPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The entry contains PVST active configuration per specific Vlan and Port."
    INDEX { rlBrgPvstOperPortVlanId, rlBrgPvstOperPortPort }
    ::= { rlBrgPvstOperPortTable 1 }

RlBrgPvstOperPortEntry ::= SEQUENCE {
        rlBrgPvstOperPortVlanId             INTEGER,
        rlBrgPvstOperPortPort               INTEGER,
        rlBrgPvstOperPortEnable             TruthValue,
        rlBrgPvstOperPortPathCost           INTEGER,
        rlBrgPvstOperPortPriority           INTEGER,
        rlBrgPvstOperPortState              INTEGER,
        rlBrgPvstOperPortRole               INTEGER,
        rlBrgPvstOperPortBpduType           INTEGER,
        rlBrgPvstOperPortDesignatedRoot     BridgeId,
        rlBrgPvstOperPortDesignatedCost     INTEGER,
        rlBrgPvstOperPortDesignatedBridge   BridgeId,
        rlBrgPvstOperPortDesignatedPort     OCTET STRING,
        rlBrgPvstOperPortForwardTransitions Counter32,
        rlBrgPvstOperPortEdgePort           TruthValue,
        rlBrgPvstOperPortBpduSent           Counter32,
        rlBrgPvstOperPortBpduReceived       Counter32
    }

rlBrgPvstOperPortVlanId OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan number for this entry which contains PVST configuration."
    ::= { rlBrgPvstOperPortEntry 1 }

rlBrgPvstOperPortPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port for which this entry
         contains Per Vlan Spanning Tree Protocol management
         information."
    ::= { rlBrgPvstOperPortEntry 2 }

rlBrgPvstOperPortEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The enabled/disabled status of the port."
    ::= { rlBrgPvstOperPortEntry 3 }

rlBrgPvstOperPortPathCost OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Operational contribution of this port to the path cost of
         paths towards the spanning tree root which include
         this port.
         Default path cost is determined by port speed and path cost method
         (long or short)."
    ::= { rlBrgPvstOperPortEntry 4 }

rlBrgPvstOperPortPriority OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Operational value of the priority field which is
         contained in the more significant 4 bits of the most
         significant octet of the (2 octet long) Port ID.
         The other octet of the Port ID is given by the value
         of rlBrgPvstOperPortPort."
    ::= { rlBrgPvstOperPortEntry 5 }

rlBrgPvstOperPortState OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled  (1),
        blocking  (2),
        listening (3),
        learning  (4),
        forwarding(5),
        broken    (6)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port's current state as defined by application of
         the Spanning Tree Protocol. This state controls what
         action a port takes on reception of a frame.
         If the bridge has detected a port that is malfunctioning
         it will place that port into the broken(6)state."
    ::= { rlBrgPvstOperPortEntry 6 }

rlBrgPvstOperPortRole OBJECT-TYPE
    SYNTAX  INTEGER {
        unknown    (0),
        disabled   (1),
        alternate  (2),
        backup     (3),
        root       (4),
        designated (5)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specify the STP role of this this port."
    ::= { rlBrgPvstOperPortEntry 7 }

rlBrgPvstOperPortBpduType OBJECT-TYPE
    SYNTAX  INTEGER {
        pvst (2),
        rpvst(3)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified the type of BPDU transmitted by this port."
    ::= { rlBrgPvstOperPortEntry 8 }

rlBrgPvstOperPortDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the root of the spanning
         tree as determined by the Spanning Tree Protocol
         as executed by this node. This value is used as
         the Root Identifier parameter in all Configuration
         Bridge PDUs originated by this node."
    ::= { rlBrgPvstOperPortEntry 9 }

rlBrgPvstOperPortDesignatedCost OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The path cost of the Designated Port of the
         segment connected to this port.  This value is
         compared to the Root Path Cost field in received
         bridge PDUs."
    ::= { rlBrgPvstOperPortEntry 10 }

rlBrgPvstOperPortDesignatedBridge OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Bridge Identifier of the bridge which this
         port considers to be the Designated Bridge for
         this port's segment."
    REFERENCE
        "IEEE 802.1D-1990: Section 4.5.5.6"
    ::= { rlBrgPvstOperPortEntry 11 }

rlBrgPvstOperPortDesignatedPort OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Port Identifier of the port on the Designated
         Bridge for this port's segment."
    ::= { rlBrgPvstOperPortEntry 12 }

rlBrgPvstOperPortForwardTransitions OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of times this port has transitioned
         from the Learning state to the Forwarding state."
    ::= { rlBrgPvstOperPortEntry 13 }

rlBrgPvstOperPortEdgePort OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational value of the Edge Port parameter.  The
         object is initialized to the value of
         dot1dStpPortAdminEdgePort and is set FALSE on reception of
         a BPDU."
    REFERENCE
        "IEEE 802.1t clause 14.8.2, 18.3.4"
    ::= { rlBrgPvstOperPortEntry 14 }

rlBrgPvstOperPortBpduSent OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified the number of bpdu sent from this port."
    ::= { rlBrgPvstOperPortEntry 15 }

rlBrgPvstOperPortBpduReceived OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specified the number of bpdu received in this port."
    ::= { rlBrgPvstOperPortEntry 16 }

-- rlBrgPvstInconsistencyPortTable

rlBrgPvstInconsistencyPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlBrgPvstInconsistencyPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table contains Per Vlan Spanning-Tree Ports Inconsistency
         information."
    ::= { rlBrgPvst 5 }

rlBrgPvstInconsistencyPortEntry OBJECT-TYPE
    SYNTAX RlBrgPvstInconsistencyPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Entry contains Per Vlan Spanning-Tree Port Inconsistency information."
    INDEX { rlBrgPvstInconsistencyVlanId, rlBrgPvstInconsistencyPort}
    ::= { rlBrgPvstInconsistencyPortTable 1 }

RlBrgPvstInconsistencyPortEntry ::= SEQUENCE {
        rlBrgPvstInconsistencyVlanId   INTEGER,
        rlBrgPvstInconsistencyPort     INTEGER,
        rlBrgPvstInconsistencyState    BITS
    }

rlBrgPvstInconsistencyVlanId OBJECT-TYPE
    SYNTAX  INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Vlan number for this entry which contains PVST Port Inconsistency
         information."
    ::= { rlBrgPvstInconsistencyPortEntry 1 }

rlBrgPvstInconsistencyPort OBJECT-TYPE
    SYNTAX  INTEGER (1..4096)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port for which this entry
         contains Per Vlan Spanning Tree Port Inconsistency information."
    ::= { rlBrgPvstInconsistencyPortEntry 2 }


rlBrgPvstInconsistencyState OBJECT-TYPE
    SYNTAX BITS {
                type(0), -- a port-type inconsistency
                pvid(1)  -- a PVID inconsistency
           }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port PVST Inconsistency state."
    ::= { rlBrgPvstInconsistencyPortEntry 3 }

END

