RADLAN-WBA-MIB DEFINITIONS ::= BEGIN

IMPORTS
    rnd                                             FROM RADLAN-MIB
    InetAddressType,InetAddress,InetAddressIPv6     FROM INET-ADDRESS-MIB -- RFC2851
    SnmpAdminString                                 FROM SNMP-FRAMEWORK-MIB
    TEXTUAL-CONVENTION, DisplayString,MacAddress    FROM SNMPv2-TC
    OBJECT-TYPE                                     FROM SNMPv2-SMI;


rlWBA   MODULE-IDENTITY
        LAST-UPDATED "201007050000Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
                "The private MIB module definition for Web Based Authentication."
        REVISION "201007050000Z"
        DESCRIPTION
                "Added this MODULE-IDENTITY clause."
        ::= { rnd 230 }

RlWBAStatusType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "The host(mac,ifindex) authentication status"
     SYNTAX INTEGER {
            unknown(0),
            inProcess(1),
            failAuthen(2),
            pending(3),
            authenticating(4),
            authenticated(5),
            waitAck(6)
     }

RlWBARetryFlagOp ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "The retry flag options"
     SYNTAX INTEGER {
            off(0),
            on(1)
     }

rlWBAAuxiliaryTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlWBAAuxiliaryEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION        "The table is an auxiliary table with 1 entry only. Used
                       to pass user credentials to authentication manager and provide
                       the users' authentication status."
   ::= { rlWBA 1 }

rlWBAAuxiliaryEntry OBJECT-TYPE
    SYNTAX  RlWBAAuxiliaryEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The row definition for this table."
    INDEX { rlWBAIp }
    ::= { rlWBAAuxiliaryTable 1 }

RlWBAAuxiliaryEntry ::= SEQUENCE {
    rlWBAIp                 InetAddress,
    rlWBAStatus             RlWBAStatusType,
    rlAuxFailReason         INTEGER,
    rlIsRetryFlag           RlWBARetryFlagOp,
    rlWBAUsername           DisplayString,
    rlWBAPassword           DisplayString
}


rlWBAIp OBJECT-TYPE
   SYNTAX InetAddress
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION       "User remote IP address."
   ::= { rlWBAAuxiliaryEntry 1 }

rlWBAStatus OBJECT-TYPE
    SYNTAX  RlWBAStatusType
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The host authentication status."
    ::= { rlWBAAuxiliaryEntry 2 }

rlAuxFailReason OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION    "Web Based Authentication fail reason"

   ::= { rlWBAAuxiliaryEntry 3 }

rlIsRetryFlag OBJECT-TYPE
    SYNTAX  RlWBARetryFlagOp
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION    "Web Based Authentication retry flag.
                    If flag is on it means the host that started authentication process was out
                    due to higher priority session. The host must retry authenticating until higher session
                    is accepted/failed. The default value is OFF"
    DEFVAL{ off }
   ::= { rlWBAAuxiliaryEntry 4 }

rlWBAUsername OBJECT-TYPE
   SYNTAX DisplayString (SIZE(0..32))
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION       "Web Based Authentication User Name"
   ::= { rlWBAAuxiliaryEntry 5 }

rlWBAPassword OBJECT-TYPE
   SYNTAX DisplayString (SIZE(0..16))
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION    "Web Based Authentication User Password."

   ::= { rlWBAAuxiliaryEntry 6 }







-- -------------------------------------------------------------
-- ---------   Image Tables     --------------------------------
-- -------------------------------------------------------------




 rlWBAImageTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlWBAImageEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The table holds the images content."
    ::= {rlWBA 2 }

    rlWBAImageEntry  OBJECT-TYPE
    SYNTAX      RlWBAImageEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the rlWBAImageTable."
    INDEX    { rlWBAImageNumber,rlWBAImageIndex}
    ::= {rlWBAImageTable  1 }

    RlWBAImageEntry ::= SEQUENCE {
    rlWBAImageNumber     INTEGER (1..10),
    rlWBAImageIndex      INTEGER (1..1000),
    rlWBAImageText       OCTET STRING
    }


    rlWBAImageNumber OBJECT-TYPE
    SYNTAX      INTEGER (1..10)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable identifies the Image number ... "
    ::= { rlWBAImageEntry 1 }

    rlWBAImageIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..1000)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "This variable identifies the Data of index of the image cut into octetes of 160 bytes"

    ::= { rlWBAImageEntry 2 }


    rlWBAImageText OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "This variable identifies the MIB which holds image content ."
    ::= { rlWBAImageEntry 3 }



-- -------------------------------------------------------------
-- ---------   Image Tables     --------------------------------
-- -------------------------------------------------------------

 rlWBADataTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlWBADataEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The table holds the Data content."
    ::= {rlWBA 3 }

    rlWBADataEntry  OBJECT-TYPE
    SYNTAX      RlWBADataEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the rlWBADataTable."
    INDEX    { rlWBADataNumber,rlWBADataIndex}
    ::= {rlWBADataTable  1 }

    RlWBADataEntry ::= SEQUENCE {
    rlWBADataNumber     INTEGER (1..10),
    rlWBADataIndex      INTEGER (1..1000),
    rlWBADataText       SnmpAdminString
    }


    rlWBADataNumber OBJECT-TYPE
    SYNTAX      INTEGER (1..10)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable identifies the Data of index of the image cut into octets of 160 bytes"
    ::= { rlWBADataEntry 1 }

    rlWBADataIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..1000)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "TBD"

    ::= { rlWBADataEntry 2 }


    rlWBADataText OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "This variable identifies the MIB which holds a section of the Data content in the table.(chunk of 160 bytes)"
    ::= { rlWBADataEntry 3 }


-- image information
 rlWBAImageInfoTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlWBAImageInfoEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The table holds the images content."
    ::= {rlWBA 4 }

    rlWBAImageInfoEntry  OBJECT-TYPE
    SYNTAX      RlWBAImageInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the rlWBAImageInfoTable."
    INDEX    { rlWBAImageInfoNumber}
    ::= {rlWBAImageInfoTable  1 }

    RlWBAImageInfoEntry ::= SEQUENCE {
    rlWBAImageInfoNumber     INTEGER (1..10),
    rlWBAImageInfoName       SnmpAdminString,
    rlWBAImageInfoSize       INTEGER

    }


    rlWBAImageInfoNumber OBJECT-TYPE
    SYNTAX      INTEGER (1..10)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable identifies the Image number ... "
    ::= { rlWBAImageInfoEntry 1 }

    rlWBAImageInfoName OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "This variable identifies the Name of the image eg: myImage.png"

    ::= { rlWBAImageInfoEntry 2 }


    rlWBAImageInfoSize OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "This variable identifies the size of the image."
    ::= { rlWBAImageInfoEntry 3 }



    rlWBAImageClear OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION    "Action to Clear a certain image "

   ::= {rlWBA 5}

    rlWBADataClear OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION    "Action to Clear a certain image "

   ::= {rlWBA 6 }

    rlWBAImageDownloadFinishStatus OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION    "Finish status of customization image download"

   ::= {rlWBA 7}

END






