RADLAN-MIR-MIB DEFINITIONS ::= BEGIN

-- Title:                RADLAN ROS
--                       Private MIR MIB
-- Version:              7.46
-- Date:                 15-Jan-2007

IMPORTS
    rnd                                                     FROM RADLAN-MIB
    OBJECT-TYPE, MODULE-IDENTITY                            FROM SNMPv2-SMI
    RowStatus                                               FROM SNMPv2-TC
    InterfaceIndex                                          FROM IF-MIB;

rlMir MODULE-IDENTITY
                LAST-UPDATED "200701020000Z"
                ORGANIZATION "Marvell Semiconductor, Inc."
                CONTACT-INFO
					"5488 Marvell Lane
					Santa Clara, CA 95054
					USA

					Website:  www.marvell.com"
                DESCRIPTION
                      "This private MIB module defines MIR private MIBs."
                REVISION "200701020000Z"
                DESCRIPTION
                      "Initial revision."
        ::= { rnd 61 }

rlMirMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "MIB's version, the current version is 1."
    ::= { rlMir 1 }

rlMirMaxNumOfMRIsAfterReset OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The maximun instanses of IP Multi Instance Routers after the
         following reset."
    DEFVAL { 1 }
    ::= { rlMir 2 }

rlMirMaxNumOfMRIs OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximun instanses of IP Multi Instance Routers."
    ::= { rlMir 3 }

rlMirCurMriNum OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The number of the MRI of which MIB variables are treated at
        the same time by the SNMP agent."
    ::= { rlMir 4 }

rlMirInterfaceTable  OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlMirInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list of the assignment ifinterfaces to IP Router instances."
    ::= { rlMir 5 }

rlMirInterfaceEntry OBJECT-TYPE
    SYNTAX  RlMirInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "An entry of this table specifies the MRID assignement to a L2
        interfrace."
    INDEX  { rlMirInterfaceIfIndex }
    ::= { rlMirInterfaceTable 1 }

RlMirInterfaceEntry ::= SEQUENCE {
    rlMirInterfaceIfIndex       InterfaceIndex,
    rlMirInterfaceMrid          INTEGER
}

rlMirInterfaceIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS      read-write
    STATUS      current
    DESCRIPTION
        "The L2 interface for which this entry contains information."
    ::= { rlMirInterfaceEntry 1 }

rlMirInterfaceMrid OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Multi IP Router Instance Identifier to which the
         interface is assgned."
    DEFVAL { 1 }
    ::= { rlMirInterfaceEntry 2 }

rlMirVlanBaseReservedPortsTable  OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlMirVlanBaseReservedPortsEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list VLAN based reserved physical ports."
    ::= { rlMir 6 }

rlMirVlanBaseReservedPortsEntry OBJECT-TYPE
    SYNTAX  RlMirVlanBaseReservedPortsEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A VLAN based reserved physical port."
    INDEX  { rlMirVlanBaseReservedPortsIfIndex }
    ::= { rlMirVlanBaseReservedPortsTable 1 }

RlMirVlanBaseReservedPortsEntry ::= SEQUENCE {
    rlMirVlanBaseReservedPortsIfIndex       InterfaceIndex,
    rlMirVlanBaseReservedPortsStatus        RowStatus
}

rlMirVlanBaseReservedPortsIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS      read-create
    STATUS      current
    DESCRIPTION
        "IfIndex of VLAN based reserved physical port."
    ::= { rlMirVlanBaseReservedPortsEntry 1 }

rlMirVlanBaseReservedPortsStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "It is used to delete an entry"
    ::= { rlMirVlanBaseReservedPortsEntry 2 }

rlMirVlanBaseLogicalPortsTable  OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlMirVlanBaseLogicalPortsEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A list VLAN based logical ports."
    ::= { rlMir 7 }

rlMirVlanBaseLogicalPortsEntry OBJECT-TYPE
    SYNTAX  RlMirVlanBaseLogicalPortsEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A VLAN based logical point-to-point port."
    INDEX  { rlMirVlanBaseLogicalPortsIfIndex }
    ::= { rlMirVlanBaseLogicalPortsTable 1 }

RlMirVlanBaseLogicalPortsEntry ::= SEQUENCE {
    rlMirVlanBaseLogicalPortsIfIndex                InterfaceIndex,
    rlMirVlanBaseLogicalPortsReservedIfIndex        InterfaceIndex,
    rlMirVlanBaseLogicalPortsVlanTag                INTEGER,
    rlMirVlanBaseLogicalPortsStatus                 RowStatus
}

rlMirVlanBaseLogicalPortsIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS      read-create
    STATUS      current
    DESCRIPTION
        "IfIndex of VLAN based Logical point-to-point port."
    ::= { rlMirVlanBaseLogicalPortsEntry 1 }

rlMirVlanBaseLogicalPortsReservedIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS      read-create
    STATUS      current
    DESCRIPTION
        "IfIndex of VLAN based reserved physical port on which the logical
         port is defined."
    ::= { rlMirVlanBaseLogicalPortsEntry 2 }

rlMirVlanBaseLogicalPortsVlanTag OBJECT-TYPE
    SYNTAX      INTEGER (1..4095)
    MAX-ACCESS      read-create
    STATUS      current
    DESCRIPTION
        "VLAN tag."
    ::= { rlMirVlanBaseLogicalPortsEntry 3 }

rlMirVlanBaseLogicalPortsStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "It is used to add, update and delete an entry"
    ::= { rlMirVlanBaseLogicalPortsEntry 4 }

rlMirCurMriNumRouter OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Returns Router Mri Number."
    ::= { rlMir 8 }

rlMirCurMriNumOob OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Returns Router Mri Number."
    ::= { rlMir 9 }

END

