ELTEX-BGP-MIB DEFINITIONS ::= BEGIN

  IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Integer32,
    Counter32,
    Gauge32,
    Unsigned32,
    IpAddress
      FROM SNMPv2-SMI

    TEXTUAL-CONVENTION,
    DisplayString,
    TruthValue,
    RowStatus,
    TimeStamp,
    TimeInterval,
    MacAddress
      FROM SNMPv2-TC

    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
      FROM SNMPv2-CONF

    InetAddressType,
    InetAddress,
    InetPortNumber,
    InetAddressPrefixLength
      FROM INET-ADDRESS-MIB

    InterfaceIndexOrZero
      FROM IF-MIB

    eltexLtd
      FROM ELTEX-SMI-ACTUAL;

  eltexBgpMIB MODULE-IDENTITY
    LAST-UPDATED "201709040000Z" -- Mon Sep 04 00:00:00 GMT 2017
    ORGANIZATION "Eltex Enterprise Co, Ltd."
    CONTACT-INFO 
        "www.eltex.nsk.ru"
    DESCRIPTION  
        "The MIB module for management of the BGP protocol."

  ::= { eltexLtd 45 }

-------------------------------------------------------------------------------
-- Textual Conventions.

  EltexBgpIdentifier ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION "The representation of a BGP Identifier. Could be any 32-bit
                 number in a form of 4-octet IPv4 address."
    SYNTAX       OCTET STRING (SIZE (4))

  EltexBgpAfi ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION "The representation of a BGP AFI (Address Family Identifier)"
    SYNTAX      INTEGER {
                  other(0),
                  ipv4(1),
                  ipv6(2),
                  l2vpn(25)
                }

  EltexBgpSafi ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION 
        "The representation of a BGP SAFI (Sub-Address Family Identifier)"
    SYNTAX      INTEGER {
                  none(0),
                  unicast(1),
                  multicast(2),
                  both(3),
                  labeled(4),
                  vpls(65),
                  evpn(70),
                  mplsBgpVpn(128),
                  private(241)
                }

  EltexBgpAutonomousSystemNumber ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION "An autonomous System Number.  If <AsSize> is
                 two-octet, the range is 0..65535.  If it is
                 four-octet, it is the full range of Unsigned32."
    SYNTAX      Unsigned32

  EltexBgpAsSize ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "The size of the AS number."
    SYNTAX      INTEGER {
                  twoOctet(1),
                  fourOctet(2)
                }

  EltexBgpAdminStatus ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "The desired administrative state of an entry."
    SYNTAX      INTEGER {
                  adminStatusUp(1),
                  adminStatusDown(2)
                }

  EltexBgpOperStatus ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "The current operational state of an entity."
    SYNTAX      INTEGER {
                  operStatusUp(1),        -- active
                  operStatusDown(2),      -- inactive
                  operStatusGoingUp(3),   -- activating
                  operStatusGoingDown(4), -- deactivating
                  operStatusActFailed(5)  -- activation failed
                }

  EltexBgpOriginCode ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "A BGP origin code."
    SYNTAX      INTEGER {
                  originIgp(0),           -- path interior to originating AS
                  originEgp(1),           -- path learned via EGP protocol
                  originIncomplete(2)     -- path was learned by other means
                }

  EltexBgpConfigDropOrWarn ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Whether to drop a session or just warn a parameter has been
                 exceeded."
    SYNTAX      INTEGER {
                  drop(1),                -- the session is dropped
                  warn(2)                 -- a warning is produced
                }

  EltexBgpPeerOrRib ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Whether an index refers to a BGP Peer Index or a RIB index."
    SYNTAX      INTEGER {
                  peerIndex(1),
                  ribIndex(2),
                  noIndex(3)
                }

  EltexBgpPeerStates ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "The current state of a connection to a BGP peer."
    SYNTAX      INTEGER {
                  none(0),
                  idle(1),
                  connect(2),
                  active(3),
                  opensent(4),
                  openconfirm(5),
                  established(6)
                }

  EltexBgpPeerEvents ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "An event that has occurred to a connection to a BGP peer."
    SYNTAX      INTEGER {
                  noEvent(0),             -- no event has yet occurred
                  start(1),               -- the connection has been activated
                                          --  (either outgoing or incoming)
                  stop(2),                -- the connection has been
                                          --  deactivated
                  transportOpen(3),       -- the transport connection has been
                                          --  opened
                  transportClosed(4),     -- the transport connection has been
                                          --  closed
                  transportOpenFailed(5), -- an attempt to open the transport
                                          --  connection has failed
                  transportFatalError(6), -- a fatal error has occurred on the
                                          --  transport connection
                  connectRetryTimer(7),   -- the ConnectRetry timer has popped
                  holdTimer(8),           -- the Hold timer has popped
                  keepaliverTimer(9),     -- the Keepalive timer has popped
                  recvOpen(10),           -- a BGP Open message has been
                                          --  received
                  recvKeepAlive(11),      -- a BGP KeepAlive message has been
                                          --  received
                  recvUpdate(12),         -- a BGP Update message has been
                                          --  received
                  recvNotification(13),   -- a BGP Notification message has
                                          --  been received
                  connParmsUpdate(14)     -- Connection parameters have been
                                          --  updated
                }

  EltexBgpCapabilities ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "The capabilities advertised by a BGP instance."
    SYNTAX      BITS {
                  mpIpv4Unicast(0),             -- multiprotocol BGP support
                                                --  for IPv4 unicast routes
                  mpIpv4Multicast(1),           -- multiprotocol BGP support
                                                --  for IPv4 multicast routes
                  mpIpv4Vpn(2),                 -- multiprotocol BGP support
                                                --  for IPv4 VPN routes
                  mpIpv4Label(3),               -- multiprotocol BGP support
                                                --  for labeled IPv4 VPN
                                                --  routes
                  mpIpv6Unicast(4),             -- multiprotocol BGP support
                                                --  for IPv6 unicast routes
                  mpIpv6Multicast(5),           -- multiprotocol BGP support
                                                --  for IPv6 multicast routes
                  mpIpv6Vpn(6),                 -- multiprotocol BGP support
                                                --  for IPv6 VPN routes
                  mpIpv6Label(7),               -- multiprotocol BGP support
                                                --  for labeled IPv6 VPN
                                                --  routes
                  routeRefresh(8),              -- support for Route Refresh
                                                --  messages
                  gracefulRestart(9),           -- support for graceful restart
                                                --  processing
                  routeRefreshCisco(10),        -- support for pre-standard
                                                --  (Cisco) Route Refresh
                                                --  messages
                  outboundRouteFilter(11),      -- support for Outbound Route
                                                --  Filtering, for one or more
                                                --  AFI/SAFI types
                  outboundRouteFilterCisco(12), -- support for pre-standard
                                                --  (Cisco) Outbound Route
                                                --  Filtering, for one or more
                                                --  AFI/SAFI types
                  fourOctetAs(13),              -- support for four-octet AS
                                                --  numbers
                  mpL2vpnVpls(14),              -- multiprotocol BGP support
                                                --  for AFI/SAFI = L2VPN/VPLS
                  addPath(15),                  -- support for additional BGP
                                                --  paths
                  mpL2vpnEvpn(16),              -- multiprotocol BGP support
                                                --  for AFI/SAFI = L2VPN/EVPN
                  mpIpv4Private(17),            -- multiprotocol BGP support
                                                --  for AFI/SAFI = IPv4/Private
                  enhancedRouteRefresh(18)      -- support for enhanced route
                                                --  refresh (RFC7313)
                }

  EltexBgpCeaseErrorSubcode ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "The error subcode to be sent in the Cease Notification message."
    SYNTAX      INTEGER {
                  none(0),          -- no subcode is specified.
                  adminShutdown(2), -- administrative Shutdown.
                  peerUnconfig(3),  -- peer De-configured.
                  adminReset(4),    -- administrative Reset.
                  configChange(6),  -- other Configuration Change.
                  noResource(8)     -- out of Resources.
                }

  EltexBgpNlriIsActiveFlag ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Indicates whether an NLRI is active in the routing table."
    SYNTAX      INTEGER {
                  notTracked(1),    -- BGP is not tracking active routes
                  inactive(2),      -- The BGP route is inactive
                  active(3)         -- The BGP route is active
                }

  EltexBgpPeerConfigStates ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "Reports the state of the peer configuration."
     SYNTAX     INTEGER {
                  stateUpToDate (1),            -- Up to date.
                  stateOutOfDateAdminDown (2),  -- Out of date, requiring the
                                                -- peer's admin status to be
                                                -- set to down.
                  stateOutOfDateRowInactive (3) -- Out of date, requiring the
                                                -- peer's row status to be set
                                                -- to inactive.
                }

  EltexBgpReasonNotBest ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Reports the reason a route was determined to be not the
                 best route to that destination."
    SYNTAX      INTEGER {
                  notConsidered(0),       -- The route has not been considered
                                          -- for best route
                  routeIsBest(1),         -- The is the best route
                  weight(2),              -- The route was beaten by one with a
                                          -- better weight
                  localPref(3),           -- The route was beaten by one with a
                                          -- better local preference
                  localOrigPreferred(4),  -- The route was beaten by a
                                          -- locally-originated route
                  asPathLen(5),           -- The route was beaten by one with a
                                          -- shorter AS Path
                  origin(6),              -- The route was beaten by one with a
                                          -- lower origin code
                  med(7),                 -- The route was beaten by one with a
                                          -- lower MED
                  localOrigTieBreaker(8), -- The route was beaten by another
                                          -- locally originated route
                  ebgpVsibgp(9),          -- The IBGP route was beaten by a
                                          -- route from an external peer
                  adminDistance(10),      -- The route was beaten by a route
                                          -- with a lower admin distance
                  pathCostToNextHop(11),  -- The route was beaten by a route
                                          -- with a lower path cost to the
                                          -- next hop.
                  prefExisting(12),       -- The route was beaten because
                                          -- existing route was preferred
                  identifier(13),         -- The route was beaten by a route
                                          -- with a lower identifier either
                                          -- ORIGINATOR ID or BGP identifier
                  clusterLen(14),         -- The route was beaten by a route
                                          -- with a lower cluster length
                  peerType(15),           -- The route was beaten by a route
                                          -- with a preferred peer address
                                          -- type.  IPv6 is preferred to IPv4
                  peerAddress(16),        -- The route was beaten by a route
                                          -- with a lower peer address
                  peerPort(17),           -- The route was beaten by a route
                                          -- with a lower peer port
                  pathId(18)              -- The route was beaten by a route
                                          -- with a lower path id
                }

  EltexBgpNlriPeerTypes ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "The type of peer than a route was received from."
    SYNTAX      INTEGER {
                  none(1),    -- The route was not received from a BGP peer.
                  iBGP(2),    -- The route was received from an iBGP BGP peer.
                  eBGP(3)     -- The route was received from an eBGP BGP peer.
                }

  EltexBgpASNotation ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Selecting the AS number notation."
    SYNTAX      INTEGER {
                  asplainASNumber(1),                -- AS_PLAIN notation
                  asdotASnumber(2)                   -- AS_DOT notation
                }

  EltexBgpPeerReflectorClientType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "What type of client this BGP Peer is.  A client of a route
                 reflector is a meshed client if and only if it is fully meshed
                 with all meshed clients of that route reflector."
    SYNTAX      INTEGER {
                  nonClient(0),
                  client(1),
                  meshedClient(2)
                }

  EltexBgpRouteMapAsPathAction ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "How to handle setting an AS-Path attribute."
    SYNTAX      INTEGER {
                  none(0),          -- No action is carried out
                  set(1)            -- The local AS number is prepended to the AS path
                }

  EltexBgpAddPathSrCap ::= TEXTUAL-CONVENTION
     STATUS     current
     DESCRIPTION "BGP additional path send/receive capability."
     SYNTAX     INTEGER {
                  disable (0),               -- disable sending and receiving
                  receive (1),               -- receive but do not send
                  send (2),                  -- send but do not receive
                  both (3),                  -- send and receive
                  inherit (4),               -- inherit configuration from
                                             -- the entity AFI/SAFI level
                  unknown (5)                -- unknown
                }

  EltexBfdSessionStatus ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "The current BFD session state of a peer."
    SYNTAX      INTEGER {
                bfdSessNotRequired(0),    -- not required
                bfdSessInitial(1),        -- initial
                bfdSessActivating(2),     -- activating
                bfdSessActive(3),         -- active
                bfdSessInactive(4),       -- inactive
                bfdSessAdminDown(5),      -- admin down
                bfdSessNoContact(6)       -- no contact
                }

  EltexBgpRouteDistinguisher ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Syntax for a route distinguisher."
    SYNTAX      OCTET STRING (SIZE (0 | 8))

  EltexBgpEvpnRouteTypes ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Evpn route type:
                 1 -- Ethernet Auto-Discovery (A-D) route
                 2 -- MAC/IP Advertisement route
                 3 -- Inclusive Multicast Ethernet Tag route
                 4 -- Ethernet Segment route
                 5 -- IP prefix route"
    SYNTAX      Unsigned32

  EltexBgpEvpnESI ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Syntax for an Ethernet Segment Identifier."
    SYNTAX      OCTET STRING (SIZE (0 | 10))

  EltexBgpEvpnEthernetTag ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "An Ethernet tag identifier, representing a broadcast domain
                 in an EVPN instance."
    SYNTAX      Unsigned32


  EltexBgpCommListType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Community List type standard or extended."
    SYNTAX      INTEGER {
                  standardCommunity(1),    -- List use for a standard community
                  extendedCommunity(2)     -- List use for a extended community
                }

  EltexBgpCommListEntryType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "How an entry in the eltexBgpCommunityListTable is used to match
                 route commmunities or an entry in the eltexBgpExtCommListTable is
                 used to match route extended commmunities."
    SYNTAX      INTEGER {
                  communityGroup(1),    -- Use a community group
                  regularExpression(2)  -- Use a regular expression
                }

  EltexBgpPermitOrDeny ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "Whether the behavior is to permit or deny."
    SYNTAX      INTEGER {
                  permit(1),  -- Unmatched routes are permitted
                  deny(2)     -- Unmatched routes are denied
                }

  EltexBgpCommunity ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION "The representation of a BGP Community form of 4-octet or  BGP
                 Extended Community form of 8-octet."
    SYNTAX      OCTET STRING (SIZE (4 | 8))


  EltexBgpExtendedCommunity ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "8x"
    STATUS       current
    DESCRIPTION "The representation of a BGP Extended Community."
    SYNTAX OCTET STRING (SIZE(8))

  EltexBgpAggregateOptions ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "The option used when aggregating."
    SYNTAX      INTEGER {
                  none(1),           -- No options.  An aggregate entry is
                                     --  generated if more specific entries are
                                     --  present
                  summary(2),        -- Only the summary option.  More specific
                                     --  routes that make the aggregate are not
                                     --  advertised
                  asSet(3),          -- Aggregates the AS-PATH using the
                                     --  algorithm described in RFC 1771.  This
                                     --  maintains the longest AS-Sequence common
                                     --  common to the aggregated routes and
                                     --  adds AS numbers from the other routes
                                     --  to an AS-Set
                  summaryAsSet(4)    -- Both summary and AS-Set options
                }

  EltexBgpInetAddressType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A value that represents a type of Internet address.

         unknown(0)  An unknown address type.  This value MUST
                     be used if the value of the corresponding
                     InetAddress object is a zero-length string.
                     It may also be used to indicate an IP address
                     that is not in one of the formats defined
                     below.

         ipv4(1)     An IPv4 address as defined by the
                     InetAddressIPv4 textual convention.

         ipv6(2)     An IPv6 address as defined by the
                     InetAddressIPv6 textual convention.

         ipv4z(3)    A non-global IPv4 address including a zone
                     index as defined by the InetAddressIPv4z
                     textual convention.

         ipv6z(4)    A non-global IPv6 address including a zone
                     index as defined by the InetAddressIPv6z
                     textual convention.

         dns(16)     A DNS domain name as defined by the
                     InetAddressDNS textual convention."
    SYNTAX       INTEGER {
                     unknown(0),
                     ipv4(1),
                     ipv6(2),
                     ipv4z(3),
                     ipv6z(4),
                     dns(16)
                 }

-------------------------------------------------------------------------------

  eltexBgpObjects    OBJECT IDENTIFIER ::= { eltexBgpMIB 1 }

  eltexBgpProcess       OBJECT IDENTIFIER ::= { eltexBgpObjects 1 }

--
-- BGP Process Table.
--
-- This is the top-level MIB for the BGP Router feature. It controls
-- creation and global configuration of the protocol.
--

  eltexBgpProcessTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpProcessEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Each entry in this table represents a single instance of
                 BGP Router process. Only some fields in an entry can be 
                 changed while the admin status is up.
                 
                 The current implementation allows only a single process of
                 BGP is configured on the router. The single BGP process
                 could be created only with process ID 1."
    ::= { eltexBgpProcess 1 }

  eltexBgpProcessEntry OBJECT-TYPE
    SYNTAX      EltexBgpProcessEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Each entry represents a BGP Router entity."
    INDEX       { eltexBgpProcessId }
    ::= { eltexBgpProcessTable 1 }

  EltexBgpProcessEntry ::= SEQUENCE {
      eltexBgpProcessId                     Unsigned32,
      eltexBgpProcessRowStatus              RowStatus,
      eltexBgpProcessAdminStatus            EltexBgpAdminStatus,
      eltexBgpProcessOperStatus             EltexBgpOperStatus,
      eltexBgpProcessLocalAs                EltexBgpAutonomousSystemNumber,
      eltexBgpProcessLocalIdentifier        EltexBgpIdentifier,
      eltexBgpProcessOperLocalIdentifier    EltexBgpIdentifier,
      eltexBgpProcessTableVersion           Unsigned32,
      eltexBgpProcessASNotation             EltexBgpASNotation,
      eltexBgpProcessClusterIdentifier      EltexBgpIdentifier,
      eltexBgpProcessOperClusterIdentifier  EltexBgpIdentifier,
      eltexBgpProcessInterClientReflEnabled TruthValue,
      eltexBgpProcessPathMtuDiscovery       TruthValue,
      eltexBgpProcessAsPathMultipathRelax   TruthValue
    }

  eltexBgpProcessId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Identifies a BGP Router entity."
    ::= { eltexBgpProcessEntry 1 }

  eltexBgpProcessRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The row status for this BGP Process Table entry, used to
                 create and destroy table entries."
    ::= { eltexBgpProcessEntry 2 }

  eltexBgpProcessAdminStatus OBJECT-TYPE
    SYNTAX      EltexBgpAdminStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The administrative status of this BGP Process entity, used to
                 activate and deactivate the protocol."
    DEFVAL      { adminStatusDown }
    ::= { eltexBgpProcessEntry 3 }

  eltexBgpProcessOperStatus OBJECT-TYPE
    SYNTAX      EltexBgpOperStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The current operational status of this BGP Process entity."
    ::= { eltexBgpProcessEntry 4 }

  eltexBgpProcessLocalAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The local autonomous system number.

                 For a router not in a confederation, it is equivalent to
                 the Base Scalar bgpM2LocalAs.  For a router in a
                 confederation, it is equivalent to the Base Scalar
                 bgpM2ConfederationId.  If eltexBgpProcessConfederationId
                 is not 0, then this router is in a confederation.

                 If the eltexBgpProcessAsSize is twoOctet, then the range is
                 constrained to be 0-65535.  A non-mappable 4-octet AS
                 number should only be used when all BGP speakers within
                 the AS support 4-octet AS numbers.

                 This field can only be changed when the Admin Status is
                 down."
    ::= { eltexBgpProcessEntry 5 }

  eltexBgpProcessLocalIdentifier OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The BGP Identifier of the local system. This is a generic
                 identifier and not necessarily an IP address.  This field
                 can only be changed when the Admin Status is down.
                 It is equivalent to the Base Scalar bgpM2LocalIdentifier.
                 
                 The null value turns on ID election algorithm that chooses
                 the highest loopback interface if any, or the highest IP
                 interface otherwise."
    DEFVAL       { '00000000'H }
    ::= { eltexBgpProcessEntry 6 }

  eltexBgpProcessOperLocalIdentifier OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The BGP Identifier of the local system that is used in the
                 present moment. It could be selected by election algorithm
                 or configured by user."
    ::= { eltexBgpProcessEntry 7 }

  eltexBgpProcessTableVersion OBJECT-TYPE
       SYNTAX       Unsigned32 (0..4294967295)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
                 "The table version number of the Loc-RIB.  Initialized to 1
                  when BGP starts or restarts, and is incremented every time
                  the Loc-RIB is recalculated."
    ::= { eltexBgpProcessEntry 8 }

  eltexBgpProcessASNotation OBJECT-TYPE
    SYNTAX      EltexBgpASNotation
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The choice between asplain and asdot notation AS numbers."
    DEFVAL      { asplainASNumber }
    ::= { eltexBgpProcessEntry 9 }

  eltexBgpProcessClusterIdentifier OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The configured Cluster-ID of the local router.
                 A value of 0.0.0.0 indicates the absence of this
                 value.  This field can only be changed when the Admin
                 Status is down. The BGP router will act as a route reflector
                 if any peer is configured to be a client.  If no cluster ID is
                 explicitly configured here, the Router ID will be used."
    DEFVAL       { '00000000'H }
    ::= { eltexBgpProcessEntry 10 }

  eltexBgpProcessOperClusterIdentifier OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The Cluster-ID that is used in the present moment."
    DEFVAL       { '00000000'H }
    ::= { eltexBgpProcessEntry 11 }

  eltexBgpProcessInterClientReflEnabled OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Routes will not be reflected between two peers that are
                configured to be route reflector clients in the
                eltexBgpPeerReflectorClient field if this field takes the value
                FALSE."
    DEFVAL       { true }
    ::= { eltexBgpProcessEntry 12 }

  eltexBgpProcessPathMtuDiscovery OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Enable path MTU discovery on all neighbors"
    DEFVAL       { false }
    ::= { eltexBgpProcessEntry 13 }

  eltexBgpProcessAsPathMultipathRelax OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This field indicates whether BGP routes with different
                 AS_PATHs can be used as equal cost routes.

                 If this is FALSE then BGP only treats two BGP routes as
                 equal cost if several of their attributes, including the
                 AS_PATH, are identical.  This is the default behavior.

                 If this is TRUE then BGP can treat two BGP routes as
                 equal cost even if their AS_PATHs differ, as long as their
                 AS_PATH lengths and other relevant attributes are the
                 same.  This allows routes with different AS_PATHs to be
                 programmed into the forwarding table as equal cost
                 multipath routes.

                 When multipath-relax is enabled BGP still selects one
                 of the multipath routes as the best route to advertise to
                 its peers.  The AS_PATH advertised to peers reflects the
                 best route but not other equal cost routes, so it does not
                 reflect the full set of ASs on the forwarding path.  This
                 means that enabling multipath-relax can cause routing
                 loops.  Therefore multipath-relax should only be enabled
                 if the network administrator is sure that routing loops
                 cannot occur.

                 This field can only be changed when the Admin Status is
                 down."
    DEFVAL       { false }
    ::= { eltexBgpProcessEntry 14 }

--
-- <AFI, SAFI> supported table
--

  eltexBgpProcessAddrFamilyTable OBJECT-TYPE
  -- FAMILY-SHORT-NAME BGP_AFI
    SYNTAX      SEQUENCE OF EltexBgpProcessAddrFamilyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Table of per-<AFI, SAFI> configuration information."
    ::= { eltexBgpProcess 2 }

  eltexBgpProcessAddrFamilyEntry OBJECT-TYPE
    SYNTAX      EltexBgpProcessAddrFamilyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Entry containing information about support for an
                 <AFI, SAFI>."
    INDEX { eltexBgpProcessId,
            eltexBgpProcessAddrFamilyAfi,
            eltexBgpProcessAddrFamilySafi }
    ::= { eltexBgpProcessAddrFamilyTable 1 }

  EltexBgpProcessAddrFamilyEntry ::= SEQUENCE {
      eltexBgpProcessAddrFamilyAfi                 EltexBgpAfi,
      eltexBgpProcessAddrFamilySafi                EltexBgpSafi,
      eltexBgpProcessAddrFamilyRowStatus           RowStatus,
      eltexBgpProcessAddrFamilyAddPathCapCfg       EltexBgpAddPathSrCap,
      eltexBgpProcessAddrFamilyAddPathBestN        Unsigned32
      }

  eltexBgpProcessAddrFamilyAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The AFI index into the <AFI, SAFI> table."
    ::= { eltexBgpProcessAddrFamilyEntry 2 }

  eltexBgpProcessAddrFamilySafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The SAFI index into the <AFI, SAFI> table."
    ::= { eltexBgpProcessAddrFamilyEntry 3 }

  eltexBgpProcessAddrFamilyRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The row status for this <AFI, SAFI> entry, used to
                 create and destroy table entries. This field can
                 only be set while Process is admin down."
    ::= { eltexBgpProcessAddrFamilyEntry 4 }

  eltexBgpProcessAddrFamilyAddPathCapCfg OBJECT-TYPE
    SYNTAX      EltexBgpAddPathSrCap
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The default BGP additional path capability for I-BGP
                 sessions.

                 This can be overridden at the BGP peer AFI/SAFI level
                 (eltexBgpPeerAddrFamilyAddPathCapCfg).

                 BGP additional path capability is never enabled by default
                 for E-BGP sessions - instead it should be configured for
                 specific E-BGP peers at the peer AFI/SAFI level.

                 Valid values are:
                 -  disable (0)
                    Disable sending and receiving additional BGP paths
                 -  receive (1)
                    Receive but do not send additional BGP paths
                 -  send (2)
                    Send but do not receive additional BGP paths
                 -  both (3)
                    Send and receive additional BGP paths.

                 Any update to this object will take effect the next time
                 that the peer session reactivates."
    DEFVAL { disable }
    ::= { eltexBgpProcessAddrFamilyEntry 5 }

  eltexBgpProcessAddrFamilyAddPathBestN OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The number of best paths to calculate as candidate BGP
                 additional paths.

                 BGP calculates the N best paths for each destination as
                 candidates for advertisement to BGP peers as additional
                 paths.

                 The candidate paths are the N best paths avoiding duplicate
                 BGP next hops.  They include the best path, and alternative
                 lower preference / higher cost paths.

                 For the default value of 1 the only candidate path is the
                 best path for each destination.

                 A value of 2 is sufficient to calculate the best path and
                 a backup path (if available) for each destination.

                 For small values of N the benefit of fast convergence after
                 N-1 failures can outweigh the cost of calculating and
                 advertising the best N routes, but for larger values of N
                 the benefit does not justify the cost.  Therefore this field
                 should only be set to a small value.

                 The number of paths advertised to each BGP peer can be
                 restricted at the BGP peer level
                 (eltexBgpPeerAddrFamilyAddPathBestN), but it is not possible to
                 advertise more paths than are specified here as candidates.

                 This field can only be modified while BGP process is admin down."
    DEFVAL { 1 }
    ::= { eltexBgpProcessAddrFamilyEntry 6 }

-------------------------------------------------------------------------------

  eltexBgpPeer          OBJECT IDENTIFIER ::= { eltexBgpObjects 2 }

  eltexBgpPeerData      OBJECT IDENTIFIER ::= { eltexBgpPeer 1 }

  --
  -- BGP Peer Data Table.
  --
  -- This table contains all the information required for each peer including
  -- protocol parameters, statistics and policy configuration.  A row in this
  -- table is created for each peer the BGP process knows about.
  --

  eltexBgpPeerTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPeerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "BGP peer configuration table.

                 This table allows a user to configure individual BGP peers.

                 This table is a configuration table - all status, statistics
                 and control fields are located in the BGP peer status table
                 (eltexBgpPeerStatusTable).

                 This table does not contain entries for dynamic peers."
    ::= { eltexBgpPeerData 1 }

  eltexBgpPeerEntry OBJECT-TYPE
    SYNTAX      EltexBgpPeerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Entry containing information about the connection with
                 a BGP peer."
    INDEX { eltexBgpProcessId,
            eltexBgpPeerRemoteAddrType,
            eltexBgpPeerRemoteAddr }
    ::= { eltexBgpPeerTable 1 }

  EltexBgpPeerEntry ::= SEQUENCE {
      eltexBgpPeerRemoteAddrType            InetAddressType,
      eltexBgpPeerRemoteAddr                InetAddress,
      eltexBgpPeerRowStatus                 RowStatus,
      eltexBgpPeerAdminStatus               EltexBgpAdminStatus,
      eltexBgpPeerOperStatus                EltexBgpOperStatus,
      eltexBgpPeerRemoteAs                  EltexBgpAutonomousSystemNumber,
      eltexBgpPeerSourceInterface           InterfaceIndexOrZero,
      eltexBgpPeerNxtHopSlf                 TruthValue,
      eltexBgpPeerConfigMaxPrfx             Unsigned32,
      eltexBgpPeerConfigDropWarn            EltexBgpConfigDropOrWarn,
      eltexBgpPeerMaxPrfxHold               Unsigned32,
      eltexBgpPeerConfigThreshold           Unsigned32,
      eltexBgpPeerConnectRetryInterval      Unsigned32,
      eltexBgpPeerHoldTimeConfigd           Unsigned32,
      eltexBgpPeerKeepAliveConfigd          Unsigned32,
      eltexBgpPeerMinRouteAdvertiseInterval Unsigned32,
      eltexBgpPeerMinASOriginationInterval  Unsigned32,
      eltexBgpPeerMinRouteWithdrawInterval  Unsigned32,
      eltexBgpPeerConfigOpenDelay           Unsigned32,
      eltexBgpPeerConfigIdleHold            Unsigned32,
      eltexBgpPeerDistListPlIn              DisplayString,
      eltexBgpPeerDistListPlOut             DisplayString,
      eltexBgpPeerReflectorClient           EltexBgpPeerReflectorClientType,
      eltexBgpPeerSoftResetWithStoredInfo   TruthValue,
      eltexBgpPeerConfigPeerGroup           DisplayString,
      eltexBgpPeerBfdDesired                TruthValue,
      eltexBgpPeerPassword                  OCTET STRING,
      eltexBgpPeerPasswordKeyChain          OCTET STRING,
      eltexBgpPeerAsPathListIn              DisplayString,
      eltexBgpPeerAsPathListOut             DisplayString,
      eltexBgpPeerEbgpMultihop              TruthValue,
      eltexBgpPeerCoreTracking              TruthValue,
      eltexBgpPeerAsOverride                TruthValue,
      eltexBgpPeerAllowAsIn                 Unsigned32
    }

  eltexBgpPeerRemoteAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the remote address for the peering
                 session."
    ::= { eltexBgpPeerEntry 1 }

  eltexBgpPeerRemoteAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The remote address for the peering session.

                 This is the address of the BGP peer.  It must be specified
                 so the address length must be non-zero."
    ::= { eltexBgpPeerEntry 2 }

  eltexBgpPeerRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The row status for this BGP peer table entry, used to
                create and destroy table entries."
    ::= { eltexBgpPeerEntry 3 }

  eltexBgpPeerAdminStatus OBJECT-TYPE
    SYNTAX      EltexBgpAdminStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The desired state of the BGP connection.

                 This parameter can be used to restart BGP peer
                 connections.  Care should be used in providing write
                 access to this object without adequate authentication."
    DEFVAL      { adminStatusDown }
    ::= { eltexBgpPeerEntry 4 }

  eltexBgpPeerOperStatus OBJECT-TYPE
    SYNTAX      EltexBgpOperStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The current operational status of this peer.  This usually
                 reflects the desired AdminStatus, but can contain transitional
                 values and failures."
    ::= { eltexBgpPeerEntry 5 }

  eltexBgpPeerRemoteAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The remote autonomous system number.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin status DOWN and then UP, thus forcing the
                 peer session to be restarted.  In this case, until the
                 peer is set admin_status DOWN, the peer will be marked as
                 out of date (as reported by the config state field in the
                 eltexBgpPeerStatusTable row for the peer)."
    ::= { eltexBgpPeerEntry 6 }

  eltexBgpPeerSourceInterface OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The interface index for the interface from which the
                 source address for session is chosen.  If non-zero, BGP
                 will look for the first address on this interface with a
                 type matching eltexBgpPeerRemoteAddrType, and use that as the
                 source address.

                 This field can be changed at any time, causing the peer to
                 be immediately deactivated and reactivated.

                 If the configured interface (or address on that interface)
                 did not exist when the peer was activated, and is
                 subsequently added, the peer will automatically use the
                 configured interface address.  This will cause the peer to
                 be immediately deactivated and reactivated."
    DEFVAL       { 0 }
    ::= { eltexBgpPeerEntry 7 }

  eltexBgpPeerNxtHopSlf OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "When eltexBgpPeerNxtHopSlf is 'true', routes will be 
                 advertised to the peer with NEXT_HOP attribute set to 
                 BGP router local address."
    DEFVAL       { false }
    ::= { eltexBgpPeerEntry 8 }

    eltexBgpPeerConfigMaxPrfx OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This object is used to limit the number of prefixes that
                 can be accepted from this peer.

                 Setting eltexBgpPeerConfigMaxPrfx to a non-zero value sets 
                 the maximum number of prefixes that can be accepted from 
                 this peer."
    DEFVAL       { 0 }
    ::= { eltexBgpPeerEntry 9 }

    eltexBgpPeerConfigDropWarn OBJECT-TYPE
    SYNTAX      EltexBgpConfigDropOrWarn
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This object is used  to determine whether the session is
                 dropped or a warning is generated when the maximum number
                 of prefixes set is exceeded.

                 Setting eltexBgpPeerConfigDropWarn to 'drop' will cause the
                 session to be dropped when the prefix limit is reached."
    DEFVAL       { warn }
    ::= { eltexBgpPeerEntry 10 }

    eltexBgpPeerMaxPrfxHold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The time interval in seconds between when this BGP session
                 is turn down due to the number of prefixes received from
                 this peer exceeding the maximum in
                 eltexBgpPeerConfigMaxPrfx and when BGP attempts to
                 reestablish the session."
    DEFVAL       { 90 }
    ::= { eltexBgpPeerEntry 11 }

    eltexBgpPeerConfigThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "A percentage of the limit set by eltexBgpPeerConfigMaxPrfx.
                 When the number of prefixes received from this peer reaches
                 this threshold, BGP issues a warning.

                 This field is not used if eltexBgpPeerConfigMaxPrfx is set to
                 zero."
    DEFVAL       { 75 }
    ::= { eltexBgpPeerEntry 12 }

    eltexBgpPeerConnectRetryInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval for the ConnectRetry timer.  The suggested
                 value for this timer is 120 seconds.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 120 }
    ::= { eltexBgpPeerEntry 13 }

    eltexBgpPeerHoldTimeConfigd OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the Hold Time configured for
                 this BGP speaker with this peer.  This value is placed in
                 an OPEN message sent to this peer by this BGP speaker, and
                 is compared with the Hold Time field in an OPEN message
                 received from the peer when determining the Hold Time
                 (eltexBgpPeerStatusHoldTime) with the peer.  This value must not be
                 less than three seconds if it is not zero (0) in which
                 case the Hold Time is NOT to be established with the peer.
                 The value of this object is only allowed to be zero (0) if
                 the value of eltexBgpPeerKeepAliveConfigd is also zero (0).
                 The suggested value for this timer is 90 seconds.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 90 }
    ::= { eltexBgpPeerEntry 14 }

    eltexBgpPeerKeepAliveConfigd OBJECT-TYPE
    SYNTAX      Unsigned32 ( 0 | 1..21845 )
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the KeepAlive configured for
                 this BGP speaker with this peer.  The value of this object
                 will only determine the KEEPALIVE messages frequency
                 relative to the value specified in eltexBgpPeerHoldTimeConfigd
                 the actual time interval for the KEEPALIVE messages is
                 indicated by eltexBgpPeerStatusKeepAlive.  A reasonable 
                 maximum value for this timer would be configured to be one 
                 third of that of eltexBgpPeerHoldTimeConfigd.

                 The value of this object is only allowed to be zero (0) if
                 the value of eltexBgpPeerHoldTimeConfigd is also zero (0).  If
                 the value of this object is zero (0), no periodical
                 KEEPALIVE messages are sent to the peer after the BGP
                 connection has been established.  The suggested value for
                 this timer is 30 seconds.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 30 }
    ::= { eltexBgpPeerEntry 15 }

    eltexBgpPeerMinRouteAdvertiseInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the
                 MinRouteAdvertisementInterval timer.  This determines the
                 minimum time between a BGP UPDATE to a peer advertising or
                 withdrawing a route and a subsequent BGP UPDATE to the
                 peer advertising a route to the same destination.

                 The default value for this timer is 30 seconds.  Its value
                 must not be less than eltexBgpPeerMinRouteWithdrawInterval."
    DEFVAL       { 30 }
    ::= { eltexBgpPeerEntry 16 }

    eltexBgpPeerMinASOriginationInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for determining the minimum amount
                 of time that must elapse between successive advertisements of
                 UPDATE messages that report changes to a route within the
                 advertising BGP speaker's own autonomous system. The
                 suggested value for this timer is 15 seconds."
    DEFVAL       { 15 }
    ::= { eltexBgpPeerEntry 17 }

    eltexBgpPeerMinRouteWithdrawInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the MinRouteWithdrawInterval
                 timer.  This is the interval which is enforced between
                 advertisement and subsequent withdrawal of a route.

                 The default value for this timer is 30 seconds.  The value
                 must not exceed that of eltexBgpPeerMinRouteAdvertiseInterval."
    DEFVAL       { 30 }
    ::= { eltexBgpPeerEntry 18 }

    eltexBgpPeerConfigOpenDelay OBJECT-TYPE
    SYNTAX      Unsigned32 (0..240)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The delay to enforce in between a TCP connection with this
                 peer becoming established and a BGP Open message being
                 sent.  If this delay is zero, then no delay will be
                 injected, and a BGP Open message will be sent as soon as
                 the TCP connection allows it.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 0 }
    ::= { eltexBgpPeerEntry 19 }

    eltexBgpPeerConfigIdleHold OBJECT-TYPE
    SYNTAX      Unsigned32 (1..32767)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The time to hold this peer in Idle state after a BGP
                 session has progressed beyond Idle state initially and
                 then returned to it.  No new connections will be initiated
                 or accepted until the peer comes out of Idle state.  By
                 setting this field to a large value, this timer can be
                 used to provide some level of peer oscillation damping, if
                 desired.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 15 }
    ::= { eltexBgpPeerEntry 20 }

    eltexBgpPeerDistListPlIn OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The Prefix List name identifying the Prefix List to use
                 to filter routes received from the peer."
    ::= { eltexBgpPeerEntry 21 }

    eltexBgpPeerDistListPlOut OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The Prefix List name identifying the Prefix List to use
                 to filter routes advertised to the peer."
    ::= { eltexBgpPeerEntry 22 }

  eltexBgpPeerReflectorClient OBJECT-TYPE
    SYNTAX      EltexBgpPeerReflectorClientType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This value indicates whether the given peer is a reflector
                client of this router, or not.  A value of nonClient(0)
                indicates that this peer is not a reflector client.  A
                value of client(1) indicates that this peer is a reflector
                client that is not fully meshed with other reflector
                clients.  A value of meshedClient(2) indicates that the
                peer is a reflector client and is fully meshed with all
                other reflector clients.

                For specific AFI/SAFI, this can be configured using
                eltexBgpPeerAddrFamilyReflectorClient."
    DEFVAL       { nonClient }
    ::= { eltexBgpPeerEntry 23 }

  eltexBgpPeerSoftResetWithStoredInfo OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This option causes all routes learned from a peer to be stored
                 so that the ARI can be recalculated (for example, due to a 
                 change in import policy) without performing a route refresh or
                 restarting the peer session.

                 This field can only be changed when the peer is admin_status
                 DOWN.

                 This option overlaps with route refresh (RR) behavior. If the
                 option is enabled, Route refresh capability continues to be
                 advertized and the BGP router still responds to RR request
                 from the peer. However, route refresh messages will never
                 be sent to this peer."
    DEFVAL { false }
    ::= { eltexBgpPeerEntry 24 }

  eltexBgpPeerConfigPeerGroup OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This is the index of the peer group. If a peer is  not in
                 a peer group then its eltexBgpPeerConfigPeerGroup value is 0"
    ::= { eltexBgpPeerEntry 25 }

   eltexBgpPeerBfdDesired OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Indicates whether Bidirectional Forwarding Detection (BFD) is
                 desired for this peer.

                 This field can be changed at any time."
    DEFVAL { false }
    ::= { eltexBgpPeerEntry 27 }

  eltexBgpPeerPassword OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..80))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The MD5 password used by this peer. This field can only be
                 changed when the row is not active."
    ::= { eltexBgpPeerEntry 28 }

  eltexBgpPeerPasswordKeyChain OBJECT-TYPE
      SYNTAX      OCTET STRING (SIZE (0..32))
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "Name of key chain for MD5 digest calculation."
  ::= { eltexBgpPeerEntry 29 }

  eltexBgpPeerAsPathListIn OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The AS Path Access List name identifying the AS Path Access List
                 to use to filter routes received from the peer.

                 If this name is non-NULL string and the AS Path Access List with
                 this name is defined, then routes received from this peer
                 are matched against this filter list and permitted or
                 denied as defined by the filter list."
    ::= { eltexBgpPeerEntry 30 }

  eltexBgpPeerAsPathListOut OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The AS Path Access List name identifying the AS Path Access List
                 to use to filter routes advertised to the peer.

                 If this name is non-NULL string and the AS Path Access List with
                 this name is defined, then routes to be advertised to this peer
                 are matched against this filter list and advertised or
                 not as defined by the filter list."
    ::= { eltexBgpPeerEntry 31 }

  eltexBgpPeerEbgpMultihop OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "If this field is set to TRUE and this is an eBGP neighbor,
                 then the TTL value will change to default value
                 (value in MIB_ipDefaultTTL_CNS).

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN."
    DEFVAL { false }
    ::= { eltexBgpPeerEntry 33 }

  eltexBgpPeerCoreTracking OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "If this field is set to TRUE, the core availability is monitored. 
                 When all BGP sessions with the core are broken, an emergency shutdown 
                 of the connections of all ES participants must be called.
                 This field can be changed at any time."
    DEFVAL { false }
    ::= { eltexBgpPeerEntry 34 }

  eltexBgpPeerAsOverride OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This field is used in conjunction with eltexBgpPeerAddrFamilyAsOverride
                 to indicate whether BGP should perform AS-override on routes
                 advertised to the peer.

                 If AS-override is enabled, then when advertising routes to this
                 peer for this address-family, any instance of the peer's AS
                 number will be replaced in the advertised AS path with the
                 local AS number.

                 The peer may be configured to ignore this field and instead
                 obtain the value from a peer group as explained in the table
                 description.

                 AS-override may be enabled independently for each address family.
                 When eltexBgpPeerAsOverride is set to 'true', set
                 eltexBgpPeerAddrFamilyAsOverride to 'true' or 'false' to enable
                 or disable as-override for each address family.

                 If the value of this object is changed while the peer session is
                 active, BGP will check for any routes that need to be advertised
                 or withdrawn as a result of the change.

                 Note that this field has no effect when set for iBGP peers."
    DEFVAL      { false }
    ::= { eltexBgpPeerEntry 35 }

  eltexBgpPeerAllowAsIn OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The number of instances of the local AS identifier that may
                 be contained in the route's AS-Path without rejecting the
                 route.

                 The AS-Path attribute of a BGP route contains the identifiers
                 of the Autonomous Systems traversed by the route.  When
                 a route is received with an AS-Path containing the local
                 AS identifier, it normally indicates a routing loop, and
                 the default behavior is to reject the route.  This object
                 allows this behavior to be over-ridden.

                 This is useful, for example, for VPN routes, where routes
                 from one CE router are advertised to other CE routers
                 through a provider's BGP network.  Two CE routers in
                 the same AS can enable this feature to prevent routes from
                 the other CE from being discarded.

                 When eltexBgpPeerAllowAsIn is set to a non-zero value, that
                 value is used for all address families, and the value of
                 eltexBgpPeerAddrFamilyAllowAsIn is ignored.

                 Alternatively, the value may be configured independently for
                 each address family.  To do this, set eltexBgpPeerAllowAsIn to 0
                 and set the value of eltexBgpPeerAddrFamilyAllowAsIn for each
                 address family.

                 Changing the value of this object while the peer is active
                 triggers BGP to refresh its routes from the peer."
    DEFVAL { 0 }
    ::= { eltexBgpPeerEntry 36 }

--
-- BGP Peer <AFI, SAFI> configuration table.
--

  eltexBgpPeerAddrFamilyTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPeerAddrFamilyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "BGP Peer <AFI, SAFI> configuration table.

                 This table allows a user to configure peer characteristics
                 on a per AFI/SAFI basis.

                 This table is a configuration table - all status, statistics
                 and control fields are deprecated in favor of the BGP peer
                 AFI/SAFI status table (etlexBgpPeerAddrFamilyStatusTable).

                 This table does not contain entries for dynamic peers."
    ::= { eltexBgpPeerData 2 }
    
  eltexBgpPeerAddrFamilyEntry OBJECT-TYPE
    SYNTAX      EltexBgpPeerAddrFamilyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Peer <AFI, SAFI> configuration table entry."
    INDEX { eltexBgpProcessId,
            eltexBgpPeerRemoteAddrType,
            eltexBgpPeerRemoteAddr,
            eltexBgpPeerAddrFamilyAfi,
            eltexBgpPeerAddrFamilySafi }
    ::= { eltexBgpPeerAddrFamilyTable 1 }

  EltexBgpPeerAddrFamilyEntry ::= SEQUENCE {
      eltexBgpPeerAddrFamilyAfi               EltexBgpAfi,
      eltexBgpPeerAddrFamilySafi              EltexBgpSafi,
      eltexBgpPeerAddrFamilyDisable           TruthValue,
      eltexBgpPeerAddrFamilyNxtHopSlf         TruthValue,
      eltexBgpPeerAddrFamilyConfigMaxPrfx     Unsigned32,
      eltexBgpPeerAddrFamilyConfigDropWarn    EltexBgpConfigDropOrWarn,
      eltexBgpPeerAddrFamilyMaxPrfxHold       Unsigned32,
      eltexBgpPeerAddrFamilyConfigThreshold   Unsigned32,
      eltexBgpPeerAddrFamilyMinRteAdvertInt   Unsigned32,
      eltexBgpPeerAddrFamilyMinASOrigInt      Unsigned32,
      eltexBgpPeerAddrFamilyMinRteWithdrawInt Unsigned32,
      eltexBgpPeerAddrFamilyReflectorClient   EltexBgpPeerReflectorClientType,
      eltexBgpPeerAddrFamilyRouteMapIn        DisplayString,
      eltexBgpPeerAddrFamilyRouteMapOut       DisplayString,
      eltexBgpPeerAddrFamilyOrigDefault       TruthValue,
      eltexBgpPeerAddrFamilyOrigDefaultMap    DisplayString,
      eltexBgpPeerAddrFamilyPreserveNextHop   TruthValue,
      eltexBgpPeerAddrFamilyAsOverride        TruthValue,
      eltexBgpPeerAddrFamilyAllowAsIn         Unsigned32,
      eltexBgpPeerAddrFamilyAddPathCapCfg     EltexBgpAddPathSrCap,
      eltexBgpPeerAddrFamilyAddPathBestN      Unsigned32
    }

  eltexBgpPeerAddrFamilyAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The AFI index into the peer <AFI, SAFI> table."
    ::= { eltexBgpPeerAddrFamilyEntry 1 }

  eltexBgpPeerAddrFamilySafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The SAFI index into the peer <AFI, SAFI> table."
    ::= { eltexBgpPeerAddrFamilyEntry 2 }

  eltexBgpPeerAddrFamilyDisable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "When eltexBgpPeerAddrFamilyDisable is 'true', BGP will not
                 advertise Multiprotocol support to the peer for this
                 address family.

                 When eltexBgpPeerAddrFamilyDisable is 'false', BGP will
                 advertise Multiprotocol support to the peer if support 
                 for the address family has been enabled in the 
                 corresponding bgpRmAfiSafiTable entry.

                 Any update to this object will take effect the next time
                 that the eltexBgpPeerTable entry is activated
                 (eltexBgpPeerAdminStatus is changed to 'adminStatusUp').

                 If config usage bit eltexBgpPeerAddrFamilyGroupDisable 
                 is set, and the peer belongs to a peer group, then the
                 eltexBgpPeerAddrFamilyGroupDisable value is used instead 
                 of this value."
    DEFVAL { true }
    ::= { eltexBgpPeerAddrFamilyEntry 3 }

  eltexBgpPeerAddrFamilyNxtHopSlf OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Gives finer control of the next-hop-self configuration
                 provided by eltexBgpPeerNxtHopSlf.

                 When eltexBgpPeerNxtHopSlf is 'false', BGP does not perform
                 next-hop-self for any address family.

                 When eltexBgpPeerNxtHopSlf is 'true', BGP performs 
                 next-hop-self for those address families for which 
                 eltexBgpPeerAddrFamilyNxtHopSlf is 'true'.

                 If the value of this object is changed while the peer session
                 is active, BGP will check for any routes that need to be
                 advertised or withdrawn as a result of the change."
    DEFVAL { true }
    ::= { eltexBgpPeerAddrFamilyEntry 4 }

  eltexBgpPeerAddrFamilyConfigMaxPrfx OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Gives finer control of the maximum prefix configuration
                 provided by eltexBgpPeerConfigMaxPrfx.

                 To configure address family specific values for the maximum
                 number of prefixes that can be accepted from the peer,
                 set eltexBgpPeerConfigMaxPrfx to zero, and set
                 eltexBgpPeerAddrFamilyConfigMaxPrfx to the limit 
                 for this address family."
    DEFVAL { 0 }
    ::= { eltexBgpPeerAddrFamilyEntry 5 }

  eltexBgpPeerAddrFamilyConfigDropWarn OBJECT-TYPE
    SYNTAX      EltexBgpConfigDropOrWarn
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Gives finer control of the configuration provided by
                 eltexBgpPeerConfigDropWarn, which determines the behavior
                 when the maximum prefix limit is reached.

                 To configure whether the session is dropped or a warning is
                 behavior independently for different address
                 families, set eltexBgpPeerConfigDropWarn to 'warn', and set
                 the value of eltexBgpPeerAddrFamilyConfigDropWarn for 
                 each address family as needed."
    DEFVAL { warn }
    ::= { eltexBgpPeerAddrFamilyEntry 6 }

  eltexBgpPeerAddrFamilyMaxPrfxHold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Gives finer control of the configuration provided by
                 eltexBgpPeerMaxPrfxHold, which determines the time interval in
                 seconds between when this BGP session is torn down due to
                 the number of prefixes received from this peer exceeding the
                 maximum in eltexBgpPeerConfigMaxPrfx(AfiSafi) and when BGP
                 attempts to reestablish the session.

                 To configure a time interval for individual families, set
                 eltexBgpPeerMaxPrfxHold to zero and set 
                 eltexBgpPeerAddrFamilyMaxPrfxHold to the required time 
                 interval for each address family."
    DEFVAL { 90 }
    ::= { eltexBgpPeerAddrFamilyEntry 7 }

  eltexBgpPeerAddrFamilyConfigThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Gives finer control of the threshold configuration
                 provided by eltexBgpPeerConfigThreshold.  When the number of
                 prefixes received from this peer for this address family
                 reaches this threshold, BGP issues a warning.

                 This field is not used if eltexBgpPeerConfigMaxPrfx and
                 eltexBgpPeerAddrFamilyConfigThreshold are set to zero.

                 To configure a threshold for individual families, set
                 eltexBgpPeerConfigMaxPrfx to zero and set
                 eltexBgpPeerAddrFamilyConfigThreshold to the required 
                 threshold for each address family."
    DEFVAL { 75 }
    ::= { eltexBgpPeerAddrFamilyEntry 8 }

  eltexBgpPeerAddrFamilyMinRteAdvertInt OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the
                 MinRouteAdvertisementInterval timer.  This determines the
                 minimum time between a BGP UPDATE to a peer advertising or
                 withdrawing a route and a subsequent BGP UPDATE to the
                 peer advertising a route to the same destination."
    DEFVAL      { 30 }
    ::= { eltexBgpPeerAddrFamilyEntry 9 }

  eltexBgpPeerAddrFamilyMinASOrigInt OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for determining the minimum
                 amount of time that must elapse between successive
                 advertisements of UPDATE messages that report changes to a
                 route within the advertising BGP speaker's own autonomous
                 system.

                 This field has no effect if
                 eltexBgpPeerMinASOriginationInterval is set to a non-zero
                 value.  To configure values independently for each address
                 family, set eltexBgpPeerMinASOriginationInterval to 0 and set
                 the values of eltexBgpPeerAddrFamilyMinASOrigInt as required."
    DEFVAL      { 15 }
    ::= { eltexBgpPeerAddrFamilyEntry 10 }

  eltexBgpPeerAddrFamilyMinRteWithdrawInt OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the MinRouteWithdrawInterval
                 timer.  This is the interval which is enforced between
                 advertisement and subsequent withdrawal of a route.

                 This field has no effect if 
                 eltexBgpPeerMinRouteWithdrawInterval is set to a non-zero 
                 value. To configure values independently for each address 
                 family, set eltexBgpPeerMinRouteWithdrawInterval to 0 and
                 set the values of eltexBgpPeerAddrFamilyMinRteWithdrawInt 
                 as required."
    DEFVAL      { 0 }
    ::= { eltexBgpPeerAddrFamilyEntry 11 }

  eltexBgpPeerAddrFamilyReflectorClient OBJECT-TYPE
    SYNTAX      EltexBgpPeerReflectorClientType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Gives finer control of the configuration provided by
                 eltexBgpPeerReflectorClient.

                 This value indicates whether the given peer is a reflector
                 client of this router for this AFI/SAFI, or not.  A value
                 of nonClient(0) indicates that this peer is not a
                 reflector client for this AFI/SAFI.  A value of client(1)
                 indicates that this peer is a reflector client for this
                 AFI/SAFI that is not fully meshed with other reflector
                 clients.  A value of meshedClient(2) indicates that the
                 peer is a reflector client for this AFI/SAFI and is fully
                 meshed with all other reflector clients.

                 The peer's reflector-client setting for this AFI/SAFI is
                 chosen as follows.

                 -  If the peer is not a member of a peer group
                    o  If eltexBgpPeerReflectorClient is NOT non-client then use
                       that
                    o  Otherwise use eltexBgpPeerAddrFamilyReflectorClient.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL      { nonClient }
    ::= { eltexBgpPeerAddrFamilyEntry 12 }

  eltexBgpPeerAddrFamilyRouteMapIn OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The name of the Route Map to use for route imports from
                 the peer for this AFI/SAFI."
    ::= { eltexBgpPeerAddrFamilyEntry 13 }

  eltexBgpPeerAddrFamilyRouteMapOut OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The name of the Route Map to use for route exports to the
                 peer for this AFI/SAFI."
    ::= { eltexBgpPeerAddrFamilyEntry 14 }

    eltexBgpPeerAddrFamilyOrigDefault OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Indicates whether BGP should originate a default route to
                 the peer for this AFI/SAFI."
    DEFVAL       { false }
    ::= { eltexBgpPeerAddrFamilyEntry 15 }

    eltexBgpPeerAddrFamilyOrigDefaultMap OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The name of the Route Map to use for default route exports to the
                 peer for this AFI/SAFI."
    ::= { eltexBgpPeerAddrFamilyEntry 16 }
    
    eltexBgpPeerAddrFamilyPreserveNextHop OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This field is used to preserve the BGP next hop when
                 forwarding routes to this eBGP peer.

                 By default, the next hop of a route is preserved when
                 advertising the route to an iBGP peer, but is updated when
                 advertising the route to an eBGP peer.  Setting this to
                 'true' over-rides this behavior and preserves the next hop
                 when routes are advertised to this eBGP peer.

                 The peer may be configured to ignore this field and
                 instead obtain the value from a peer-group as explained in
                 the table description."
    DEFVAL { false }
    ::= { eltexBgpPeerAddrFamilyEntry 17 }

  eltexBgpPeerAddrFamilyAsOverride OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This field is used in conjunction with eltexBgpPeerAsOverride
                 to indicate whether BGP should perform AS-override on routes
                 advertised to the peer.

                 If AS-override is enabled, then when advertising routes to this
                 peer for this address-family, any instance of the peer's AS
                 number will be replaced in the advertised AS path with the
                 local AS number.

                 The peer may be configured to ignore this field and instead
                 obtain the value from a peer group as explained in the table
                 description.

                 AS-override may be enabled independently for each address family.
                 When eltexBgpPeerAddrFamilyAsOverride is set to 'true', set
                 eltexBgpPeerAsOverride to 'true' or 'false' to enable
                 or disable as-override for each address family.

                 If the value of this object is changed while the peer session is
                 active, BGP will check for any routes that need to be advertised
                 or withdrawn as a result of the change.

                 Note that this field has no effect when set for iBGP peers."
    DEFVAL { true }
    ::= { eltexBgpPeerAddrFamilyEntry 18 }

  eltexBgpPeerAddrFamilyAllowAsIn OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The number of instances of the local AS identifier that may
                 be contained in the route's AS-Path without rejecting the
                 route.

                 The AS-Path attribute of a BGP route contains the identifiers
                 of the Autonomous Systems traversed by the route.  When
                 a route is received with an AS-Path containing the local
                 AS identifier, it normally indicates a routing loop, and
                 the default behavior is to reject the route.  This object
                 allows this behavior to be over-ridden.

                 This is useful, for example, for VPN routes, where routes
                 from one CE router are advertised to other CE routers sites
                 through a provider's BGP network.  Two CE routers in
                 the same AS can enable this feature to prevent routes from
                 the other CE from being discarded.

                 If eltexBgpPeerAllowAsIn is set to a non-zero value, then that
                 value is used for all address families, and the value of
                 eltexBgpPeerAddrFamilyAllowAsIn is ignored.

                 To configure values independently for each address family, set
                 eltexBgpPeerAllowAsIn to 0 and set the values of
                 eltexBgpPeerAddrFamilyAllowAsIn as required.

                 Changing the value of this object while the peer is active
                 triggers BGP to refresh its routes from the peer."
    DEFVAL { 0 }
    ::= { eltexBgpPeerAddrFamilyEntry 19 }

  eltexBgpPeerAddrFamilyAddPathCapCfg OBJECT-TYPE
    SYNTAX      EltexBgpAddPathSrCap
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The configured BGP additional path capability for this
                 peer and AFI/SAFI.

                 Valid values are:
                 -  disable (0)
                    Disable sending and receiving additional BGP paths
                 -  receive (1)
                    Receive but do not send additional BGP paths
                 -  send (2)
                    Send but do not receive additional BGP paths
                 -  both (3)
                    Send and receive additional BGP paths
                 -  inherit (4)
                    Inherit configuration from the BGP process AFI/SAFI
                    level (eltexBgpProcessAddrFamilyAddPathCapCfg).

                 The effective BGP additional path capabilities for the
                 session are negotiated with the peer and are reported by
                 the eltexBgpPeerAddrFamilyStatusAddPathCapNeg field.

                 Any update to this object will take effect the next time
                 that the eltexBgpPeerTable entry is activated
                 (eltexBgpPeerAdminStatus is changed to 'adminStatusUp')."
    DEFVAL { inherit }
    ::= { eltexBgpPeerAddrFamilyEntry 20 }

  eltexBgpPeerAddrFamilyAddPathBestN OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The number of best paths to advertise to this peer as
                 additional paths for this AFI/SAFI.

                 The number of candidate paths available to advertise to
                 the peer depends on the value of the
                 eltexBgpProcessAddrFamilyAddPathBestN field.
                 This field specifies how many of
                 the candidate paths to advertise to this peer.

                 For the default value of 1 only the best path for each
                 destination is advertised.

                 A value of 2 is sufficient to advertise the best path and
                 2nd best path for each destination.

                 Any additional paths are advertised to peers subject to
                 split horizon rules, export policy, and BGP ADD-PATH
                 capability negotiation. These filters apply after
                 selecting the best N paths to advertise, so the actual
                 number of paths advertised may be smaller.

                 Changing the value of this field while the peer is active
                 triggers BGP to advertise additional paths according to
                 the new configuration."
    DEFVAL { 1 }
    ::= { eltexBgpPeerAddrFamilyEntry 21 }

  --
  -- BGP peer status table.
  --
  -- This table reports BGP peer status and statistics.
  --

  eltexBgpPeerStatusTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPeerStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "BGP peer status table.

                 This table reports BGP peer status and statistics.  It also
                 allows a user to control BGP peer statistics and peer
                 sessions.

                 This table does not contain any BGP peer configuration -
                 the eltexBgpPeerTable MIB is the BGP peer configuration MIB.

                 This table contains entries for both configured and dynamic
                 peers.

                 For configured peers the corresponding rows in the
                 eltexBgpPeerTable MIB and eltexBgpPeerStatusTable MIB have
                 identical index fields.

                 The lifetime of a BGP peer status entry depends on whether
                 the BGP peer is configured or dynamic.
                 -  The entry for a configured peer is created and destroyed
                 when the corresponding entry in the BGP peer
                 configuration table (eltexBgpPeerTable) is created and
                 destroyed.
                 -  The entry for a dynamic peer is created when the BGP
                 peering session is established.  It is destroyed when
                 the BGP session has terminated."
    ::= { eltexBgpPeerData 3 }

  eltexBgpPeerStatusEntry OBJECT-TYPE
    SYNTAX      EltexBgpPeerStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Entry containing information about the status of a BGP peer."
    INDEX { eltexBgpProcessId,
            eltexBgpPeerRemoteAddrType,
            eltexBgpPeerRemoteAddr }
    ::= { eltexBgpPeerStatusTable 1 }

  EltexBgpPeerStatusEntry ::= SEQUENCE {
      eltexBgpPeerStatusIdentifier              EltexBgpIdentifier,
      eltexBgpPeerStatusState                   EltexBgpPeerStates,
      eltexBgpPeerStatusDynamicPeer             TruthValue,
      eltexBgpPeerStatusRemoteAs                EltexBgpAutonomousSystemNumber,
      eltexBgpPeerStatusPeerIndex               Unsigned32,
      eltexBgpPeerStatusCapsSupport             TruthValue,
      eltexBgpPeerStatusLastError               OCTET STRING,
      eltexBgpPeerStatusLastErrorDataLen        Unsigned32,
      eltexBgpPeerStatusLastErrorData           OCTET STRING,
      eltexBgpPeerStatusFsmEstablishedTime      Gauge32,
      eltexBgpPeerStatusInUpdatesElpsTime       Gauge32,
      eltexBgpPeerStatusHoldTime                Integer32,
      eltexBgpPeerStatusKeepAlive               Integer32,
      eltexBgpPeerStatusInOpens                 Counter32,
      eltexBgpPeerStatusOutOpens                Counter32,
      eltexBgpPeerStatusInNotifications         Counter32,
      eltexBgpPeerStatusOutNotifications        Counter32,
      eltexBgpPeerStatusInUpdates               Counter32,
      eltexBgpPeerStatusOutUpdates              Counter32,
      eltexBgpPeerStatusInKeepalives            Counter32,
      eltexBgpPeerStatusOutKeepalives           Counter32,
      eltexBgpPeerStatusInRefreshes             Counter32,
      eltexBgpPeerStatusOutRefreshes            Counter32,
      eltexBgpPeerStatusInTotalMessages         Counter32,
      eltexBgpPeerStatusOutTotalMessages        Counter32,
      eltexBgpPeerStatusFsmEstTransitions       Counter32,
      eltexBgpPeerStatusConnectRetryCount       Counter32,
      eltexBgpPeerStatusClearCnts               TruthValue,
      eltexBgpPeerStatusRtRefresh               TruthValue,
      eltexBgpPeerStatusLastErrorRcvd           OCTET STRING,
      eltexBgpPeerStatusLastErrorRcvdTime       TimeStamp,
      eltexBgpPeerStatusLastErrorSent           OCTET STRING,
      eltexBgpPeerStatusLastErrorSentTime       TimeStamp,
      eltexBgpPeerStatusLastState               EltexBgpPeerStates,
      eltexBgpPeerStatusLastEvent               EltexBgpPeerEvents,
      eltexBgpPeerStatusCapsSent                EltexBgpCapabilities,
      eltexBgpPeerStatusCapsRcvd                EltexBgpCapabilities,
      eltexBgpPeerStatusCapsNegotiated          EltexBgpCapabilities,
      eltexBgpPeerStatusRcvdMsgElpsTime         TimeInterval,
      eltexBgpPeerStatusIdleHoldRemTime         TimeInterval,
      eltexBgpPeerStatusRouteRefrSent           Counter32,
      eltexBgpPeerStatusRouteRefrRcvd           Counter32,
      eltexBgpPeerStatusSelLocalAddrType        InetAddressType,
      eltexBgpPeerStatusSelLocalAddr            InetAddress,
      eltexBgpPeerStatusSelLocalPort            InetPortNumber,
      eltexBgpPeerStatusSelRemotePort           InetPortNumber,
      eltexBgpPeerStatusSelLocalAs              EltexBgpAutonomousSystemNumber,
      eltexBgpPeerStatusSelRemoteAs             EltexBgpAutonomousSystemNumber,
      eltexBgpPeerStatusInPrfxes                Gauge32,
      eltexBgpPeerStatusOutPrfxes               Gauge32,
      eltexBgpPeerStatusOutPrfxesAdvertised     Gauge32,
      eltexBgpPeerStatusConfigState             EltexBgpPeerConfigStates,
      eltexBgpPeerStatusConnectRetryInt         Unsigned32,
      eltexBgpPeerStatusConfigPassive           TruthValue,
      eltexBgpPeerStatusConfigOpenDelay         Unsigned32,
      eltexBgpPeerStatusConfigIdleHold          Unsigned32,
      eltexBgpPeerStatusTtl                     Integer32,
      eltexBgpPeerStatusHoldTimeConfigd         Unsigned32,
      eltexBgpPeerStatusKeepAliveConfigd        Unsigned32,
      eltexBgpPeerStatusResendAllRoutes         TruthValue,
      eltexBgpPeerStatusOutUpdateElpsTime       Gauge32,
      eltexBgpPeerStatusOutPrfxesDenied         Counter32,
      eltexBgpPeerStatusOutPrfxesImpWdr         Counter32,
      eltexBgpPeerStatusOutPrfxesExpWdr         Counter32,
      eltexBgpPeerStatusInPrfxesImpWdr          Counter32,
      eltexBgpPeerStatusInPrfxesExpWdr          Counter32,
      eltexBgpPeerStatusReceivedHoldTime        Integer32,
      eltexBgpPeerStatusDropSession             TruthValue,
      eltexBgpPeerStatusCeaseErrorSubcode       EltexBgpCeaseErrorSubcode,
      eltexBgpPeerStatusBfdStatus               EltexBfdSessionStatus,
      eltexBgpPeerStatusPeerGroup               DisplayString
    }

  eltexBgpPeerStatusIdentifier OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The BGP Identifier of this entry's BGP peer.

                 This entry is zero unless the eltexBgpPeerStatusState is in the
                 openconfirm or the established state."
    ::= { eltexBgpPeerStatusEntry 1 }

  eltexBgpPeerStatusState OBJECT-TYPE
    SYNTAX      EltexBgpPeerStates
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The BGP peer's FSM state."
    ::= { eltexBgpPeerStatusEntry 2 }

  eltexBgpPeerStatusDynamicPeer OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether the peer is dynamic (true) or individually
                 configured (false)."
    ::= { eltexBgpPeerStatusEntry 3 }

  eltexBgpPeerStatusRemoteAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The remote autonomous system number in use on the session.
                 For configured peers not yet active, this is the
                 configured value."
    ::= { eltexBgpPeerStatusEntry 4 }

  eltexBgpPeerStatusPeerIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The peer index.

                 The peer index is a unique index for the peer entry in the
                 eltexBgpPeerStatusTable.  It is used to provide an index value
                 for other tables whose data is logically per-peer."
    ::= { eltexBgpPeerStatusEntry 5 }

  eltexBgpPeerStatusCapsSupport OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether or not this peer accepted our local capabilities
                 optional parameter sent on the OPEN message.  This field
                 will not be relevant until the peer has reached open_confirm
                 state.  Note that this field indicates support or otherwise
                 of the capabilities optional parameter, not a specific
                 capability."
    ::= { eltexBgpPeerStatusEntry 6 }

  eltexBgpPeerStatusLastError OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The last error code and subcode sent or received on this
                 connection.  If no error has occurred, this field is zero.
                 Otherwise, the first byte of this two byte OCTET STRING
                 contains the error code, and the second byte contains the
                 subcode."
    ::= { eltexBgpPeerStatusEntry 7 }

  eltexBgpPeerStatusLastErrorDataLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The length of the last error data.  If this is zero no
                 error data was provided or generated."
    ::= { eltexBgpPeerStatusEntry 8 }

  eltexBgpPeerStatusLastErrorData OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The last error code's data seen by this peer on this
                 connection."
    ::= { eltexBgpPeerStatusEntry 9 }

  eltexBgpPeerStatusFsmEstablishedTime OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This timer indicates how long in seconds this peer has
                 been in the Established state or how long since this peer
                 was last in the Established state.  It is set to zero when
                 a new peer is configured or the router is booted."
    ::= { eltexBgpPeerStatusEntry 10 }

  eltexBgpPeerStatusInUpdatesElpsTime OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Elapsed time in seconds since the last BGP Update message
                 was received from the peer."
    ::= { eltexBgpPeerStatusEntry 11 }

  eltexBgpPeerStatusHoldTime OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Time interval in seconds for the Hold Timer established
                 with the peer.

                 The Hold Timer interval is calculated by this BGP speaker by
                 using the smaller of the configured eltexBgpPeerHoldTimeConfigd
                 value and the Hold Time received in the OPEN message.

                 For dynamic peers the Hold Timer interval is calculated
                 using the default eltexBgpPeerHoldTimeConfigd value rather than
                 a configured value.

                 A value of zero indicates that the Hold Timer has not been
                 established with the peer."
    ::= { eltexBgpPeerStatusEntry 12 }

  eltexBgpPeerStatusKeepAlive OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Time interval in seconds for the KeepAlive Timer
                 established with the peer.

                 The KeepAlive Timer interval is calculated by this BGP speaker
                 such that, when compared with eltexBgpPeerStatusHoldTime,
                 it has the same proportion as the configured
                 eltexBgpPeerKeepAliveConfigd has when compared with
                 eltexBgpPeerHoldTimeConfigd.

                 For dynamic peers the KeepAlive Timer interval is calculated
                 using the default eltexBgpPeerKeepAliveConfigd and
                 eltexBgpPeerHoldTimeConfigd values rather than configured values.

                 A value of zero indicates that the KeepAlive Timer has not
                 been established with the peer."
    ::= { eltexBgpPeerStatusEntry 13 }

  eltexBgpPeerStatusInOpens OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP OPEN messages received on this
                 connection."
    ::= { eltexBgpPeerStatusEntry 14 }

  eltexBgpPeerStatusOutOpens OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP OPEN messages transmitted on this
                 connection."
    ::= { eltexBgpPeerStatusEntry 15 }

  eltexBgpPeerStatusInNotifications OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP NOTIFICATION messages received on this
                 connection."
    ::= { eltexBgpPeerStatusEntry 16 }

  eltexBgpPeerStatusOutNotifications OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP NOTIFICATION messages transmitted on
                 this connection."
    ::= { eltexBgpPeerStatusEntry 17 }

  eltexBgpPeerStatusInUpdates OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP UPDATE messages received on this
                 connection."
    ::= { eltexBgpPeerStatusEntry 18 }

  eltexBgpPeerStatusOutUpdates OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP UPDATE messages transmitted on this
                 connection."
    ::= { eltexBgpPeerStatusEntry 19 }

  eltexBgpPeerStatusInKeepalives OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP KEEPALIVE messages received on this
                 connection."
    ::= { eltexBgpPeerStatusEntry 20 }

  eltexBgpPeerStatusOutKeepalives OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP KEEPALIVE messages transmitted on this
                 connection."
    ::= { eltexBgpPeerStatusEntry 21 }

  eltexBgpPeerStatusInRefreshes OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP ROUTE REFRESH messages received on this
                 connection."
    ::= { eltexBgpPeerStatusEntry 22 }

  eltexBgpPeerStatusOutRefreshes OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of BGP ROUTE REFRESH messages transmitted on
                 this connection."
    ::= { eltexBgpPeerStatusEntry 23 }

  eltexBgpPeerStatusInTotalMessages OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The total number of messages received from the remote peer
                 on this connection."
    ::= { eltexBgpPeerStatusEntry 24 }

  eltexBgpPeerStatusOutTotalMessages OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The total number of messages transmitted to the remote
                 peer on this connection."
    ::= { eltexBgpPeerStatusEntry 25 }

  eltexBgpPeerStatusFsmEstTransitions OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The total number of times the BGP FSM transitioned into
                 the established state for this peer."
    ::= { eltexBgpPeerStatusEntry 26 }

  eltexBgpPeerStatusConnectRetryCount OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The current connect retry count of this peer.

                 This is incremented each time the peer session flaps, and is
                 used to determine the time to wait before retrying the
                 session.

                 Note this is only incremented when an active session
                 terminates abnormally, and not when it simply fails to come
                 up."
    ::= { eltexBgpPeerStatusEntry 27 }

  eltexBgpPeerStatusClearCnts OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this field to 'true' to clear the counters associated
                 with this peer.

                 Reading the value of this field has no meaning.  The field
                 is not returned on a MIB Get."
    ::= { eltexBgpPeerStatusEntry 28 }

  eltexBgpPeerStatusRtRefresh OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this field to 'true' to trigger sending a route
                 refresh request for this peer.

                 Setting this field will only have an effect if a BGP
                 session to the peer is active.  Peers that do not support
                 route refresh will have their sessions toggled.

                 Reading the value of this field has no meaning.  The field
                 is not returned on a MIB Get."
    ::= { eltexBgpPeerStatusEntry 29 }

  eltexBgpPeerStatusLastErrorRcvd OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The last error code and subcode received from the peer on
                 this connection.

                 If no error has been received from the peer, this field is
                 zero.  Otherwise, the first byte of this two byte OCTET
                 STRING contains the error code, and the second byte contains
                 the subcode."
    ::= { eltexBgpPeerStatusEntry 30 }

  eltexBgpPeerStatusLastErrorRcvdTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The value of sysUpTime when the last error was received
                 from the peer on this connection.

                 If no error has been received from the peer, this field is
                 zero."
    ::= { eltexBgpPeerStatusEntry 31 }

  eltexBgpPeerStatusLastErrorSent OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The last error code and subcode sent to the peer on this
                 connection.

                 If no error has been sent to the peer, this field is zero.
                 Otherwise, the first byte of this two byte OCTET STRING
                 contains the error code, and the second byte contains the
                 subcode."
    ::= { eltexBgpPeerStatusEntry 32 }

  eltexBgpPeerStatusLastErrorSentTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The value of sysUpTime when the last error was sent to the
                 peer on this connection.

                 If no error has been sent to the peer, this field is zero."
    ::= { eltexBgpPeerStatusEntry 33 }

  eltexBgpPeerStatusLastState OBJECT-TYPE
    SYNTAX      EltexBgpPeerStates
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The BGP peer's previous FSM state."
    ::= { eltexBgpPeerStatusEntry 34 }

  eltexBgpPeerStatusLastEvent OBJECT-TYPE
    SYNTAX      EltexBgpPeerEvents
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The last input to be made to the BGP peer's FSM."
    ::= { eltexBgpPeerStatusEntry 35 }

  eltexBgpPeerStatusCapsSent OBJECT-TYPE
    SYNTAX      EltexBgpCapabilities
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The capabilities announced to the peer on the most recent
                 Open message sent to the peer.  This field is set to zero
                 before the first Open message is sent to the peer, and
                 is unchanged if the session comes down."
    ::= { eltexBgpPeerStatusEntry 36 }

  eltexBgpPeerStatusCapsRcvd OBJECT-TYPE
    SYNTAX      EltexBgpCapabilities
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The capabilities received on the most recent Open message
                 received from the peer.  This field is set to zero before
                 the first Open message is received from the peer, and is
                 unchanged if the session comes down.

                 In the event that the peer signals a capability that BGP
                 does not recognize, this field will only contain those
                 capabilities that BGP recognizes.  A user should walk the
                 eltexBgpPeerCapsRcvdTable to confirm the full list of
                 capabilities received from the peer."
    ::= { eltexBgpPeerStatusEntry 37 }

  eltexBgpPeerStatusCapsNegotiated OBJECT-TYPE
    SYNTAX      EltexBgpCapabilities
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The capabilities negotiated for the session with the peer.
                 This field is set to zero before Open messages have been
                 exchanged with the peer, and is unchanged if the session
                 comes down."
    ::= { eltexBgpPeerStatusEntry 38 }

  eltexBgpPeerStatusRcvdMsgElpsTime OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The elapsed time in hundredths of a second since anything
                 was received from this peer.  If nothing has been received
                 from this peer, this field is set to zero.  If the session
                 comes down this value continues to increase."
    ::= { eltexBgpPeerStatusEntry 39 }

  eltexBgpPeerStatusIdleHoldRemTime OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "For a peer in 'idle' state, the time remaining in
                 hundredths of a second until BGP will try to reactivate
                 the connection.  If the peer is not in 'idle' state, this is
                 set to zero."
    ::= { eltexBgpPeerStatusEntry 40 }

  eltexBgpPeerStatusRouteRefrSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of Route Refresh messages sent to the peer.

                 If the session comes down this value is unchanged, and will
                 continue to increment if the session is reestablished.

                 However, for dynamic peers the peer status entry is lost
                 if the BGP session is not re-established within the graceful
                 restart period, and in this case the value of this field
                 is lost."
    ::= { eltexBgpPeerStatusEntry 41 }

  eltexBgpPeerStatusRouteRefrRcvd OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of Route Refresh messages received from the
                 peer.

                 If the session comes down this value is unchanged, and will
                 continue to increment if the session is reestablished.

                 However, for dynamic peers the peer status entry is lost
                 if the BGP session is not re-established within the graceful
                 restart period, and in this case the value of this field
                 is lost."
    ::= { eltexBgpPeerStatusEntry 42 }

  eltexBgpPeerStatusSelLocalAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The address family of the local address used by the
                 transport connection for the peering session.

                 A value of none implies that there is currently no
                 connection to this peer."
    ::= { eltexBgpPeerStatusEntry 43 }

  eltexBgpPeerStatusSelLocalAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The local address used by the transport connection for the
                 peering session."
    ::= { eltexBgpPeerStatusEntry 44 }

  eltexBgpPeerStatusSelLocalPort OBJECT-TYPE
    SYNTAX      InetPortNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The local port used by the transport connection for the
                 peering session.

                 A value of zero implies that there is currently no
                 connection to this peer."
    ::= { eltexBgpPeerStatusEntry 45 }

  eltexBgpPeerStatusSelRemotePort OBJECT-TYPE
    SYNTAX      InetPortNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The remote port used by the transport connection for the
                 peering session.

                 A value of zero implies that there is currently no
                 connection to this peer."
    ::= { eltexBgpPeerStatusEntry 46 }

  eltexBgpPeerStatusSelLocalAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The local AS number used on this session.

                 If the eltexBgpPeerStatusState is not 'established', then this
                 field is zero."
    ::= { eltexBgpPeerStatusEntry 47 }

  eltexBgpPeerStatusSelRemoteAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The remote AS number used on this session.

                 If the eltexBgpPeerStatusState is not 'established', then this
                 field is zero."
    ::= { eltexBgpPeerStatusEntry 48 }

  eltexBgpPeerStatusInPrfxes OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The total number of prefixes received from this peer."
    ::= { eltexBgpPeerStatusEntry 49 }

  eltexBgpPeerStatusOutPrfxes OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of prefixes that are installed in all of this
                 peer's Adj-RIBs-Out."
    ::= { eltexBgpPeerStatusEntry 50 }

  eltexBgpPeerStatusOutPrfxesAdvertised OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The total number of prefixes advertised to this peer."
    ::= { eltexBgpPeerStatusEntry 51 }

  eltexBgpPeerStatusConfigState OBJECT-TYPE
    SYNTAX      EltexBgpPeerConfigStates
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This field reports the state of the peer configuration.
                 The peer configuration may be in one of the following
                 states.

                 -  Up to date.  That is, all configuration set by MIBs for
                 this peer has been applied to the current peer session
                 (if it exists).

                 -  Out of date, requiring the peer's admin status to be
                 set to down before all the current MIB configuration
                 for this peer can be applied.

                 -  Out of date, requiring the peer's row status to be set
                 to inactive before all the current MIB configuration
                 for this peer can be applied."
    ::= { eltexBgpPeerStatusEntry 52 }

  eltexBgpPeerStatusConnectRetryInt OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The currently active time interval for the ConnectRetry
                 timer.

                 This value may be different from the current peer MIB
                 value (eltexBgpPeerConnectRetryInterval) if the peer takes its
                 value from a peer group MIB
                 (eltexBgpPeergrConnectRetryInterval) or the MIB which provides
                 the value has been changed since the peer session was
                 started."
    ::= { eltexBgpPeerStatusEntry 53 }

  eltexBgpPeerStatusConfigPassive OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The current active passive flag.  If TRUE, then no
                 outbound connections will be initiated, and only incoming
                 connections will be accepted.  If FALSE, then outbound
                 connections will be attempted to this peer, and incoming
                 connections will be accepted from this peer."
    ::= { eltexBgpPeerStatusEntry 54 }

  eltexBgpPeerStatusConfigOpenDelay OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The currently active delay to enforce in between a TCP
                 connection with this peer becoming established and a BGP
                 Open message being sent."
    ::= { eltexBgpPeerStatusEntry 55 }

  eltexBgpPeerStatusConfigIdleHold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The currently active time to hold this peer in Idle state
                 after a BGP session has progressed beyond Idle state
                 initially and then returned to it."
    ::= { eltexBgpPeerStatusEntry 56 }

  eltexBgpPeerStatusTtl OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The currently active Time To Live used by the connection
                 on this peer."
    ::= { eltexBgpPeerStatusEntry 57 }

  eltexBgpPeerStatusHoldTimeConfigd OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The currently active time interval in seconds for the Hold
                 Time configured for this BGP speaker with this peer."
    ::= { eltexBgpPeerStatusEntry 58 }

  eltexBgpPeerStatusKeepAliveConfigd OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The currently active time interval in seconds for the
                 KeepAlive configured for this BGP speaker with this peer."
    ::= { eltexBgpPeerStatusEntry 59 }

  eltexBgpPeerStatusResendAllRoutes OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this to 'true' to trigger BGP to re-send all routes
                to the peer.  If the peer supports enhanced route refresh,
                then the routes will be sent as an unsolicited enhanced
                route refresh.

                Setting this field will only have an effect if a BGP
                session to the peer is active.

                This field always has the value 'false' when read."
    DEFVAL     { false }
    ::= { eltexBgpPeerStatusEntry 60 }

  eltexBgpPeerStatusOutUpdateElpsTime OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Elapsed time in seconds since the last BGP UPDATE message
                was sent to this peer.  Each time eltexBgpPeerStatusOutUpdates
                is incremented, the value of this object is set to zero
                (0)."
    ::= { eltexBgpPeerStatusEntry 61 }

  eltexBgpPeerStatusOutPrfxesDenied OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This is the number of prefixes in the Loc-RIB that have
                have failed export policy checks and so have not been
                installed in the Adj-RIB-Out for this peer."
    ::= { eltexBgpPeerStatusEntry 62 }

  eltexBgpPeerStatusOutPrfxesImpWdr OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The total number of routes for which an implicit withdraw
                has been sent to this peer.  A route is implicitly
                withdrawn if a replacement route with the same NLRI is
                advertised to the peer."
    ::= { eltexBgpPeerStatusEntry 63 }

  eltexBgpPeerStatusOutPrfxesExpWdr OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The total number of routes for which an explicit withdraw
                has been sent to this peer.  A route is explicitly
                withdrawn if it is advertised in the WITHDRAWN ROUTES
                field in an UPDATE message sent to the peer."
    ::= { eltexBgpPeerStatusEntry 64 }

  eltexBgpPeerStatusInPrfxesImpWdr OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The total number of routes that have been implicitly
                withdrawn by this peer.  A route is implicitly withdrawn
                if a replacement route with the same NLRI is received from
                the peer."
    ::= { eltexBgpPeerStatusEntry 65 }

  eltexBgpPeerStatusInPrfxesExpWdr OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The total number of routes that have been explicitly
                withdrawn by this peer.  A route is explicitly withdrawn
                if it is advertised in the WITHDRAWN ROUTES field in an
                UPDATE message received from the peer."
    ::= { eltexBgpPeerStatusEntry 66 }

  eltexBgpPeerStatusReceivedHoldTime OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The Hold Time value received in the OPEN message from this
                 peer.

                 A value of zero indicates that no Hold Time has been
                 received from the peer."
    ::= { eltexBgpPeerStatusEntry 67 }

  eltexBgpPeerStatusDropSession OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this field to 'true' to drop the current session with
                 the BGP peer.  For a dynamic BGP peer this causes the
                 peer status entry to disappear if the BGP session is not
                 re-established within the graceful restart period.

                 Reading the value of this field has no meaning.  The field
                 is not returned on a MIB Get."
    ::= { eltexBgpPeerStatusEntry 68 }

  eltexBgpPeerStatusCeaseErrorSubcode OBJECT-TYPE
    SYNTAX      EltexBgpCeaseErrorSubcode
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The error subcode to be sent in the Cease Notification
                 messages triggered by setting eltexBgpPeerStatusDropSession to
                 'true'.  If set to 'none' then DC-BGP chooses the subcode
                 itself.

                 This field does not affect the error subcode for Cease
                 Notification messages triggered for other reasons."
    DEFVAL      { none }
    ::= { eltexBgpPeerStatusEntry 69 }

  eltexBgpPeerStatusBfdStatus OBJECT-TYPE
    SYNTAX      EltexBfdSessionStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "BFD session state for this peer."
    ::= { eltexBgpPeerStatusEntry 70 }

  eltexBgpPeerStatusPeerGroup OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The peer group name this neighbor belongs to, or
                 empty string if this neighbor does not belong to a peer group.

                 For dynamic peers, this is the peer group name for the
                 peer range that this peer belongs to."
    ::= { eltexBgpPeerStatusEntry 71 }

  --
  -- BGP peer <AFI, SAFI> status table.
  --
  -- This table allows a user to control BGP peer AFI/SAFI operations.
  --

  eltexBgpPeerAddrFamilyStatusTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPeerAddrFamilyStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "BGP peer <AFI, SAFI> status table.

                 This table allows a user to control BGP peer AFI/SAFI
                 operations.

                 In future this table may also report BGP peer AFI/SAFI
                 status and statistics.

                 This table does not contain any BGP peer AFI/SAFI
                 configuration - the eltexBgpPeerAddrFamilyTable MIB is the BGP
                 peer AFI/SAFI configuration MIB.

                 This table contains entries for both configured and dynamic
                 peers.

                 Rows in this table cannot be created or destroyed manually.
                 A table entry for each supported address family is created
                 automatically when an entry in the eltexBgpPeerStatusTable is
                 created.  The entries are destroyed when the
                 eltexBgpPeerStatusTable entry is destroyed."
    ::= { eltexBgpPeerData 4 }

  eltexBgpPeerAddrFamilyStatusEntry OBJECT-TYPE
    SYNTAX      EltexBgpPeerAddrFamilyStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Entry containing information about the status of a BGP peer
                 for a particular AFI/SAFI."
    INDEX { eltexBgpProcessId,
            eltexBgpPeerRemoteAddrType,
            eltexBgpPeerRemoteAddr,
            eltexBgpPeerAddrFamilyAfi,
            eltexBgpPeerAddrFamilySafi }
    ::= { eltexBgpPeerAddrFamilyStatusTable 1 }

  EltexBgpPeerAddrFamilyStatusEntry ::= SEQUENCE {
      eltexBgpPeerAddrFamilyStatusRtRefresh              TruthValue,
      eltexBgpPeerAddrFamilyStatusAddPathCapNeg          EltexBgpAddPathSrCap,
      eltexBgpPeerAddrFamilyStatusReflectorClient        EltexBgpPeerReflectorClientType,
      eltexBgpPeerAddrFamilyStatusUpdateGroup            Unsigned32,
      eltexBgpPeerAddrFamilyStatusResendAllRoutes        TruthValue
    }

  eltexBgpPeerAddrFamilyStatusRtRefresh OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this to 'true' to trigger BGP to send a Route Refresh
                 request to the peer for this AFI/SAFI.

                 Setting this field will only have an effect if a BGP
                 session to the peer is active.  Peers that do not support
                 route refresh will have their sessions toggled.

                 This field always has the value 'false' when read."
    DEFVAL { false }
    ::= { eltexBgpPeerAddrFamilyStatusEntry 1 }

  eltexBgpPeerAddrFamilyStatusAddPathCapNeg OBJECT-TYPE
    SYNTAX      EltexBgpAddPathSrCap
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The BGP additional path capability negotiated with this
                 peer for this AFI/SAFI."
    ::= { eltexBgpPeerAddrFamilyStatusEntry 2 }

  eltexBgpPeerAddrFamilyStatusReflectorClient OBJECT-TYPE
    SYNTAX      EltexBgpPeerReflectorClientType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The currently active value which indicates whether the
                 given peer is a reflector client of this router for this
                 AFI/SAFI, or not.

                 This value may be different from the current peer AFI/SAFI
                 MIB value (eltexBgpPeerAddrFamilyReflectorClient) if any of the
                 following are true.
                 -  The peer takes its reflector client status from the
                    current peer MIB value (eltexBgpPeerReflectorClient) or from
                    a peer group MIB (eltexBgpPeerGroupReflectorClient).
                 -  The peer takes its value from a peer group AFI/SAFI MIB
                    (eltexBgpPeerAddrFamilyGroupReflectorClient).
                 -  The MIB which provides the value has been changed since
                    the peer session was started."
    ::= { eltexBgpPeerAddrFamilyStatusEntry 3 }

  eltexBgpPeerAddrFamilyStatusUpdateGroup OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The index of the update group that the peer is a member of
                for this AFI/SAFI.

                Zero if the peer is not a member of an update group."
    ::= { eltexBgpPeerAddrFamilyStatusEntry 4 }

  eltexBgpPeerAddrFamilyStatusResendAllRoutes OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Set this to 'true' to trigger BGP to re-send all routes
                to the peer for this AFI/SAFI.  If the peer supports
                enhanced route refresh, then this will be sent as an
                unsolicited enhanced route refresh.

                Setting this field will only have an effect if a BGP
                session to the peer is active.

                This field always has the value 'false' when read."
    DEFVAL { false }
    ::= { eltexBgpPeerAddrFamilyStatusEntry 5 }

-------------------------------------------------------------------------------

  eltexBgpPeerGroup      OBJECT IDENTIFIER ::= { eltexBgpPeer 2 }

  --
  -- BGP Peer Group Table
  --
  -- This table is used to create and manage Peer Groups.
  --


  eltexBgpPeerGroupTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPeerGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The table of peer groups.

                 A peer group is a set of peers that share a common peer
                 group configuration.

                 Using peer groups simplifies peer configuration.  Instead of
                 configuring many peers with the same set of configuration
                 values, you can configure a single peer group and then
                 assign peers to the peer group.

                 Each peer in a peer group has its eltexBgpPeerConfigPeerGroup value
                 set to the peer group index.  If a peer is  not in a peer group then
                 its eltexBgpPeerConfigPeerGroup value is 0."
    ::= { eltexBgpPeerGroup 1 }

  eltexBgpPeerGroupEntry OBJECT-TYPE
    SYNTAX      EltexBgpPeerGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Entry containing information about the connection with
                 a BGP peer."
    INDEX { eltexBgpProcessId,
            eltexBgpPeerGroupName }
    ::= { eltexBgpPeerGroupTable 1 }

  EltexBgpPeerGroupEntry ::= SEQUENCE {
      eltexBgpPeerGroupName                      DisplayString,
      eltexBgpPeerGroupRowStatus                 RowStatus,
      eltexBgpPeerGroupRemoteAs                  EltexBgpAutonomousSystemNumber,
      eltexBgpPeerGroupSourceInterface           InterfaceIndexOrZero,
      eltexBgpPeerGroupNxtHopSlf                 TruthValue,
      eltexBgpPeerGroupConfigMaxPrfx             Unsigned32,
      eltexBgpPeerGroupConfigDropWarn            EltexBgpConfigDropOrWarn,
      eltexBgpPeerGroupMaxPrfxHold               Unsigned32,
      eltexBgpPeerGroupConfigThreshold           Unsigned32,
      eltexBgpPeerGroupConnectRetryInterval      Unsigned32,
      eltexBgpPeerGroupHoldTimeConfigd           Unsigned32,
      eltexBgpPeerGroupKeepAliveConfigd          Unsigned32,
      eltexBgpPeerGroupMinRouteAdvertiseInterval Unsigned32,
      eltexBgpPeerGroupMinASOriginationInterval  Unsigned32,
      eltexBgpPeerGroupMinRouteWithdrawInterval  Unsigned32,
      eltexBgpPeerGroupConfigOpenDelay           Unsigned32,
      eltexBgpPeerGroupConfigIdleHold            Unsigned32,
      eltexBgpPeerGroupDistListPlIn              DisplayString,
      eltexBgpPeerGroupDistListPlOut             DisplayString,
      eltexBgpPeerGroupReflectorClient           EltexBgpPeerReflectorClientType,
      eltexBgpPeerGroupSoftResetWithStoredInfo   TruthValue,
      eltexBgpPeerGroupBfdDesired                TruthValue,
      eltexBgpPeerGroupPassword                  OCTET STRING,
      eltexBgpPeerGroupPasswordKeyChain          OCTET STRING,
      eltexBgpPeerGroupAsPathListIn              DisplayString,
      eltexBgpPeerGroupAsPathListOut             DisplayString,
      eltexBgpPeerGroupAsOverride                TruthValue,
      eltexBgpPeerGroupAllowAsIn                 Unsigned32,
      eltexBgpPeerGroupEbgpMultihop              TruthValue
    }

  eltexBgpPeerGroupName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The name of this eltexBgpPeerGroupEntry.  This is the index of the
                 peer group."
    ::= { eltexBgpPeerGroupEntry 1 }

  eltexBgpPeerGroupRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The row status for this BGP peer group table entry, used to
                create and destroy table entries."
    ::= { eltexBgpPeerGroupEntry 2 }

  eltexBgpPeerGroupRemoteAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The remote autonomous system number.

                 For individual peers, this can be configured using
                 eltexBgpPeerRemoteAs.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin status DOWN and then UP, thus forcing the
                 peer session to be restarted.  In this case, until the
                 peer is set admin_status DOWN, the peer will be marked as
                 out of date (as reported by the config state field in the
                 eltexBgpPeerStatusTable row for the peer)."
    ::= { eltexBgpPeerGroupEntry 3 }

  eltexBgpPeerGroupSourceInterface OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The interface index for the interface from which the
                 source address for session is chosen.  If non-zero, BGP
                 will look for the first address on this interface with a
                 type matching eltexBgpPeerRemoteAddrType, and use that as the
                 source address.

                 This field can be changed at any time, causing the peer to
                 be immediately deactivated and reactivated.

                 If the configured interface (or address on that interface)
                 did not exist when the peer was activated, and is
                 subsequently added, the peer will automatically use the
                 configured interface address.  This will cause the peer to
                 be immediately deactivated and reactivated."
    DEFVAL       { 0 }
    ::= { eltexBgpPeerGroupEntry 4 }

  eltexBgpPeerGroupNxtHopSlf OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "When eltexBgpPeerGroupNxtHopSlf is 'true', routes will be 
                 advertised to the peer with NEXT_HOP attribute set to 
                 BGP router local address."
    DEFVAL       { false }
    ::= { eltexBgpPeerGroupEntry 5 }

    eltexBgpPeerGroupConfigMaxPrfx OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This object is used to limit the number of prefixes that
                 can be accepted from this peer.

                 Setting eltexBgpPeerGroupConfigMaxPrfx to a non-zero value sets 
                 the maximum number of prefixes that can be accepted from 
                 this peer."
    DEFVAL       { 0 }
    ::= { eltexBgpPeerGroupEntry 6 }

    eltexBgpPeerGroupConfigDropWarn OBJECT-TYPE
    SYNTAX      EltexBgpConfigDropOrWarn
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This object is used  to determine whether the session is
                 dropped or a warning is generated when the maximum number
                 of prefixes set is exceeded.

                 Setting eltexBgpPeerGroupConfigDropWarn to 'drop' will cause the
                 session to be dropped when the prefix limit is reached."
    DEFVAL       { warn }
    ::= { eltexBgpPeerGroupEntry 7 }

    eltexBgpPeerGroupMaxPrfxHold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The time interval in seconds between when this BGP session
                 is turn down due to the number of prefixes received from
                 this peer exceeding the maximum in
                 eltexBgpPeerGroupConfigMaxPrfx and when BGP attempts to
                 reestablish the session."
    DEFVAL       { 90 }
    ::= { eltexBgpPeerGroupEntry 8 }

    eltexBgpPeerGroupConfigThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "A percentage of the limit set by eltexBgpPeerGroupConfigMaxPrfx.
                 When the number of prefixes received from this peer reaches
                 this threshold, BGP issues a warning.

                 This field is not used if eltexBgpPeerGroupConfigMaxPrfx is set to
                 zero."
    DEFVAL       { 75 }
    ::= { eltexBgpPeerGroupEntry 9 }

    eltexBgpPeerGroupConnectRetryInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval for the ConnectRetry timer.  The suggested
                 value for this timer is 120 seconds.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 120 }
    ::= { eltexBgpPeerGroupEntry 10 }

    eltexBgpPeerGroupHoldTimeConfigd OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the Hold Time configured for
                 this BGP speaker with this peer.  This value is placed in
                 an OPEN message sent to this peer by this BGP speaker, and
                 is compared with the Hold Time field in an OPEN message
                 received from the peer when determining the Hold Time
                 (eltexBgpPeerStatusHoldTime) with the peer.  This value must not be
                 less than three seconds if it is not zero (0) in which
                 case the Hold Time is NOT to be established with the peer.
                 The value of this object is only allowed to be zero (0) if
                 the value of eltexBgpPeerKeepAliveConfigd is also zero (0).
                 The suggested value for this timer is 90 seconds.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 90 }
    ::= { eltexBgpPeerGroupEntry 11 }

    eltexBgpPeerGroupKeepAliveConfigd OBJECT-TYPE
    SYNTAX      Unsigned32 ( 0 | 1..21845 )
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the KeepAlive configured for
                 this BGP speaker with this peer.  The value of this object
                 will only determine the KEEPALIVE messages frequency
                 relative to the value specified in eltexBgpPeerGroupHoldTimeConfigd
                 the actual time interval for the KEEPALIVE messages is
                 indicated by eltexBgpPeerStatusKeepAlive.  A reasonable 
                 maximum value for this timer would be configured to be one 
                 third of that of eltexBgpPeerGroupHoldTimeConfigd.

                 The value of this object is only allowed to be zero (0) if
                 the value of eltexBgpPeerGroupHoldTimeConfigd is also zero (0).
                 If the value of this object is zero (0), no periodical
                 KEEPALIVE messages are sent to the peer after the BGP
                 connection has been established.  The suggested value for
                 this timer is 30 seconds.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 30 }
    ::= { eltexBgpPeerGroupEntry 12 }

    eltexBgpPeerGroupMinRouteAdvertiseInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the
                 MinRouteAdvertisementInterval timer.  This determines the
                 minimum time between a BGP UPDATE to a peer advertising or
                 withdrawing a route and a subsequent BGP UPDATE to the
                 peer advertising a route to the same destination.

                 The default value for this timer is 30 seconds.  Its value
                 must not be less than eltexBgpPeerGroupMinRouteAdvertiseInterval."
    DEFVAL       { 30 }
    ::= { eltexBgpPeerGroupEntry 13 }

    eltexBgpPeerGroupMinASOriginationInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for determining the minimum amount
                 of time that must elapse between successive advertisements of
                 UPDATE messages that report changes to a route within the
                 advertising BGP speaker's own autonomous system. The
                 suggested value for this timer is 15 seconds."
    DEFVAL       { 15 }
    ::= { eltexBgpPeerGroupEntry 14 }

    eltexBgpPeerGroupMinRouteWithdrawInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Time interval in seconds for the MinRouteWithdrawInterval
                 timer.  This is the interval which is enforced between
                 advertisement and subsequent withdrawal of a route.

                 The default value for this timer is 30 seconds.  The value
                 must not exceed that of eltexBgpPeerGroupMinRouteAdvertiseInterval."
    DEFVAL       { 30 }
    ::= { eltexBgpPeerGroupEntry 15 }

    eltexBgpPeerGroupConfigOpenDelay OBJECT-TYPE
    SYNTAX      Unsigned32 (0..240)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The delay to enforce in between a TCP connection with this
                 peer becoming established and a BGP Open message being
                 sent.  If this delay is zero, then no delay will be
                 injected, and a BGP Open message will be sent as soon as
                 the TCP connection allows it.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 0 }
    ::= { eltexBgpPeerGroupEntry 16 }

    eltexBgpPeerGroupConfigIdleHold OBJECT-TYPE
    SYNTAX      Unsigned32 (1..32767)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The time to hold this peer in Idle state after a BGP
                 session has progressed beyond Idle state initially and
                 then returned to it.  No new connections will be initiated
                 or accepted until the peer comes out of Idle state.  By
                 setting this field to a large value, this timer can be
                 used to provide some level of peer oscillation damping, if
                 desired.

                 This field can be changed at any time.  However, if the
                 field is changed while the peer is admin_status UP, the
                 change will only take effect after the peer has been
                 cycled admin_status DOWN and then UP, thus forcing the
                 peer session to be restarted."
    DEFVAL       { 15 }
    ::= { eltexBgpPeerGroupEntry 17 }

    eltexBgpPeerGroupDistListPlIn OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The Prefix List name identifying the Prefix List to use
                 to filter routes received from the peer."
    ::= { eltexBgpPeerGroupEntry 18 }

    eltexBgpPeerGroupDistListPlOut OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The Prefix List name identifying the Prefix List to use
                 to filter routes advertised to the peer."
    ::= { eltexBgpPeerGroupEntry 19 }

  eltexBgpPeerGroupReflectorClient OBJECT-TYPE
    SYNTAX      EltexBgpPeerReflectorClientType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This value indicates whether the given peer is a reflector
                client of this router, or not.  A value of nonClient(0)
                indicates that this peer is not a reflector client.  A
                value of client(1) indicates that this peer is a reflector
                client that is not fully meshed with other reflector
                clients.  A value of meshedClient(2) indicates that the
                peer is a reflector client and is fully meshed with all
                other reflector clients."
    DEFVAL       { nonClient }
    ::= { eltexBgpPeerGroupEntry 20 }

  eltexBgpPeerGroupSoftResetWithStoredInfo OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "This option causes all routes learned from a peer to be stored
                 so that the ARI can be recalculated (for example, due to a 
                 change in import policy) without performing a route refresh or
                 restarting the peer session.

                 This field can only be changed when the peer is admin_status
                 DOWN.

                 This option overlaps with route refresh (RR) behavior. If the
                 option is enabled, Route refresh capability continues to be
                 advertized and the BGP router still responds to RR request
                 from the peer. However, route refresh messages will never
                 be sent to this peer."
    DEFVAL { false }
    ::= { eltexBgpPeerGroupEntry 21 }

  eltexBgpPeerGroupBfdDesired OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Indicates whether Bidirectional Forwarding Detection (BFD)
                 is desired for peers in this peer group.

                 This field can be changed at any time."
    DEFVAL { false }
    ::= { eltexBgpPeerGroupEntry 22 }

  eltexBgpPeerGroupPassword OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..80))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The MD5 password used by this peer. This field can only be
                 changed when the row is not active."
    ::= { eltexBgpPeerGroupEntry 23 }

  eltexBgpPeerGroupPasswordKeyChain OBJECT-TYPE
      SYNTAX      OCTET STRING (SIZE (0..32))
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "Name of key chain for MD5 digest calculation."
  ::= { eltexBgpPeerGroupEntry 24 }

  eltexBgpPeerGroupAsPathListIn OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The Filter List index identifying the Filter List to use
                 to filter routes received from peers in this peer group.

                 If this name is non-NULL string and the AS Path Access List with
                 this name is defined, then routes received from peers
                 are matched against this filter list and permitted or
                 denied as defined by the filter list."
    ::= { eltexBgpPeerGroupEntry 25 }

  eltexBgpPeerGroupAsPathListOut OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The AS Path Access List name identifying the AS Path Access List
                 to use to filter routes advertised to peers in this peer group.

                 If this name is non-NULL string and the AS Path Access List with
                 this name is defined, then routes to be advertised to peers
                 are matched against this filter list and advertised or
                 not as defined by the filter list."
    ::= { eltexBgpPeerGroupEntry 26 }

eltexBgpPeerGroupAsOverride OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "If AS-override is enabled, then when advertising routes to a
                 peer in this group, any instance of the peer's AS number will
                 be replaced in the advertised AS path with the local AS number.

                 This field is only taken into account for peer-group
                 members if the conditions described in the eltexBgpPeerTable
                 description are met.

                 If the value of this object is changed while the peer session is
                 active, BGP will check for any routes that need to be advertised
                 or withdrawn as a result of the change.

                 Note that this field has no effect when set for iBGP peers."
    DEFVAL { false }
    ::= { eltexBgpPeerGroupEntry 27 }

  eltexBgpPeerGroupAllowAsIn OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The number of instances of the local AS identifier that
                 may be contained in the route's AS-Path without rejecting
                 the route.

                 The AS-Path attribute of a BGP route contains the
                 identifiers of the Autonomous Systems traversed by the
                 route.  When a route is received with an AS-Path
                 containing the local AS identifier, it normally indicates
                 a routing loop, and the default behavior is to reject the
                 route.  This object allows this behavior to be
                 over-ridden.

                 This is useful, for example, for VPN routes, where routes
                 from one CE router are advertised to other CE routers
                 through a provider's BGP network.  Two CE routers in the
                 same AS can enable this feature to prevent routes from the
                 other CE from being discarded.

                 When eltexBgpPeerGroupAllowAsIn is set to a non-zero value,
                 that value is used for all address families, and the value
                 of eltexBgpPeerAddrFamilyAllowAsIn is ignored.

                 Alternatively, the value may be configured independently
                 for each address family.  To do this, set
                 eltexBgpPeerGroupAllowAsIn to 0 and set the value of
                 eltexBgpPeerAddrFamilyAllowAsIn for each address family.

                 Changing the value of this object while the peer is active
                 triggers BGP to refresh its routes from the peer.

                 This field overrides the peer eltexBgpPeerAllowAsIn field."
    DEFVAL { 0 }
    ::= { eltexBgpPeerGroupEntry 28 }
    
    eltexBgpPeerGroupEbgpMultihop OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "When this field is set to TRUE for an eBGP peer group,
                 the TTL value will be adjusted to the default setting
                 (as defined in MIB_ipDefaultTTL_CNS) for all peers within
                 the group. This field overrides the peer 
                 eltexBgpPeerEbgpMultihop field."
    DEFVAL { false }
    ::= { eltexBgpPeerGroupEntry 29 }

-------------------------------------------------------------------------------

  eltexBgpPeerRange      OBJECT IDENTIFIER ::= { eltexBgpPeer 3 }

  --
  -- BGP Peer Range Table
  --
  -- This table is used to create and manage Peer Ranges.
  --


  eltexBgpPeerRangeTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPeerRangeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Peer range table.

                 This table allows a user to configure BGP dynamic neighbors.
                 Instead of being configured individually in the BGP peer
                 table, BGP dynamic neighbors are configured as ranges of
                 remote addresses with associated peer groups.  Each range
                 is configured as a remote address prefix.  Any BGP peer with
                 a remote address that matches the remote address prefix
                 becomes a member of the associated peer group.

                 Each entry in this table configures a remote address prefix
                 and specifies the associated peer group.

                 If an incoming connection matches multiple peer range
                 entries then the entry with the longest remote address
                 prefix is selected.

                 Although it is possible to configure overlapping peer ranges
                 with different remote address prefix lengths, this is not
                 recommended - peer range configuration is simpler and
                 clearer if peer ranges do not overlap.

                 Dynamic peers are always passive.  It is not possible to
                 initiate outbound connections to dynamic peers because
                 their addresses aren't known until they initiate an
                 incoming connection.

                 Deactivating a peer range entry causes BGP sessions with
                 matching dynamic BGP peers to be dropped.  This does not
                 apply to configured BGP peers with matching remote
                 addresses, nor to dynamic BGP peers with remote addresses
                 matching peer range entries with longer remote address
                 prefixes."
    ::= { eltexBgpPeerRange 1 }

  eltexBgpPeerRangeEntry OBJECT-TYPE
    SYNTAX      EltexBgpPeerRangeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Each entry represents a Peer Range entity."
    INDEX { eltexBgpProcessId,
            eltexBgpPeerRangeRemoteAddrType,
            eltexBgpPeerRangeRemoteAddr,
            eltexBgpPeerRangeRemotePrefixLen,
            eltexBgpPeerRangeRemoteAddrScopeId }
    ::= { eltexBgpPeerRangeTable 1 }

  EltexBgpPeerRangeEntry ::= SEQUENCE {
    eltexBgpPeerRangeRemoteAddrType      InetAddressType,
    eltexBgpPeerRangeRemoteAddr          InetAddress,
    eltexBgpPeerRangeRemotePrefixLen     InetAddressPrefixLength,
    eltexBgpPeerRangeRemoteAddrScopeId   Unsigned32,
    eltexBgpPeerRangeRowStatus           RowStatus,
    eltexBgpPeerRangeAdminStatus         EltexBgpAdminStatus,
    eltexBgpPeerRangeConfigPeerGroup     DisplayString,
    eltexBgpPeerRangeNumPeers            Unsigned32,
    eltexBgpPeerRangeMaxPeers            Unsigned32
  }

  eltexBgpPeerRangeRemoteAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the remote address prefix."
    ::= { eltexBgpPeerRangeEntry 1 }

  eltexBgpPeerRangeRemoteAddr OBJECT-TYPE
    SYNTAX      InetAddress (SIZE(0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The remote address prefix.

                 The length must be consistent with eltexBgpPeerRangeRemoteAddrType,
                 4 for ipv4 and 16 for ipv6.

                 The prefix length is specified by eltexBgpPeerRangeRemotePrefixLen.
                 Any bits beyond the specified prefix length must be zero."
    ::= { eltexBgpPeerRangeEntry 2 }

  eltexBgpPeerRangeRemotePrefixLen OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The remote address prefix length in bits."
    ::= { eltexBgpPeerRangeEntry 3 }

  eltexBgpPeerRangeRemoteAddrScopeId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The scope ID of the remote address prefix.  The scope ID
                 is required if the address is an IPv6 link-local address.
                 Otherwise, this field must be set to zero."
    ::= { eltexBgpPeerRangeEntry 4 }

  eltexBgpPeerRangeRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The row status for this peer range table entry, used to
                 create and destroy table entries."
    ::= { eltexBgpPeerRangeEntry 5 }

  eltexBgpPeerRangeAdminStatus OBJECT-TYPE
    SYNTAX      EltexBgpAdminStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The administrative status of this table entry, used to
                 activate and deactivate the peer range."
    DEFVAL      { adminStatusUp }
    ::= { eltexBgpPeerRangeEntry 6 }

  eltexBgpPeerRangeConfigPeerGroup OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The peer group name that neighbors in this peer
                 range belongs to.

                 The peer range must be assigned to a peer group so this
                 field cannot be empty.

                 If this field is changed while active then all dynamic peers
                 based on the peer range entry are immediately updated."
    ::= { eltexBgpPeerRangeEntry 7 }

  eltexBgpPeerRangeNumPeers OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The current number of dynamic BGP peers for this peer
                 range."
    ::= { eltexBgpPeerRangeEntry 8 }

  eltexBgpPeerRangeMaxPeers OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The maximum number of dynamic BGP peers for this peer range.

                 If this limit is reached then BGP rejects incoming
                 connections from new dynamic BGP peers until BGP session
                 termination causes the number of dynamic BGP peers to fall
                 back below the limit.

                 If this limit is reduced below the current number of
                 dynamic BGP peers then BGP will reject incoming
                 connections from new dynamic BGP peers until the number
                 of dynamic BGP peers falls below the new limit. BGP
                 does not terminate existing BGP sessions with dynamic BGP
                 peers in this case."
    DEFVAL      { 32 }
    ::= { eltexBgpPeerRangeEntry 9 }

-------------------------------------------------------------------------------

  eltexBgpRib OBJECT IDENTIFIER ::= { eltexBgpObjects 3 }

  --
  -- BGP Local RIB Table
  --
  -- This table contains per route information including routes and attributes.
  -- It is ordered by route prefix and basically represent Loc-RIB table.
  --

  eltexBgpLocRibTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpLocRibEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "This table contains information about paths to destination
                 networks received from all BGP4 peers.

                 This table reports routes and path attributes after import
                 policy has been applied.  Only routes accepted by import
                 policy are reported."
    ::= { eltexBgpRib 1 }

  eltexBgpLocRibEntry OBJECT-TYPE
    SYNTAX      EltexBgpLocRibEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a path to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpLocRibAfi,
            eltexBgpLocRibSafi,
            eltexBgpLocRibPrfxType,
            eltexBgpLocRibPrfx,
            eltexBgpLocRibPrfxLen,
            eltexBgpLocRibPeerOrRib,
            eltexBgpLocRibPeerRibIndex,
            eltexBgpLocRibPathId }
    ::= { eltexBgpLocRibTable 1 }

  EltexBgpLocRibEntry ::= SEQUENCE {
      eltexBgpLocRibAfi                  EltexBgpAfi,
      eltexBgpLocRibSafi                 EltexBgpSafi,
      eltexBgpLocRibPrfxType             EltexBgpInetAddressType,
      eltexBgpLocRibPrfx                 OCTET STRING,
      eltexBgpLocRibPrfxLen              Unsigned32,
      eltexBgpLocRibPeerOrRib            EltexBgpPeerOrRib,
      eltexBgpLocRibPeerRibIndex         Unsigned32,
      eltexBgpLocRibPathId               Unsigned32,
      eltexBgpLocRibBest                 TruthValue,
      eltexBgpLocRibAsSize               EltexBgpAsSize,
      eltexBgpLocRibASPathStr            OCTET STRING,
      eltexBgpLocRibPathAttrOrigin       EltexBgpOriginCode,
      eltexBgpLocRibPathAttrNextHopType  InetAddressType,
      eltexBgpLocRibPathAttrNextHop      InetAddress,
      eltexBgpLocRibPathAttrMultExtDisc  Unsigned32,
      eltexBgpLocRibPathAttrLocalPref    Unsigned32,
      eltexBgpLocRibPathAttrAtomicAgg    TruthValue,
      eltexBgpLocRibPathAttrAggAS        EltexBgpAutonomousSystemNumber,
      eltexBgpLocRibPathAttrAggAddr      EltexBgpIdentifier,
      eltexBgpLocRibPathAttrCalcLclPref  Unsigned32,
      eltexBgpLocRibPathAttrOrigId       EltexBgpIdentifier,
      eltexBgpLocRibPathAttrWeight       Unsigned32,
      eltexBgpLocRibEcmp                 TruthValue,
      eltexBgpLocRibPathAttrAsPathLimAs  EltexBgpAutonomousSystemNumber,
      eltexBgpLocRibPthAttAsPthLimUpper  Unsigned32,
      eltexBgpLocRibIsActive             EltexBgpNlriIsActiveFlag,
      eltexBgpLocRibPathAttrMEDPrsnt     TruthValue,
      eltexBgpLocRibReasonNotBest        EltexBgpReasonNotBest,
      eltexBgpLocRibPeerType             EltexBgpNlriPeerTypes,
      eltexBgpLocRibAggrType             INTEGER
    }

  eltexBgpLocRibAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this Loc-RIB route."
    ::= { eltexBgpLocRibEntry 1 }

  eltexBgpLocRibSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this Loc-RIB
                 route."
    ::= { eltexBgpLocRibEntry 2 }

  eltexBgpLocRibPrfxType OBJECT-TYPE
    SYNTAX      EltexBgpInetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A type of address prefix in the Network Layer Reachability
                 Information field."
    ::= { eltexBgpLocRibEntry 3 }

  eltexBgpLocRibPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information from NLRI field.

                 The prefix length is specified by eltexBgpLocRibPrfxLen. Any
                 bits beyond the length specified by eltexBgpLocRibPrfxLen are
                 zeroed."
    ::= { eltexBgpLocRibEntry 4 }

  eltexBgpLocRibPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The prefix length is specified by eltexBgpLocRibPrfxLen. Any
                 bits beyond the length specified by eltexBgpLocRibPrfxLen are
                 zeroed."
    ::= { eltexBgpLocRibEntry 5 }

  eltexBgpLocRibPeerOrRib OBJECT-TYPE
    SYNTAX      EltexBgpPeerOrRib
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Whether this route was learned from a BGP peer or redistributed
                 from Routing Information Base."
    ::= { eltexBgpLocRibEntry 6 }

  eltexBgpLocRibPeerRibIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of either the BGP peer or RIB this route was
                 learned from.  If eltexBgpNlriPrefixPeerOrRib is peer, this field
                 is equivalent to a eltexBgpPeerStatusPeerIndex.  If
                 eltexBgpNlriPrefixPeerOrRib is afm, this field is equivalent to
                 an internal index of RIB entity."
    ::= { eltexBgpLocRibEntry 7 }

  eltexBgpLocRibPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                 If BGP additional path receive capability was negotiated
                 with the peer for this AFI/SAFI then this is the received
                 path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpLocRibEntry 8 }

  eltexBgpLocRibBest OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "An indication of whether or not this route was chosen as the
                 best BGP4 route."
    ::= { eltexBgpLocRibEntry 9 }

  eltexBgpLocRibAsSize OBJECT-TYPE
    SYNTAX      EltexBgpAsSize
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether the eltexBgpLocRibASPathStr field contains two or
                 four byte AS numbers."
    ::= { eltexBgpLocRibEntry 10 }

  eltexBgpLocRibASPathStr OBJECT-TYPE
    SYNTAX      OCTET STRING  (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This is a string depicting the autonomous system path to this
                 network which was received from the peer which advertised it.
                 Two-octet AS numbers appear as four-octet numbers by adding
                 two bytes of zero padding."
    ::= { eltexBgpLocRibEntry 11 }

  eltexBgpLocRibPathAttrOrigin OBJECT-TYPE
    SYNTAX      EltexBgpOriginCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The ultimate origin of the path information."
    ::= { eltexBgpLocRibEntry 12 }

  eltexBgpLocRibPathAttrNextHopType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of nexthop address received in the UPDATE packet."
    ::= { eltexBgpLocRibEntry 13 }

  eltexBgpLocRibPathAttrNextHop OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The address of the border router that should be used to access
                 the destination network.  This address is the nexthop address
                 received in the UPDATE packet.  The address family of this
                 object will be the same as that of the prefix in this row."
    ::= { eltexBgpLocRibEntry 14 }

  eltexBgpLocRibPathAttrMultExtDisc OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This metric is used to discriminate between multiple exit
                 points to an adjacent autonomous system.
                 Valid only if eltexBgpLocRibPathAttrMEDPrsnt is TRUE."
    ::= { eltexBgpLocRibEntry 15 }

  eltexBgpLocRibPathAttrLocalPref OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The originating BGP4 speaker's degree of preference for an
                 advertised route."
    ::= { eltexBgpLocRibEntry 16 }

  eltexBgpLocRibPathAttrAtomicAgg OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "When this object is set to TRUE, the ATOMIC_AGGREGATE Path
                 Attribute is present and indicates that the NLRI MUST NOT
                 be made more specific."
    ::= { eltexBgpLocRibEntry 17 }

  eltexBgpLocRibPathAttrAggAS OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the last BGP4 speaker that performed route
                 aggregation."
    ::= { eltexBgpLocRibEntry 18 }

  eltexBgpLocRibPathAttrAggAddr OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address of the last BGP4 speaker that performed route
                 aggregation.  A value of zero indicates the absence of this
                 attribute.  Note propagation of AS of zero is illegal in
                 the Internet."
    ::= { eltexBgpLocRibEntry 19 }

  eltexBgpLocRibPathAttrCalcLclPref OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The degree of preference calculated by the receiving BGP4
                 speaker for an advertised route."
    ::= { eltexBgpLocRibEntry 20 }

  eltexBgpLocRibPathAttrOrigId OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The Originator-ID identifying the router that initially
                 advertised this destination to a Route Reflector.  A
                 value of 0.0.0.0 indicates the absence of this attribute."
    ::= { eltexBgpLocRibEntry 21 }

  eltexBgpLocRibPathAttrWeight OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The local degree of preference assigned to this route."
    ::= { eltexBgpLocRibEntry 22 }

  eltexBgpLocRibEcmp   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether or not this route was installed into the
                 Forwarding Table as an ECMP route (it may or may not be
                 the best BGP4 route advertised to BGP peers)."
    ::= { eltexBgpLocRibEntry 23 }

  eltexBgpLocRibPathAttrAsPathLimAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the speaker that attached the AS_PATHLIMIT
                 attribute.  A value of 0 indicates the absence of this
                 attribute.  Note that propagation of AS of zero is illegal in
                 the Internet."
    ::= { eltexBgpLocRibEntry 24 }

  eltexBgpLocRibPthAttAsPthLimUpper OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The upper bound on the number of ASes in the AS_PATH
                 associated with this route before the route will be filtered.
                 Only valid if eltexBgpLocRibPathAttrAsPathLimAs is non-zero."
    ::= { eltexBgpLocRibEntry 25 }

  eltexBgpLocRibIsActive OBJECT-TYPE
    SYNTAX      EltexBgpNlriIsActiveFlag
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "An indication of whether or not this route is installed in
                 the forwarding table.

                 - 'active' if the route is installed in the forwarding
                   table, or is a route redistributed from another routing
                   protocol instance

                 - 'inactive' otherwise.

                 - 'notTracked' if BGP does not track active routes."
    ::= { eltexBgpLocRibEntry 26 }

  eltexBgpLocRibPathAttrMEDPrsnt OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If true, then the route has an associated MED attribute,
                 whose value is given in eltexBgpLocRibPathAttrMultExitDisc.
                 If false, the route has no MED attribute, and the value of
                 eltexBgpLocRibPathAttrMultExitDisc is undefined."
    ::= { eltexBgpLocRibEntry 27 }

  eltexBgpLocRibReasonNotBest OBJECT-TYPE
    SYNTAX      EltexBgpReasonNotBest
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If eltexBgpLocRibBest is 'true', then this field is set to
                'routeIsBest'.  Otherwise, it reports the stage in the
                decision process when the route was determined to be
                non-best.

                This is the reason that the route was discarded from the
                decision process.  There may be other reasons why this route
                is less preferred than the best route."
    ::= { eltexBgpLocRibEntry 28 }

  eltexBgpLocRibPeerType OBJECT-TYPE
    SYNTAX      EltexBgpNlriPeerTypes
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If eltexBgpLocRibPeerOrRib is peer, this field indicates
                 whether the source peer is an iBGP or eBGP peer.  If false,
                 this field is set to 'none'."
    ::= { eltexBgpLocRibEntry 29 }

  eltexBgpLocRibAggrType OBJECT-TYPE
    SYNTAX      INTEGER {
                  noAggregation(1),
                  aggregateRoute(2),
                  unsuppAggregatedRoute(3),
                  suppressedAggregatedRoute(4)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This object indicates any aggregation processing that
                 has been applied to this route.

                 A value of noAggregation(1) indicates that this route
                 does not aggregate any other routes, and is not
                 aggregated by any route.

                 A value of aggregateRoute(2) indicates that this route
                 is a locally configured aggregating route,
                 corresponding to an entry in the eltexBgpAggregateTable.

                 A value of unsuppAggregatedRoute(3) indicates that this
                 route has been aggregated by a locally configured
                 aggregate route and is not suppressed - the route is
                 still explicitly advertised to peers.

                 A value of suppressedAggregatedRoute(4) indicates that
                 this route has been aggregated by a locally configured
                 aggregate route and is flagged such that it should not be
                 advertised along with the aggregate route."
    ::= { eltexBgpLocRibEntry 30 }

-------------------------------------------------------------------------------

  --
  -- BGP Adj-Rib-In Table
  --
  -- This table contains per route information including routes and attributes.
  -- All routes received from peers are contained within this table, regardless
  -- of whether they have been accepted by policy.  Routes that are 
  -- redistributed from other routing protocols are not present.
  --

  eltexBgpAdjRibInTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpAdjRibInEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP-4 Adj-RIB-In Table contains information about all
                 paths to destination networks received from all BGP4 peers.
                 Paths from AFMs are not contained within this table.

                 This table reports received routes and path attributes before
                 import policy has been applied."
    ::= { eltexBgpRib 2 }

  eltexBgpAdjRibInEntry OBJECT-TYPE
    SYNTAX      EltexBgpAdjRibInEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a path to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpAdjRibInPeerIndex,
            eltexBgpAdjRibInAfi,
            eltexBgpAdjRibInSafi,
            eltexBgpAdjRibInPrfxType,
            eltexBgpAdjRibInPrfx,
            eltexBgpAdjRibInPrfxLen,
            eltexBgpAdjRibInPathId }
    ::= { eltexBgpAdjRibInTable 1 }

  EltexBgpAdjRibInEntry ::= SEQUENCE {
      eltexBgpAdjRibInPeerIndex                Unsigned32,
      eltexBgpAdjRibInAfi                      EltexBgpAfi,
      eltexBgpAdjRibInSafi                     EltexBgpSafi,
      eltexBgpAdjRibInPrfxType                 InetAddressType,
      eltexBgpAdjRibInPrfx                     InetAddress,
      eltexBgpAdjRibInPrfxLen                  InetAddressPrefixLength,
      eltexBgpAdjRibInPathId                   Unsigned32,
      eltexBgpAdjRibInAsSize                   EltexBgpAsSize,
      eltexBgpAdjRibInASPathStr                OCTET STRING,
      eltexBgpAdjRibInPathAttrOrigin           EltexBgpOriginCode,
      eltexBgpAdjRibInPathAttrNextHopType      InetAddressType,
      eltexBgpAdjRibInPathAttrNextHop          InetAddress,
      eltexBgpAdjRibInPathAttrMultiExitDisc    Unsigned32,
      eltexBgpAdjRibInPathAttrLocalPref        Unsigned32,
      eltexBgpAdjRibInPathAttrAtomicAggregate  TruthValue,
      eltexBgpAdjRibInPathAttrAggregatorAS     EltexBgpAutonomousSystemNumber,
      eltexBgpAdjRibInPathAttrAggregatorAddr   EltexBgpIdentifier,
      eltexBgpAdjRibInPathAttrOrigId           EltexBgpIdentifier,
      eltexBgpAdjRibInPathAttrAsPathLimAs      EltexBgpAutonomousSystemNumber,
      eltexBgpAdjRibInPathAttrAsPathLimUpper   Unsigned32,
      eltexBgpAdjRibInPathAttrMEDPrsnt         TruthValue,
      eltexBgpAdjRibInPathAccepted             TruthValue
    }

  eltexBgpAdjRibInPeerIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of the BGP peer this route was learned from.
                 This field is equivalent to a eltexBgpPeerStatusPeerIndex."
    ::= { eltexBgpAdjRibInEntry 1 }

  eltexBgpAdjRibInAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this Adj-RIB-In route."
    ::= { eltexBgpAdjRibInEntry 2 }

  eltexBgpAdjRibInSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this
                 Adj-RIB-In route."
    ::= { eltexBgpAdjRibInEntry 3 }

  eltexBgpAdjRibInPrfxType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A type of address prefix in the Network Layer Reachability
                 Information field."
    ::= { eltexBgpAdjRibInEntry 4 }

  eltexBgpAdjRibInPrfx OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field.

                 The prefix length is specified by eltexBgpAdjRibInPrfxLen.  Any
                 bits beyond the length specified by eltexBgpAdjRibInPrfxLen are
                 zeroed."
    ::= { eltexBgpAdjRibInEntry 5 }

  eltexBgpAdjRibInPrfxLen OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the IP address prefix in the Network Layer
                 Reachability Information field."
    ::= { eltexBgpAdjRibInEntry 6 }

  eltexBgpAdjRibInPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                If BGP additional path receive capability was negotiated
                with the peer for this AFI/SAFI then this is the received
                path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpAdjRibInEntry 7 }

  eltexBgpAdjRibInAsSize OBJECT-TYPE
    SYNTAX      EltexBgpAsSize
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether the eltexBgpAdjRibInASPathStr field contains two or
                 four byte AS numbers."
    ::= { eltexBgpAdjRibInEntry 8 }

  eltexBgpAdjRibInASPathStr OBJECT-TYPE
    SYNTAX      OCTET STRING  (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This is a string depicting the autonomous system path to this
                 network which was received from the peer which advertised it.
                 Two-octet AS numbers appear as four-octet numbers by adding
                 two bytes of zero padding."
    ::= { eltexBgpAdjRibInEntry 9 }

  eltexBgpAdjRibInPathAttrOrigin OBJECT-TYPE
    SYNTAX      EltexBgpOriginCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The ultimate origin of the path information."
    ::= { eltexBgpAdjRibInEntry 10 }

  eltexBgpAdjRibInPathAttrNextHopType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of the nexthop address received in the UPDATE packet."
    ::= { eltexBgpAdjRibInEntry 11 }

  eltexBgpAdjRibInPathAttrNextHop OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The address of the border router that should be used to access
                 the destination network.  This address is the nexthop address
                 received in the UPDATE packet.  The address family of this
                 object will be the same as that of the prefix in this row."
    ::= { eltexBgpAdjRibInEntry 12 }

  eltexBgpAdjRibInPathAttrMultiExitDisc OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This metric is used to discriminate between multiple exit
                 points to an adjacent autonomous system.
                 Valid only if eltexBgpAdjRibInPathAttrMEDPrsnt is TRUE."
    ::= { eltexBgpAdjRibInEntry 13 }

  eltexBgpAdjRibInPathAttrLocalPref OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The originating BGP4 speaker's degree of preference for an
                 advertised route."
    ::= { eltexBgpAdjRibInEntry 14 }

  eltexBgpAdjRibInPathAttrAtomicAggregate OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "When this object is set to true, the ATOMIC_AGGREGATE Path 
                 Attribute is present and indicates that the NLRI MUST NOT
                 be made more specific."
    ::= { eltexBgpAdjRibInEntry 15 }

  eltexBgpAdjRibInPathAttrAggregatorAS OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the last BGP4 speaker that performed route
                 aggregation."
    ::= { eltexBgpAdjRibInEntry 16 }

  eltexBgpAdjRibInPathAttrAggregatorAddr OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address of the last BGP4 speaker that performed route
                 aggregation.  A value of zero indicates the absence of this
                 attribute.  Note propagation of AS of zero is illegal in
                 the Internet."
    ::= { eltexBgpAdjRibInEntry 17 }

  eltexBgpAdjRibInPathAttrOrigId OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The Originator-ID identifying the router that initially
                 advertised this destination to a Route Reflector.  A
                 value of 0.0.0.0 indicates the absence of this attribute."
    ::= { eltexBgpAdjRibInEntry 18 }

  eltexBgpAdjRibInPathAttrAsPathLimAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the speaker that attached the AS_PATHLIMIT
                 attribute.  A value of 0 indicates the absence of this
                 attribute.  Note that propagation of AS of zero is illegal in
                 the Internet."
    ::= { eltexBgpAdjRibInEntry 19 }

  eltexBgpAdjRibInPathAttrAsPathLimUpper OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The upper bound on the number of ASes in the AS_PATH
                 associated with this route before the route will be filtered.
                 Only valid if eltexBgpAdjRibInPathAttrAsPathLimAs is non-zero."
    ::= { eltexBgpAdjRibInEntry 20 }

  eltexBgpAdjRibInPathAttrMEDPrsnt OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If true, then the route has an associated MED attribute,
                 whose value is given in eltexBgpAdjRibInPathAttMultiExitDisc.
                 If false, the route has no MED attribute, and the value of
                 eltexBgpAdjRibInPathAttMultiExitDisc is undefined."
    ::= { eltexBgpAdjRibInEntry 21 }

  eltexBgpAdjRibInPathAccepted OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If true, then the route was accepted by policy.  If false it
                 was denied."
    ::= { eltexBgpAdjRibInEntry 22 }

-------------------------------------------------------------------------------

  --
  -- BGP Adj-RIB Out Table
  --
  -- This table contains the set of routes advertised to each peer.
  --

  eltexBgpAdjRibOutTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpAdjRibOutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP Adj-RIB-Out Table contains the set of routes
                 advertised to each peer."
    ::= { eltexBgpRib 3 }

  eltexBgpAdjRibOutEntry OBJECT-TYPE
    SYNTAX      EltexBgpAdjRibOutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a path to a network that has been
                 advertised to a peer.  The route has been
                 explicitly advertised in an UPDATE message sent to the
                 peer, unless eltexBgpAdjRibOutLocalAggrType has the value
                 suppressedAggregatedRoute(4), in which case the route
                 has only been advertised as part of an aggregate
                 route."
    INDEX { eltexBgpProcessId,
            eltexBgpPeerStatusPeerIndex,
            eltexBgpAdjRibOutAfi,
            eltexBgpAdjRibOutSafi,
            eltexBgpAdjRibOutPrfxType,
            eltexBgpAdjRibOutPrfx,
            eltexBgpAdjRibOutPrfxLen,
            eltexBgpAdjRibOutPathId }
    ::= { eltexBgpAdjRibOutTable 1 }

  EltexBgpAdjRibOutEntry ::= SEQUENCE {
      eltexBgpAdjRibOutAfi                  EltexBgpAfi,
      eltexBgpAdjRibOutSafi                 EltexBgpSafi,
      eltexBgpAdjRibOutPrfxType             InetAddressType,
      eltexBgpAdjRibOutPrfx                 InetAddress,
      eltexBgpAdjRibOutPrfxLen              InetAddressPrefixLength,
      eltexBgpAdjRibOutPathId               Unsigned32,
      eltexBgpAdjRibOutBest                 TruthValue,
      eltexBgpAdjRibOutAdvertStatus         INTEGER,
      eltexBgpAdjRibOutLocalAggrType        INTEGER,
      eltexBgpAdjRibOutAsSize               EltexBgpAsSize,
      eltexBgpAdjRibOutASPathStr            OCTET STRING,
      eltexBgpAdjRibOutOrigin               EltexBgpOriginCode,
      eltexBgpAdjRibOutNextHopType          InetAddressType,
      eltexBgpAdjRibOutNextHop              InetAddress,
      eltexBgpAdjRibOutMultiExitDisc        Unsigned32,
      eltexBgpAdjRibOutLocalPref            Unsigned32,
      eltexBgpAdjRibOutAtomicAggregate      TruthValue,
      eltexBgpAdjRibOutAggregatorAS         EltexBgpAutonomousSystemNumber,
      eltexBgpAdjRibOutAggregatorAddr       EltexBgpIdentifier,
      eltexBgpAdjRibOutOrigId               EltexBgpIdentifier,
      eltexBgpAdjRibOutEcmp                 TruthValue,
      eltexBgpAdjRibOutAsLimAs              EltexBgpAutonomousSystemNumber,
      eltexBgpAdjRibOutAsLimUpper           Unsigned32,
      eltexBgpAdjRibOutIsActive             EltexBgpNlriIsActiveFlag,
      eltexBgpAdjRibOutMEDPrsnt             TruthValue,
      eltexBgpAdjRibOutPeerType             EltexBgpNlriPeerTypes
    }

  eltexBgpAdjRibOutAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this Adj-RIB Out
                 route."
    ::= { eltexBgpAdjRibOutEntry 1 }

  eltexBgpAdjRibOutSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for
                 this Adj-RIB Out route."
    ::= { eltexBgpAdjRibOutEntry 2 }

  eltexBgpAdjRibOutPrfxType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "A type of the address prefix in the Network Layer Reachability
                 Information field for this Adj-RIB Out route."
    ::= { eltexBgpAdjRibOutEntry 3 }

  eltexBgpAdjRibOutPrfx OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field for this Adj-RIB Out route.

                 The prefix length is specified by eltexBgpAdjRibOutPrfxLen.
                 Any bits beyond the length specified by
                 eltexBgpAdjRibOutPrfxLen are zeroed.

                 This field contains the full line format BGP NLRI omitting
                 any NLRI length field.

                 For SAFI 128 the NLRI includes the MPLS label and Route
                 Distinguisher as well as the IPv4 or IPv6 address prefix."
    ::= { eltexBgpAdjRibOutEntry 4 }

  eltexBgpAdjRibOutPrfxLen OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the address prefix contained in the
                 eltexBgpAdjRibOutPrfx object."
    ::= { eltexBgpAdjRibOutEntry 5 }

  eltexBgpAdjRibOutPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this Adj-RIB Out route.

                 If BGP additional path send capability was negotiated with
                 the peer for this AFI/SAFI then this is the path ID sent for
                 this Adj-RIB Out route, otherwise it is zero."
    ::= { eltexBgpAdjRibOutEntry 6 }

  eltexBgpAdjRibOutBest OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "An indication of whether or not this route was chosen as the
                 best BGP4 route."
    ::= { eltexBgpAdjRibOutEntry 7 }

  eltexBgpAdjRibOutAdvertStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                  advertised(1),
                  suppressed(2),
                  pendingWithdrawal(3),
                  withdrawn(4)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This object indicates the current state of
                 advertisement of the route to the peer.

                 A value of advertised(1) indicates that the route has
                 been advertised to the peer.

                 A value of suppressed(2) indicates that the route is
                 not currently advertised to the peer, but will be
                 advertised when a minimum advertisement interval timer
                 expires.

                 A value of pendingWithdrawal(3) indicates that the
                 route is currently advertised to the peer, but will be
                 withdrawn when the timer expires.

                 A value of withdrawn(4) indicates that the route has
                 been withdrawn from the peer, and this entry will be
                 removed from the Adj-RIB-Out on the expiry of the
                 timer."
    ::= { eltexBgpAdjRibOutEntry 8 }

  eltexBgpAdjRibOutLocalAggrType OBJECT-TYPE
    SYNTAX      INTEGER {
                  noAggregation(1),
                  aggregateRoute(2),
                  unsuppAggregatedRoute(3),
                  suppressedAggregatedRoute(4)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This object indicates any aggregation processing that
                 has been applied to this Adj-RIB-Out route.

                 A value of noAggregation(1) indicates that this route
                 does not aggregate any other routes, and is not
                 aggregated by any route.

                 A value of aggregateRoute(2) indicates that this route
                 is a locally configured aggregating route.

                 A value of unsuppAggregatedRoute(3) indicates that this
                 route has been aggregated by a locally configured
                 aggregate route and is not suppressed - the route is
                 still explicitly advertised to the peer.

                 A value of suppressedAggregatedRoute(4) indicates that
                 this route has been aggregated by a locally configured
                 aggregate route and is flagged such that it should not be
                 advertised along with the aggregate route.  Typically such
                 routes are not installed on an Adj-RIB-Out.  If however the
                 aggregate route itself is not permitted to be added to the
                 Adj-RIB-Out then suppressed routes are advertised if they
                 themselves are permitted by policy."
    ::= { eltexBgpAdjRibOutEntry 9 }

  eltexBgpAdjRibOutAsSize OBJECT-TYPE
    SYNTAX      EltexBgpAsSize
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether the eltexBgpAdjRibOutASPathStr object contains
                 two or four byte AS numbers."
    ::= { eltexBgpAdjRibOutEntry 10 }

  eltexBgpAdjRibOutASPathStr OBJECT-TYPE
    SYNTAX      OCTET STRING  (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This is a string containing the autonomous system path sent to
                 this peer in the AS_PATH attribute for this Adj-RIB-Out route.
                 Two-octet AS numbers appear as four-octet numbers by adding
                 two bytes of zero padding."
    ::= { eltexBgpAdjRibOutEntry 11 }

  eltexBgpAdjRibOutOrigin OBJECT-TYPE
    SYNTAX      EltexBgpOriginCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The ultimate origin of the path information."
    ::= { eltexBgpAdjRibOutEntry 12 }

  eltexBgpAdjRibOutNextHopType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of the next hop address transmitted 
                 in the UPDATE packet."
    ::= { eltexBgpAdjRibOutEntry 13 }

  eltexBgpAdjRibOutNextHop OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The next hop address transmitted in the UPDATE packet.
                 The address family of this object is the same as that
                 of eltexBgpAdjRibOutPrfx."
    ::= { eltexBgpAdjRibOutEntry 14 }

  eltexBgpAdjRibOutMultiExitDisc OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This metric is used to discriminate between multiple
                 exit points to an adjacent autonomous system.
                 Valid only if eltexBgpAdjRibOutMEDPrsnt is TRUE."
    ::= { eltexBgpAdjRibOutEntry 15 }

  eltexBgpAdjRibOutLocalPref OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The local preference for this Adj-RIB-Out route, as
                 transmitted in the UPDATE message sent to the peer."
    ::= { eltexBgpAdjRibOutEntry 16 }

  eltexBgpAdjRibOutAtomicAggregate OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "When this object is set to true, the ATOMIC_AGGREGATE Path 
                 Attribute was included in the UPDATE sent to the peer
                 for this Adj-RIB-Out route."
    ::= { eltexBgpAdjRibOutEntry 17 }

  eltexBgpAdjRibOutAggregatorAS OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the last BGP4 speaker that performed
                 route aggregation."
    ::= { eltexBgpAdjRibOutEntry 18 }

  eltexBgpAdjRibOutAggregatorAddr OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address of the last BGP4 speaker that performed
                 route aggregation.  A value of 0.0.0.0 indicates that
                 this attribute was not included in the UPDATE message
                 sent to the peer."
    ::= { eltexBgpAdjRibOutEntry 19 }

  eltexBgpAdjRibOutOrigId OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The Originator-ID identifying the router that initially
                 advertised this destination to a Route Reflector.  A
                 value of 0.0.0.0 indicates the absence of this
                 attribute."
    ::= { eltexBgpAdjRibOutEntry 20 }

  eltexBgpAdjRibOutEcmp   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether or not this route was installed into the
                 Forwarding Table as an ECMP route (it may or may not be
                 the best BGP4 route advertised to BGP peers)."
    ::= { eltexBgpAdjRibOutEntry 21 }

  eltexBgpAdjRibOutAsLimAs OBJECT-TYPE
    SYNTAX       EltexBgpAutonomousSystemNumber
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION  "If non-zero this is the number of the AS that attached the
                  AS_PATHLIMIT attribute."
    ::= { eltexBgpAdjRibOutEntry 22 }

  eltexBgpAdjRibOutAsLimUpper OBJECT-TYPE
    SYNTAX      Unsigned32  (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The upper bound on the number of ASes in the AS_PATH attribute
                 after which the route will be filtered.  Only valid if
                 eltexBgpAdjRibOutAsLimAs is non-zero."
    ::= { eltexBgpAdjRibOutEntry 23 }

  eltexBgpAdjRibOutIsActive OBJECT-TYPE
    SYNTAX      EltexBgpNlriIsActiveFlag
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "An indication of whether or not this route is installed in
                 the forwarding table.

                 - 'active' if the route is installed in the forwarding
                   table, or is a route redistributed from another routing
                   protocol instance

                 - 'inactive' otherwise.

                 - 'notTracked' if BGP does not track active routes."
    ::= { eltexBgpAdjRibOutEntry 24 }

  eltexBgpAdjRibOutMEDPrsnt OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If true, then the route has an associated MED attribute,
                 whose value is given in eltexBgpAdjRibOutMultiExitDisc. 
                 If false, the route has no MED attribute, and the value of
                 eltexBgpAdjRibOutMultiExitDisc is undefined."
    ::= { eltexBgpAdjRibOutEntry 25 }

  eltexBgpAdjRibOutPeerType OBJECT-TYPE
    SYNTAX      EltexBgpNlriPeerTypes
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This field indicates whether the source peer is an iBGP or
                 eBGP peer."
    ::= { eltexBgpAdjRibOutEntry 26 }

-------------------------------------------------------------------------------

  --
  -- BGP VPN Local RIB Table
  --
  -- This table contains per VPN route information including routes and attributes.
  --

  eltexBgpVpnLocRibTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpVpnLocRibEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "This table contains information about paths to destination
                 networks received from all BGP4 peers.

                 This table reports routes and path attributes after import
                 policy has been applied.  Only routes accepted by import
                 policy are reported."
    ::= { eltexBgpRib 6 }

  eltexBgpVpnLocRibEntry OBJECT-TYPE
    SYNTAX      EltexBgpVpnLocRibEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a path to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpVpnLocRibAfi,
            eltexBgpVpnLocRibSafi,
            eltexBgpVpnLocRibPrfx,
            eltexBgpVpnLocRibPrfxLen,
            eltexBgpVpnLocRibPeerOrRib,
            eltexBgpVpnLocRibPeerRibIndex,
            eltexBgpVpnLocRibPathId }
    ::= { eltexBgpVpnLocRibTable 1 }

  EltexBgpVpnLocRibEntry ::= SEQUENCE {
      eltexBgpVpnLocRibAfi                      EltexBgpAfi,
      eltexBgpVpnLocRibSafi                     EltexBgpSafi,
      eltexBgpVpnLocRibPrfx                     OCTET STRING,
      eltexBgpVpnLocRibPrfxLen                  Unsigned32,
      eltexBgpVpnLocRibPeerOrRib                EltexBgpPeerOrRib,
      eltexBgpVpnLocRibPeerRibIndex             Unsigned32,
      eltexBgpVpnLocRibPathId                   Unsigned32,
      eltexBgpVpnLocRibBest                     TruthValue,
      eltexBgpVpnLocRibAsSize                   EltexBgpAsSize,
      eltexBgpVpnLocRibASPathStr                OCTET STRING,
      eltexBgpVpnLocRibPathAttrOrigin           EltexBgpOriginCode,
      eltexBgpVpnLocRibPathAttrNextHopType      InetAddressType,
      eltexBgpVpnLocRibPathAttrNextHop          InetAddress,
      eltexBgpVpnLocRibPathAttrMultExtDisc      Unsigned32,
      eltexBgpVpnLocRibPathAttrLocalPref        Unsigned32,
      eltexBgpVpnLocRibPathAttrAtomicAgg        TruthValue,
      eltexBgpVpnLocRibPathAttrAggAS            EltexBgpAutonomousSystemNumber,
      eltexBgpVpnLocRibPathAttrAggAddr          EltexBgpIdentifier,
      eltexBgpVpnLocRibPathAttrCalcLclPref      Unsigned32,
      eltexBgpVpnLocRibPathAttrOrigId           EltexBgpIdentifier,
      eltexBgpVpnLocRibPathAttrWeight           Unsigned32,
      eltexBgpVpnLocRibEcmp                     TruthValue,
      eltexBgpVpnLocRibPathAttrAsPathLimAs      EltexBgpAutonomousSystemNumber,
      eltexBgpVpnLocRibPthAttAsPthLimUpper      Unsigned32,
      eltexBgpVpnLocRibIsActive                 EltexBgpNlriIsActiveFlag,
      eltexBgpVpnLocRibPathAttrMEDPrsnt         TruthValue,
      eltexBgpVpnLocRibReasonNotBest            EltexBgpReasonNotBest,
      eltexBgpVpnLocRibPeerType                 EltexBgpNlriPeerTypes,
      eltexBgpVpnLocRibRd                       EltexBgpRouteDistinguisher,
      eltexBgpVpnLocRibEvpnRouteType            EltexBgpEvpnRouteTypes,
      eltexBgpVpnLocRibEvpnPrefixLen            Unsigned32,
      eltexBgpVpnLocRibEvpnEsi                  EltexBgpEvpnESI,
      eltexBgpVpnLocRibEvpnEthernetTagId        EltexBgpEvpnEthernetTag,
      eltexBgpVpnLocRibEvpnMacAddressLen        Unsigned32,
      eltexBgpVpnLocRibEvpnMacAddress           MacAddress,
      eltexBgpVpnLocRibEvpnPrefixAddressLen     Unsigned32,
      eltexBgpVpnLocRibEvpnPrefixAddressType    InetAddressType,
      eltexBgpVpnLocRibEvpnPrefixAddress        InetAddress,
      eltexBgpVpnLocRibEvpnOrigAddressLen       Unsigned32,
      eltexBgpVpnLocRibEvpnOrigAddressType      InetAddressType,
      eltexBgpVpnLocRibEvpnOrigAddress          InetAddress,
      eltexBgpVpnLocRibEvpnGatewayAddressType   InetAddressType,
      eltexBgpVpnLocRibEvpnGatewayAddress       InetAddress,
      eltexBgpVpnLocRibEvpnVni1                 Unsigned32,
      eltexBgpVpnLocRibEvpnVni2                 Unsigned32,
      eltexBgpVpnLocRibMplsLabel                Unsigned32,
      eltexBgpVpnLocRibMplsPrefixAddressLen     Unsigned32,
      eltexBgpVpnLocRibMplsPrefixAddressType    InetAddressType,
      eltexBgpVpnLocRibMplsPrefixAddress        InetAddress
    }

  eltexBgpVpnLocRibAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this VPN Loc-RIB route."
    ::= { eltexBgpVpnLocRibEntry 1 }

  eltexBgpVpnLocRibSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this VPN Loc-RIB
                 route."
    ::= { eltexBgpVpnLocRibEntry 2 }

  eltexBgpVpnLocRibPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information from NLRI field.

                 The prefix length is specified by eltexBgpVpnLocRibPrfxLen. Any
                 bits beyond the length specified by eltexBgpVpnLocRibPrfxLen are
                 zeroed."
    ::= { eltexBgpVpnLocRibEntry 3 }

  eltexBgpVpnLocRibPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of prefix in the Network Layer
                 Reachability Information field."
    ::= { eltexBgpVpnLocRibEntry 4 }

  eltexBgpVpnLocRibPeerOrRib OBJECT-TYPE
    SYNTAX      EltexBgpPeerOrRib
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Whether this route was learned from a BGP peer or redistributed
                 from Routing Information Base."
    ::= { eltexBgpVpnLocRibEntry 5 }

  eltexBgpVpnLocRibPeerRibIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of either the BGP peer or RIB this route was
                 learned from.  If eltexBgpVpnLocRibPeerOrRib is peer, this field
                 is equivalent to a eltexBgpPeerStatusPeerIndex.  If
                 eltexBgpVpnLocRibPeerOrRib is afm, this field is equivalent to
                 an internal index of RIB entity."
    ::= { eltexBgpVpnLocRibEntry 6 }

  eltexBgpVpnLocRibPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                 If BGP additional path receive capability was negotiated
                 with the peer for this AFI/SAFI then this is the received
                 path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpVpnLocRibEntry 7 }

  eltexBgpVpnLocRibBest OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "An indication of whether or not this route was chosen as the
                 best BGP4 route."
    ::= { eltexBgpVpnLocRibEntry 8 }

  eltexBgpVpnLocRibAsSize OBJECT-TYPE
    SYNTAX      EltexBgpAsSize
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether the eltexBgpVpnLocRibASPathStr field contains two or
                 four byte AS numbers."
    ::= { eltexBgpVpnLocRibEntry 9 }

  eltexBgpVpnLocRibASPathStr OBJECT-TYPE
    SYNTAX      OCTET STRING  (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This is a string depicting the autonomous system path to this
                 network which was received from the peer which advertised it.
                 Two-octet AS numbers appear as four-octet numbers by adding
                 two bytes of zero padding."
    ::= { eltexBgpVpnLocRibEntry 10 }

  eltexBgpVpnLocRibPathAttrOrigin OBJECT-TYPE
    SYNTAX      EltexBgpOriginCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The ultimate origin of the path information."
    ::= { eltexBgpVpnLocRibEntry 11 }

  eltexBgpVpnLocRibPathAttrNextHopType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of nexthop address received in the UPDATE packet."
    ::= { eltexBgpVpnLocRibEntry 12 }

  eltexBgpVpnLocRibPathAttrNextHop OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The address of the border router that should be used to access
                 the destination network.  This address is the nexthop address
                 received in the UPDATE packet."
    ::= { eltexBgpVpnLocRibEntry 13 }

  eltexBgpVpnLocRibPathAttrMultExtDisc OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This metric is used to discriminate between multiple exit
                 points to an adjacent autonomous system.
                 Valid only if eltexBgpVpnLocRibPathAttrMEDPrsnt is TRUE."
    ::= { eltexBgpVpnLocRibEntry 14 }

  eltexBgpVpnLocRibPathAttrLocalPref OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The originating BGP4 speaker's degree of preference for an
                 advertised route."
    ::= { eltexBgpVpnLocRibEntry 15 }

  eltexBgpVpnLocRibPathAttrAtomicAgg OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "When this object is set to TRUE, the ATOMIC_AGGREGATE Path
                 Attribute is present and indicates that the NLRI MUST NOT
                 be made more specific."
    ::= { eltexBgpVpnLocRibEntry 16 }

  eltexBgpVpnLocRibPathAttrAggAS OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the last BGP4 speaker that performed route
                 aggregation."
    ::= { eltexBgpVpnLocRibEntry 17 }

  eltexBgpVpnLocRibPathAttrAggAddr OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address of the last BGP4 speaker that performed route
                 aggregation.  A value of zero indicates the absence of this
                 attribute.  Note propagation of AS of zero is illegal in
                 the Internet."
    ::= { eltexBgpVpnLocRibEntry 18 }

  eltexBgpVpnLocRibPathAttrCalcLclPref OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The degree of preference calculated by the receiving BGP4
                 speaker for an advertised route."
    ::= { eltexBgpVpnLocRibEntry 19 }

  eltexBgpVpnLocRibPathAttrOrigId OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The Originator-ID identifying the router that initially
                 advertised this destination to a Route Reflector.  A
                 value of 0.0.0.0 indicates the absence of this attribute."
    ::= { eltexBgpVpnLocRibEntry 20 }

  eltexBgpVpnLocRibPathAttrWeight OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The local degree of preference assigned to this route."
    ::= { eltexBgpVpnLocRibEntry 21 }

  eltexBgpVpnLocRibEcmp   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether or not this route was installed into the
                 Forwarding Table as an ECMP route (it may or may not be
                 the best BGP4 route advertised to BGP peers)."
    ::= { eltexBgpVpnLocRibEntry 22 }

  eltexBgpVpnLocRibPathAttrAsPathLimAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the speaker that attached the AS_PATHLIMIT
                 attribute.  A value of 0 indicates the absence of this
                 attribute.  Note that propagation of AS of zero is illegal in
                 the Internet."
    ::= { eltexBgpVpnLocRibEntry 23 }

  eltexBgpVpnLocRibPthAttAsPthLimUpper OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The upper bound on the number of ASes in the AS_PATH
                 associated with this route before the route will be filtered.
                 Only valid if eltexBgpVpnLocRibPathAttrAsPathLimAs is non-zero."
    ::= { eltexBgpVpnLocRibEntry 24 }

  eltexBgpVpnLocRibIsActive OBJECT-TYPE
    SYNTAX      EltexBgpNlriIsActiveFlag
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "An indication of whether or not this route is installed in
                 the forwarding table.

                 - 'active' if the route is installed in the forwarding
                   table, or is a route redistributed from another routing
                   protocol instance

                 - 'inactive' otherwise.

                 - 'notTracked' if BGP does not track active routes."
    ::= { eltexBgpVpnLocRibEntry 25 }

  eltexBgpVpnLocRibPathAttrMEDPrsnt OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If true, then the route has an associated MED attribute,
                 whose value is given in eltexBgpVpnLocRibPathAttrMultExitDisc.
                 If false, the route has no MED attribute, and the value of
                 eltexBgpVpnLocRibPathAttrMultExitDisc is undefined."
    ::= { eltexBgpVpnLocRibEntry 26 }

  eltexBgpVpnLocRibReasonNotBest OBJECT-TYPE
    SYNTAX      EltexBgpReasonNotBest
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If eltexBgpVpnLocRibBest is 'true', then this field is set to
                'routeIsBest'.  Otherwise, it reports the stage in the
                decision process when the route was determined to be
                non-best.

                This is the reason that the route was discarded from the
                decision process.  There may be other reasons why this route
                is less preferred than the best route."
    ::= { eltexBgpVpnLocRibEntry 27 }

  eltexBgpVpnLocRibPeerType OBJECT-TYPE
    SYNTAX      EltexBgpNlriPeerTypes
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If eltexBgpVpnLocRibPeerOrRib is peer, this field indicates
                 whether the source peer is an iBGP or eBGP peer.  If false,
                 this field is set to 'none'."
    ::= { eltexBgpVpnLocRibEntry 28 }

  eltexBgpVpnLocRibRd OBJECT-TYPE
    SYNTAX      EltexBgpRouteDistinguisher
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Route Distinguisher of the route."
    ::= { eltexBgpVpnLocRibEntry 29 }

  eltexBgpVpnLocRibEvpnRouteType OBJECT-TYPE
    SYNTAX      EltexBgpEvpnRouteTypes
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "EVPN route type."
    ::= { eltexBgpVpnLocRibEntry 30 }

  eltexBgpVpnLocRibEvpnPrefixLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "EVPN route length in bits without Route Distinguisher."
    ::= { eltexBgpVpnLocRibEntry 31 }

  eltexBgpVpnLocRibEvpnEsi OBJECT-TYPE
    SYNTAX      EltexBgpEvpnESI
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Ethernet Segment Identifier."
    ::= { eltexBgpVpnLocRibEntry 32 }

  eltexBgpVpnLocRibEvpnEthernetTagId OBJECT-TYPE
    SYNTAX      EltexBgpEvpnEthernetTag
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "VLAN ID."
    ::= { eltexBgpVpnLocRibEntry 33 }

  eltexBgpVpnLocRibEvpnMacAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Length in bits field eltexBgpVpnLocRibEvpnMacAddress."
    ::= { eltexBgpVpnLocRibEntry 34 }

  eltexBgpVpnLocRibEvpnMacAddress OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "MAC address from route type 2."
    ::= { eltexBgpVpnLocRibEntry 35 }

  eltexBgpVpnLocRibEvpnPrefixAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The length of field eltexBgpVpnLocRibEvpnPrefixAddress, for 
                 IPv4 it is 32 bits, and for IPv6 - 128. This field is
                 optional and may not contain any values (all zeros)."
    ::= { eltexBgpVpnLocRibEntry 36 }

  eltexBgpVpnLocRibEvpnPrefixAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of the address prefix in the Network Layer Reachability
                 Information field for this route. Optional field for route type 2."
    ::= { eltexBgpVpnLocRibEntry 37 }

  eltexBgpVpnLocRibEvpnPrefixAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "IP address optional field for route type 2."
    ::= { eltexBgpVpnLocRibEntry 38 }

  eltexBgpVpnLocRibEvpnOrigAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The length field eltexBgpVpnLocRibEvpnOrigAddress for the IP
                 address of the originator of the route. "
    ::= { eltexBgpVpnLocRibEntry 39 }

  eltexBgpVpnLocRibEvpnOrigAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "IP address type field eltexBgpVpnLocRibEvpnOrigAddress."
    ::= { eltexBgpVpnLocRibEntry 40 }

  eltexBgpVpnLocRibEvpnOrigAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address of the originator of the route, usually 
                 the VTEP router loopback."
    ::= { eltexBgpVpnLocRibEntry 41 }

  eltexBgpVpnLocRibEvpnGatewayAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of the Gateway IP address in the Network Layer Reachability
                 Information field for route type 5."
    ::= { eltexBgpVpnLocRibEntry 42 }

  eltexBgpVpnLocRibEvpnGatewayAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Gateway IP address field for route type 5."
    ::= { eltexBgpVpnLocRibEntry 43 }

  eltexBgpVpnLocRibEvpnVni1 OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "VNI field for route type 1, 2, 5."
    ::= { eltexBgpVpnLocRibEntry 44 }

  eltexBgpVpnLocRibEvpnVni2 OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The second VNI field for route type 2"
    ::= { eltexBgpVpnLocRibEntry 45 }

  eltexBgpVpnLocRibMplsLabel OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The value of bottom MPLS label in label stack field presenting
                 in the Network Layer Reachability Information for this route"
    ::= { eltexBgpVpnLocRibEntry 46 }
  
  eltexBgpVpnLocRibMplsPrefixAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The length of field eltexBgpVpnLocRibMplsPrefixAddress, for 
                 IPv4 it is 32 bits, and for IPv6 - 128. This field is
                 optional and may not contain any values (all zeros)."
    ::= { eltexBgpVpnLocRibEntry 47 }

  eltexBgpVpnLocRibMplsPrefixAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of the address prefix in the Network Layer Reachability
                 Information field for this route."
    ::= { eltexBgpVpnLocRibEntry 48 }

  eltexBgpVpnLocRibMplsPrefixAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Address prefix in the Network Layer Reachability Information
                 field for this route."
    ::= { eltexBgpVpnLocRibEntry 49 }

-------------------------------------------------------------------------------

  --
  -- BGP VPN Adj-Rib-In Table
  --
  -- This table contains per VPN route information including routes and attributes.
  -- All vpn routes received from peers are contained within this table, 
  -- regardless of whether they have been accepted by policy.  Routes that are 
  -- redistributed from other routing protocols are not present.
  --

  eltexBgpVpnAdjRibInTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpVpnAdjRibInEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP-4 VPN Adj-RIB-In Table contains information about all vpn
                 paths to destination networks received from all BGP4 peers.
                 Paths from AFMs are not contained within this table.

                 This table reports received routes and path attributes before
                 import policy has been applied."
    ::= { eltexBgpRib 7 }

  eltexBgpVpnAdjRibInEntry OBJECT-TYPE
    SYNTAX      EltexBgpVpnAdjRibInEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a path to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpVpnAdjRibInPeerIndex,
            eltexBgpVpnAdjRibInAfi,
            eltexBgpVpnAdjRibInSafi,
            eltexBgpVpnAdjRibInPrfx,
            eltexBgpVpnAdjRibInPrfxLen,
            eltexBgpVpnAdjRibInPathId }
    ::= { eltexBgpVpnAdjRibInTable 1 }

  EltexBgpVpnAdjRibInEntry ::= SEQUENCE {
      eltexBgpVpnAdjRibInPeerIndex                Unsigned32,
      eltexBgpVpnAdjRibInAfi                      EltexBgpAfi,
      eltexBgpVpnAdjRibInSafi                     EltexBgpSafi,
      eltexBgpVpnAdjRibInPrfx                     OCTET STRING,
      eltexBgpVpnAdjRibInPrfxLen                  Unsigned32,
      eltexBgpVpnAdjRibInPathId                   Unsigned32,
      eltexBgpVpnAdjRibInAsSize                   EltexBgpAsSize,
      eltexBgpVpnAdjRibInASPathStr                OCTET STRING,
      eltexBgpVpnAdjRibInPathAttrOrigin           EltexBgpOriginCode,
      eltexBgpVpnAdjRibInPathAttrNextHopType      InetAddressType,
      eltexBgpVpnAdjRibInPathAttrNextHop          InetAddress,
      eltexBgpVpnAdjRibInPathAttrMultiExitDisc    Unsigned32,
      eltexBgpVpnAdjRibInPathAttrLocalPref        Unsigned32,
      eltexBgpVpnAdjRibInPathAttrAtomicAggregate  TruthValue,
      eltexBgpVpnAdjRibInPathAttrAggregatorAS     EltexBgpAutonomousSystemNumber,
      eltexBgpVpnAdjRibInPathAttrAggregatorAddr   EltexBgpIdentifier,
      eltexBgpVpnAdjRibInPathAttrOrigId           EltexBgpIdentifier,
      eltexBgpVpnAdjRibInPathAttrAsPathLimAs      EltexBgpAutonomousSystemNumber,
      eltexBgpVpnAdjRibInPathAttrAsPathLimUpper   Unsigned32,
      eltexBgpVpnAdjRibInPathAttrMEDPrsnt         TruthValue,
      eltexBgpVpnAdjRibInPathAccepted             TruthValue,
      eltexBgpVpnAdjRibInRd                       EltexBgpRouteDistinguisher,
      eltexBgpVpnAdjRibInEvpnRouteType            EltexBgpEvpnRouteTypes,
      eltexBgpVpnAdjRibInEvpnPrefixLen            Unsigned32,
      eltexBgpVpnAdjRibInEvpnEsi                  EltexBgpEvpnESI,
      eltexBgpVpnAdjRibInEvpnEthernetTagId        EltexBgpEvpnEthernetTag,
      eltexBgpVpnAdjRibInEvpnMacAddressLen        Unsigned32,
      eltexBgpVpnAdjRibInEvpnMacAddress           MacAddress,
      eltexBgpVpnAdjRibInEvpnPrefixAddressLen     Unsigned32,
      eltexBgpVpnAdjRibInEvpnPrefixAddressType    InetAddressType,
      eltexBgpVpnAdjRibInEvpnPrefixAddress        InetAddress,
      eltexBgpVpnAdjRibInEvpnOrigAddressLen       Unsigned32,
      eltexBgpVpnAdjRibInEvpnOrigAddressType      InetAddressType,
      eltexBgpVpnAdjRibInEvpnOrigAddress          InetAddress

    }

  eltexBgpVpnAdjRibInPeerIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of the BGP peer this route was learned from.
                 This field is equivalent to a eltexBgpPeerStatusPeerIndex."
    ::= { eltexBgpVpnAdjRibInEntry 1 }

  eltexBgpVpnAdjRibInAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this VPN Adj-RIB-In route."
    ::= { eltexBgpVpnAdjRibInEntry 2 }

  eltexBgpVpnAdjRibInSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this VPN
                 Adj-RIB-In route."
    ::= { eltexBgpVpnAdjRibInEntry 3 }

  eltexBgpVpnAdjRibInPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field.

                 The prefix length is specified by eltexBgpVpnAdjRibInPrfxLen. Any
                 bits beyond the length specified by eltexBgpVpnAdjRibInPrfxLen are
                 zeroed."
    ::= { eltexBgpVpnAdjRibInEntry 4 }

  eltexBgpVpnAdjRibInPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the IP address prefix in the Network Layer
                 Reachability Information field."
    ::= { eltexBgpVpnAdjRibInEntry 5 }

  eltexBgpVpnAdjRibInPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                 If BGP additional path receive capability was negotiated
                 with the peer for this AFI/SAFI then this is the received
                 path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpVpnAdjRibInEntry 6 }

  eltexBgpVpnAdjRibInAsSize OBJECT-TYPE
    SYNTAX      EltexBgpAsSize
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether the eltexBgpVpnAdjRibInASPathStr field contains two or
                 four byte AS numbers."
    ::= { eltexBgpVpnAdjRibInEntry 7 }

  eltexBgpVpnAdjRibInASPathStr OBJECT-TYPE
    SYNTAX      OCTET STRING  (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This is a string depicting the autonomous system path to this
                 network which was received from the peer which advertised it.
                 Two-octet AS numbers appear as four-octet numbers by adding
                 two bytes of zero padding."
    ::= { eltexBgpVpnAdjRibInEntry 8 }

  eltexBgpVpnAdjRibInPathAttrOrigin OBJECT-TYPE
    SYNTAX      EltexBgpOriginCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The ultimate origin of the path information."
    ::= { eltexBgpVpnAdjRibInEntry 9 }

  eltexBgpVpnAdjRibInPathAttrNextHopType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of the nexthop address received in the UPDATE packet."
    ::= { eltexBgpVpnAdjRibInEntry 10 }

  eltexBgpVpnAdjRibInPathAttrNextHop OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The address of the border router that should be used to access
                 the destination network.  This address is the nexthop address
                 received in the UPDATE packet."
    ::= { eltexBgpVpnAdjRibInEntry 11 }

  eltexBgpVpnAdjRibInPathAttrMultiExitDisc OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This metric is used to discriminate between multiple exit
                 points to an adjacent autonomous system.
                 Valid only if eltexBgpVpnAdjRibInPathAttrMEDPrsnt is TRUE."
    ::= { eltexBgpVpnAdjRibInEntry 12 }

  eltexBgpVpnAdjRibInPathAttrLocalPref OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The originating BGP4 speaker's degree of preference for an
                 advertised route."
    ::= { eltexBgpVpnAdjRibInEntry 13 }

  eltexBgpVpnAdjRibInPathAttrAtomicAggregate OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "When this object is set to true, the ATOMIC_AGGREGATE Path 
                 Attribute is present and indicates that the NLRI MUST NOT
                 be made more specific."
    ::= { eltexBgpVpnAdjRibInEntry 14 }

  eltexBgpVpnAdjRibInPathAttrAggregatorAS OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the last BGP4 speaker that performed route
                 aggregation."
    ::= { eltexBgpVpnAdjRibInEntry 15 }

  eltexBgpVpnAdjRibInPathAttrAggregatorAddr OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address of the last BGP4 speaker that performed route
                 aggregation.  A value of zero indicates the absence of this
                 attribute.  Note propagation of AS of zero is illegal in
                 the Internet."
    ::= { eltexBgpVpnAdjRibInEntry 16 }

  eltexBgpVpnAdjRibInPathAttrOrigId OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The Originator-ID identifying the router that initially
                 advertised this destination to a Route Reflector.  A
                 value of 0.0.0.0 indicates the absence of this attribute."
    ::= { eltexBgpVpnAdjRibInEntry 17 }

  eltexBgpVpnAdjRibInPathAttrAsPathLimAs OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the speaker that attached the AS_PATHLIMIT
                 attribute.  A value of 0 indicates the absence of this
                 attribute.  Note that propagation of AS of zero is illegal in
                 the Internet."
    ::= { eltexBgpVpnAdjRibInEntry 18 }

  eltexBgpVpnAdjRibInPathAttrAsPathLimUpper OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The upper bound on the number of ASes in the AS_PATH
                 associated with this route before the route will be filtered.
                 Only valid if eltexBgpVpnAdjRibInPathAttrAsPathLimAs is non-zero."
    ::= { eltexBgpVpnAdjRibInEntry 19 }

  eltexBgpVpnAdjRibInPathAttrMEDPrsnt OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If true, then the route has an associated MED attribute,
                 whose value is given in eltexBgpVpnAdjRibInPathAttMultiExitDisc.
                 If false, the route has no MED attribute, and the value of
                 eltexBgpVpnAdjRibInPathAttMultiExitDisc is undefined."
    ::= { eltexBgpVpnAdjRibInEntry 20 }

  eltexBgpVpnAdjRibInPathAccepted OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If true, then the route was accepted by policy.  If false it
                 was denied."
    ::= { eltexBgpVpnAdjRibInEntry 21 }

  eltexBgpVpnAdjRibInRd OBJECT-TYPE
    SYNTAX      EltexBgpRouteDistinguisher
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Route Distinguisher of the route."
    ::= { eltexBgpVpnAdjRibInEntry 22 }

  eltexBgpVpnAdjRibInEvpnRouteType OBJECT-TYPE
    SYNTAX      EltexBgpEvpnRouteTypes
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "EVPN route type."
    ::= { eltexBgpVpnAdjRibInEntry 23 }

  eltexBgpVpnAdjRibInEvpnPrefixLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "EVPN route length in bits without Route Distinguisher."
    ::= { eltexBgpVpnAdjRibInEntry 24 }

  eltexBgpVpnAdjRibInEvpnEsi OBJECT-TYPE
    SYNTAX      EltexBgpEvpnESI
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Ethernet Segment Identifier."
    ::= { eltexBgpVpnAdjRibInEntry 25 }

  eltexBgpVpnAdjRibInEvpnEthernetTagId OBJECT-TYPE
    SYNTAX      EltexBgpEvpnEthernetTag
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "VLAN ID."
    ::= { eltexBgpVpnAdjRibInEntry 26 }

  eltexBgpVpnAdjRibInEvpnMacAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Length in bits field eltexBgpVpnAdjRibInEvpnMacAddress."
    ::= { eltexBgpVpnAdjRibInEntry 27 }

  eltexBgpVpnAdjRibInEvpnMacAddress OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "MAC address from route type 2."
    ::= { eltexBgpVpnAdjRibInEntry 28 }

  eltexBgpVpnAdjRibInEvpnPrefixAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The length of field eltexBgpVpnAdjRibInEvpnPrefixAddress, for 
                 IPv4 it is 32 bits, and for IPv6 - 128. This field is
                 optional and may not contain any values (all zeros)."
    ::= { eltexBgpVpnAdjRibInEntry 29 }

  eltexBgpVpnAdjRibInEvpnPrefixAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of the address prefix in the Network Layer Reachability
                 Information field for this route. Optional field for route type 2."
    ::= { eltexBgpVpnAdjRibInEntry 30 }

  eltexBgpVpnAdjRibInEvpnPrefixAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "IP address optional field for route type 2."
    ::= { eltexBgpVpnAdjRibInEntry 31 }

  eltexBgpVpnAdjRibInEvpnOrigAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The length field eltexBgpVpnAdjRibInEvpnOrigAddress for the IP
                 address of the originator of the route."
    ::= { eltexBgpVpnAdjRibInEntry 32 }

  eltexBgpVpnAdjRibInEvpnOrigAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "IP address type field eltexBgpVpnAdjRibInEvpnOrigAddress."
    ::= { eltexBgpVpnAdjRibInEntry 33 }

  eltexBgpVpnAdjRibInEvpnOrigAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address of the originator of the route, usually 
                 the VTEP router loopback."
    ::= { eltexBgpVpnAdjRibInEntry 34 }


-------------------------------------------------------------------------------

  --
  -- BGP VPN Adj-RIB Out Table
  --
  -- This table contains the set of VPN routes advertised to each peer.
  --

  eltexBgpVpnAdjRibOutTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpVpnAdjRibOutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP vpn Adj-RIB-Out Table contains the set of routes
                 advertised to each peer."
    ::= { eltexBgpRib 8 }

  eltexBgpVpnAdjRibOutEntry OBJECT-TYPE
    SYNTAX      EltexBgpVpnAdjRibOutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a path to a network that has been
                 advertised to a peer.  The route has been
                 explicitly advertised in an UPDATE message sent to the
                 peer, unless eltexBgpVpnAdjRibOutLocalAggrType has the value
                 suppressedAggregatedRoute(4), in which case the route
                 has only been advertised as part of an aggregate
                 route."
    INDEX { eltexBgpProcessId,
            eltexBgpPeerStatusPeerIndex,
            eltexBgpVpnAdjRibOutAfi,
            eltexBgpVpnAdjRibOutSafi,
            eltexBgpVpnAdjRibOutPrfx,
            eltexBgpVpnAdjRibOutPrfxLen,
            eltexBgpVpnAdjRibOutPathId }
    ::= { eltexBgpVpnAdjRibOutTable 1 }

  EltexBgpVpnAdjRibOutEntry ::= SEQUENCE {
      eltexBgpVpnAdjRibOutAfi                      EltexBgpAfi,
      eltexBgpVpnAdjRibOutSafi                     EltexBgpSafi,
      eltexBgpVpnAdjRibOutPrfx                     OCTET STRING,
      eltexBgpVpnAdjRibOutPrfxLen                  Unsigned32,
      eltexBgpVpnAdjRibOutPathId                   Unsigned32,
      eltexBgpVpnAdjRibOutBest                     TruthValue,
      eltexBgpVpnAdjRibOutAdvertStatus             INTEGER,
      eltexBgpVpnAdjRibOutLocalAggrType            INTEGER,
      eltexBgpVpnAdjRibOutAsSize                   EltexBgpAsSize,
      eltexBgpVpnAdjRibOutASPathStr                OCTET STRING,
      eltexBgpVpnAdjRibOutOrigin                   EltexBgpOriginCode,
      eltexBgpVpnAdjRibOutNextHopType              InetAddressType,
      eltexBgpVpnAdjRibOutNextHop                  InetAddress,
      eltexBgpVpnAdjRibOutMultiExitDisc            Unsigned32,
      eltexBgpVpnAdjRibOutLocalPref                Unsigned32,
      eltexBgpVpnAdjRibOutAtomicAggregate          TruthValue,
      eltexBgpVpnAdjRibOutAggregatorAS             EltexBgpAutonomousSystemNumber,
      eltexBgpVpnAdjRibOutAggregatorAddr           EltexBgpIdentifier,
      eltexBgpVpnAdjRibOutOrigId                   EltexBgpIdentifier,
      eltexBgpVpnAdjRibOutEcmp                     TruthValue,
      eltexBgpVpnAdjRibOutAsLimAs                  EltexBgpAutonomousSystemNumber,
      eltexBgpVpnAdjRibOutAsLimUpper               Unsigned32,
      eltexBgpVpnAdjRibOutIsActive                 EltexBgpNlriIsActiveFlag,
      eltexBgpVpnAdjRibOutMEDPrsnt                 TruthValue,
      eltexBgpVpnAdjRibOutPeerType                 EltexBgpNlriPeerTypes,
      eltexBgpVpnAdjRibOutRd                       EltexBgpRouteDistinguisher,
      eltexBgpVpnAdjRibOutEvpnRouteType            EltexBgpEvpnRouteTypes,
      eltexBgpVpnAdjRibOutEvpnPrefixLen            Unsigned32,
      eltexBgpVpnAdjRibOutEvpnEsi                  EltexBgpEvpnESI,
      eltexBgpVpnAdjRibOutEvpnEthernetTagId        EltexBgpEvpnEthernetTag,
      eltexBgpVpnAdjRibOutEvpnMacAddressLen        Unsigned32,
      eltexBgpVpnAdjRibOutEvpnMacAddress           MacAddress,
      eltexBgpVpnAdjRibOutEvpnPrefixAddressLen     Unsigned32,
      eltexBgpVpnAdjRibOutEvpnPrefixAddressType    InetAddressType,
      eltexBgpVpnAdjRibOutEvpnPrefixAddress        InetAddress,
      eltexBgpVpnAdjRibOutEvpnOrigAddressLen       Unsigned32,
      eltexBgpVpnAdjRibOutEvpnOrigAddressType      InetAddressType,
      eltexBgpVpnAdjRibOutEvpnOrigAddress          InetAddress

    }

  eltexBgpVpnAdjRibOutAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this VPN Adj-RIB Out
                 route."
    ::= { eltexBgpVpnAdjRibOutEntry 1 }

  eltexBgpVpnAdjRibOutSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for
                 this VPN Adj-RIB Out route."
    ::= { eltexBgpVpnAdjRibOutEntry 2 }

  eltexBgpVpnAdjRibOutPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field for this VPN Adj-RIB Out route.

                 The prefix length is specified by eltexBgpVpnAdjRibOutPrfxLen.
                 Any bits beyond the length specified by
                 eltexBgpVpnAdjRibOutPrfxLen are zeroed.

                 This field contains the full line format BGP NLRI omitting
                 any NLRI length field."
    ::= { eltexBgpVpnAdjRibOutEntry 3 }

  eltexBgpVpnAdjRibOutPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the address prefix contained in the
                 eltexBgpVpnAdjRibOutPrfx object."
    ::= { eltexBgpVpnAdjRibOutEntry 4 }

  eltexBgpVpnAdjRibOutPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this VPN Adj-RIB Out route.

                 If BGP additional path send capability was negotiated with
                 the peer for this AFI/SAFI then this is the path ID sent for
                 this VPN Adj-RIB Out route, otherwise it is zero."
    ::= { eltexBgpVpnAdjRibOutEntry 5 }

  eltexBgpVpnAdjRibOutBest OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "An indication of whether or not this route was chosen as the
                 best BGP4 route."
    ::= { eltexBgpVpnAdjRibOutEntry 6 }

  eltexBgpVpnAdjRibOutAdvertStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                  advertised(1),
                  suppressed(2),
                  pendingWithdrawal(3),
                  withdrawn(4)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This object indicates the current state of
                 advertisement of the route to the peer.

                 A value of advertised(1) indicates that the route has
                 been advertised to the peer.

                 A value of suppressed(2) indicates that the route is
                 not currently advertised to the peer, but will be
                 advertised when a minimum advertisement interval timer
                 expires.

                 A value of pendingWithdrawal(3) indicates that the
                 route is currently advertised to the peer, but will be
                 withdrawn when the timer expires.

                 A value of withdrawn(4) indicates that the route has
                 been withdrawn from the peer, and this entry will be
                 removed from the VPN Adj-RIB-Out on the expiry of the
                 timer."
    ::= { eltexBgpVpnAdjRibOutEntry 7 }

  eltexBgpVpnAdjRibOutLocalAggrType OBJECT-TYPE
    SYNTAX      INTEGER {
                  noAggregation(1),
                  aggregateRoute(2),
                  unsuppAggregatedRoute(3),
                  suppressedAggregatedRoute(4)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This object indicates any aggregation processing that
                 has been applied to this VPN Adj-RIB-Out route.

                 A value of noAggregation(1) indicates that this route
                 does not aggregate any other routes, and is not
                 aggregated by any route.

                 A value of aggregateRoute(2) indicates that this route
                 is a locally configured aggregating route.

                 A value of unsuppAggregatedRoute(3) indicates that this
                 route has been aggregated by a locally configured
                 aggregate route and is not suppressed - the route is
                 still explicitly advertised to the peer.

                 A value of suppressedAggregatedRoute(4) indicates that
                 this route has been aggregated by a locally configured
                 aggregate route and is flagged such that it should not be
                 advertised along with the aggregate route.  Typically such
                 routes are not installed on an VPN Adj-RIB-Out.  If however the
                 aggregate route itself is not permitted to be added to the
                 VPN Adj-RIB-Out then suppressed routes are advertised if they
                 themselves are permitted by policy."
    ::= { eltexBgpVpnAdjRibOutEntry 8 }

  eltexBgpVpnAdjRibOutAsSize OBJECT-TYPE
    SYNTAX      EltexBgpAsSize
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether the eltexBgpVpnAdjRibOutASPathStr object contains
                 two or four byte AS numbers."
    ::= { eltexBgpVpnAdjRibOutEntry 9 }

  eltexBgpVpnAdjRibOutASPathStr OBJECT-TYPE
    SYNTAX      OCTET STRING  (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This is a string containing the autonomous system path sent to
                 this peer in the AS_PATH attribute for this VPN Adj-RIB-Out route.
                 Two-octet AS numbers appear as four-octet numbers by adding
                 two bytes of zero padding."
    ::= { eltexBgpVpnAdjRibOutEntry 10 }

  eltexBgpVpnAdjRibOutOrigin OBJECT-TYPE
    SYNTAX      EltexBgpOriginCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The ultimate origin of the path information."
    ::= { eltexBgpVpnAdjRibOutEntry 11 }

  eltexBgpVpnAdjRibOutNextHopType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of the next hop address transmitted 
                 in the UPDATE packet."
    ::= { eltexBgpVpnAdjRibOutEntry 12 }

  eltexBgpVpnAdjRibOutNextHop OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The next hop address transmitted in the UPDATE packet."
    ::= { eltexBgpVpnAdjRibOutEntry 13 }

  eltexBgpVpnAdjRibOutMultiExitDisc OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This metric is used to discriminate between multiple
                 exit points to an adjacent autonomous system.
                 Valid only if eltexBgpVpnAdjRibOutMEDPrsnt is TRUE."
    ::= { eltexBgpVpnAdjRibOutEntry 14 }

  eltexBgpVpnAdjRibOutLocalPref OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The local preference for this VPN Adj-RIB-Out route, as
                 transmitted in the UPDATE message sent to the peer."
    ::= { eltexBgpVpnAdjRibOutEntry 15 }

  eltexBgpVpnAdjRibOutAtomicAggregate OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "When this object is set to true, the ATOMIC_AGGREGATE Path 
                 Attribute was included in the UPDATE sent to the peer
                 for this VPN Adj-RIB-Out route."
    ::= { eltexBgpVpnAdjRibOutEntry 16 }

  eltexBgpVpnAdjRibOutAggregatorAS OBJECT-TYPE
    SYNTAX      EltexBgpAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The AS number of the last BGP4 speaker that performed
                 route aggregation."
    ::= { eltexBgpVpnAdjRibOutEntry 17 }

  eltexBgpVpnAdjRibOutAggregatorAddr OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address of the last BGP4 speaker that performed
                 route aggregation.  A value of 0.0.0.0 indicates that
                 this attribute was not included in the UPDATE message
                 sent to the peer."
    ::= { eltexBgpVpnAdjRibOutEntry 18 }

  eltexBgpVpnAdjRibOutOrigId OBJECT-TYPE
    SYNTAX      EltexBgpIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The Originator-ID identifying the router that initially
                 advertised this destination to a Route Reflector.  A
                 value of 0.0.0.0 indicates the absence of this
                 attribute."
    ::= { eltexBgpVpnAdjRibOutEntry 19 }

  eltexBgpVpnAdjRibOutEcmp   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Whether or not this route was installed into the
                 Forwarding Table as an ECMP route (it may or may not be
                 the best BGP4 route advertised to BGP peers)."
    ::= { eltexBgpVpnAdjRibOutEntry 20 }

  eltexBgpVpnAdjRibOutAsLimAs OBJECT-TYPE
    SYNTAX       EltexBgpAutonomousSystemNumber
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION  "If non-zero this is the number of the AS that attached the
                  AS_PATHLIMIT attribute."
    ::= { eltexBgpVpnAdjRibOutEntry 21 }

  eltexBgpVpnAdjRibOutAsLimUpper OBJECT-TYPE
    SYNTAX      Unsigned32  (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The upper bound on the number of ASes in the AS_PATH attribute
                 after which the route will be filtered.  Only valid if
                 eltexBgpVpnAdjRibOutAsLimAs is non-zero."
    ::= { eltexBgpVpnAdjRibOutEntry 22 }

  eltexBgpVpnAdjRibOutIsActive OBJECT-TYPE
    SYNTAX      EltexBgpNlriIsActiveFlag
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "An indication of whether or not this route is installed in
                 the forwarding table.

                 - 'active' if the route is installed in the forwarding
                   table, or is a route redistributed from another routing
                   protocol instance

                 - 'inactive' otherwise.

                 - 'notTracked' if BGP does not track active routes."
    ::= { eltexBgpVpnAdjRibOutEntry 23 }

  eltexBgpVpnAdjRibOutMEDPrsnt OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If true, then the route has an associated MED attribute,
                 whose value is given in eltexBgpVpnAdjRibOutMultiExitDisc. 
                 If false, the route has no MED attribute, and the value of
                 eltexBgpVpnAdjRibOutMultiExitDisc is undefined."
    ::= { eltexBgpVpnAdjRibOutEntry 24 }

  eltexBgpVpnAdjRibOutPeerType OBJECT-TYPE
    SYNTAX      EltexBgpNlriPeerTypes
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "This field indicates whether the source peer is an iBGP or
                 eBGP peer."
    ::= { eltexBgpVpnAdjRibOutEntry 25 }

  eltexBgpVpnAdjRibOutRd OBJECT-TYPE
    SYNTAX      EltexBgpRouteDistinguisher
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Route Distinguisher of the route."
    ::= { eltexBgpVpnAdjRibOutEntry 26 }

  eltexBgpVpnAdjRibOutEvpnRouteType OBJECT-TYPE
    SYNTAX      EltexBgpEvpnRouteTypes
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "EVPN route type."
    ::= { eltexBgpVpnAdjRibOutEntry 27 }

  eltexBgpVpnAdjRibOutEvpnPrefixLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "EVPN route length in bits without Route Distinguisher."
    ::= { eltexBgpVpnAdjRibOutEntry 28 }

  eltexBgpVpnAdjRibOutEvpnEsi OBJECT-TYPE
    SYNTAX      EltexBgpEvpnESI
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Ethernet Segment Identifier."
    ::= { eltexBgpVpnAdjRibOutEntry 29 }

  eltexBgpVpnAdjRibOutEvpnEthernetTagId OBJECT-TYPE
    SYNTAX      EltexBgpEvpnEthernetTag
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "VLAN ID."
    ::= { eltexBgpVpnAdjRibOutEntry 30 }

  eltexBgpVpnAdjRibOutEvpnMacAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "Length in bits field eltexBgpVpnAdjRibOutEvpnMacAddress."
    ::= { eltexBgpVpnAdjRibOutEntry 31 }

  eltexBgpVpnAdjRibOutEvpnMacAddress OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "MAC address from route type 2."
    ::= { eltexBgpVpnAdjRibOutEntry 32 }

  eltexBgpVpnAdjRibOutEvpnPrefixAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The length of field eltexBgpVpnAdjRibOutEvpnPrefixAddress, for 
                 IPv4 it is 32 bits, and for IPv6 - 128. This field is
                 optional and may not contain any values (all zeros)."
    ::= { eltexBgpVpnAdjRibOutEntry 33 }

  eltexBgpVpnAdjRibOutEvpnPrefixAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A type of the address prefix in the Network Layer Reachability
                 Information field for this route. Optional field for route type 2."
    ::= { eltexBgpVpnAdjRibOutEntry 34 }

  eltexBgpVpnAdjRibOutEvpnPrefixAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "IP address optional field for route type 2."
    ::= { eltexBgpVpnAdjRibOutEntry 35 }

  eltexBgpVpnAdjRibOutEvpnOrigAddressLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The length field eltexBgpVpnAdjRibOutEvpnOrigAddress for the IP
                 address of the originator of the route."
    ::= { eltexBgpVpnAdjRibOutEntry 36 }

  eltexBgpVpnAdjRibOutEvpnOrigAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "IP address type field eltexBgpVpnAdjRibOutEvpnOrigAddress."
    ::= { eltexBgpVpnAdjRibOutEntry 37 }

  eltexBgpVpnAdjRibOutEvpnOrigAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The IP address of the originator of the route, usually 
                 the VTEP router loopback."
    ::= { eltexBgpVpnAdjRibOutEntry 38 }
-------------------------------------------------------------------------------

  --
  -- BGP Network Table
  --
  -- This table contains the set of internal routes BGP advertised to each peer.
  --

  eltexBgpNetworkTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpNetworkEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "BGP network configuration table.

                 This table allows a user to configure internal networks
                 advertised via BGP."
    ::= { eltexBgpRib 4 }

  eltexBgpNetworkEntry OBJECT-TYPE
    SYNTAX      EltexBgpNetworkEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Entry containing information about the internal network
                 announced via BGP."
    INDEX { eltexBgpProcessId,
            eltexBgpNetworkAfi,
            eltexBgpNetworkSafi,
            eltexBgpNetworkPrfxType,
            eltexBgpNetworkPrfx,
            eltexBgpNetworkPrfxLen }
    ::= { eltexBgpNetworkTable 1 }

  EltexBgpNetworkEntry ::= SEQUENCE {
      eltexBgpNetworkAfi                    EltexBgpAfi,
      eltexBgpNetworkSafi                   EltexBgpSafi,
      eltexBgpNetworkPrfxType               InetAddressType,
      eltexBgpNetworkPrfx                   InetAddress,
      eltexBgpNetworkPrfxLen                InetAddressPrefixLength,
      eltexBgpNetworkRowStatus              RowStatus
    }

  eltexBgpNetworkAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The address family of the prefix for this route."
    DEFVAL      { ipv4 }
    ::= { eltexBgpNetworkEntry 1 }

  eltexBgpNetworkSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this
                 route."
    DEFVAL      { unicast }
    ::= { eltexBgpNetworkEntry 2 }

  eltexBgpNetworkPrfxType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "A type of address prefix."
    ::= { eltexBgpNetworkEntry 3 }

  eltexBgpNetworkPrfx OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "An address prefix."
    ::= { eltexBgpNetworkEntry 4 }

  eltexBgpNetworkPrfxLen OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Length in bits of the address prefix contained in the
                 eltexBgpNetworkPrfx object."
    ::= { eltexBgpNetworkEntry 5 }

  eltexBgpNetworkRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The row status for this BGP Network Table entry, used to
                 create and destroy table entries."
    ::= { eltexBgpNetworkEntry 6 }

-------------------------------------------------------------------------------

  --
  -- Path Attribute Extensions
  --

  eltexBgpPathAttrExtensions OBJECT IDENTIFIER ::= { eltexBgpRib 5 }

  --
  -- Path Attribute Route Reflection Extensions
  --

  eltexBgpPathAttrRouteReflectionExts OBJECT IDENTIFIER ::= { eltexBgpPathAttrExtensions 1 }


  --
  -- Cluster table
  --
  -- This table holds the clusters passed through on a given path.
  --

  eltexBgpPathAttrClusterLocTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPathAttrClusterLocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP-4 Path Attribute Cluster Table contains the per
                 network path (NLRI) data on the reflection path which a
                 route has traversed.  The absence of row data for a given
                 network path indicates a lack of this attribute information
                 for the indicated network path.

                 This table reports received routes and path attributes after
                 import policy has been applied.  Only routes accepted by
                 import policy are reported."
    ::= { eltexBgpPathAttrRouteReflectionExts 1 }

  eltexBgpPathAttrClusterLocEntry OBJECT-TYPE
    SYNTAX      EltexBgpPathAttrClusterLocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a cluster traversal provided with a path to
                 a network."
    INDEX { eltexBgpProcessId,
            eltexBgpLocRibPeerOrRib,
            eltexBgpLocRibPeerRibIndex,
            eltexBgpLocRibAfi,
            eltexBgpLocRibSafi,
            eltexBgpLocRibPrfx,
            eltexBgpLocRibPrfxLen,
            eltexBgpLocRibPathId,
            eltexBgpPathAttrClusterLocIndex }
    ::= { eltexBgpPathAttrClusterLocTable 1 }


  EltexBgpPathAttrClusterLocEntry ::= SEQUENCE {
      eltexBgpPathAttrClusterLocIndex      Unsigned32,
      eltexBgpPathAttrClusterLocValue      Unsigned32
      }

  eltexBgpPathAttrClusterLocIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An integral index for a row in this table."
    ::= { eltexBgpPathAttrClusterLocEntry 1 }

  eltexBgpPathAttrClusterLocValue OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A four octet long value representing a part of the
                 reflection path that the route has passed.  Each such four
                 octet long value represents the ID of a cluster that
                 the route has traversed.  The sequence of this path as
                 received in the route advertisement will be preserved in
                 the sequence of eltexBgpPathAttrClusterTable rows (and the
                 eltexBgpLocPathAttrClusterValue's in each row) as returned for a given
                 network path, and the monotonically increasing sequence of
                 eltexBgpLocPathAttrClusterIndex values for that network path."
    ::= { eltexBgpPathAttrClusterLocEntry 2 }

-------------------------------------------------------------------------------

  eltexBgpCommList OBJECT IDENTIFIER ::= { eltexBgpObjects 4 }

  --
  -- BGP Community List Table.
  --
  -- This table contains BGP Community List for set or matching in a route.
  --

  eltexBgpCommunityListTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpCommunityListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The table of BGP Community List entries.

                 A Community List is used to match against communities in a
                 route or to set communities in a route.  A Community List
                 consists of the set of entries in this table with a common
                 eltexBgpCommunityListName.  This set of entries is then ordered
                 by the eltexBgpCommunityListEntryIndex value and this ordering is
                 important when matching against communities in a route.

                 When used to match against communities in a route, the
                 method used for a Community List entry depends on
                 eltexBgpCommunityListEntryType.

                 - If 'community-group', the route communities are matched
                 against entries in the eltexBgpCommunityGroupTable.

                 - If 'regular-expression', the route communities are
                 matched against eltexBgpCommunityListRegexp.

                 When used to set communities in a route, a Community List
                 entry is only used if eltexBgpCommunityListEntryType is
                 'community-group' and eltexBgpCommunityListPermit is 'permit'.

                 The entries in the eltexBgpCommunityGroupTable which correspond
                 to this entry in the eltexBgpCommunityListTable have the same
                 eltexBgpCommunityListName and eltexBgpCommunityListEntryIndex
                 indices."
     ::= { eltexBgpCommList 1 }

  eltexBgpCommunityListEntry OBJECT-TYPE
    SYNTAX      EltexBgpCommunityListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Each entry represents a BGP Community"
    INDEX { eltexBgpCommunityListType,
            eltexBgpCommunityListName,
            eltexBgpCommunityListEntryIndex }
    ::= { eltexBgpCommunityListTable 1 }

  EltexBgpCommunityListEntry ::= SEQUENCE {
      eltexBgpCommunityListType          EltexBgpCommListType,
      eltexBgpCommunityListName          DisplayString,
      eltexBgpCommunityListEntryIndex    Unsigned32,
      eltexBgpCommunityListRowStatus     RowStatus,
      eltexBgpCommunityListEntryType     EltexBgpCommListEntryType,
      eltexBgpCommunityListPermit        EltexBgpPermitOrDeny,
      eltexBgpCommunityListRegexp        DisplayString
      }


  eltexBgpCommunityListType OBJECT-TYPE
    SYNTAX      EltexBgpCommListType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Community type Standard or Extended."
    ::= { eltexBgpCommunityListEntry 1 }

  eltexBgpCommunityListName OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Name (identifier) of the the Community
                 List."
    ::= { eltexBgpCommunityListEntry 2 }

  eltexBgpCommunityListEntryIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of this entry in the Community List.

                 This ordering is important when the Community List is used
                 to match against communities in a route."
    ::= { eltexBgpCommunityListEntry 3 }

  eltexBgpCommunityListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Used to create and delete a Community List entry."
    ::= { eltexBgpCommunityListEntry 4 }

  eltexBgpCommunityListEntryType OBJECT-TYPE
    SYNTAX      EltexBgpCommListEntryType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "This field indicates how this entry is used to match route
                 commmunities.

                 - If 'community-group', the route communities are matched
                 against entries in the eltexBgpCommunityGroupTable.

                 - If 'regular-expression', the route communities are
                 matched against eltexBgpCommunityListRegexp.

                 When used to set route communities, this entry is only
                 used if this field is 'community-group' and
                 eltexBgpCommunityListPermit is 'permit'."
    DEFVAL { communityGroup }
    ::= { eltexBgpCommunityListEntry 5 }

  eltexBgpCommunityListPermit OBJECT-TYPE
    SYNTAX      EltexBgpPermitOrDeny
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "When matching routes, this field indicates whether the set
                 of matched routes should be permitted or denied.

                 When setting routes, this Community List entry is ignored
                 if this field is 'deny'."
    DEFVAL { permit }
    ::= { eltexBgpCommunityListEntry 6 }

  eltexBgpCommunityListRegexp OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "If eltexBgpCommunityListType value set to 'standardCommunity',
                 contains the regular expression to use when matching
                 elements of the community list for a route.  This is
                 stored here in ASCII format.  Communities are matched
                 using new-format decimal notation.  For example, the
                 community '0x00120101' should be represented in the string
                 as '18:257'.  The string is not NULL-terminated.  A NULL
                 string or a comm_exp_len of zero indicates that the field
                 is not in use.

                 If eltexBgpCommunityListType value set to 'extendedCommunity',
                 contains the regular expression to use when matching
                 elements of the extended community list for a route.  This
                 is stored here in ASCII format.  Extended communities are
                 matched as hexadecimal numbers.  For example, the extended
                 community '0x11223344556677' should be represented in the
                 string as '0011223344556677' (leading zeroes are necessary
                 to make the length up to 8 bytes).  The string is not
                 NULL-terminated.  A NULL string or a ext_comm_exp_len of
                 zero indicates that the field is not in use.

                 This field is only relevant if eltexBgpCommunityListEntryType
                 is 'regular-expression'.  It is otherwise ignored."
    ::= { eltexBgpCommunityListEntry 7 }

-------------------------------------------------------------------------------

  --
  -- BGP Community Group Table.
  --
  -- This table contains a community for Community List.
  --

  eltexBgpCommunityGroupTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpCommunityGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The table of BGP Community Group entries.

                 Each entry in this table contains a single community.

                 A Community List entry with an event type of
                 'community-group' uses a Community Group.  The set of
                 eltexBgpCommunityGroupTable entries corresponding to a
                 eltexBgpCommunityListTable entry are those with the same
                 eltexBgpCommunityListName and eltexBgpCommunityListEntryIndex values.

                 This set of entries gives a group of communities.  The
                 ordering of this group of communities is not important,
                 hence we can directly use the community value as the third
                 MIB index for this table."
     ::= { eltexBgpCommList 2 }

  eltexBgpCommunityGroupEntry OBJECT-TYPE
    SYNTAX      EltexBgpCommunityGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Each entry represents a BGP Community"
    INDEX { eltexBgpCommunityListType,
            eltexBgpCommunityListName,
            eltexBgpCommunityListEntryIndex,
            eltexBgpCommunityGroupCommunity}
    ::= { eltexBgpCommunityGroupTable 1 }

  EltexBgpCommunityGroupEntry ::= SEQUENCE {
      eltexBgpCommunityGroupCommunity     EltexBgpCommunity,
      eltexBgpCommunityGroupRowStatus     RowStatus
      }

  eltexBgpCommunityGroupCommunity OBJECT-TYPE
    SYNTAX      EltexBgpCommunity
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The community value to use when matching against or
                 setting the route communities.

                 Note that the community value itself is used as an index
                 field.  This is OK as the order of communities with a
                 Community Group is irrelevant."
    ::= { eltexBgpCommunityGroupEntry 1 }

  eltexBgpCommunityGroupRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Used to create and delete a Community Group entry."
    ::= { eltexBgpCommunityGroupEntry 2 }

-------------------------------------------------------------------------------

  --
  -- BGP local RIB communities table
  --
  -- This table holds information on the communities the indexed route belongs
  -- to.
  --

  eltexBgpPathAttrCommunityExts OBJECT IDENTIFIER ::= { eltexBgpPathAttrExtensions 2 }

  eltexBgpPathAttrCommLocTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPathAttrCommLocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP-4 Path Attribute Community Table contains the per
                 network path (NLRI) data on the community membership
                 advertised with a route.  The absence of row data for a given
                 network path indicates a lack of this attribute information
                 for the indicated network path.

                 This table reports received routes and path attributes after
                 import policy has been applied.  Only routes accepted by
                 import policy are reported."
    ::= { eltexBgpPathAttrCommunityExts 1 }

  eltexBgpPathAttrCommLocEntry OBJECT-TYPE
    SYNTAX      EltexBgpPathAttrCommLocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a community association provided with a path
                 to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpPathAttrCommLocPeerOrRib,
            eltexBgpPathAttrCommLocPeerRibIndex,
            eltexBgpPathAttrCommLocAfi,
            eltexBgpPathAttrCommLocSafi,
            eltexBgpPathAttrCommLocPrfx,
            eltexBgpPathAttrCommLocPrfxLen,
            eltexBgpPathAttrCommLocPathId,
            eltexBgpPathAttrCommLocIndex }
    ::= { eltexBgpPathAttrCommLocTable 1 }


  EltexBgpPathAttrCommLocEntry ::= SEQUENCE {
      eltexBgpPathAttrCommLocPeerOrRib     EltexBgpPeerOrRib,
      eltexBgpPathAttrCommLocPeerRibIndex  Unsigned32,
      eltexBgpPathAttrCommLocAfi           EltexBgpAfi,
      eltexBgpPathAttrCommLocSafi          EltexBgpSafi,
      eltexBgpPathAttrCommLocPrfx          OCTET STRING,
      eltexBgpPathAttrCommLocPrfxLen       Unsigned32,
      eltexBgpPathAttrCommLocPathId        Unsigned32,
      eltexBgpPathAttrCommLocIndex         Unsigned32,
      eltexBgpPathAttrCommLocValue         EltexBgpCommunity,
      eltexBgpPathAttrCommLocUserData      OCTET STRING
      }

  eltexBgpPathAttrCommLocPeerOrRib OBJECT-TYPE
    SYNTAX      EltexBgpPeerOrRib
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Whether this route was learned from a BGP peer or redistributed
                 from Routing Information Base."
    ::= { eltexBgpPathAttrCommLocEntry 1 }

  eltexBgpPathAttrCommLocPeerRibIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of either the BGP peer or RIB this route was
                 learned from.  If eltexBgpPathAttrCommLocPeerOrRib is peer, this
                 field is equivalent to a eltexBgpPeerStatusPeerIndex.  If
                 eltexBgpPathAttrCommLocPeerOrRib is afm, this field is equivalent to
                 an internal index of RIB entity."
    ::= { eltexBgpPathAttrCommLocEntry 2 }

  eltexBgpPathAttrCommLocAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this Loc-RIB route."
    ::= { eltexBgpPathAttrCommLocEntry 3 }

  eltexBgpPathAttrCommLocSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this Loc-RIB
                 route."
    ::= { eltexBgpPathAttrCommLocEntry 4 }

  eltexBgpPathAttrCommLocPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field.

                 The prefix length is specified by eltexBgpPathAttrCommLocPrfxLen.  Any bits
                 beyond the length specified by eltexBgpPathAttrCommLocPrfxLen are zeroed.

                 This field contains the full line format BGP NLRI omitting
                 any NLRI length field.

                 For SAFI 128 the NLRI includes the MPLS label and Route
                 Distinguisher as well as the IPv4 or IPv6 address prefix."
  ::= { eltexBgpPathAttrCommLocEntry 5 }

  eltexBgpPathAttrCommLocPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the prefix in the Network Layer Reachability
                 Information field."
    ::= { eltexBgpPathAttrCommLocEntry 6 }

  eltexBgpPathAttrCommLocPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                 If BGP additional path receive capability was negotiated
                 with the peer for this AFI/SAFI then this is the received
                 path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpPathAttrCommLocEntry 7 }

  eltexBgpPathAttrCommLocIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An integer index for a row in this table."
    ::= { eltexBgpPathAttrCommLocEntry 8 }

  eltexBgpPathAttrCommLocValue OBJECT-TYPE
    SYNTAX      EltexBgpCommunity
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A value representing a community.   There are certain
                 4-octet long values which could be returned in this
                 columnar row data that carry additional semantics."
    ::= { eltexBgpPathAttrCommLocEntry 9 }

  eltexBgpPathAttrCommLocUserData OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE (4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "User data for this path attribute."
    ::= { eltexBgpPathAttrCommLocEntry 10 }

-------------------------------------------------------------------------------

  --
  -- BGP  Adj-RIB In communities table
  --
  -- This table holds information on the communities the indexed route belongs
  -- to.

  eltexBgpPathAttrCommAdjInTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPathAttrCommAdjInEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP-4 Received Path Attribute Community Table contains the
                 per network path (NLRI) data on the community membership
                 advertised with a route.  The absence of row data for a given
                 network path indicates a lack of this attribute information
                 for the indicated network path.

                 This table is similar to eltexBgpPathAttrCommLocTable but
                 reports path attributes before import policy has been applied."
    ::= { eltexBgpPathAttrCommunityExts 2 }

  eltexBgpPathAttrCommAdjInEntry OBJECT-TYPE
    SYNTAX      EltexBgpPathAttrCommAdjInEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a community association provided with a path
                 to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpPathAttrCommAdjInPeerRibIndex,
            eltexBgpPathAttrCommAdjInAfi,
            eltexBgpPathAttrCommAdjInSafi,
            eltexBgpPathAttrCommAdjInPrfx,
            eltexBgpPathAttrCommAdjInPrfxLen,
            eltexBgpPathAttrCommAdjInPathId,
            eltexBgpPathAttrCommAdjInIndex }
    ::= { eltexBgpPathAttrCommAdjInTable 1 }

  EltexBgpPathAttrCommAdjInEntry ::= SEQUENCE {
      eltexBgpPathAttrCommAdjInPeerRibIndex  Unsigned32,
      eltexBgpPathAttrCommAdjInAfi           EltexBgpAfi,
      eltexBgpPathAttrCommAdjInSafi          EltexBgpSafi,
      eltexBgpPathAttrCommAdjInPrfx          OCTET STRING,
      eltexBgpPathAttrCommAdjInPrfxLen       Unsigned32,
      eltexBgpPathAttrCommAdjInPathId        Unsigned32,
      eltexBgpPathAttrCommAdjInIndex         Unsigned32,
      eltexBgpPathAttrCommAdjInValue         EltexBgpCommunity,
      eltexBgpPathAttrCommAdjInUserData      OCTET STRING
      }

  eltexBgpPathAttrCommAdjInPeerRibIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of the BGP peer this route was learned from.
                 This field is equivalent to a eltexBgpPeerStatusPeerIndex."
    ::= { eltexBgpPathAttrCommAdjInEntry 1 }

  eltexBgpPathAttrCommAdjInAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this Adj-RIB In route."
    ::= { eltexBgpPathAttrCommAdjInEntry 2 }

  eltexBgpPathAttrCommAdjInSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this Adj-RIB In
                 route."
    ::= { eltexBgpPathAttrCommAdjInEntry 3 }

  eltexBgpPathAttrCommAdjInPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field.

                 The prefix length is specified by eltexBgpPathAttrCommAdjInPrfxLen.  Any bits
                 beyond the length specified by eltexBgpPathAttrCommAdjInPrfxLen are zeroed.

                 This field contains the full line format BGP NLRI omitting
                 any NLRI length field.

                 For SAFI 128 the NLRI includes the MPLS label and Route
                 Distinguisher as well as the IPv4 or IPv6 address prefix."
  ::= { eltexBgpPathAttrCommAdjInEntry 4 }

  eltexBgpPathAttrCommAdjInPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the prefix in the Network Layer Reachability
                 Information field."
    ::= { eltexBgpPathAttrCommAdjInEntry 5 }

  eltexBgpPathAttrCommAdjInPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                 If BGP additional path receive capability was negotiated
                 with the peer for this AFI/SAFI then this is the received
                 path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpPathAttrCommAdjInEntry 6 }

  eltexBgpPathAttrCommAdjInIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An integer index for a row in this table."
    ::= { eltexBgpPathAttrCommAdjInEntry 7 }

  eltexBgpPathAttrCommAdjInValue  OBJECT-TYPE
    SYNTAX      EltexBgpCommunity
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A value representing a community.   There are certain
                 4-octet long values which could be returned in this
                 columnar row data that carry additional semantics."
    ::= { eltexBgpPathAttrCommAdjInEntry 8 }

  eltexBgpPathAttrCommAdjInUserData OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE (4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "User data for this path attribute."
    ::= { eltexBgpPathAttrCommAdjInEntry 9 }

-------------------------------------------------------------------------------

  --
  -- BGP Adj-RIB Out Communities table
  --
  -- This table holds information on the communities the indexed route belongs
  -- to.

  eltexBgpPathAttrCommAdjOutTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPathAttrCommAdjOutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP-4 Adj-RIB Out Path Attribute Community Table contains the
                 per network path (NLRI) data on the community membership
                 advertised with a route.  The absence of row data for a given
                 network path indicates a lack of this attribute information
                 for the indicated network path.

                 This table reports transmitted routes and path attributes
                 after export policy has been applied.  Only routes accepted by
                 export policy are reported."
    ::= { eltexBgpPathAttrCommunityExts 3 }

  eltexBgpPathAttrCommAdjOutEntry OBJECT-TYPE
    SYNTAX      EltexBgpPathAttrCommAdjOutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about a community association provided with a path
                 to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpPathAttrCommAdjOutPeerRibIndex,
            eltexBgpPathAttrCommAdjOutAfi,
            eltexBgpPathAttrCommAdjOutSafi,
            eltexBgpPathAttrCommAdjOutPrfx,
            eltexBgpPathAttrCommAdjOutPrfxLen,
            eltexBgpPathAttrCommAdjOutPathId,
            eltexBgpPathAttrCommAdjOutIndex }
    ::= { eltexBgpPathAttrCommAdjOutTable 1 }

  EltexBgpPathAttrCommAdjOutEntry ::= SEQUENCE {
      eltexBgpPathAttrCommAdjOutPeerRibIndex  Unsigned32,
      eltexBgpPathAttrCommAdjOutAfi           EltexBgpAfi,
      eltexBgpPathAttrCommAdjOutSafi          EltexBgpSafi,
      eltexBgpPathAttrCommAdjOutPrfx          OCTET STRING,
      eltexBgpPathAttrCommAdjOutPrfxLen       Unsigned32,
      eltexBgpPathAttrCommAdjOutPathId        Unsigned32,
      eltexBgpPathAttrCommAdjOutIndex         Unsigned32,
      eltexBgpPathAttrCommAdjOutValue         EltexBgpCommunity,
      eltexBgpPathAttrCommAdjOutUserData      OCTET STRING
      }

  eltexBgpPathAttrCommAdjOutPeerRibIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of the BGP peer this route was learned from.
                 This field is equivalent to a eltexBgpPeerStatusPeerIndex."
    ::= { eltexBgpPathAttrCommAdjOutEntry 1 }

  eltexBgpPathAttrCommAdjOutAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this Adj-RIB Out route."
    ::= { eltexBgpPathAttrCommAdjOutEntry 2 }

  eltexBgpPathAttrCommAdjOutSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this Adj-RIB Out
                 route."
    ::= { eltexBgpPathAttrCommAdjOutEntry 3 }

  eltexBgpPathAttrCommAdjOutPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field.

                 The prefix length is specified by eltexBgpPathAttrCommAdjOutPrfxLen.  Any bits
                 beyond the length specified by eltexBgpPathAttrCommAdjOutPrfxLen are zeroed.

                 This field contains the full line format BGP NLRI omitting
                 any NLRI length field.

                 For SAFI 128 the NLRI includes the MPLS label and Route
                 Distinguisher as well as the IPv4 or IPv6 address prefix."
  ::= { eltexBgpPathAttrCommAdjOutEntry 4 }

  eltexBgpPathAttrCommAdjOutPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the prefix in the Network Layer Reachability
                 Information field."
    ::= { eltexBgpPathAttrCommAdjOutEntry 5 }

  eltexBgpPathAttrCommAdjOutPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                 If BGP additional path receive capability was negotiated
                 with the peer for this AFI/SAFI then this is the received
                 path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpPathAttrCommAdjOutEntry 6 }

  eltexBgpPathAttrCommAdjOutIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An integer index for a row in this table."
    ::= { eltexBgpPathAttrCommAdjOutEntry 7 }

  eltexBgpPathAttrCommAdjOutValue  OBJECT-TYPE
    SYNTAX      EltexBgpCommunity
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A value representing a community. There are certain
                 4-octet long values which could be returned in this
                 columnar row data that carry additional semantics."
    ::= { eltexBgpPathAttrCommAdjOutEntry 8 }

  eltexBgpPathAttrCommAdjOutUserData OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE (4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "User data for this path attribute."
    ::= { eltexBgpPathAttrCommAdjOutEntry 9 }

-------------------------------------------------------------------------------

  --
  -- BGP local RIB Extended Communities
  --
  -- This table holds information on the extended communities the indexed route
  -- belongs to.
  --

  eltexBgpPathAttrExtCommunityExts OBJECT IDENTIFIER ::= { eltexBgpPathAttrExtensions 3 }

  eltexBgpPathAttrExtCommLocTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPathAttrExtCommLocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP-4 Path Attribute Extended Community Table contains the
                 per network path (NLRI) data on the extended community
                 membership advertised with a route.  The absence of row data
                 for a given network path indicates a lack of this attribute
                 information for the indicated network path.

                 This table reports received routes and path attributes after
                 import policy has been applied.  Only routes accepted by
                 import policy are reported."
    ::= { eltexBgpPathAttrExtCommunityExts 1 }

  eltexBgpPathAttrExtCommLocEntry OBJECT-TYPE
    SYNTAX      EltexBgpPathAttrExtCommLocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about an extended community association provided
                 with a path to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpPathAttrExtCommLocPeerOrRib,
            eltexBgpPathAttrExtCommLocPeerRibIndex,
            eltexBgpPathAttrExtCommLocAfi,
            eltexBgpPathAttrExtCommLocSafi,
            eltexBgpPathAttrExtCommLocPrfx,
            eltexBgpPathAttrExtCommLocPrfxLen,
            eltexBgpPathAttrExtCommLocPathId,
            eltexBgpPathAttrExtCommLocIndex }
    ::= { eltexBgpPathAttrExtCommLocTable 1 }

  EltexBgpPathAttrExtCommLocEntry ::= SEQUENCE {
      eltexBgpPathAttrExtCommLocPeerOrRib     EltexBgpPeerOrRib,
      eltexBgpPathAttrExtCommLocPeerRibIndex  Unsigned32,
      eltexBgpPathAttrExtCommLocAfi           EltexBgpAfi,
      eltexBgpPathAttrExtCommLocSafi          EltexBgpSafi,
      eltexBgpPathAttrExtCommLocPrfx          OCTET STRING,
      eltexBgpPathAttrExtCommLocPrfxLen       Unsigned32,
      eltexBgpPathAttrExtCommLocPathId        Unsigned32,
      eltexBgpPathAttrExtCommLocIndex         Unsigned32,
      eltexBgpPathAttrExtCommLocValue         EltexBgpExtendedCommunity,
      eltexBgpPathAttrExtCommLocUserData      OCTET STRING
      }

  eltexBgpPathAttrExtCommLocPeerOrRib OBJECT-TYPE
    SYNTAX      EltexBgpPeerOrRib
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Whether this route was learned from a BGP peer or redistributed
                 from Routing Information Base."
    ::= { eltexBgpPathAttrExtCommLocEntry 1 }

  eltexBgpPathAttrExtCommLocPeerRibIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of either the BGP peer or RIB this route was
                 learned from.  If eltexBgpPathAttrExtCommLocPeerOrRib is peer, this field
                 is equivalent to a eltexBgpPeerStatusPeerIndex.  If
                 eltexBgpPathAttrExtCommLocPeerOrRib is afm, this field is equivalent to
                 an internal index of RIB entity."
    ::= { eltexBgpPathAttrExtCommLocEntry 2 }

  eltexBgpPathAttrExtCommLocAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this Loc-RIB route."
    ::= { eltexBgpPathAttrExtCommLocEntry 3 }

  eltexBgpPathAttrExtCommLocSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this Loc-RIB
                 route."
    ::= { eltexBgpPathAttrExtCommLocEntry 4 }

  eltexBgpPathAttrExtCommLocPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field.

                 The prefix length is specified by eltexBgpPathAttrExtCommLocPrfxLen.  Any bits
                 beyond the length specified by eltexBgpPathAttrExtCommLocPrfxLen are zeroed.

                 This field contains the full line format BGP NLRI omitting
                 any NLRI length field.

                 For SAFI 128 the NLRI includes the MPLS label and Route
                 Distinguisher as well as the IPv4 or IPv6 address prefix."
  ::= { eltexBgpPathAttrExtCommLocEntry 5 }

  eltexBgpPathAttrExtCommLocPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the prefix in the Network Layer Reachability
                 Information field."
    ::= { eltexBgpPathAttrExtCommLocEntry 6 }

  eltexBgpPathAttrExtCommLocPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                 If BGP additional path receive capability was negotiated
                 with the peer for this AFI/SAFI then this is the received
                 path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpPathAttrExtCommLocEntry 7 }

  eltexBgpPathAttrExtCommLocIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An integer index for a row in this table."
    ::= { eltexBgpPathAttrExtCommLocEntry 8 }

  eltexBgpPathAttrExtCommLocValue  OBJECT-TYPE
    SYNTAX      EltexBgpExtendedCommunity
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A value representing an extended community.   There are
                 certain 8-octet long values which could be returned in this
                 columnar row data that carry additional semantics."
    ::= { eltexBgpPathAttrExtCommLocEntry 9 }

  eltexBgpPathAttrExtCommLocUserData OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE (4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "User data for this path attribute."
    ::= { eltexBgpPathAttrExtCommLocEntry 10 }

-------------------------------------------------------------------------------

  --
  -- BGP  Adj-RIB In Extended Communities table
  --
  -- This table holds information on the extended communities the indexed route
  -- belongs to.

  eltexBgpPathAttrExtCommAdjInTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPathAttrExtCommAdjInEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP-4 Received Path Attribute Extended Community Table contains the
                 per network path (NLRI) data on the extended community membership
                 advertised with a route.  The absence of row data for a given
                 network path indicates a lack of this attribute information
                 for the indicated network path.

                 This table is similar to eltexBgpPathAttrExtCommLocTable but reports
                 path attributes before import policy has been applied."
    ::= { eltexBgpPathAttrExtCommunityExts 2 }

  eltexBgpPathAttrExtCommAdjInEntry OBJECT-TYPE
    SYNTAX      EltexBgpPathAttrExtCommAdjInEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about an extended community association provided with a path
                 to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpPathAttrExtCommAdjInPeerRibIndex,
            eltexBgpPathAttrExtCommAdjInAfi,
            eltexBgpPathAttrExtCommAdjInSafi,
            eltexBgpPathAttrExtCommAdjInPrfx,
            eltexBgpPathAttrExtCommAdjInPrfxLen,
            eltexBgpPathAttrExtCommAdjInPathId,
            eltexBgpPathAttrExtCommAdjInIndex }
    ::= { eltexBgpPathAttrExtCommAdjInTable 1 }

  EltexBgpPathAttrExtCommAdjInEntry ::= SEQUENCE {
      eltexBgpPathAttrExtCommAdjInPeerRibIndex  Unsigned32,
      eltexBgpPathAttrExtCommAdjInAfi           EltexBgpAfi,
      eltexBgpPathAttrExtCommAdjInSafi          EltexBgpSafi,
      eltexBgpPathAttrExtCommAdjInPrfx          OCTET STRING,
      eltexBgpPathAttrExtCommAdjInPrfxLen       Unsigned32,
      eltexBgpPathAttrExtCommAdjInPathId        Unsigned32,
      eltexBgpPathAttrExtCommAdjInIndex         Unsigned32,
      eltexBgpPathAttrExtCommAdjInValue         EltexBgpExtendedCommunity,
      eltexBgpPathAttrExtCommAdjInUserData      OCTET STRING
      }

  eltexBgpPathAttrExtCommAdjInPeerRibIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of the BGP peer this route was learned from.
                 This field is equivalent to a eltexBgpPeerStatusPeerIndex."
    ::= { eltexBgpPathAttrExtCommAdjInEntry 1 }

  eltexBgpPathAttrExtCommAdjInAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this Adj-RIB In route."
    ::= { eltexBgpPathAttrExtCommAdjInEntry 2 }

  eltexBgpPathAttrExtCommAdjInSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this Adj-RIB In
                 route."
    ::= { eltexBgpPathAttrExtCommAdjInEntry 3 }

  eltexBgpPathAttrExtCommAdjInPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field.

                 The prefix length is specified by eltexBgpPathAttrExtCommAdjInPrfxLen.  Any bits
                 beyond the length specified by eltexBgpPathAttrExtCommAdjInPrfxLen are zeroed.

                 This field contains the full line format BGP NLRI omitting
                 any NLRI length field.

                 For SAFI 128 the NLRI includes the MPLS label and Route
                 Distinguisher as well as the IPv4 or IPv6 address prefix."
  ::= { eltexBgpPathAttrExtCommAdjInEntry 4 }

  eltexBgpPathAttrExtCommAdjInPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the prefix in the Network Layer Reachability
                 Information field."
    ::= { eltexBgpPathAttrExtCommAdjInEntry 5 }

  eltexBgpPathAttrExtCommAdjInPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                 If BGP additional path receive capability was negotiated
                 with the peer for this AFI/SAFI then this is the received
                 path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpPathAttrExtCommAdjInEntry 6 }

  eltexBgpPathAttrExtCommAdjInIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An integer index for a row in this table."
    ::= { eltexBgpPathAttrExtCommAdjInEntry 7 }

  eltexBgpPathAttrExtCommAdjInValue  OBJECT-TYPE
    SYNTAX      EltexBgpExtendedCommunity
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A value representing a community.   There are certain
                 8-octet long values which could be returned in this
                 columnar row data that carry additional semantics."
    ::= { eltexBgpPathAttrExtCommAdjInEntry 8 }

  eltexBgpPathAttrExtCommAdjInUserData OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE (4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "User data for this path attribute."
    ::= { eltexBgpPathAttrExtCommAdjInEntry 9 }

-------------------------------------------------------------------------------

  --
  -- BGP Adj-RIB Out ExtCommunities table
  --
  -- This table holds information on the communities the indexed route belongs
  -- to.

  eltexBgpPathAttrExtCommAdjOutTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpPathAttrExtCommAdjOutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The BGP-4 Adj-RIB Out Path Attribute ExtCommunity Table contains the
                 per network path (NLRI) data on the extended community membership
                 advertised with a route.  The absence of row data for a given
                 network path indicates a lack of this attribute information
                 for the indicated network path.

                 This table reports transmitted routes and path attributes
                 after export policy has been applied.  Only routes accepted by
                 export policy are reported."
    ::= { eltexBgpPathAttrExtCommunityExts 3 }

  eltexBgpPathAttrExtCommAdjOutEntry OBJECT-TYPE
    SYNTAX      EltexBgpPathAttrExtCommAdjOutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Information about an extended community association provided with a path
                 to a network."
    INDEX { eltexBgpProcessId,
            eltexBgpPathAttrExtCommAdjOutPeerRibIndex,
            eltexBgpPathAttrExtCommAdjOutAfi,
            eltexBgpPathAttrExtCommAdjOutSafi,
            eltexBgpPathAttrExtCommAdjOutPrfx,
            eltexBgpPathAttrExtCommAdjOutPrfxLen,
            eltexBgpPathAttrExtCommAdjOutPathId,
            eltexBgpPathAttrExtCommAdjOutIndex }
    ::= { eltexBgpPathAttrExtCommAdjOutTable 1 }

  EltexBgpPathAttrExtCommAdjOutEntry ::= SEQUENCE {
      eltexBgpPathAttrExtCommAdjOutPeerRibIndex  Unsigned32,
      eltexBgpPathAttrExtCommAdjOutAfi           EltexBgpAfi,
      eltexBgpPathAttrExtCommAdjOutSafi          EltexBgpSafi,
      eltexBgpPathAttrExtCommAdjOutPrfx          OCTET STRING,
      eltexBgpPathAttrExtCommAdjOutPrfxLen       Unsigned32,
      eltexBgpPathAttrExtCommAdjOutPathId        Unsigned32,
      eltexBgpPathAttrExtCommAdjOutIndex         Unsigned32,
      eltexBgpPathAttrExtCommAdjOutValue         EltexBgpExtendedCommunity,
      eltexBgpPathAttrExtCommAdjOutUserData      OCTET STRING
      }

  eltexBgpPathAttrExtCommAdjOutPeerRibIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of the BGP peer this route was learned from.
                 This field is equivalent to a eltexBgpPeerStatusPeerIndex."
    ::= { eltexBgpPathAttrExtCommAdjOutEntry 1 }

  eltexBgpPathAttrExtCommAdjOutAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The address family of the prefix for this Adj-RIB Out route."
    ::= { eltexBgpPathAttrExtCommAdjOutEntry 2 }

  eltexBgpPathAttrExtCommAdjOutSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The subsequent address family of the prefix for this Adj-RIB Out
                 route."
    ::= { eltexBgpPathAttrExtCommAdjOutEntry 3 }

  eltexBgpPathAttrExtCommAdjOutPrfx OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An address prefix in the Network Layer Reachability
                 Information field.

                 The prefix length is specified by eltexBgpPathAttrExtCommAdjOutPrfxLen.  Any bits
                 beyond the length specified by eltexBgpPathAttrExtCommAdjOutPrfxLen are zeroed.

                 This field contains the full line format BGP NLRI omitting
                 any NLRI length field.

                 For SAFI 128 the NLRI includes the MPLS label and Route
                 Distinguisher as well as the IPv4 or IPv6 address prefix."
  ::= { eltexBgpPathAttrExtCommAdjOutEntry 4 }

  eltexBgpPathAttrExtCommAdjOutPrfxLen OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Length in bits of the prefix in the Network Layer Reachability
                 Information field."
    ::= { eltexBgpPathAttrExtCommAdjOutEntry 5 }

  eltexBgpPathAttrExtCommAdjOutPathId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The path ID for this NLRI.

                 If BGP additional path receive capability was negotiated
                 with the peer for this AFI/SAFI then this is the received
                 path ID for this NLRI, otherwise it is zero."
    ::= { eltexBgpPathAttrExtCommAdjOutEntry 6 }

  eltexBgpPathAttrExtCommAdjOutIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "An integer index for a row in this table."
    ::= { eltexBgpPathAttrExtCommAdjOutEntry 7 }

  eltexBgpPathAttrExtCommAdjOutValue  OBJECT-TYPE
    SYNTAX      EltexBgpExtendedCommunity
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "A value representing a community. There are certain
                 8-octet long values which could be returned in this
                 columnar row data that carry additional semantics."
    ::= { eltexBgpPathAttrExtCommAdjOutEntry 8 }

  eltexBgpPathAttrExtCommAdjOutUserData OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE (4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "User data for this path attribute."
    ::= { eltexBgpPathAttrExtCommAdjOutEntry 9 }

-------------------------------------------------------------------------------

  eltexBgpPolicy          OBJECT IDENTIFIER ::= { eltexBgpObjects 5 }

  --
  -- BGP AS Path Access List.
  --
  -- This table contains the BGP AS Path Access List for matching AS Path in a route.
  --

  eltexBgpAsPathAccessListTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF EltexBgpAsPathAccessListEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION   "The table of BGP AS Path Access Lists.

                   An AS Path Access List is used to test whether the
                   AS Path in a route matches the list.  The AS Path is matched
                   against each eltexBgpAsPathAccessListEntry with the same
                   eltexBgpAsPathAccessListName in the order specified by
                   eltexBgpAsPathAccessListAsPathIndex.  If the AS Path does not match any
                   entry in the list, then there is no match.

                   This table contains AS Path regular expressions which can be
                   used to filter imported and exported routes.  Each row in
                   this table contains a single regular expression against
                   which to match."
     ::= { eltexBgpPolicy 1 }

  eltexBgpAsPathAccessListEntry OBJECT-TYPE
    SYNTAX                 EltexBgpAsPathAccessListEntry
    MAX-ACCESS             not-accessible
    STATUS                 current
    DESCRIPTION            "Each entry represents one or more AS Paths"
    INDEX { eltexBgpAsPathAccessListName,
            eltexBgpAsPathAccessListAsPathIndex }
    ::= { eltexBgpAsPathAccessListTable 1 }

  EltexBgpAsPathAccessListEntry ::= SEQUENCE {
      eltexBgpAsPathAccessListName         DisplayString,
      eltexBgpAsPathAccessListAsPathIndex  Unsigned32,
      eltexBgpAsPathAccessListRowStatus    RowStatus,
      eltexBgpAsPathAccessListAsPath       DisplayString,
      eltexBgpAsPathAccessListMatchType    EltexBgpPermitOrDeny
      }

  eltexBgpAsPathAccessListName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Name (identifier) of the AS Path List."
    ::= { eltexBgpAsPathAccessListEntry 1 }

  eltexBgpAsPathAccessListAsPathIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of this AS Path Entry in this AS Path List."
    ::= { eltexBgpAsPathAccessListEntry 2 }

  eltexBgpAsPathAccessListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Used to create and delete an AS Path List entry."
    ::= { eltexBgpAsPathAccessListEntry 3 }

  eltexBgpAsPathAccessListAsPath OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..160))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Contains the regular expression to use when matching the
                 AS Path.  This is stored here in ASCII format.  AS numbers
                 are matched as decimal numbers.  For example, the AS
                 number '0x0123' should be represented in the regular
                 expression string as '291'.  The string is not
                 NULL-terminated.  A NULL string or a zero length indicates that
                 the field is not in use and no AS Path will match this entry."
    ::= { eltexBgpAsPathAccessListEntry 4 }

  eltexBgpAsPathAccessListMatchType OBJECT-TYPE
    SYNTAX      EltexBgpPermitOrDeny
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "The type of match represented by this AS Path List entry.

                 A list entry with a match type of permit returns true if
                 the AS Path matches the regular expression and false if it
                 does not.

                 A list entry with a match type of deny returns false if
                 the AS Path matches the regular expression and true if it
                 does not.

                 Note that this field is ignored if the AS Path List entry
                 is referenced via a Route Map table entry in which case
                 the eltMesRouteMapType is used."
    DEFVAL { permit }
    ::= { eltexBgpAsPathAccessListEntry 5 }

-------------------------------------------------------------------------------

--
-- BGP Aggregate Address Table
--
-- This table is used to control how BGP aggregates addresses.
--

  eltexBgpAggregateTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF EltexBgpAggregateEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "This table is used to control how BGP aggregates
                 addresses.  Each entry in the table results in one aggregate
                 address being created.  This will result in an aggregate
                 entry in the routing table when at least one more specific
                 route matching the address specified is learnt.

                 The options allow configuration as to whether the AS_PATH
                 attribute keeps full information or not, and whether the more
                 specfic route is also entered in the routing table (the
                 summary only option).  These options can also be chosen on
                 a per route basis by matching on the advertise and suppress
                 route maps.

                 The attribute route map is used to set attributes of the
                 aggregated route if required.

                 It is possible to create overlapping entries in the table.
                 This can result in routes that match more than one
                 table entry.

                 -  If a route matches multiple aggregate addresses,
                 then it is suppressed any of the matching aggregates would
                 cause the route to be suppressed.

                 -  If a route matches the advertise map of an aggregate
                 address, then it is not aggregated by that aggregate address.
                 However, it may still be aggregated by other overlapping
                 aggregate addresses."
    ::= { eltexBgpPolicy 2 }

  eltexBgpAggregateEntry OBJECT-TYPE
    SYNTAX      EltexBgpAggregateEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "Each entry represents a member of an aggregate address option
                 set."
    INDEX { eltexBgpProcessId,
            eltexBgpAggrAfi,
            eltexBgpAggrSafi,
            eltexBgpAggrPrefixType,
            eltexBgpAggrPrefix,
            eltexBgpAggrPrefixLength }
    ::= { eltexBgpAggregateTable 1 }

  EltexBgpAggregateEntry ::= SEQUENCE {
      eltexBgpAggrAfi                       EltexBgpAfi,
      eltexBgpAggrSafi                      EltexBgpSafi,
      eltexBgpAggrPrefixType                InetAddressType,
      eltexBgpAggrPrefix                    InetAddress,
      eltexBgpAggrPrefixLength              InetAddressPrefixLength,
      eltexBgpAggrRowStatus                 RowStatus,
      eltexBgpAggrOptions                   EltexBgpAggregateOptions,
      eltexBgpAggrSuppressMap               DisplayString,
      eltexBgpAggrAdvertiseMap              DisplayString,
      eltexBgpAggrAttributeMap              DisplayString
      }

  eltexBgpAggrAfi OBJECT-TYPE
    SYNTAX      EltexBgpAfi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The AFI of the aggregating address."
    ::= { eltexBgpAggregateEntry 1 }

  eltexBgpAggrSafi OBJECT-TYPE
    SYNTAX      EltexBgpSafi
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The SAFI of the aggregating address."
    ::= { eltexBgpAggregateEntry 2 }

  eltexBgpAggrPrefixType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The type of the aggregate address."
    ::= { eltexBgpAggregateEntry 3 }

  eltexBgpAggrPrefix OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of this eltexBgpAggregateEntry.  This is the prefix of
                 the configured aggregating address."
    ::= { eltexBgpAggregateEntry 4 }

  eltexBgpAggrPrefixLength OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION "The index of this eltexBgpAggregateEntry.  This is the length of
                 the prefix (in bits) of the configured aggregating address."
    ::= { eltexBgpAggregateEntry 5 }

  eltexBgpAggrRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION "Used to create and delete an aggregate address option set."
    ::= { eltexBgpAggregateEntry 6 }

  eltexBgpAggrOptions OBJECT-TYPE
    SYNTAX      EltexBgpAggregateOptions
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Options applied to this set of aggregate addresses.  Note with
                 no options, more specific routes are installed in the routing
                 table, but the AS_PATH will lose information as it will not
                 contain AS-SETs.  This is normally OK as it reduces route
                 flap.

                 Note that a route may be aggregated by multiple overlapping
                 aggregate addresses.  In this case, the route is suppressed
                 if any of the matching aggregates would cause the route to
                 be suppressed."
    DEFVAL { none }
    ::= { eltexBgpAggregateEntry 7 }

  eltexBgpAggrSuppressMap OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The name of the Route Map used to suppress routes. The match
                 clauses of this route map are used to selectively suppress
                 more specific routes from being advertised.  No route map
                 should be defined here if a suppress option ('summary',
                 'summaryAsSet' or 'summaryAsAppend') is configured in the
                 eltexBgpAggrOptions field."
    ::= { eltexBgpAggregateEntry 8 }

  eltexBgpAggrAdvertiseMap OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The name of the Route Map used to advertise routes. The match
                 clauses of this route map are used to select routes which
                 although they match the aggregate address, should not be
                 aggregated."
    ::= { eltexBgpAggregateEntry 9 }

  eltexBgpAggrAttributeMap OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The name of the Route Map used to set aggregated routes
                 attributes.  The set clauses of this route map are used to set
                 path attributes of the aggregated route."
    ::= { eltexBgpAggregateEntry 10 }

END
