RADLAN-MGMD-ROUTER-MIB DEFINITIONS ::= BEGIN
-- Title:                RADLAN IGMP
--                       IGMP Router Private MIB
--                       based on MGMD Router standard MIB MGMD-MIB (rfc5519)
-- Version:              0.00
-- Date:                 01 July 2011

IMPORTS
    rnd                              FROM RADLAN-MIB
    MODULE-IDENTITY, OBJECT-TYPE, mib-2, Counter32, Gauge32,
    Unsigned32, TimeTicks            FROM SNMPv2-SMI
    InetAddress, InetAddressType     FROM INET-ADDRESS-MIB
    RowStatus,TruthValue,
    DisplayString                    FROM SNMPv2-TC
    NpgOperStatus                    FROM RADLAN-PIM-MIB
    mgmdRouterInterfaceEntry         FROM MGMD-STD-MIB
    MODULE-COMPLIANCE, OBJECT-GROUP  FROM SNMPv2-CONF
    InterfaceIndexOrZero,
    InterfaceIndex                   FROM IF-MIB;

rlIgmp MODULE-IDENTITY
        LAST-UPDATED "201107210000Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
                "The private MIB module definition for IGMP Router
                 in Radlan devices."
        REVISION "201107210000Z"
        DESCRIPTION
                "Added this MODULE-IDENTITY clause."
        ::= { rnd 225 }

----------------------------------------------------------
-- RLinterfaceTable
----------------------------------------------------------
--Common Textual Conventions

AdminStatus ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "The desired administrative state of a MIB row."
    SYNTAX      INTEGER {
                  adminStatusUp(1),
                  adminStatusDown(2)
                }

rlMgmdInterfaceExtTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF RlMgmdInterfaceExtEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "The (conceptual) Extension Interface table listing the entries
             with counters of the standard interface table."

    ::= { rlIgmp 1 }

rlMgmdInterfaceExtEntry OBJECT-TYPE
    SYNTAX     RlMgmdInterfaceExtEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "An entry (conceptual row) in the rlMgmdInterfaceExtTable."
    AUGMENTS   { mgmdRouterInterfaceEntry }

    ::= { rlMgmdInterfaceExtTable 1 }


RlMgmdInterfaceExtEntry ::= SEQUENCE{
    rlMgmdRouterInterfaceExtStatsUpTime             TimeTicks,
    rlMgmdRouterInterfaceExtEnableStats             TruthValue,
    rlMgmdRouterInterfaceExtNumFailedJoins          Unsigned32,
    rlMgmdRouterInterfaceExtNumIgmpV1Msgs           Unsigned32,
    rlMgmdRouterInterfaceExtNumIgmpV2MldV1Msgs      Unsigned32,
    rlMgmdRouterInterfaceExtNumIgmpV3MldV2Msgs      Unsigned32,
    rlMgmdRouterInterfaceExtNumInvalidMsgsRcvd      Unsigned32,
    rlMgmdRouterInterfaceExtNumGenQueriesSent       Unsigned32,
    rlMgmdRouterInterfaceExtNumSpecQueriesSent      Unsigned32,
    rlmgmdRouterInterfaceQrRobustness               Unsigned32,
    rlmgmdRouterInterfaceQrQueryInterval            Unsigned32,
    rlmgmdRouterInterfaceQrQueryMaxResponseTime     Unsigned32,
    rlmgmdRouterInterfaceQrLastMembQueryIntvl       Unsigned32,
    rlmgmdRouterInterfaceExtSrcAndGrpFilter         DisplayString,
    rlMgmdRouterInterfaceExtAdminStatus             AdminStatus,
    rlMgmdRouterInterfaceExtOperStatus              NpgOperStatus,
    rlMgmdRouterInterfaceExtIsQuerier               TruthValue,
    rlMgmdRouterInterfaceExtProxyDownProtected      INTEGER

}



rlMgmdRouterInterfaceExtStatsUpTime OBJECT-TYPE
    SYNTAX     TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The time since the statistics counters for this interface
             were last reset.

             This field is reset to zero when
             rlMgmdRouterInterfaceExtEnableStats is modified to 'true'.

             This value may wrap."

    ::= { rlMgmdInterfaceExtEntry 1 }

rlMgmdRouterInterfaceExtEnableStats OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "This object defines whether DC-IGMP returns
          interface-specific statistics on MIB GET operations
          for this interface's MIB row.
           If this object is modified from 'true' to 'false' and back to 'true',
           the statistics fields are reset. This field is readable and writeable."

       ::= { rlMgmdInterfaceExtEntry 2 }


rlMgmdRouterInterfaceExtNumFailedJoins OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of failed joins received for this interface - that is,
            the number of times a group membership could not be added on this
            interface."

    ::= { rlMgmdInterfaceExtEntry 3 }

rlMgmdRouterInterfaceExtNumIgmpV1Msgs OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of IGMPv1 messages received for this interface.
            This includes both valid and invalid messages."

    ::= { rlMgmdInterfaceExtEntry 4 }

rlMgmdRouterInterfaceExtNumIgmpV2MldV1Msgs OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of IGMPv2 or Mldv1 messages received for this interface.
            This includes both valid and invalid messages."

    ::= { rlMgmdInterfaceExtEntry 5}

rlMgmdRouterInterfaceExtNumIgmpV3MldV2Msgs OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of IGMPv3 or Mldv2 messages received for this interface.
            This includes both valid and invalid messages."

    ::= { rlMgmdInterfaceExtEntry 6}

rlMgmdRouterInterfaceExtNumInvalidMsgsRcvd OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of Invalid IGMP or MLD messages received for this interface."

    ::= { rlMgmdInterfaceExtEntry 7}

rlMgmdRouterInterfaceExtNumGenQueriesSent OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of General Queries sent for this interface."

    ::= { rlMgmdInterfaceExtEntry 8}

rlMgmdRouterInterfaceExtNumSpecQueriesSent OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of Specific Queries sent for this interface."

    ::= { rlMgmdInterfaceExtEntry 9}


rlmgmdRouterInterfaceQrRobustness OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The value of Robustness in use on this interface.

            The Robustness Variable allows tuning for the expected
            packet loss on a subnet.  If a subnet is expected to be
            lossy, the Robustness Variable may be increased.  IGMP and
            MLD is robust to (Robustness Variable-1) packet losses.

            For IGMPv3/MLDv2, this may differ from the value
            configured using mgmdRouterInterfaceRobustness if the
            local router is not the querier on this interface."

    ::= { rlMgmdInterfaceExtEntry 10 }

rlmgmdRouterInterfaceQrQueryInterval OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The value of Query Interval in use on this interface.

            The frequency at which IGMP or MLD General Query packets
            are transmitted on this interface.

            For IGMPv3/MLDv2, this may differ from the value
            configured using mgmdRouterInterfaceQueryInterval if the
            local router is not the querier on this interface."

    ::= { rlMgmdInterfaceExtEntry 11 }

rlmgmdRouterInterfaceQrQueryMaxResponseTime OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The value of Maximum Query Response Time in use on this
            interface.

            For IGMPv3/MLDv2, this may differ from the value
            configured using mgmdRouterInterfaceQueryMaxResponseTime
            if the local router is not the querier on this interface."

    ::= { rlMgmdInterfaceExtEntry 12 }

rlmgmdRouterInterfaceQrLastMembQueryIntvl OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The value of Last Member Query Interval in use on this
            interface.

            The Last Member Query Interval is the Max Response Time
            inserted into Group-Specific and Group-and-Source-specific
            Queries sent in response to Leave messages, and is also
            the amount of time between successive Specific Query
            messages.  This value may be tuned to modify the leave
            latency of the network.  A reduced value results in
            reduced time to detect the loss of the last member of a
            group.

            The value of this object is irrelevant if
            mgmdRouterInterfaceVersion is 1.

            The value of this object is also irrelevant if this
            interface is configured to use immediate-leave behavior
            without a last member query - that is, if
            mgmdRouterInterfaceImmedtLeave is 'true' and
            mgmdRouterInterfaceQryBefImmdLv is 'false'.

            For IGMPv3/MLDv2, this may differ from the value
            configured using mgmdRouterInterfaceLastMembQueryIntvl if
            the local router is not the querier on this interface."

    ::= { rlMgmdInterfaceExtEntry 13 }

rlmgmdRouterInterfaceExtSrcAndGrpFilter OBJECT-TYPE
    SYNTAX     DisplayString
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "The interface will ignore requests to join any
            group/source pair that is not included in the extended
            access list with a list index corresponding to the value
            configured for this object.

            If the value of this object is 0, no requests are ignored
            as a result of this object.

            This object deprecates the dcmgmdRouterInterfaceAllowSSMList
            object.  If both of these (S,G) filters are set to
            non-zero values, then both take effect for SSM groups -
            that is, a request to join an SSM group/source pair is
            only accepted if it passes through both filters.

            If both this object and the
            dcmgmdRouterInterfaceAllowASMList object are set to non-zero
            values, then a request to join an ASM group/source pair is
            only accepted if it passes through both filters."
    DEFVAL { "" }
    ::= { rlMgmdInterfaceExtEntry 14 }

rlMgmdRouterInterfaceExtAdminStatus OBJECT-TYPE
    SYNTAX       AdminStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
            "The desired administrative state of the interface."
    DEFVAL { adminStatusDown }
    ::= { rlMgmdInterfaceExtEntry 15 }

rlMgmdRouterInterfaceExtOperStatus OBJECT-TYPE
    SYNTAX     NpgOperStatus
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The current operational state of the interface."
    ::= { rlMgmdInterfaceExtEntry 16 }

rlMgmdRouterInterfaceExtIsQuerier OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "???"
    ::= { rlMgmdInterfaceExtEntry 17 }

rlMgmdRouterInterfaceExtProxyDownProtected OBJECT-TYPE
   SYNTAX      INTEGER {
    	unspecified(-1),
    	enabled(1),
    	disabled(2)
   }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
            "Enable/Disable IGMP Proxy Downstream protected on the interface."
    ::= { rlMgmdInterfaceExtEntry 18 }

END

