RADLAN-QOS-CLI-MIB DEFINITIONS ::= BEGIN

-- Version:    7.46
-- Date:       04 Jan 2007
-- 28 May 2003 Changed UNITS clause of rlQosPolicerCir to kbps
-- 28 May 2003 Added QoS Access Control Element table two indexes (rlQosAceTidxTable)
-- 29 Sep 2003 Add textual convention to QosObjectMode (service).
-- 15 Nov 2004 Add DSCP to Queue Default map table
-- 27 Jan 2005 Add new advanced action : trustCosDscp
-- 07 Feb 2005 Add vpt,ether-type,tcp-flags,icmp-type,icmp-code,igmp-type to ClassTupleType
--             Add ip-ICMP,ip-IGMP To AceObjectType
--             Add vpt,ethertype To ClassOffsetType
-- 14 March 2005 Add   rlQosPortRateLimitStatus,rlQosCirPortRateLimit, rlQosCbsPortRateLimit
--                to   rlQosIfPolicyTable
-- 17-Apr-2005 Added rlQosDscpToDpTable
-- 06-Apr-2006 Added branch rlQosStatistics and tables:
-- 08-May-2006 Added innerVlan to ClassOffsetType And inner-vlan to ClassTupleType
-- 11-Dec-2006 Added rlQosClassifierUtilization
-- 24-Dec-2006 Changed rlQosTypeQueue1 ... rlQosTypeQueue8 fields in
--                       rlQosQueueProfileTable from read-create to read-write
-- 24-Dec-2006 Added new MIB: rlQosPortToProfileMappingTable
-- 31-Dec-2006 Added support for Time Based ACL
-- 04-Jan-2007 Added rlQosTimeBasedAclTable
-- 17-Apr-2007 Added IPv6 ACL support
--             Change rlQosOffsetTable to deprecated
-- 6-Jun-2007  Added rlQosClassifierUtilizationSystem
-- 18-Jan-2008 Add rlQosClassifierUtilizationRulesNumber  to rlQosClassifierUtilizationEntry
-- 01-Jun-2009 Add udp-port-range-start-src, udp-port-range-end-src,
--                 udp-port-range-start-dest, udp-port-range-end-dest,
--                 tcp-port-range-start-src, tcp-port-range-end-src,
--                 tcp-port-range-start-dest, tcp-port-range-end-dest, to ClassTupleType
--             Add rlQosAceTidxTuple9, rlQosAceTidxTuple10 to rlQosAceTidxTable
-- 18-Aug-2009 Removed Time Based Tables : code moved to general TimeBasedInfrastrucure
-- 22-Oct-2009 Added rlQosAceTidxTuple11 to rlQosAceTidxTable in order to keep Src MAC addr of Dynamic ACLs
-- 2-Mar-2017 Added ipv6-flow-label to ClassTupleType, to be set to rlQosAceTidxTuple11
-- 02-Jul-2017 Added rlQosPolicyMapIsBoundToInterface to rlQosPolicyMapTable
--             Added rlQosAclIsBoundToInterface to lQosAclTable
-- 7-Jun-2021  rlQosOffsetTable is allowed again
IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,Counter32,
    Gauge32, Unsigned32, IpAddress, TimeTicks   FROM SNMPv2-SMI
    InterfaceIndex,InterfaceIndexOrZero         FROM IF-MIB
    TruthValue, RowStatus, RowPointer,
    TEXTUAL-CONVENTION,DisplayString            FROM SNMPv2-TC
    Counter64, OBJECT-TYPE                      FROM SNMPv2-SMI
    PortList,VlanId                             FROM Q-BRIDGE-MIB
    VlanList1, VlanList2, VlanList3, VlanList4  FROM RADLAN-BRIDGEMIBOBJECTS-MIB
    Percents,rnd                                FROM RADLAN-MIB
    StatisticsDPType,StatisticsClearActionType  FROM RADLAN-POLICY-MIB;


rlQosCliMib MODULE-IDENTITY
        LAST-UPDATED "201707020000Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
                "The private MIB module definition for Quality Of Service CLI
                 in Radlan devices."
        REVISION "201707020000Z"
        DESCRIPTION
                 "Added rlQosPolicyMapIsBoundToInterface, rlQosAclIsBoundToInterface"
        REVISION "200602120000Z"
        DESCRIPTION
                "Added:
                     StatisticsCntrNumOfBitsType
                     StatisticsCntrType
                     rlQosStatistics
                     rlQosPortPolicyStatisticsTable
                     rlQosSinglePolicerStatisticsTable
                     rlQosAggregatePolicerStatisticsTable
                     rlQosOutQueueStatisticsTable
                     rlQosGlobalStatisticsCntrsTable."
        REVISION "200602120000Z"
        DESCRIPTION
                 "Editorial changes to support new MIB compilers."
        REVISION "200503140000Z"
        DESCRIPTION
                 "Add rlQosPortRateLimitStatus,rlQosCirPortRateLimit, rlQosCbsPortRateLimit
                  to   rlQosIfPolicyTable"
        REVISION "200502070000Z"
        DESCRIPTION
                "Add vpt,ether-type,tcp-flags,icmp-type,icmp-code,igmp-type to ClassTupleType
                 Add mac-Offset,ip-ICMP,ip-IGMP To AceObjectType
                 Add vpt,ethertype To ClassOffsetType"
        REVISION "200501270000Z"
        DESCRIPTION
                "Add new advanced action : trustCosDscp"
        REVISION "200411150000Z"
        DESCRIPTION
                "Add DSCP to Queue Default map table."
        REVISION "200309290000Z"
        DESCRIPTION
                "Add textual convention to QosObjectMode (service)."
        REVISION "200309210000Z"
        DESCRIPTION
                "Added this MODULE-IDENTITY clause, changed IMPORT, removed ranges in
                 SEQUENCE elements, changed access of rlQosCliQosMode, rlQosCliBasicModeCfg and
                 rlQosMaxNumOfAce."
        REVISION "200504170000Z"
        DESCRIPTION
                "Added rlQosDscpToDpTable"

        ::= { rnd 88 }


ClassOffsetType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 6 offset types:
         1- Absolute-start of the packet.
         2- Layer 2-start of MAC header.
         3- MPLS-start of MPLS header.
         4- Layer 3-start of layer 3 header.
         5- Layer 4-start of layer 4 header.
         6- Layer 5-after TCP/UDP header.
         7- VLAN.
         8- input device port.
         9- input device port.
         10-VPT.
         11-EtherType.
         12-innerVlan.
         13-Layer 3 IPv6 - start of layer 3 IPv6 header.
         14-Layer 4 IPv6 - start of layer 4 IPv6 header.
         15-Source MAC.
         16-Destination MAC."
    SYNTAX  INTEGER {
         packetStart(1),
         layer2-start(2),
         mpls-start(3),
         layer3-start(4),
         layer4-start(5),
         layer5-start(6),
         vlan(7),
         in-port(8),
         out-port(9),
         vpt(10),
         ethertype(11),
         inner-vlan(12),
         layer3-ipv6-start(13),
         layer4-ipv6-start(14),
         src-mac(15),
         dst-mac(16)
        }

ClassTupleType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of Tuple types "
    SYNTAX  INTEGER {
         protocol(1),
         ip-src(2),
         ip-dest(3),
         dscp(4),
         ip-precedence(5),
         udp-port-src(6),
         udp-port-dest(7),
         tcp-port-src(8),
         tcp-port-dest(9),
         mac-src(10),
         mac-dest(11),
         vlan(12),
         in-port(13),
         out-port(14),
         general(15),
         vpt(16),
         ether-type(17),
         tcp-flags(18),
         icmp-type(19),
         icmp-code(20),
         igmp-type(21),
         inner-vlan(22),
         ipv6-src(23),
         ipv6-dest(24),
         udp-port-range-start-src(25),
         udp-port-range-end-src(26),
         udp-port-range-start-dest(27),
         udp-port-range-end-dest(28),
         tcp-port-range-start-src(29),
         tcp-port-range-end-src(30),
         tcp-port-range-start-dest(31),
         tcp-port-range-end-dest(32),
         ipv6-flow-label(33),
         ipv6-traffic-class(100)
        }

AceActionType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 4 ACE Actions:
         1- Permit- permit to the traffic that define
                by the parameters.
         2- Deny- deny the traffic that define
                by the parameter.
         3- Deny-DisablePort deny the traffic that defined
                by the parameters and disable the port.
         4- Deny-LogInput deny the traffic that defined
                by the parameters and log incoming traffic.
                 5- Permit-LogInput permit the traffic that defined
                by the parameters and log incoming traffic."
    SYNTAX  INTEGER {
         permit(1),
         deny(2),
         deny-DisablePort(3),
         deny-LogInput(4),
         permit-LogInput(5)
         }

AceObjectType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 13 ACE types:
        1- IP ACE.
        2- IP-TCP ACE.
        3- IP-UDP ACE.
        4- IP-offset ACE.
        5- MAC ACE.
        6- MAC-offset ACE.
        7- IP-ICMP ACE.
        8- IP-IGMP ACE.
        9- IPv6 ACE.
        10- IPv6-TCP ACE.
        11- IPv6-UDP ACE.
        12- IPv6-offset ACE.
        13- IPv6-ICMP ACE."
    SYNTAX  INTEGER {
        ip(1),
        ip-TCP(2),
        ip-UDP(3),
        ip-Offset(4),
        mac(5),
        mac-Offset(6),
        ip-ICMP(7),
        ip-IGMP(8),
        ipv6(9),
        ipv6-TCP(10),
        ipv6-UDP(11),
        ipv6-Offset(12),
        ipv6-ICMP(13)
        }

AclObjectType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 3 ACL types:
         1- MAC ACL.
         2- IPv4 ACL.
         3- IPv6 ACL."
    SYNTAX  INTEGER {
         mac(1),
         ip(2),
         ipv6(3)
         }

ClassMapType ::= TEXTUAL-CONVENTION
   STATUS  current
   DESCRIPTION
       "Specifies one of 2 Class-map types:
        1- Match all. logical and between all statements.
        2- Match any. logical or between all statements."
  SYNTAX  INTEGER {
       matchAll(1),
       matchAny(2)
       }

ClassMapAction ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 8 Class-map actios:
         1- none - action not specified - use default action.
         2 -Mark IP-Precedence.
         3- Mark DSCP.
         4- Set Egress queue
         5- Mark VPT
         6- Choose queue by global trust mode."
    SYNTAX  INTEGER {
        none(1),
        setIP-Precedence(2),
        setDSCP(3),
        setQueue(4),
        setCos(5),
        trust(6)
--v750 - trust mode it done by globalTrustMode field in RlQosModeGlobalCfgEntry.
--       the class map action is changed to "trust"
--v750 depcrated    trustCos(6),
--v750 depcrated    trustDSCP(7),
--v750 depcrated    trustTCP-UDPport(8),
--v750 depcrated    trustCosDscp(9)
        }

MarkVlanAction  ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
    "Specifies the mark vlan action type in the class map table.
      1 - noMark - No vlan marking
      2 - mark  - mark vlan tagged.
      3 - markNestedVlan - add vlan tag to the packet. "
    SYNTAX  INTEGER {
        noMark(1),
        mark(2),
        markNestedVlan(3)
    }

RedirectAction  ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
    "Specifies the packet redirection options.
     Redirection is applied only on permitted packets.
      1 - disabled  - no redirect
      2 - trap - trap to local_host (CPU)
      3 - redirectToInterface - redirect to a output interface (port, trunk or vlan)
      4 - redirectToAllPorts - redirect to all ports, except the ingress port.
      5 - mirror - forward the packet and sent a copy to local_host (CPU)
      6 - analyzerPort - forward the packet and sent a copy to egress port.
      7 - loopback - redirect the packet the the port it was received.
      8 - redirectToPortGroup - send to group of ports, defined in rlUserAssignedVidxTable table
      9 - mirror_and_redirectToInterface - send the packet to interface and send a copy to local_host(CPU)
      10 -mirror_and_redirectToInterfacesGroup - send the packet to group of ports and send a copy to local_host(CPU)  "
    SYNTAX  INTEGER {
        disabled(1),
        trap(2),
        redirectToInterface(3),
        redirectToAllPorts(4),
        mirror(5),
        analyzerPort(6),
        loopback(7),
        redirectToPortGroup(8),
        mirrorAndRedirectToInterface(9),
        mirrorAndRedirectToInterfacesGroup(10)
    }

PolicerType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 3 Policer types:
         1- Single policer only per one class map.
         2- Aggregate policer can be applied to several
            class maps.
         3- Cascade policer."
    SYNTAX  INTEGER {
        single(1),
        aggregate(2),
        cascade(3) -- Obsolete
        }


PolicerAction ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 4 Policer Action:
         1- No Action
         2- Drop out of profile packets.
         3- Remark out of profile packets.
         4- Remark to explicit value out of profile packets
         5- this policer is part of cascade chain"
    SYNTAX  INTEGER {
        none(1),
        drop(2),
        remark(3),
        explicit-remark(4),
        cascadePointer(5) -- Obsolete
        }

QosGlobalMode ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 3 QoS mode:
         1- disable no QoS on the system
         2- Basic Qos mode only trust mode with ACL are enabled.
         3- Advance mode all Qos option are enabled.
         4- Service Mode -v750 DEPEREACTED!!!  all Qos option are enabled only in
            service mode configuration"
    SYNTAX  INTEGER {
        disable(1),
        basic(2),
        advance(3)
--v750 deprecated        service(4)
}

QosTrustMode ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 6 QoS trust mode:
          - none.- v750 DEPRECATED - same as globalMode = disable. means that only ACL can be applied.
         - 802.1p. queue is set by the VPT field.
         - DSCP. queue is set by the DSCP field
         - v750 deprecated. replaced with new scalar rlQosDscpMutationEnable .
           DSCP-Mutation. the DSCP mutate in the ingress and
            then the queue is set by the DSCP
          - tcp/udp.-  v750 - DEPRECATED - not supported. the queue is set by the l4 port number.
          - cos-dscp. Queue is set for l2 traffic
             by VPT field and for l3 traffic by DSCP field. "
    SYNTAX  INTEGER {
--deprecated        none(1),
        cos(1),
        dscp(2),
--v750 deprecated :  dscp-mutation(3),
--deprecated tcp-upd(5),
        cos-dscp(3)
}

BinaryStatus ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "Specifies Disable or enable."
    SYNTAX  INTEGER {
        disable(1),
        enable(2)
}

QueueType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "Queue type Ef or WRR."
    SYNTAX  INTEGER {
        ef(1),
        wrr(2)
}

AclDefaultAction ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "Default action when the ACL reach end point."
    SYNTAX  INTEGER {
        deny-all(1),
        forward-all(2),
        application-specific(3)
}

InterfaceType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "Interface type."
    SYNTAX  INTEGER {
        vlan(1),
        port(2)
}

StatisticsCntrNumOfBitsType  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "The counter can be of different sizes - 32 bit, 48 bit, 64 bit. Maximum is 64."
   SYNTAX INTEGER {
      uint32(32),
      uint48(48),
      uint64(64)
}


StatisticsCntrType  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "The counter can be of different types, depends on actions adhered to
                    rules that the counter is working on."
   SYNTAX INTEGER {
      statisticsCntrTypeSetDSCP(1),
      statisticsCntrTypeDeny(2)
}


RlQosTimeBasedAclWeekPeriodicList  ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION  "Bitmap that includes days of week.
                 Each bit in the bitmap associated with corresponding day of the week."
    SYNTAX      BITS {
            monday(0),
            tuesday(1),
            wednesday(2),
            thursday(3),
            friday(4),
            saturday(5),
            sunday(6)
}

RlQosAceTidxActionDropType  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "The Action Drop Type."
   SYNTAX INTEGER {
      hardDrop(1),
      softDrop(2)
}

RlQosApplicationDefaultActionType  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "Application default actions."
   SYNTAX INTEGER {
      forward(1),
      hard-Drop(2),
      soft-Drop(3),
      trap(4)
}
--  CLI QOS MODE Scalar

rlQosCliQosMode OBJECT-TYPE
    SYNTAX     QosGlobalMode
    MAX-ACCESS read-write
    STATUS     deprecated
    DESCRIPTION
        " *********This Scalar is deprecated - rlQosGlobalCfgEntry - replaces its
        functionality***************
        This scalar define in which mode the
         system will work: basic , advance or none."
    ::= { rlQosCliMib 1 }

-- CLI QoS Basic Mode Config Scalar
rlQosCliBasicModeCfg OBJECT-TYPE
    SYNTAX     QosTrustMode
    MAX-ACCESS read-write
    STATUS     deprecated
    DESCRIPTION
        "*********This Scalar is deprecated - rlQosGlobalCfgEntry - replaces its
        functionality***************
         This scalar define in which trust mode the
                 system will work:802.1p or DSCP or
                 DSCP-Mutation or TCP/UDP or none or vpt-dscp."
    ::= { rlQosCliMib 2 }

-- Maximum Number of ACE per system Scalar

rlQosMaxNumOfAce OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This scalar define the max number of aces."
    ::= { rlQosCliMib 3 }

 -- QoS Offset Table

rlQosOffsetTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosOffsetEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies Offset Table information"
    ::= { rlQosCliMib 4 }

rlQosOffsetEntry OBJECT-TYPE
    SYNTAX     RlQosOffsetEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Each entry in this table describes one classifier field.
        The information includes: Offset Type the offset the mask and the
        Pattern.
        if the type is vlan then the value will be the vlan tag.
        if the Type is in/out port it will be the device in/out port.
        The index is sequential integer represent by rlQosOffsetIndex"
    INDEX { rlQosOffsetIndex }
    ::= { rlQosOffsetTable 1 }

RlQosOffsetEntry ::= SEQUENCE {
    rlQosOffsetIndex        INTEGER,
    rlQosOffsetType         ClassOffsetType,
    rlQosOffsetValue        INTEGER,
    rlQosOffsetMask         INTEGER,
    rlQosOffsetPattern      INTEGER,
    rlQosOffsetTuplePointer INTEGER,
    rlQosOffsetStatus       RowStatus
    }

rlQosOffsetIndex OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "An arbitrary incremental Index
         for the offset table."
    ::= { rlQosOffsetEntry 1 }

rlQosOffsetType OBJECT-TYPE
    SYNTAX     ClassOffsetType
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "Start of the offset."
    ::= { rlQosOffsetEntry 2 }

rlQosOffsetValue OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "The Offset value."
    ::= { rlQosOffsetEntry 3 }

rlQosOffsetMask OBJECT-TYPE
    SYNTAX     INTEGER(0..255)
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "Define which bit to be extracted from the offset."
    ::= { rlQosOffsetEntry 4 }


rlQosOffsetPattern OBJECT-TYPE
    SYNTAX     INTEGER(0..255)
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "The value to match too."
    ::= { rlQosOffsetEntry 5 }

rlQosOffsetTuplePointer OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "Pointer for the relevant Tuple."
    ::= { rlQosOffsetEntry 6 }

rlQosOffsetStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosOffsetEntry 7 }


 -- QoS Tuple Table


rlQosTupleTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosTupleEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies Tuple Table information"
    ::= { rlQosCliMib 5 }

rlQosTupleEntry OBJECT-TYPE
    SYNTAX     RlQosTupleEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Each entry in this table describes one Tuple.
        The information includes: Tuple Type and the Tuples values.
        The index is sequential integer represent by rlQosTupleIndex"
    INDEX { rlQosTupleIndex }
    ::= { rlQosTupleTable 1 }

RlQosTupleEntry ::= SEQUENCE {
    rlQosTupleIndex         INTEGER,
    rlQosTupleType          ClassTupleType,
    rlQosTupleValue1        INTEGER,
    rlQosTupleValue2        OCTET STRING,
    rlQosTupleStatus        RowStatus
    }

rlQosTupleIndex OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "An arbitrary incremental Index
         for the offset table."
    ::= { rlQosTupleEntry 1 }

rlQosTupleType OBJECT-TYPE
    SYNTAX     ClassTupleType
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "Start of the offset."
    ::= { rlQosTupleEntry 2 }

rlQosTupleValue1 OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "The Tuple no.1 value can be regular integer
         values only."
    ::= { rlQosTupleEntry 3 }

rlQosTupleValue2 OBJECT-TYPE
    SYNTAX     OCTET STRING(SIZE(0..32))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "The Tuple no.2 value can be IPv4/IPv6/MAC address
         or protocol number with mask"
    ::= { rlQosTupleEntry 4 }


rlQosTupleStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosTupleEntry 5 }

-- QoS Access Control Element table


rlQosAceTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosAceEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table specifies ACE table information"
    ::= { rlQosCliMib 6 }

rlQosAceEntry OBJECT-TYPE
    SYNTAX     RlQosAceEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Each entry in this table describes one Classifier Element.
        The information includes: Action the ACE's Type the up to 8 tuples
        pointers. The index is sequential integer represent by rlQosAceIndex"
    INDEX { rlQosAceIndex }
    ::= { rlQosAceTable 1 }

RlQosAceEntry ::= SEQUENCE {
    rlQosAceIndex          INTEGER,
    rlQosAceAction         AceActionType,
    rlQosAceType           AceObjectType,
    rlQosAceTuple1         INTEGER,
    rlQosAceTuple2         INTEGER,
    rlQosAceTuple3         INTEGER,
    rlQosAceTuple4         INTEGER,
    rlQosAceTuple5         INTEGER,
    rlQosAceTuple6         INTEGER,
    rlQosAceTuple7         INTEGER,
    rlQosAceTuple8         INTEGER,
    rlQosAceAccount        BinaryStatus,
    rlQosAceStatus         RowStatus
    }

rlQosAceIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An arbitrary incremental Index
         for the ACE table."
    ::= { rlQosAceEntry 1 }

rlQosAceAction OBJECT-TYPE
    SYNTAX AceActionType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Action to take."
    ::= { rlQosAceEntry 2 }

rlQosAceType OBJECT-TYPE
    SYNTAX AceObjectType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Type"
    ::= { rlQosAceEntry 3 }

rlQosAceTuple1 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple 1 pointer."
    ::= { rlQosAceEntry 4 }

rlQosAceTuple2 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple 1 pointer."
    ::= { rlQosAceEntry 5 }

rlQosAceTuple3 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple 1 pointer."
    ::= { rlQosAceEntry 6 }

rlQosAceTuple4 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple 1 pointer."
    ::= { rlQosAceEntry 7 }

rlQosAceTuple5 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple 1 pointer."
    ::= { rlQosAceEntry 8 }

rlQosAceTuple6 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple 1 pointer."
    ::= { rlQosAceEntry 9 }

rlQosAceTuple7 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple 1 pointer."
    ::= { rlQosAceEntry 10 }

rlQosAceTuple8 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple 1 pointer."
    ::= { rlQosAceEntry 11 }

rlQosAceAccount OBJECT-TYPE
    SYNTAX BinaryStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Accounting state.
         When set to 'enabled' than appropriate statistic's
         counter is provided for an ACE."
    ::= { rlQosAceEntry 12 }

rlQosAceStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosAceEntry 13 }


-- QoS Access Control List table

rlQosAclTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosAclEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies ACL table information"
    ::= { rlQosCliMib 7 }

rlQosAclEntry OBJECT-TYPE
    SYNTAX RlQosAclEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one Classifier Element.
         The information includes: Action and the row status. The ACE pointer
         are in the ACL-ACE reference table.
         The index is sequential integer represent by rlQosAceIndex"
    INDEX { rlQosAclIndex }
    ::= { rlQosAclTable 1 }

RlQosAclEntry ::= SEQUENCE {
    rlQosAclIndex						INTEGER,
    rlQosAclName						DisplayString,
    rlQosAclType						AclObjectType,
    rlQosAclStatus						RowStatus,
    rlQosAclNumOfAces					INTEGER,
    rlQosAclIsBoundToInterface			TruthValue	
    }

rlQosAclIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An arbitrary incremental Index
                 for the ACE table."
    ::= { rlQosAclEntry 1 }

rlQosAclName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..32))
--    Rsyntax OCTET STRING(SIZE(0..255))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Name ACL."
    ::= { rlQosAclEntry 2 }


rlQosAclType OBJECT-TYPE
    SYNTAX AclObjectType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACL Type."
    ::= { rlQosAclEntry 3 }

rlQosAclStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosAclEntry 4 }

rlQosAclNumOfAces OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "Holds number of aces in the acl."
    ::= { rlQosAclEntry 5 }

rlQosAclIsBoundToInterface OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "Indicates whether the ACL is bound to any interface or not."
    ::= { rlQosAclEntry 6 }


--QoS ACE ACL refernce table


rlQosAclAceRefTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosAclAceRefEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies the ACE to ACL
         relationship."
    ::= { rlQosCliMib 8 }

rlQosAclAceRefEntry OBJECT-TYPE
    SYNTAX RlQosAclAceRefEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the relationship
         between ACE to ACL. Show which ACE include in one ACL.
         The index is the ACE pointer represent
         by rlQosAclAceRefAcePointer"
    INDEX { rlQosAclAceRefAcePointer }
    ::= { rlQosAclAceRefTable 1 }

RlQosAclAceRefEntry ::= SEQUENCE {
    rlQosAclAceRefAcePointer    INTEGER,
    rlQosAclAceRefAclPointer    INTEGER,
    rlQosAclAceRefStatus        RowStatus
    }

rlQosAclAceRefAcePointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The Index is the ACE pointer"
    ::= { rlQosAclAceRefEntry 1 }

rlQosAclAceRefAclPointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACL index Pointer"
    ::= { rlQosAclAceRefEntry 2 }

rlQosAclAceRefStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosAclAceRefEntry 3 }


-- QoS Class-Map table


rlQosClassMapTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosClassMapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies CCL table information"
    ::= { rlQosCliMib 9 }

rlQosClassMapEntry OBJECT-TYPE
    SYNTAX RlQosClassMapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one Class Map Element.
        The information includes: Classes Name,Class Action,
        Policer pointer, and 1 match statements.
        The index is sequential integer represent by rlQosClassMapIndex"
    INDEX { rlQosClassMapIndex }
    ::= { rlQosClassMapTable 1 }

RlQosClassMapEntry ::= SEQUENCE {
    rlQosClassMapIndex          INTEGER,
    rlQosClassMapName           DisplayString,
    rlQosClassMapType           ClassMapType,
    rlQosClassMapAction         ClassMapAction,
    rlQosClassMapMarkValue      INTEGER,
    rlQosClassMapPolicer        INTEGER,
    rlQosClassMapMatch1         INTEGER,
    rlQosClassMapMatch2         INTEGER,
    rlQosClassMapMarkVlan       MarkVlanAction,
    rlQosClassMapNewVlan        INTEGER,
    rlQosClassMapRedirectAction RedirectAction,
    rlQosClassMapDestInterface  INTEGER,
    rlQosClassMapStatus         RowStatus,
    rlQosClassMapMatch3         INTEGER,
    rlQosClassMapTrapId         INTEGER,
    rlQosClassMapCounterEnable  TruthValue,
    rlQosClassMapTunnelIdx      Unsigned32
    }


rlQosClassMapIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Class Map Index"
    ::= { rlQosClassMapEntry 1 }

rlQosClassMapName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..32))
--    Rsyntax OCTET STRING(SIZE(0..255))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Name of the Class Map."
    ::= { rlQosClassMapEntry 2 }


rlQosClassMapType OBJECT-TYPE
    SYNTAX ClassMapType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Class map type"
    DEFVAL {1}
    ::= { rlQosClassMapEntry 3 }

rlQosClassMapAction OBJECT-TYPE
    SYNTAX ClassMapAction
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Class Map Action."
    DEFVAL {1}
    ::= { rlQosClassMapEntry 4 }

rlQosClassMapMarkValue OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Mark value when mark action has been chosen in
         Class Map Action field."
    DEFVAL {0}
    ::= { rlQosClassMapEntry 5 }

rlQosClassMapPolicer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Policer  pointer. 0-means no policer."
    DEFVAL {0}
    ::= { rlQosClassMapEntry 6 }
rlQosClassMapMatch1  OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Match ACL 1 pointer."
    ::= { rlQosClassMapEntry 7 }

rlQosClassMapMatch2  OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Match ACL 2 pointer."
    DEFVAL {0}
    ::= { rlQosClassMapEntry 8 }

rlQosClassMapMarkVlan  OBJECT-TYPE
    SYNTAX MarkVlanAction
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "If 'mark', than the classified
         traffic will be remarked with new VLAN id.
         If 'disabled' VLAN id is not changed.
         If markNestedVlan, if the egress interface defined as
         VLAN tagged member then a new VLAN tag is added  to the packet."
    DEFVAL {1}
    ::= { rlQosClassMapEntry 9 }

rlQosClassMapNewVlan  OBJECT-TYPE
    SYNTAX INTEGER(0..4095)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "If rlQosClassMapMarkVlan is not 'noMark',
         than the classified traffic will be
         remarked with new VLAN id.
         The value of this field sets new VLAN id."
    DEFVAL {0}
    ::= { rlQosClassMapEntry 10 }

rlQosClassMapRedirectAction  OBJECT-TYPE
    SYNTAX RedirectAction
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Specifiy the redirection action."
    DEFVAL {disabled}
    ::= { rlQosClassMapEntry 11 }

rlQosClassMapDestInterface  OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Relevant if rlQosClassMapRedirect is either
        'redirectToInterface' or 'analyzerPort' or 'toMultipleInterfaces'.
        Specified the output interface the packet is redireted to or
        the port that gets copy of the packet in addition to the port
        it was forwarded."
    DEFVAL {0}
    ::= { rlQosClassMapEntry 12 }

rlQosClassMapStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosClassMapEntry 13 }

rlQosClassMapMatch3  OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Match ACL 3 pointer."
    DEFVAL {0}
    ::= { rlQosClassMapEntry 14 }

rlQosClassMapTrapId  OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "If now zero, Indicates the trap type id the matched packets arrives with,
        relevant when RedirectAction is trap or mirror."
    DEFVAL {0}
    ::= { rlQosClassMapEntry 15 }

rlQosClassMapCounterEnable  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Enable/disable counting per class map.
        Counts packets matche the class map rules."
    DEFVAL {false}
    ::= { rlQosClassMapEntry 16 }

rlQosClassMapTunnelIdx  OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "If not zero, then the tunnel data pointed by rlQosClassMapTunnelIdx
        is added to the packet"
    DEFVAL {0}
    ::= { rlQosClassMapEntry 17 }

--- QoS Policer table


rlQosPolicerTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosPolicerEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies All the Policers in the system Information"
    ::= { rlQosCliMib 10 }

rlQosPolicerEntry OBJECT-TYPE
    SYNTAX RlQosPolicerEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one policer.
        The information includes: Policer name, Policer type, Committed Rate,
        Committed Burst, Out-of-Profile Action.
        The index is sequential integer represent by rlQosPolicerIndex"
    INDEX { rlQosPolicerIndex }
    ::= { rlQosPolicerTable 1 }

RlQosPolicerEntry ::= SEQUENCE {
    rlQosPolicerIndex            INTEGER,
    rlQosPolicerName             DisplayString,
    rlQosPolicerType             PolicerType,
    rlQosPolicerCir              Unsigned32,
    rlQosPolicerCbs              Unsigned32,   
    rlQosPolicerAction           PolicerAction,
    rlQosPolicerCasPointerRemVal INTEGER,
    rlQosPolicerStatus           RowStatus,
    rlQosPolicerPir              Unsigned32,
    rlQosPolicerPbs              Unsigned32,
    rlQosPolicerPeakAction       PolicerAction
    }

rlQosPolicerIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Policer Index."
    ::= { rlQosPolicerEntry 1 }

rlQosPolicerName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..32))
--    Rsyntax OCTET STRING(SIZE(0..255))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Name of the Policer."
    ::= { rlQosPolicerEntry 2 }


rlQosPolicerType OBJECT-TYPE
    SYNTAX PolicerType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Policer type"
    ::= { rlQosPolicerEntry 3 }

rlQosPolicerCir OBJECT-TYPE
    SYNTAX Unsigned32
    UNITS      "kbps"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Committed rate value."
    ::= { rlQosPolicerEntry 4 }
rlQosPolicerCbs OBJECT-TYPE
    SYNTAX Unsigned32
    UNITS      "bytes"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Committed burst Value."
    ::= { rlQosPolicerEntry 5 }

rlQosPolicerAction OBJECT-TYPE
    SYNTAX PolicerAction
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Out of profile Action."
    ::= { rlQosPolicerEntry 6 }

rlQosPolicerCasPointerRemVal OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Remark value in case of explicit remark.
         The functionality as cascade pointer is obsolete."
    ::= { rlQosPolicerEntry 7 }

rlQosPolicerStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosPolicerEntry 8 }

rlQosPolicerPir OBJECT-TYPE
    SYNTAX Unsigned32
    UNITS      "kbps"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Peak rate value.
         When both this and rlQosPolicerPbs are 0 this means the mode is Single Rate
         and when they are both non 0 this means the mode is Two Rate."
    ::= { rlQosPolicerEntry 9 }
    
rlQosPolicerPbs OBJECT-TYPE
    SYNTAX Unsigned32
    UNITS      "bytes"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Peak burst Value.
         When both this and rlQosPolicerPir are 0 this means the mode is Single Rate
         and when they are both non 0 this means the mode is Two Rate."
    ::= { rlQosPolicerEntry 10 }

rlQosPolicerPeakAction OBJECT-TYPE
    SYNTAX PolicerAction
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Out of profile peak action."
    ::= { rlQosPolicerEntry 11 }

-- QoS Police-Map table



rlQosPolicyMapTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosPolicyMapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies Policy Map Table Information"
    ::= { rlQosCliMib 11 }

rlQosPolicyMapEntry OBJECT-TYPE
    SYNTAX RlQosPolicyMapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one policy map.
        The information includes: Index, Policy Map name,
        Up to 6 class map names.
        The index is sequential integer represent by rlQosPolicerIndex"
    INDEX { rlQosPolicyMapIndex }
    ::= { rlQosPolicyMapTable 1 }

RlQosPolicyMapEntry ::= SEQUENCE {
    rlQosPolicyMapIndex          	INTEGER,
    rlQosPolicyMapName           	DisplayString,
    rlQosPolicyMapStatus         	RowStatus,
    rlQosPolicyMapIsBoundToInterface	TruthValue
    }

rlQosPolicyMapIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Policy map Index."
    ::= { rlQosPolicyMapEntry 1 }

rlQosPolicyMapName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..32))
--    Rsyntax OCTET STRING(SIZE(0..255))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Policy map Name."
    ::= { rlQosPolicyMapEntry 2 }

rlQosPolicyMapStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosPolicyMapEntry 3 }

rlQosPolicyMapIsBoundToInterface     OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates whether the policy map is bound to any interface or not."
    ::= { rlQosPolicyMapEntry 4 }

--QoS Policy Class map refernce table


rlQosPolicyClassRefTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosPolicyClassRefEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The relationship
         between policy map to class map"
    ::= { rlQosCliMib 12 }

rlQosPolicyClassRefEntry OBJECT-TYPE
    SYNTAX RlQosPolicyClassRefEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the connection
         between class-map entry to policy map by using pointers.
         The index is Class map pointer
         represent by rlQosPolicyClassRefClassPointer"
    INDEX { rlQosPolicyClassRefClassPointer }
    ::= { rlQosPolicyClassRefTable 1 }

RlQosPolicyClassRefEntry ::= SEQUENCE {
    rlQosPolicyClassRefClassPointer     INTEGER,
    rlQosPolicyClassRefPolicyPointer    INTEGER,
    rlQosPolicyClassRefStatus           RowStatus
    }

rlQosPolicyClassRefClassPointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The Index is the Class-map pointer"
    ::= { rlQosPolicyClassRefEntry 1 }

rlQosPolicyClassRefPolicyPointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Policy map index Pointer"
    ::= { rlQosPolicyClassRefEntry 2 }

rlQosPolicyClassRefStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosPolicyClassRefEntry 3 }




--   QoS Interface Policy table




rlQosIfPolicyTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosIfPolicyEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies for each interface
                        the Policy Map attach to it"
    ::= { rlQosCliMib 13 }

rlQosIfPolicyEntry OBJECT-TYPE
    SYNTAX RlQosIfPolicyEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes what policy
         Map attached to specific Interface.
         The index is Interface Index represent by rlIfIndex and
         the interface type represent by rlIfType"
    INDEX { rlIfIndex,
            rlIfType }
    ::= { rlQosIfPolicyTable 1 }

RlQosIfPolicyEntry ::= SEQUENCE {
        rlIfIndex                      INTEGER,
        rlIfType                       InterfaceType,
        rlQosIfPolicyMapPointerIn      INTEGER,
        rlQosIfPolicyMapPointerOut     INTEGER,
        rlQosIfTrustActive             BinaryStatus,
        rlQosPortShaperStatus          BinaryStatus,
        rlQosCirPortShaper             INTEGER,
        rlQosCbsPortShaper             INTEGER,
        rlQosIfProfilePointer          DisplayString,
        rlQosQueueProfilePointer       DisplayString,
        rlQosQueueShapeProfilePointer  INTEGER,
        rlQosAclDefaultAction          AclDefaultAction,
        rlQosIfPolicyMapStatus         RowStatus,
        rlQosIfAclIn                   INTEGER,
        rlQosIfAclOut                  INTEGER,
        rlQosIfPolicerIn               INTEGER,
        rlQosPortRateLimitStatus       BinaryStatus,
        rlQosCirPortRateLimit          INTEGER,
        rlQosCbsPortRateLimit          INTEGER,
        rlQosIfIpv6AclIn               INTEGER,
        rlQosIfIpv6AclOut              INTEGER,
        rlQosAclDefaultActionOut       AclDefaultAction
    }

rlIfIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Interface Index."
    ::= { rlQosIfPolicyEntry 1 }

rlIfType OBJECT-TYPE
    SYNTAX InterfaceType
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Interface Type(vlan/port)."
    ::= { rlQosIfPolicyEntry 2 }

rlQosIfPolicyMapPointerIn OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Policy map pointer Input."
    ::= { rlQosIfPolicyEntry 3 }

rlQosIfPolicyMapPointerOut OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Policy map pointer Output."
    ::= { rlQosIfPolicyEntry 4 }

rlQosIfTrustActive OBJECT-TYPE
   SYNTAX BinaryStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Interface Basic Mode Trust is active or not ."
    ::= { rlQosIfPolicyEntry 5 }


rlQosPortShaperStatus OBJECT-TYPE
    SYNTAX BinaryStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "If there is shaper on the port"
    ::= { rlQosIfPolicyEntry 6 }

rlQosCirPortShaper OBJECT-TYPE
    SYNTAX INTEGER
    UNITS      "bps"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The CIR for the port shaper.
         N/A when the shper is disabled"
    ::= { rlQosIfPolicyEntry 7}

rlQosCbsPortShaper OBJECT-TYPE
    SYNTAX INTEGER
    UNITS      "bytes"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The CBS for the port shaper.
         N/A when the shper is disabled"
    ::= { rlQosIfPolicyEntry 8 }

rlQosIfProfilePointer OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..32))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Interface Profile name pointer."
    ::= { rlQosIfPolicyEntry 9 }

rlQosQueueProfilePointer OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..32))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        " Queue Profile name pointer."
    ::= { rlQosIfPolicyEntry 10 }

rlQosQueueShapeProfilePointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        " Queue shape Profile pointer."
    ::= { rlQosIfPolicyEntry 11 }


rlQosAclDefaultAction OBJECT-TYPE
    SYNTAX AclDefaultAction
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        " When one ACL is enterd then what to do for the last rull."
    ::= { rlQosIfPolicyEntry 12 } 

rlQosIfPolicyMapStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosIfPolicyEntry 13 }

rlQosIfAclIn OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Index of an ACL in the rlQosAclTable, which is applied
         to the ingress of an interface.
         0 - means no ACL applied."
    DEFVAL {0}
    ::= { rlQosIfPolicyEntry 14 }

rlQosIfAclOut OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Index of an ACL in the rlQosAclTable, which is applied
         to the egress of an interface.
         0 - means no ACL applied."
    DEFVAL {0}
    ::= { rlQosIfPolicyEntry 15 }

rlQosIfPolicerIn OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Index of an Policer in the rlQosPolicerTable, which is applied
         to the ingress of an interface.
         0 - means no Policer applied."
    DEFVAL {0}
    ::= { rlQosIfPolicyEntry 16 }

rlQosPortRateLimitStatus OBJECT-TYPE
    SYNTAX BinaryStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "If there is Rate limit on the port"
    DEFVAL {disable}
    ::= { rlQosIfPolicyEntry 17 }

rlQosCirPortRateLimit OBJECT-TYPE
    SYNTAX INTEGER
    UNITS      "bps"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The CIR for the port rate limit.
         N/A when the Rate limit is disabled"
    DEFVAL {0}
    ::= { rlQosIfPolicyEntry 18}

rlQosCbsPortRateLimit OBJECT-TYPE
    SYNTAX INTEGER
    UNITS      "bytes"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The CBS for the port Rate limit.
         N/A when the Rate limit is disabled"
    DEFVAL {0}
    ::= { rlQosIfPolicyEntry 19 }

rlQosIfIpv6AclIn OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Index of an IPv6 ACL in the rlQosAclTable, which is applied
         to the ingress of an interface.
         0 - means no ACL applied."
    DEFVAL {0}
    ::= { rlQosIfPolicyEntry 20 }

rlQosIfIpv6AclOut OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Index of an IPv6 ACL in the rlQosAclTable, which is applied
         to the egress of an interface.
         0 - means no ACL applied."
    DEFVAL {0}
    ::= { rlQosIfPolicyEntry 21 }
    
rlQosAclDefaultActionOut OBJECT-TYPE
    SYNTAX AclDefaultAction
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        " When one egress ACL is enterd then what to do for the last rull."
    ::= { rlQosIfPolicyEntry 22 }       

-- QoS Interface Profile table



rlQosIfProfileCfgTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosIfProfileCfgEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies for each Queue the Tail
         Drop or WRED parameters and the EF of WRR
         parameters."
    ::= { rlQosCliMib 14 }

rlQosIfProfileCfgEntry OBJECT-TYPE
    SYNTAX RlQosIfProfileCfgEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one queue
         parameters: Tail-drop threshold for drop precedence
         0,1,3 and the WRED min-max threshold and the probability
         factor for Drop precedence 0,1,2 and the WRED Q factor
         and the EF priority and the WRR weight.
         The index is Interface Index represent by rlIfProfileName
         and queue-id represent by rlQosQueueId"
    INDEX { rlIfProfileName,
            rlQosQueueId
                  }
    ::= { rlQosIfProfileCfgTable 1 }

RlQosIfProfileCfgEntry ::= SEQUENCE {
        rlIfProfileName          DisplayString,
        rlQosQueueId             INTEGER,
        rlQosTdThersholdDp0      INTEGER,
        rlQosTdThersholdDp1      INTEGER,
        rlQosTdThersholdDp2      INTEGER,
        rlQosRedMinDp0           INTEGER,
        rlQosRedMaxDp0           INTEGER,
        rlQosRedProbDp0          INTEGER,
        rlQosRedMinDp1           INTEGER,
        rlQosRedMaxDp1           INTEGER,
        rlQosRedProbDp1          INTEGER,
        rlQosRedMinDp2           INTEGER,
        rlQosRedMaxDp2           INTEGER,
        rlQosRedProbDp2          INTEGER,
        rlQosRedQweight          INTEGER,
        rlQosIfprofileStatus     RowStatus
    }

rlIfProfileName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Interface Index."
    ::= { rlQosIfProfileCfgEntry 1 }

rlQosQueueId OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Queue id Index."
    ::= { rlQosIfProfileCfgEntry 2 }

rlQosTdThersholdDp0 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    UNITS      "percent"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 0."
    ::= { rlQosIfProfileCfgEntry 3 }
rlQosTdThersholdDp1 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    UNITS      "percent"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 1."
    ::= { rlQosIfProfileCfgEntry 4 }
rlQosTdThersholdDp2 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    UNITS      "percent"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 2."
    ::= { rlQosIfProfileCfgEntry 5 }
rlQosRedMinDp0 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    UNITS      "percent"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 2."
    ::= { rlQosIfProfileCfgEntry 6 }
rlQosRedMaxDp0 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    UNITS      "percent"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 0."
    ::= { rlQosIfProfileCfgEntry 7 }
rlQosRedProbDp0 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 0."
    ::= { rlQosIfProfileCfgEntry 8 }
rlQosRedMinDp1 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    UNITS      "percent"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 2."
    ::= { rlQosIfProfileCfgEntry 9 }
rlQosRedMaxDp1 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    UNITS      "percent"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 1."
    ::= { rlQosIfProfileCfgEntry 10 }
rlQosRedProbDp1 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 1."
    ::= { rlQosIfProfileCfgEntry 11 }
rlQosRedMinDp2 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    UNITS      "percent"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 2."
    ::= { rlQosIfProfileCfgEntry 12 }
rlQosRedMaxDp2 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    UNITS      "percent"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 2."
    ::= { rlQosIfProfileCfgEntry 13 }
rlQosRedProbDp2 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 2."
    ::= { rlQosIfProfileCfgEntry 14 }
rlQosRedQweight OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Q factor for WRED."
    ::= { rlQosIfProfileCfgEntry 15 }

rlQosIfprofileStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosIfProfileCfgEntry 16 }


-- QoS DSCP Mutation Map


rlQosDscpMutationTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosDscpMutationEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The DSCP
         Mutation table"
    ::= { rlQosCliMib 15 }

rlQosDscpMutationEntry OBJECT-TYPE
    SYNTAX RlQosDscpMutationEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the new
         DSCP for the packet.
         The index is Old DSCP represent by rlQosOldDscp"
    INDEX { rlQosOldDscp }
    ::= { rlQosDscpMutationTable 1 }

RlQosDscpMutationEntry ::= SEQUENCE {
        rlQosOldDscp                INTEGER,
        rlQosNewDscp                INTEGER
    }

rlQosOldDscp OBJECT-TYPE
    SYNTAX INTEGER (0..63)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Old DSCP."
    ::= { rlQosDscpMutationEntry 1 }

rlQosNewDscp OBJECT-TYPE
    SYNTAX INTEGER (0..63)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "New DSCP."
    ::= { rlQosDscpMutationEntry 2 }



-- QoS DSCP Police Transmit(Remark) map



rlQosDscpRemarkTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosDscpRemarkEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The DSCP
         Remark table"
    ::= { rlQosCliMib 16 }

rlQosDscpRemarkEntry OBJECT-TYPE
    SYNTAX RlQosDscpRemarkEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the new
         DSCP for the packet.
         The index is Old DSCP represent by rlQosOldDscp"
    INDEX { rlQosRmOldDscp }
    ::= { rlQosDscpRemarkTable 1 }

RlQosDscpRemarkEntry ::= SEQUENCE {
        rlQosRmOldDscp                INTEGER,
        rlQosRmNewDscp                INTEGER,
        rlQosRmNewExceedDscp          INTEGER
    }

rlQosRmOldDscp OBJECT-TYPE
    SYNTAX INTEGER (0..63)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Old DSCP."
    ::= { rlQosDscpRemarkEntry 1 }

rlQosRmNewDscp OBJECT-TYPE
    SYNTAX INTEGER (0..63)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Specifies new DSCP in the violation action."
    ::= { rlQosDscpRemarkEntry 2 }
    
rlQosRmNewExceedDscp OBJECT-TYPE
    SYNTAX INTEGER (0..63)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Specifies new DSCP in the exceed action."
    ::= { rlQosDscpRemarkEntry 3 }


--  QoS CoS (VPT) to Queue map


rlQosCosQueueTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosCosQueueEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The Cos
         to queue map table"
    ::= { rlQosCliMib 17 }

rlQosCosQueueEntry OBJECT-TYPE
    SYNTAX RlQosCosQueueEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes queue ID.
         The index is CoS represent by rlQosCosIndex"
    INDEX { rlQosCosIndex }
    ::= { rlQosCosQueueTable 1 }

RlQosCosQueueEntry::= SEQUENCE {
        rlQosCosIndex                INTEGER,
        rlQosCosQueueId                INTEGER
    }

rlQosCosIndex OBJECT-TYPE
    SYNTAX INTEGER (0..7)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "CoS value (0-7)."
    ::= { rlQosCosQueueEntry 1 }

rlQosCosQueueId OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Queue ID."
    ::= { rlQosCosQueueEntry 2 }





--  QoS DSCP to Queue (VPT) map



rlQosDscpQueueTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosDscpQueueEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The DSCP
         to Queue map table"
    ::= { rlQosCliMib 18 }

rlQosDscpQueueEntry OBJECT-TYPE
    SYNTAX RlQosDscpQueueEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes The
         Queue Number.
         The index is DSCP represent by rlQosDscpIndex"
    INDEX { rlQosDscpIndex }
    ::= { rlQosDscpQueueTable 1 }

RlQosDscpQueueEntry ::= SEQUENCE {
        rlQosDscpIndex                INTEGER,
        rlQosQueueNum                 INTEGER
    }

rlQosDscpIndex OBJECT-TYPE
    SYNTAX INTEGER (0..63)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "DSCP value."
    ::= { rlQosDscpQueueEntry 1 }

rlQosQueueNum OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Queue Number."
    ::= { rlQosDscpQueueEntry 2 }



-- QoS TCP port to Queue map



rlQosTcpPortQueueTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosTcpPortQueueEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies TCP
         Port to Queue map table"
    ::= { rlQosCliMib 19 }

rlQosTcpPortQueueEntry OBJECT-TYPE
    SYNTAX RlQosTcpPortQueueEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes The
         Queue Number.
         The index is TCP/UDP port represent by rlQosTcpUdpPort"
    INDEX { rlQosTcpPort }
    ::= { rlQosTcpPortQueueTable 1 }

RlQosTcpPortQueueEntry ::= SEQUENCE {
        rlQosTcpPort                  INTEGER,
        rlQosTcpQueueValue            INTEGER,
        rlQosTcpPortQueueStatus       RowStatus
    }

rlQosTcpPort OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "TCP port number."
    ::= { rlQosTcpPortQueueEntry 1 }

rlQosTcpQueueValue OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Queue Number."
    ::= { rlQosTcpPortQueueEntry 2 }

rlQosTcpPortQueueStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosTcpPortQueueEntry 3 }


-- QoS UDP port to Queue map



rlQosUdpPortQueueTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosUdpPortQueueEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies UDP
         Port to Queue map table"
    ::= { rlQosCliMib 20 }

rlQosUdpPortQueueEntry OBJECT-TYPE
    SYNTAX RlQosUdpPortQueueEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes The
         Queue Number.
         The index is UDP port represent by rlQosTcpUdpPort"
    INDEX { rlQosUdpPort }
    ::= { rlQosUdpPortQueueTable 1 }

RlQosUdpPortQueueEntry ::= SEQUENCE {
        rlQosUdpPort                  INTEGER,
        rlQosUdpQueueValue            INTEGER,
        rlQosUdpPortQueueStatus       RowStatus
    }

rlQosUdpPort OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "UDP port number."
    ::= { rlQosUdpPortQueueEntry 1 }

rlQosUdpQueueValue OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Queue value."
    ::= { rlQosUdpPortQueueEntry 2 }

rlQosUdpPortQueueStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosUdpPortQueueEntry 3 }

-- CLI QoS Number of EF Scalar

rlQosEfManageTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosEfManageEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies UDP
         Port to DSCP map table"
    ::= { rlQosCliMib 21 }

rlQosEfManageEntry OBJECT-TYPE
    SYNTAX RlQosEfManageEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This Table describes The
         EF management for the system.
         The index is UDP port represent by rlQosEfQueueId"
    INDEX { rlQosEfQueueId }
    ::= { rlQosEfManageTable 1 }

RlQosEfManageEntry ::= SEQUENCE {
        rlQosEfQueueId                INTEGER,
        rlQosEfState                  BinaryStatus,
        rlQosEfPriority               INTEGER
    }

rlQosEfQueueId OBJECT-TYPE
    SYNTAX INTEGER(1..8)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Queue-ID."
    ::= { rlQosEfManageEntry 1 }

rlQosEfState OBJECT-TYPE
    SYNTAX BinaryStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Enable/disable"
    ::= { rlQosEfManageEntry 2 }

rlQosEfPriority OBJECT-TYPE
    SYNTAX INTEGER(1..8)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The priority of the queue"
    ::= { rlQosEfManageEntry 3 }


-- CLI QoS Queue Profile

rlQosQueueProfileTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosQueueProfileEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table describes the queue managment profiles "
    ::= { rlQosCliMib 22 }

rlQosQueueProfileEntry OBJECT-TYPE
    SYNTAX RlQosQueueProfileEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes The
         queue managment profile Value.
         The index is profile name represent by rlQueueProfileName"
    INDEX { rlQueueProfileName }
    ::= { rlQosQueueProfileTable 1 }

RlQosQueueProfileEntry ::= SEQUENCE {
        rlQueueProfileName          DisplayString,
        rlQosTypeQueue1             QueueType,
        rlQosValueQueue1            INTEGER,
        rlQosTypeQueue2             QueueType,
        rlQosValueQueue2            INTEGER,
        rlQosTypeQueue3             QueueType,
        rlQosValueQueue3            INTEGER,
        rlQosTypeQueue4             QueueType,
        rlQosValueQueue4            INTEGER,
        rlQosTypeQueue5             QueueType,
        rlQosValueQueue5            INTEGER,
        rlQosTypeQueue6             QueueType,
        rlQosValueQueue6            INTEGER,
        rlQosTypeQueue7             QueueType,
        rlQosValueQueue7            INTEGER,
        rlQosTypeQueue8             QueueType,
        rlQosValueQueue8            INTEGER,
        rlQosQueueProfileStatus     RowStatus,
        rlQosNumOfIfConnections     INTEGER
    }

rlQueueProfileName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Profile name for the Queue profile."
    ::= { rlQosQueueProfileEntry 1 }

rlQosTypeQueue1 OBJECT-TYPE
    SYNTAX QueueType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "EF or WRR"
    ::= { rlQosQueueProfileEntry 2 }

rlQosValueQueue1 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "for EF read-only for wrr the weight"
    ::= { rlQosQueueProfileEntry 3 }

rlQosTypeQueue2 OBJECT-TYPE
    SYNTAX QueueType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "EF or WRR"
    ::= { rlQosQueueProfileEntry 4 }

rlQosValueQueue2 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "for EF read-only for wrr the weight"
    ::= { rlQosQueueProfileEntry 5 }
rlQosTypeQueue3 OBJECT-TYPE
    SYNTAX QueueType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "EF or WRR"
    ::= { rlQosQueueProfileEntry 6 }

rlQosValueQueue3 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "for EF read-only for wrr the weight"
    ::= { rlQosQueueProfileEntry 7 }

rlQosTypeQueue4 OBJECT-TYPE
    SYNTAX QueueType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "EF or WRR"
    ::= { rlQosQueueProfileEntry 8 }

rlQosValueQueue4 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "for EF read-only for wrr the weight"
    ::= { rlQosQueueProfileEntry 9 }

rlQosTypeQueue5 OBJECT-TYPE
    SYNTAX QueueType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "EF or WRR"
    ::= { rlQosQueueProfileEntry 10 }

    rlQosValueQueue5 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "for EF read-only for wrr the weight"
    ::= { rlQosQueueProfileEntry 11 }

rlQosTypeQueue6 OBJECT-TYPE
    SYNTAX QueueType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "EF or WRR"
    ::= { rlQosQueueProfileEntry 12 }

rlQosValueQueue6 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "for EF read-only for wrr the weight"
    ::= { rlQosQueueProfileEntry 13 }
rlQosTypeQueue7 OBJECT-TYPE
    SYNTAX QueueType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "EF or WRR"
    ::= { rlQosQueueProfileEntry 14}

rlQosValueQueue7 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "for EF read-only for wrr the weight"
    ::= { rlQosQueueProfileEntry 15 }

rlQosTypeQueue8 OBJECT-TYPE
    SYNTAX QueueType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "EF or WRR"
    ::= { rlQosQueueProfileEntry 16 }

rlQosValueQueue8 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "for EF read-only for wrr the weight"
    ::= { rlQosQueueProfileEntry 17 }

rlQosQueueProfileStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosQueueProfileEntry 18 }

rlQosNumOfIfConnections OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "how many time this entry connected to the if policy table"
    ::= { rlQosQueueProfileEntry 19 }



-- CLI QoS Queue Shape Profile



rlQosQueueShapeProfileTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosQueueShapeProfileEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies the queue shaper profile"
    ::= { rlQosCliMib 23 }

rlQosQueueShapeProfileEntry OBJECT-TYPE
    SYNTAX RlQosQueueShapeProfileEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes The
         shaper profile for all queues.
         The index sequencial index represent by rlQosQueueShapeIndex"
    INDEX { rlQosQueueShapeIndex}
    ::= { rlQosQueueShapeProfileTable 1 }

RlQosQueueShapeProfileEntry ::= SEQUENCE {
        rlQosQueueShapeIndex           INTEGER,
        rlQosCirQueue1                 INTEGER,
        rlQosCbsQueue1                 INTEGER,
        rlQosCirQueue2                 INTEGER,
        rlQosCbsQueue2                 INTEGER,
        rlQosCirQueue3                 INTEGER,
        rlQosCbsQueue3                 INTEGER,
        rlQosCirQueue4                 INTEGER,
        rlQosCbsQueue4                 INTEGER,
        rlQosCirQueue5                 INTEGER,
        rlQosCbsQueue5                 INTEGER,
        rlQosCirQueue6                 INTEGER,
        rlQosCbsQueue6                 INTEGER,
        rlQosCirQueue7                 INTEGER,
        rlQosCbsQueue7                 INTEGER,
        rlQosCirQueue8                 INTEGER,
        rlQosCbsQueue8                 INTEGER,
        rlQosQueueShapeProfileStatus   RowStatus
    }

rlQosQueueShapeIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Profile Index."
    ::= { rlQosQueueShapeProfileEntry 1 }

rlQosCirQueue1 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CIR for Queue1 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 2 }

rlQosCbsQueue1 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CBS for Queue1 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 3 }

rlQosCirQueue2 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CIR for Queue2 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 4 }

rlQosCbsQueue2 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CBS for Queue2 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 5 }

rlQosCirQueue3 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CIR for Queue3 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 6 }

rlQosCbsQueue3 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CBS for Queue3 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 7 }

rlQosCirQueue4 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CIR for Queue4 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 8 }

rlQosCbsQueue4 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CBS for Queue4 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 9 }

rlQosCirQueue5 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CIR for Queue5 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 10 }

rlQosCbsQueue5 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CBS for Queue5 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 11 }

rlQosCirQueue6 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CIR for Queue6 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 12 }

rlQosCbsQueue6 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CBS for Queue6 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 13 }

rlQosCirQueue7 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CIR for Queue7 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 14 }

rlQosCbsQueue7 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CBS for Queue7 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 15 }

rlQosCirQueue8 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CIR for Queue8 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 16 }

rlQosCbsQueue8 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "CBS for Queue8 0 for not active"
    ::= { rlQosQueueShapeProfileEntry 17 }

rlQosQueueShapeProfileStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosQueueShapeProfileEntry 18 }

-- ACL counters table

rlQosAclCounterTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlQosAclCounterEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The  table is used to show statistics for
         ACL applied on an interface."
    ::= { rlQosCliMib 24 }

rlQosAclCounterEntry OBJECT-TYPE
    SYNTAX  RlQosAclCounterEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This entry shows value of conter for a
         particular ACE of an ACL."
    INDEX  {  rlQosAclCounterInterface,
              rlQosAclCounterAclIndex,
              rlQosAclCounterAceIndex}
    ::= { rlQosAclCounterTable 1 }

RlQosAclCounterEntry ::= SEQUENCE  {
    rlQosAclCounterInterface          InterfaceIndex,
    rlQosAclCounterAclIndex           INTEGER,
    rlQosAclCounterAceIndex           INTEGER,
    rlQosAclCounterValue              Counter32
}

rlQosAclCounterInterface OBJECT-TYPE
    SYNTAX  InterfaceIndex
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Interface Index on which ACL is applied."
    ::= { rlQosAclCounterEntry 1 }

rlQosAclCounterAclIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Index of ACL, which was applied on the IfIndex."
    ::= { rlQosAclCounterEntry 2 }

rlQosAclCounterAceIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Index of ACE, which is belong to an ACL."
    ::= { rlQosAclCounterEntry 3 }

rlQosAclCounterValue OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value of the ACE counter."
    ::= { rlQosAclCounterEntry 4 }


-- Free indexes table

rlQosFreeIndexesTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlQosFreeIndexesEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The  table is used to get free indexes of tables to create
         new entries. The algorithm for free indexes depends on
         table's type:
         Tuple table      - first free index.
         Offset table     - first free index.
         ACE table        - last used index + ACE indexes delta.
         ACL table        - first free index.
         Class Map table  - last used index + Class Map indexes delta.
         Policy Map table - first free index.
         Policer Table    - first free index.
         The ACE indexes delta and Class Map indexes delta are used
         to supply QoS MIB user easy insert entry capabilities.
         Values of these deltas depend on the MIB implementation.
         The 'Get and increment' approach is used in all cases. "
    ::= { rlQosCliMib 25 }

rlQosFreeIndexesEntry OBJECT-TYPE
    SYNTAX  RlQosFreeIndexesEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The entry is used to get free index for particular table."
    INDEX  {  rlQosFreeIndexesTableId}
    ::= { rlQosFreeIndexesTable 1 }

RlQosFreeIndexesEntry ::= SEQUENCE  {
    rlQosFreeIndexesTableId           INTEGER,
    rlQosFreeIndexesValue             INTEGER
}

rlQosFreeIndexesTableId OBJECT-TYPE
    SYNTAX INTEGER {
        tuple (1),
        offset(2),
        ace(3),
        acl(4),
        class(5),
        policy(6),
        policer(7),
        shaper(8)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Identification of the table, for which free index
         is retrieved."
    ::= { rlQosFreeIndexesEntry 1 }

rlQosFreeIndexesValue OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Free index for table. 0 means no free entries."
    ::= { rlQosFreeIndexesEntry 2 }

-- names to indexes table

rlQosNamesToIndexesTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlQosNamesToIndexesEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table is used to get the ACL,Class-Map and Policy-Map
          indexes from the name."
    ::= { rlQosCliMib 26 }

rlQosNamesToIndexesEntry OBJECT-TYPE
    SYNTAX  RlQosNamesToIndexesEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The entry is used to get index form particular name and table type."
    INDEX  {  rlQosNamesToIndexesTableId,
              rlQosNamesToIndexesName}
    ::= { rlQosNamesToIndexesTable 1 }

RlQosNamesToIndexesEntry ::= SEQUENCE  {
    rlQosNamesToIndexesTableId           INTEGER,
    rlQosNamesToIndexesName              DisplayString,
    rlQosNamesToIndexesValue             INTEGER
}

rlQosNamesToIndexesTableId OBJECT-TYPE
    SYNTAX INTEGER {
        acl(1),
        class(2),
        policy(3),
        policer(4)
    }
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Identification of the table, for which the index
         is retrieved."
    ::= { rlQosNamesToIndexesEntry 1 }

rlQosNamesToIndexesName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The name of the entry"
    ::= { rlQosNamesToIndexesEntry 2 }

rlQosNamesToIndexesValue OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "the index for table"
    ::= { rlQosNamesToIndexesEntry 3 }

-- Stack Control Queue number
rlQosStackControlQueue OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This scalar object defines queue ID, which is
         used for stack control information transfer.
         For standalone systems the scalar value equals 0.
         This scalar object can be used for warning messages
         when users assign a QoS map item, or a Class to the
         stack control queue."
    ::= { rlQosCliMib 27 }

-- Stack Control CoS
rlQosStackControlCos OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This scalar object defines CoS (VPT), which is used
         for stack control information transfer.
         For standalone systems the scalar value equals 8
         (not valid for VPT).
         This scalar object can be used for warning messages
         when users assign a stack control CoS to a non-stacking
         control queue."
    ::= { rlQosCliMib 28 }





-- Cos to Queue Default map table

rlQosCosQueueDefaultMapTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlQosCosQueueDefaultMapEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table is used to set default 802.1p map (vpt to queue)"
    ::= { rlQosCliMib 29 }

rlQosCosQueueDefaultMapEntry OBJECT-TYPE
    SYNTAX  RlQosCosQueueDefaultMapEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The entry is used to get index form particular name and table type."
    INDEX  {  rlQosCosQueueDefaultMapVpt }
    ::= { rlQosCosQueueDefaultMapTable 1 }

RlQosCosQueueDefaultMapEntry ::= SEQUENCE  {
    rlQosCosQueueDefaultMapVpt           INTEGER,
    rlQosCosQueueDefaultMapQueueId       INTEGER
}

rlQosCosQueueDefaultMapVpt OBJECT-TYPE
    SYNTAX INTEGER (0..7)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "vlan priority tag , 3 bits of priority which determine
        the service class."
    ::= { rlQosCosQueueDefaultMapEntry 1 }

rlQosCosQueueDefaultMapQueueId OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "the queue id vary from the first queue id to Max Number of queues supported"

    ::= { rlQosCosQueueDefaultMapEntry 2 }


-- Predefined ACLs interface table

rlQosPredefBlockAclTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlQosPredefBlockAclEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table is used apply predefined ACLs to interfaces.
         Predefined ACLs is ACL to filter particular protocol or
         protocol's family. These ACL may operate simultaneously
         with IP and MAC ACLs."
    ::= { rlQosCliMib 30 }


rlQosPredefBlockAclEntry OBJECT-TYPE
    SYNTAX  RlQosPredefBlockAclEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The entry is used to apply predefined ACLs to the interface."
    INDEX { rlQosPredefBlockAclIfIndex, rlQosPredefBlockAclIfType }
    ::= { rlQosPredefBlockAclTable 1 }


RlQosPredefBlockAclEntry ::= SEQUENCE  {
    rlQosPredefBlockAclIfIndex    InterfaceIndex,
    rlQosPredefBlockAclIfType     InterfaceType,
    rlQosPredefBlockAclMask       OCTET STRING,
    rlQosPredefBlockAclStatus     RowStatus
}

rlQosPredefBlockAclIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "IfIndex of port/trunk or VLAN tag of VLAN
         on which predefined ACLa will be configured."
    ::= { rlQosPredefBlockAclEntry 1 }

rlQosPredefBlockAclIfType OBJECT-TYPE
    SYNTAX InterfaceType
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Interface Type(vlan/port)."
    ::= { rlQosPredefBlockAclEntry 2 }


rlQosPredefBlockAclMask OBJECT-TYPE
--    SYNTAX      BITS {
--            LLCNetBueiNetBios(0),
--            IPNetBueiNetBios(1)
--    }
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "This bitmap defines predefined ACL which are applied
         on an interface. The table below defines bitmasks for
         supported predefined ACL.
         Protocol/Family     bitmask Description
         =====================================================
         LLC NetBuei/NetBios 0x01    ACL filters out LLC encapsulated
                                      NetBuei/NetBios frames
         IP NetBuei/NetBios  0x02    ACL filters out IP encapsulated
                                      NetBuei/NetBios frames
         "
    ::= { rlQosPredefBlockAclEntry 3 }

rlQosPredefBlockAclStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosPredefBlockAclEntry 4 }


 -- QoS Access Control Element table two indexes


rlQosAceTidxTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosAceTidxEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table specifies ACE table with two index information"
    ::= { rlQosCliMib 31 }

rlQosAceTidxEntry OBJECT-TYPE
    SYNTAX     RlQosAceTidxEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Each entry in this table describes one Classifier Element.
        The information includes: Action the ACE's Type the up to 11 tuples
        pointers. The index is sequential integer represent by
        rlQosAceTidxAclIndex ACL index and rlQosAceTidxIndex ACE index"
    INDEX { rlQosAceTidxAclIndex,
            rlQosAceTidxIndex}
    ::= { rlQosAceTidxTable 1 }

RlQosAceTidxEntry ::= SEQUENCE {
    rlQosAceTidxAclIndex       INTEGER,
    rlQosAceTidxIndex          INTEGER,
    rlQosAceTidxAction         AceActionType,
    rlQosAceTidxType           AceObjectType,
    rlQosAceTidxTuple1         INTEGER,
    rlQosAceTidxTuple2         INTEGER,
    rlQosAceTidxTuple3         INTEGER,
    rlQosAceTidxTuple4         INTEGER,
    rlQosAceTidxTuple5         INTEGER,
    rlQosAceTidxTuple6         INTEGER,
    rlQosAceTidxTuple7         INTEGER,
    rlQosAceTidxTuple8         INTEGER,
    rlQosAceTidxAccount        BinaryStatus,
    rlQosAceTidxStatus         RowStatus,
    rlQosAceTidxTimeRange      DisplayString,
    rlQosAceTidxTimeRangeIsActive TruthValue,
    rlQosAceTidxTuple9         INTEGER,
    rlQosAceTidxTuple10        INTEGER,
    rlQosAceTidxTuple11        INTEGER,
    rlQosAceTidxActionDropType RlQosAceTidxActionDropType

    }

rlQosAceTidxAclIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An arbitrary incremental Index
         for the ACL ACE connection."
    ::= { rlQosAceTidxEntry 1 }

rlQosAceTidxIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An arbitrary incremental Index
         for the ACE table."
    ::= { rlQosAceTidxEntry 2 }

rlQosAceTidxAction OBJECT-TYPE
    SYNTAX AceActionType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Action to take."
    ::= { rlQosAceTidxEntry 3 }

rlQosAceTidxType OBJECT-TYPE
    SYNTAX AceObjectType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Type"
    ::= { rlQosAceTidxEntry 4 }

rlQosAceTidxTuple1 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 5 }

rlQosAceTidxTuple2 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 6 }

rlQosAceTidxTuple3 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 7 }

rlQosAceTidxTuple4 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 8 }

rlQosAceTidxTuple5 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 9 }

rlQosAceTidxTuple6 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 10 }

rlQosAceTidxTuple7 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 11 }

rlQosAceTidxTuple8 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 12 }

rlQosAceTidxAccount OBJECT-TYPE
    SYNTAX BinaryStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Accounting state.
         When set to 'enabled' than appropriate statistic's
         counter is provided for an ACE."
    ::= { rlQosAceTidxEntry 13 }

rlQosAceTidxStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosAceTidxEntry 14 }

rlQosAceTidxTimeRange OBJECT-TYPE
    SYNTAX     DisplayString( SIZE(0..32))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "ACE time range name."
    ::= { rlQosAceTidxEntry 15 }

rlQosAceTidxTimeRangeIsActive OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "ACE time range is rule active state shows is ACE currently active or not."
    ::= { rlQosAceTidxEntry 16 }

rlQosAceTidxTuple9 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 17 }

rlQosAceTidxTuple10 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 18 }

rlQosAceTidxTuple11 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "ACE Tuple pointer."
    ::= { rlQosAceTidxEntry 19 }


rlQosAceTidxActionDropType OBJECT-TYPE
    SYNTAX RlQosAceTidxActionDropType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "This field is valid only if AceActionType is
        deny or deny-DisablePort."
    ::= { rlQosAceTidxEntry 20 }


rlQosMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "MIB's version, the current version is 11
         1 - original version
         2 - Add new two MIB's items.
             - rlQosAceTidxTable - Ace table with two indexes
             - rlQosMibVersion.
             Change the unit in Policer table from bps to kbps
         3 - Add new MIB's value for Textual convention QosObjectMode
         4 - Add new MIBs rlQosDscpQueueDefaultMapTable
         5 - Add new advanced action : trustCosDscp
         6 - Add vpt,ether-type,tcp-flags,icmp-type,icmp-code,igmp-type to ClassTupleType
             Add ip-ICMP,ip-IGMP To AceObjectType
             Add vpt,ethertype To ClassOffsetType
         7-  Add rlQosPortRateLimitStatus,rlQosCirPortRateLimit, rlQosCbsPortRateLimit
             to   rlQosIfPolicyTable
         8 - Add Added rlQosDscpToDpTable
         9 - Add statistics
         10 - Add innerVlan to ClassOffsetType And inner-vlan to ClassTupleType
         11 - Added rlQosCPUSafeGuardEnable"
    ::= { rlQosCliMib 32 }

-- DSCP to Queue Default map table

rlQosDscpQueueDefaultMapTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlQosDscpQueueDefaultMapEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table is used to set default dscp to queue map"
    ::= { rlQosCliMib 33 }

rlQosDscpQueueDefaultMapEntry OBJECT-TYPE
    SYNTAX  RlQosDscpQueueDefaultMapEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The entry is used to get index form particular name and table type."
    INDEX  {  rlQosDscpQueueDefaultMapDscp }
    ::= { rlQosDscpQueueDefaultMapTable 1 }

RlQosDscpQueueDefaultMapEntry ::= SEQUENCE  {
    rlQosDscpQueueDefaultMapDscp           INTEGER,
    rlQosDscpQueueDefaultMapQueueId       INTEGER
}

rlQosDscpQueueDefaultMapDscp OBJECT-TYPE
    SYNTAX INTEGER (0..63)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "dscp , 6 bits of priority which determine
        the service class."
    ::= { rlQosDscpQueueDefaultMapEntry 1 }

rlQosDscpQueueDefaultMapQueueId OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "the queue id vary from the first queue id to Max Number of queues supported"

    ::= { rlQosDscpQueueDefaultMapEntry 2 }

-- QoS DSCP to DP Map


rlQosDscpToDpTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosDscpToDpEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The DSCP
         To Dp table"
    ::= { rlQosCliMib 34 }

rlQosDscpToDpEntry OBJECT-TYPE
    SYNTAX RlQosDscpToDpEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the new
         DP for the packet.
         The index is DSCP represent by rlQosDscp"
    INDEX { rlQosDscp }
    ::= { rlQosDscpToDpTable 1 }

RlQosDscpToDpEntry ::= SEQUENCE {
        rlQosDscp                INTEGER,
        rlQosDp                  INTEGER
    }

rlQosDscp OBJECT-TYPE
    SYNTAX INTEGER (0..63)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Packet DSCP."
    ::= { rlQosDscpToDpEntry 1 }

rlQosDp OBJECT-TYPE
    SYNTAX INTEGER (0..2)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "New DP."
    ::= { rlQosDscpToDpEntry 2 }


rlQosStatistics
        OBJECT IDENTIFIER ::= { rlQosCliMib 35 }

rlQosPortPolicyStatisticsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosPortPolicyStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies statistics counter for policies with specific actions "
    ::= { rlQosStatistics 1 }

rlQosPortPolicyStatisticsEntry OBJECT-TYPE
    SYNTAX RlQosPortPolicyStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes counter per port.
        The index is port represent by rlIfIndex.
        In each entry represents counter, it's type , it's size and whether it's enabled."
    INDEX { rlIfIndex,rlIfType, rlQosPortPolicyStatisticsCntrType }
    ::= { rlQosPortPolicyStatisticsTable 1 }

RlQosPortPolicyStatisticsEntry::= SEQUENCE {
        rlQosPortPolicyStatisticsCntrType        StatisticsCntrType,
        rlQosPortPolicyStatisticsCntrNumOfBits   StatisticsCntrNumOfBitsType,
        rlQosPortPolicyStatisticsEnableCounting  TruthValue,
        rlQosPortPolicyStatisticsCounterValue    Counter64
    }

rlQosPortPolicyStatisticsCntrType          OBJECT-TYPE
    SYNTAX StatisticsCntrType
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Counter type."
    ::= { rlQosPortPolicyStatisticsEntry 1 }

rlQosPortPolicyStatisticsCntrNumOfBits          OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits."
    ::= { rlQosPortPolicyStatisticsEntry 2 }

rlQosPortPolicyStatisticsEnableCounting     OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication whether the counter is enabled."
    DEFVAL { false }
    ::= { rlQosPortPolicyStatisticsEntry 3 }

rlQosPortPolicyStatisticsCounterValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter value."
    ::= { rlQosPortPolicyStatisticsEntry 4 }


rlQosSinglePolicerStatisticsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosSinglePolicerStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies statistics counters per QoS meter "
    ::= { rlQosStatistics 2 }

rlQosSinglePolicerStatisticsEntry OBJECT-TYPE
    SYNTAX RlQosSinglePolicerStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes counter per meter. The index is port represent by                 RlQosMeterStatisticsPort and RlQosMeterStatisticsPolicerPointer. In each entry there are fields representing whether the counter for the meter is enabled and two counters value - for in-profile bytes and for out-of-profile bytes. "
    INDEX { rlIfIndex, rlQosPolicerIndex }
    ::= { rlQosSinglePolicerStatisticsTable 1 }

RlQosSinglePolicerStatisticsEntry::= SEQUENCE {
        rlQosSinglePolicerStatisticsInProfileCounterValue     Counter64,
        rlQosSinglePolicerStatisticsInProfileCntrNumOfBits    StatisticsCntrNumOfBitsType,
        rlQosSinglePolicerStatisticsOutProfileCounterValue    Counter64,
        rlQosSinglePolicerStatisticsOutProfileCntrNumOfBits   StatisticsCntrNumOfBitsType,
        rlQosSinglePolicerStatisticsStatus                    RowStatus
}

rlQosSinglePolicerStatisticsInProfileCounterValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        " Counter value of in profile traffic."
    ::= { rlQosSinglePolicerStatisticsEntry 1 }

rlQosSinglePolicerStatisticsInProfileCntrNumOfBits       OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits for in profile counter."
    ::= { rlQosSinglePolicerStatisticsEntry 2 }

rlQosSinglePolicerStatisticsOutProfileCounterValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        " Counter value of Out Profile traffic."
    ::= { rlQosSinglePolicerStatisticsEntry 3 }

rlQosSinglePolicerStatisticsOutProfileCntrNumOfBits       OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits for out profile counter."
    ::= { rlQosSinglePolicerStatisticsEntry 4 }

rlQosSinglePolicerStatisticsStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of a table entry.
         It is used to delete an entry from this table."
    ::= { rlQosSinglePolicerStatisticsEntry 5 }


rlQosAggregatePolicerStatisticsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosAggregatePolicerStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies statistics counters per QoS aggregate meter "
    ::= { rlQosStatistics 3 }

rlQosAggregatePolicerStatisticsEntry OBJECT-TYPE
    SYNTAX RlQosAggregatePolicerStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes counter per aggregate meter.
        The index is rlQosPolicerIndex.
        In each entry there are fields representing whether the counter for the
        meter is enabled and three counters values - for green, yellow and red
        profiles bytes. "
    INDEX { rlQosPolicerIndex }
    ::= { rlQosAggregatePolicerStatisticsTable 1 }

RlQosAggregatePolicerStatisticsEntry::= SEQUENCE {
        rlQosAggregatePolicerStatisticsInProfileCounterValue      Counter64,
        rlQosAggregatePolicerStatisticsInProfileCntrNumOfBits     StatisticsCntrNumOfBitsType,
        rlQosAggregatePolicerStatisticsOutProfileCounterValue     Counter64,
        rlQosAggregatePolicerStatisticsOutProfileCntrNumOfBits    StatisticsCntrNumOfBitsType,
        rlQosAggregatePolicerStatisticsStatus                     RowStatus
}

rlQosAggregatePolicerStatisticsInProfileCounterValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter value of In Profile amount of bytes."
    ::= { rlQosAggregatePolicerStatisticsEntry 1}

rlQosAggregatePolicerStatisticsInProfileCntrNumOfBits       OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits for In Profile ."
    ::= { rlQosAggregatePolicerStatisticsEntry 2 }

rlQosAggregatePolicerStatisticsOutProfileCounterValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        " Counter value of Out Profile amount of bytes."
    ::= { rlQosAggregatePolicerStatisticsEntry 3 }

rlQosAggregatePolicerStatisticsOutProfileCntrNumOfBits       OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits for Out Profile."
    ::= { rlQosAggregatePolicerStatisticsEntry 4 }

rlQosAggregatePolicerStatisticsStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of a table entry.
         It is used to delete an entry from this table."
    ::= { rlQosAggregatePolicerStatisticsEntry 5 }

rlQosOutQueueStatisticsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosOutQueueStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies statistics counters per VLAN/Port/Queue/Drop Precedence "
    ::= { rlQosStatistics 4 }

rlQosOutQueueStatisticsEntry OBJECT-TYPE
    SYNTAX RlQosOutQueueStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes counter per any permutation of
        Port/VLAN/Queue/Drop Precedence. Each of the above can a group off 'All'.
        The index is port represent by rlQosOutQueueStatisticsCountrID.
        In each entry there are fields representing
        whether the counter is enabled and counters value. "
    INDEX {rlQosOutQueueStatisticsCountrID}
    ::= { rlQosOutQueueStatisticsTable 1 }

RlQosOutQueueStatisticsEntry::= SEQUENCE {
       rlQosOutQueueStatisticsCountrID                 INTEGER,
       rlQosOutQueueStatisticsIfIndexList              PortList,
       rlQosOutQueueStatisticsPortAll                  TruthValue,
       rlQosOutQueueStatisticsVlan                     INTEGER,
       rlQosOutQueueStatisticsVlanAll                  TruthValue,
       rlQosOutQueueStatisticsQueue                    INTEGER,
       rlQosOutQueueStatisticsQueueAll                 TruthValue,
       rlQosOutQueueStatisticsDP                       StatisticsDPType,
       rlQosOutQueueStatisticsDPAll                    TruthValue,
       rlQosOutQueueStatisticsCounterTailDropValue     Counter64,
       rlQosOutQueueStatisticsCounterAllValue          Counter64,
       rlQosOutQueueStatisticsCntrNumOfBits            StatisticsCntrNumOfBitsType,
       rlQosOutQueueStatisticsStatus                   RowStatus
}

rlQosOutQueueStatisticsCountrID OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Counter id, the key of the table."
    ::= { rlQosOutQueueStatisticsEntry  1 }

rlQosOutQueueStatisticsIfIndexList OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Port for which the flow is counted."
    ::= { rlQosOutQueueStatisticsEntry 2 }

rlQosOutQueueStatisticsPortAll  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication for whether the port is configured as range of all the ports"
    ::= {rlQosOutQueueStatisticsEntry  3 }

rlQosOutQueueStatisticsVlan OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "VLAN for which the flow is counted."
    ::= { rlQosOutQueueStatisticsEntry  4 }

rlQosOutQueueStatisticsVlanAll  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication for whether the VLAN is configured as range of all the VLANS"
    ::= { rlQosOutQueueStatisticsEntry  5 }

rlQosOutQueueStatisticsQueue OBJECT-TYPE
    SYNTAX INTEGER(1..8)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Queue for which the flow is counted."
    ::= { rlQosOutQueueStatisticsEntry  6 }


rlQosOutQueueStatisticsQueueAll  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication for whether the queue is configured as range of all the Queues"
    ::= { rlQosOutQueueStatisticsEntry  7 }

rlQosOutQueueStatisticsDP OBJECT-TYPE
    SYNTAX StatisticsDPType
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Drop Precedence for which the flow is counted."
    ::= { rlQosOutQueueStatisticsEntry  8 }

rlQosOutQueueStatisticsDPAll  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication for whether the DP is configured as range of all the DPs"
    ::= { rlQosOutQueueStatisticsEntry  9}


rlQosOutQueueStatisticsCounterTailDropValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The counter for tail dropped value."
    ::= { rlQosOutQueueStatisticsEntry  10 }

rlQosOutQueueStatisticsCounterAllValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The counter for all traffic value."
    ::= { rlQosOutQueueStatisticsEntry  11 }

rlQosOutQueueStatisticsCntrNumOfBits       OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits for the counter."
    ::= { rlQosOutQueueStatisticsEntry 12 }

rlQosOutQueueStatisticsStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of a table entry.
         It is used to delete an entry from this table."
    ::= { rlQosOutQueueStatisticsEntry  13 }


-- Global Counter for statistics

rlQosGlobalStatisticsCntrsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosGlobalStatisticsCntrsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies statistics global counters  for specific rules for all ports
        that they are connected to "
    ::= { rlQosStatistics 5 }

rlQosGlobalStatisticsCntrsEntry OBJECT-TYPE
    SYNTAX RlQosGlobalStatisticsCntrsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry represents global counter."
    INDEX {rlQosGlobalStatisticsCntrsType}
    ::= { rlQosGlobalStatisticsCntrsTable 1 }

RlQosGlobalStatisticsCntrsEntry::= SEQUENCE {
       rlQosGlobalStatisticsCntrsType            StatisticsCntrType,
       rlQosGlobalStatisticsCntrsNumOfBits       StatisticsCntrNumOfBitsType,
       rlQosGlobalStatisticsCntrsCounterValue    Counter64,
       rlQosGlobalStatisticsStatus               RowStatus
}

rlQosGlobalStatisticsCntrsType          OBJECT-TYPE
    SYNTAX StatisticsCntrType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter type."
    ::= { rlQosGlobalStatisticsCntrsEntry 1 }

rlQosGlobalStatisticsCntrsNumOfBits          OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits."
    ::= { rlQosGlobalStatisticsCntrsEntry 2 }

rlQosGlobalStatisticsCntrsCounterValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter value."
    ::= { rlQosGlobalStatisticsCntrsEntry 3 }

rlQosGlobalStatisticsStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of a table entry.
         It is used to delete an entry from this table."
    ::= { rlQosGlobalStatisticsCntrsEntry 4 }

    -- clear scalar

rlQosClearCounters OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This scalar indicates to clear all the counters."
    ::= { rlQosStatistics 6 }

-- CLI QoS Classifier Utilization

    rlQosClassifierUtilization OBJECT IDENTIFIER
      ::= { rlQosCliMib 36 }

    rlQosClassifierUtilizationTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF RlQosClassifierUtilizationEntry
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "A table containing Classifier utilization information.
           Each row represents objects for a particular Unit
           present in this system."
      ::= { rlQosClassifierUtilization 1 }

    rlQosClassifierUtilizationEntry OBJECT-TYPE
      SYNTAX         RlQosClassifierUtilizationEntry
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "A Single entry containing Classifier utilization information."
      INDEX          { rlQosClassifierUtilizationUnitId }
      ::= { rlQosClassifierUtilizationTable 1 }

    RlQosClassifierUtilizationEntry ::= SEQUENCE {
      rlQosClassifierUtilizationUnitId            Unsigned32,
      rlQosClassifierUtilizationPercent           Unsigned32,
      rlQosClassifierUtilizationRulesNumber       Unsigned32,
      rlQosClassifierUtilizationFreeRulesNumber   Unsigned32
    }

     rlQosClassifierUtilizationUnitId OBJECT-TYPE
      SYNTAX         Unsigned32  (1..4294967295)
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "The Unit ID of this Classifier. must be unique per entry.
            This is an index into the table."
      ::= { rlQosClassifierUtilizationEntry 1 }


    rlQosClassifierUtilizationPercent OBJECT-TYPE
      SYNTAX         Unsigned32  (0..100)
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "The classifier utilization percentage. "
      DEFVAL { 0 }
      ::= { rlQosClassifierUtilizationEntry 2 }

   rlQosClassifierUtilizationRulesNumber OBJECT-TYPE
      SYNTAX         Unsigned32  (0..4294967295)
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "The classifier utilization number of used rules, in short rules resolution."
      DEFVAL { 0 }
      ::= { rlQosClassifierUtilizationEntry 3 }

   rlQosClassifierUtilizationFreeRulesNumber OBJECT-TYPE
      SYNTAX         Unsigned32  (0..4294967295)
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "The classifier utilization number of not used yet rules on the unit, in short rules resolution."
      DEFVAL { 0 }
      ::= { rlQosClassifierUtilizationEntry 4 }

rlQosClassifierUtilizationSystem OBJECT-TYPE
    SYNTAX         Unsigned32  (0..100)
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "The system classifier utilization percentage. "
      ::= { rlQosClassifierUtilization 2 }

rlQosClassifierRulesNumberUtilizationSystem OBJECT-TYPE
    SYNTAX         Unsigned32  (0..4294967295)
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "Number of used rules per system, in short rule resolution "
      ::= { rlQosClassifierUtilization 3 }

rlQosClassifierFreeRulesNumUtilizationSystem OBJECT-TYPE
   SYNTAX         Unsigned32  (0..4294967295)
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "Number of free rules per system, in short rule resolution "
      ::= { rlQosClassifierUtilization 4 }

rlQosClassifierMaxRulesNumberUtilizationSystem OBJECT-TYPE
    SYNTAX         Unsigned32  (0..4294967295)
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "Maximum number of rules per system, in short rule resolution "
      ::= { rlQosClassifierUtilization 5 }



-- CLI QoS Port to Profile Mapping Table

rlQosPortToProfileMappingTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosPortToProfileMappingEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table maps between port and profile"
    ::= { rlQosCliMib 37 }

rlQosPortToProfileMappingEntry OBJECT-TYPE
    SYNTAX RlQosPortToProfileMappingEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes
         mapping between port and profile"
    INDEX { rlQosPort }
    ::= { rlQosPortToProfileMappingTable 1 }

RlQosPortToProfileMappingEntry ::= SEQUENCE {
        rlQosPort                   INTEGER,
        rlQosProfileName            DisplayString
    }

rlQosPort OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Port number"
    ::= { rlQosPortToProfileMappingEntry 1 }

rlQosProfileName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "profile"
    ::= { rlQosPortToProfileMappingEntry 2 }



rlQosCPUSafeGuardEnable OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This scalar enables/disables CPU Safeguard."
    ::= { rlQosCliMib 38 }

--QoS Policy Class map priotiry refernce table


rlQosPolicyClassPriorityRefTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosPolicyClassPriorityRefEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The relationship
         between policy map to class map"
    ::= { rlQosCliMib 39 }


rlQosPolicyClassPriorityRefEntry OBJECT-TYPE
    SYNTAX RlQosPolicyClassPriorityRefEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the connection
         between class-map entry to policy map by using pointers.
         The index is Class map pointer
         represent by rlQosPolicyClassRefClassPointer.
         It is also specifies the class-map priotiry in the policy-map, which set the
         rules order within the policy-map"
    INDEX { rlQosPolicyClassPriorityRefPriority, rlQosPolicyClassPriorityRefClassPointer}
    ::= { rlQosPolicyClassPriorityRefTable 1 }

RlQosPolicyClassPriorityRefEntry ::= SEQUENCE {
    rlQosPolicyClassPriorityRefPriority        INTEGER,
    rlQosPolicyClassPriorityRefClassPointer    INTEGER,
    rlQosPolicyClassPriorityRefPolicyPointer   INTEGER,
    rlQosPolicyClassPriorityRefStatus          RowStatus
    }

rlQosPolicyClassPriorityRefPriority OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The class-map priority within the policy-map"
    ::= { rlQosPolicyClassPriorityRefEntry 1 }

rlQosPolicyClassPriorityRefClassPointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Class-map index Pointer"
    ::= { rlQosPolicyClassPriorityRefEntry 2 }

rlQosPolicyClassPriorityRefPolicyPointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Policy map index Pointer"
    ::= { rlQosPolicyClassPriorityRefEntry 3 }

rlQosPolicyClassPriorityRefStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosPolicyClassPriorityRefEntry 4 }

rlQosDenyAceStatisticsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosDenyAceStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table holds statistics for deny ACEs."
    ::= { rlQosCliMib 42 }

rlQosDenyAceStatisticsEntry  OBJECT-TYPE
    SYNTAX RlQosDenyAceStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table holds number of hits for deny ACEs
         attached to specific Interface."
    INDEX { rlQosDenyAceStatisticsIfIndex }
    ::= { rlQosDenyAceStatisticsTable 1 }

RlQosDenyAceStatisticsEntry ::= SEQUENCE {
        rlQosDenyAceStatisticsIfIndex      INTEGER,
        rlQosDenyAceStatisticsIfCounter    INTEGER
    }

rlQosDenyAceStatisticsIfIndex      OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Interface Index."
    ::= { rlQosDenyAceStatisticsEntry  1 }

rlQosDenyAceStatisticsIfCounter    OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "Number of hits on deny ACEs for this interface."
    ::= { rlQosDenyAceStatisticsEntry  2 }

rlQosDenyAceStatisticsOtherFlowCounter OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of hits on deny ACEs for 'Other'-type flow."
    ::= { rlQosCliMib  43 }

rlQosDenyAceStatisticsClearIfCounters OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Keeps ifIndex a port or trunk or vlan that
         its hit counters should be reset.
                 If the value is 0 then all interfaces counters must be reset. "
    ::= { rlQosCliMib 44 }

rlQosDenyAceStatisticsClearOtherFlowCounter OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This scalar indicates clearing 'Other'-type flow counter operation."
    ::= { rlQosCliMib 45 }

rlQosModeGlobalCfgTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosModeGlobalCfgEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table responsible to set the global qos mode configuration:
        qos mode, qos trust mode, and if port are trusted by default in qos advanced
        mode."
    ::= { rlQosCliMib 46 }

rlQosModeGlobalCfgEntry OBJECT-TYPE
    SYNTAX RlQosModeGlobalCfgEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table responsible to set the global qos mode configuration:
        qos mode, qos trust mode, and if port are trusted by default in qos advanced
        mode.
        Current implemnetaion assumes only one entry exist."
    INDEX { rlQosGlobalIndex}
    ::= { rlQosModeGlobalCfgTable 1 }

RlQosModeGlobalCfgEntry ::= SEQUENCE {
    rlQosGlobalIndex                  INTEGER,
    rlQosGlobalQoSMode                QosGlobalMode,
    rlQosBasicGlobalTrustMode         QosTrustMode,
    rlQosAdvcGlobalTrustMode          QosTrustMode,
    rlQoSPortTrustAdvancedMode        TruthValue,
    rlQosDscpMutationEnable           TruthValue,
    rlQosModeGlobalCfgStatus          RowStatus
    }

rlQosGlobalIndex OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entry index - currenly only one entry can exist, indexes hard coded with value '1'."
    ::= { rlQosModeGlobalCfgEntry 1 }

rlQosGlobalQoSMode OBJECT-TYPE
    SYNTAX     QosGlobalMode
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This field replaces deprecated scalar rlQosCliQosMode.
        Defines the global qos operation mode: disable, basic or advnaced. "
    ::= { rlQosModeGlobalCfgEntry 2 }

rlQosBasicGlobalTrustMode OBJECT-TYPE
    SYNTAX     QosTrustMode
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This field replaces deprecated scalar rlQosCliBasicModeCfg.
        Defines the global qos trust operation mode relevant for qos basic mode. "
    ::= { rlQosModeGlobalCfgEntry 3 }

rlQosAdvcGlobalTrustMode OBJECT-TYPE
    SYNTAX     QosTrustMode
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This field replaces deprecated scalar rlQosCliBasicModeCfg.
        Defines the global qos trust operation mode relevant for qos advanced mode. "
    ::= { rlQosModeGlobalCfgEntry 4 }

rlQoSPortTrustAdvancedMode OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This field specified whether ports are set to trused or not-trusted by
        default when switching to qos advanced mode."
    DEFVAL{ false }
    ::= { rlQosModeGlobalCfgEntry 5 }

rlQosDscpMutationEnable  OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This field indicates if dscp to dscp mutation mode is enable.
        It can be set to true in the following terms:
        1.rlQosGlobalTrustMode is in {dscp, vpt-dscp} ( rlQosGlobalQoSMode must be basic or advanced)
        2.if rlQosGlobalQoSMode is advanced then rlQoSPortTrustAdvancedMode must be set to true."
    DEFVAL{ false }
    ::= { rlQosModeGlobalCfgEntry 6 }

rlQosModeGlobalCfgStatus OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This status of entry action.
        In current implementation only one entry exist, therefor only status = active is
        acceptable."
    ::= { rlQosModeGlobalCfgEntry 7 }

-- ClassMapCounterTable
rlQosClassMapCounterTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlQosClassMapCounterEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The  table is used to show statistics for
         ACL applied on an interface."
    ::= { rlQosCliMib 47 }

rlQosClassMapCounterEntry OBJECT-TYPE
    SYNTAX  RlQosClassMapCounterEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This entry returns the value of the class map counter.
        Entry is added/deleted to this MIB when counting is enabled/disabled
        on the class map.
        The counter is set to zero upon reading its value."
    INDEX  {  rlQosClassMapIndex }
    ::= { rlQosClassMapCounterTable 1 }

RlQosClassMapCounterEntry ::= SEQUENCE {
    rlQosClassMapCounterValue           Counter64
}
rlQosClassMapCounterValue OBJECT-TYPE
    SYNTAX     Counter64
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This field returns the current value of the class map counter. "
    ::= { rlQosClassMapCounterEntry 2 }

--- rlQosApplicationTrapIdTable
rlQosApplicationTrapIdTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlQosApplicationTrapIdEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The  read only table is used to get the trapId
        assisated to application wants to use the trap action in
        the class map table"
    ::= { rlQosCliMib 48 }

rlQosApplicationTrapIdEntry OBJECT-TYPE
    SYNTAX  RlQosApplicationTrapIdEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This entry holds the trapId for application using the trap
        action in the class map table."
    INDEX  { IMPLIED rlQosApplicationName }
    ::= { rlQosApplicationTrapIdTable 1 }

RlQosApplicationTrapIdEntry ::= SEQUENCE {
    rlQosApplicationName           DisplayString,
    rlQosApplicationTrapId         INTEGER
}
rlQosApplicationName OBJECT-TYPE
    SYNTAX     DisplayString(SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This field represents the application name and traffic type. "
    ::= { rlQosApplicationTrapIdEntry 1 }

rlQosApplicationTrapId OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This field defines the trap id to be use in the class map entry. "
    ::= { rlQosApplicationTrapIdEntry 2 }

-- RevitalR 1-Feb-2012: add new scalar to define application-specific default action
rlQoSApplicationDefaultAction OBJECT-TYPE
    SYNTAX     RlQosApplicationDefaultActionType
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This scalar specifies application-specific default action"
    ::= { rlQosCliMib 49 }

rlQosLogInputInterfacesAceMatchedTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosLogInputInterfacesAceMatchedEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table holds a list and  of ACE matched log-input option interfaces."
    ::= { rlQosCliMib 50 }

rlQosLogInputInterfacesAceMatchedEntry  OBJECT-TYPE
    SYNTAX RlQosLogInputInterfacesAceMatchedEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table holds only one entry of port list and vlan list."
    INDEX { rlQosLogInputInterfacesAceMatchedIndex }
    ::= { rlQosLogInputInterfacesAceMatchedTable 1 }

RlQosLogInputInterfacesAceMatchedEntry ::= SEQUENCE {
        rlQosLogInputInterfacesAceMatchedIndex                  INTEGER,
        rlQosLogInputInterfacesAceMatchedPorts                  PortList,
        rlQosLogInputInterfacesAceMatchedVlanList1to1024        VlanList1,
        rlQosLogInputInterfacesAceMatchedVlanList1025to2048     VlanList2,
        rlQosLogInputInterfacesAceMatchedVlanList2049to3072     VlanList3,
        rlQosLogInputInterfacesAceMatchedVlanList3073to4094     VlanList4
    }

rlQosLogInputInterfacesAceMatchedIndex      OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
     "An index is entrie's sequence."
    ::= { rlQosLogInputInterfacesAceMatchedEntry  1 }


rlQosLogInputInterfacesAceMatchedPorts  OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "the matched log-input ACEs port list"
    ::= { rlQosLogInputInterfacesAceMatchedEntry 2}

rlQosLogInputInterfacesAceMatchedVlanList1to1024 OBJECT-TYPE
   SYNTAX      VlanList1
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
     "the matched log-input ACEs vlan list from 1 to 1024."

   ::= { rlQosLogInputInterfacesAceMatchedEntry 3}

rlQosLogInputInterfacesAceMatchedVlanList1025to2048 OBJECT-TYPE
   SYNTAX      VlanList2
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
     "the matched log-input ACEs vlan list from 1025 to 2048."

   ::= { rlQosLogInputInterfacesAceMatchedEntry 4}


rlQosLogInputInterfacesAceMatchedVlanList2049to3072 OBJECT-TYPE
   SYNTAX      VlanList3
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
     "the matched log-input ACEs vlan list from 2049 to 3072."

   ::= { rlQosLogInputInterfacesAceMatchedEntry 5}

rlQosLogInputInterfacesAceMatchedVlanList3073to4094 OBJECT-TYPE
   SYNTAX      VlanList4
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
     "the matched log-input ACEs vlan list from 3073 to 4094."

   ::= { rlQosLogInputInterfacesAceMatchedEntry 6}


-- rlQosCosProfileTable
rlQosCosProfileTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosCosProfileEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION        "This table specifies the Cos to queue map per-profile table"
    ::= { rlQosCliMib 51 }

rlQosCosProfileEntry OBJECT-TYPE
    SYNTAX RlQosCosProfileEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION        "Each entry in this table describes a QoS profile. The indices are 
         Application index, represented by rlQosCosProfileAppIndex
	 Profile index, represent by rlQosCosProfileIndex 
	 and CoS represent by rlQosCosProfileCosIndex"
    INDEX { rlQosCosProfileAppIndex, rlQosCosProfileIndex , rlQosCosProfileCosIndex }
    ::= { rlQosCosProfileTable 1 }

RlQosCosProfileEntry::= SEQUENCE {
	rlQosCosProfileAppIndex     INTEGER,	
        rlQosCosProfileIndex        INTEGER,
        rlQosCosProfileCosIndex     INTEGER,
	rlQosCosProfileEgressCos    INTEGER,
        rlQosCosProfileEgressQueue  INTEGER
--        rlQosCosProfileEgressDSCP      INTEGER,
--        rlQosCosProfileEgressDP        INTEGER,
    }

rlQosCosProfileAppIndex OBJECT-TYPE
    SYNTAX INTEGER 
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION        "Application index."
    ::= { rlQosCosProfileEntry 1 }

rlQosCosProfileIndex    OBJECT-TYPE
    SYNTAX INTEGER 
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION        "Profile index per-application."
    ::= { rlQosCosProfileEntry 2 }

rlQosCosProfileCosIndex OBJECT-TYPE
    SYNTAX INTEGER (0..7)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION        "CoS value of an incoming packet."
    ::= { rlQosCosProfileEntry 3 }

rlQosCosProfileEgressCos OBJECT-TYPE
    SYNTAX INTEGER (0..7)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION        "CoS value to (optionally) set in 802.1p User Priority field of matching packets."
    ::= { rlQosCosProfileEntry 4 }

rlQosCosProfileEgressQueue OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION        
        "Traffic class queue assigned to matching packets."
    ::= { rlQosCosProfileEntry 5 }

-- rlQosCosProfileEgressDSCP OBJECT-TYPE
--    SYNTAX INTEGER (0..63)
--    MAX-ACCESS read-write
--    STATUS current
--    DESCRIPTION
--        "DSCP value to (optionally) set in IP header of matching packets."
--    ::= { rlQosCosProfileEntry 6 }

-- rlQosCosProfileEgressDP OBJECT-TYPE
--    SYNTAX INTEGER (0..2)
--    MAX-ACCESS read-write
--    STATUS current
--    DESCRIPTION
--        "Drop precedence assigned to matching packets."
--    ::= { rlQosCosProfileEntry 7 }

-- rlQosCosProfileInterfaceTable
rlQosCosProfileInterfaceTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosCosProfileInterfaceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION        "This table specifies the Cos profile per-interface"
    ::= { rlQosCliMib 52 }

rlQosCosProfileInterfaceEntry OBJECT-TYPE
    SYNTAX RlQosCosProfileInterfaceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION        "Each entry in this table describes a CoS profile for an interface"
    INDEX { rlQosCosProfileInterfaceIfIndex }
    ::= { rlQosCosProfileInterfaceTable 1 }

RlQosCosProfileInterfaceEntry::= SEQUENCE {
	rlQosCosProfileInterfaceIfIndex             InterfaceIndex,
	rlQosCosProfileInterfaceAppIndex            INTEGER,	
        rlQosCosProfileInterfaceCosProfileIndex     INTEGER
    }

rlQosCosProfileInterfaceIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex 
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION        "Interface index."
    ::= { rlQosCosProfileInterfaceEntry 1 }

rlQosCosProfileInterfaceAppIndex OBJECT-TYPE
    SYNTAX INTEGER 
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION        "Application index."
    ::= { rlQosCosProfileInterfaceEntry 2 }

rlQosCosProfileInterfaceCosProfileIndex    OBJECT-TYPE
    SYNTAX INTEGER 
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION        "CoS-Profile index per-application."
    ::= { rlQosCosProfileInterfaceEntry 3 }

-- QoS Access Control List bound interfaces table

rlQosAclBoundIfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosAclBoundIfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies per ACL its bound interfaces"
    ::= { rlQosCliMib 53 }

rlQosAclBoundIfEntry OBJECT-TYPE
    SYNTAX RlQosAclBoundIfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the interfaces bound to ACL,
		 Ports and Vlans.
         The index is represented by rlQosAclBoundIfAclId"
    INDEX { rlQosAclBoundIfAclId }
    ::= { rlQosAclBoundIfTable 1 }

RlQosAclBoundIfEntry ::= SEQUENCE {
    rlQosAclBoundIfAclId			      INTEGER,        
	rlQosAclBoundedIfPortsList			  PortList,
	rlQosAclBoundedIfVlansList1to1024     VlanList1,
    rlQosAclBoundedIfVlansList1025to2048  VlanList2,
    rlQosAclBoundedIfVlansList2049to3072  VlanList3,
    rlQosAclBoundedIfVlansList3073to4094  VlanList4
    }

rlQosAclBoundIfAclId OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Acl index"
    ::= { rlQosAclBoundIfEntry 1 }

rlQosAclBoundedIfPortsList OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-only
    STATUS current  
    DESCRIPTION
       "Ports list bounded to Acl "
    ::= { rlQosAclBoundIfEntry 2 }
 
rlQosAclBoundedIfVlansList1to1024 OBJECT-TYPE
   SYNTAX      VlanList1
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
     "Vlan list bounded to Acl from 1 to 1024."
   ::= { rlQosAclBoundIfEntry 3}

rlQosAclBoundedIfVlansList1025to2048 OBJECT-TYPE
   SYNTAX      VlanList2
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
     "Vlan list bounded to Acl from 1025 to 2048."
   ::= { rlQosAclBoundIfEntry 4}

rlQosAclBoundedIfVlansList2049to3072 OBJECT-TYPE
   SYNTAX      VlanList3
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
     "Vlan list bounded to Acl from 2048 to 3072."
   ::= { rlQosAclBoundIfEntry 5}

rlQosAclBoundedIfVlansList3073to4094 OBJECT-TYPE
   SYNTAX      VlanList4
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
     "Vlan list bounded to Acl from 3073 to 4094."
   ::= { rlQosAclBoundIfEntry 6}


END

