RADLAN-DNSCL-MIB DEFINITIONS ::= BEGIN

-- Title:                RADLAN DNSCL Private Extension
--                       This Private MIB supports the DNS Client for ROS
-- Version:              7.60
-- Date:                 20-May-2012



IMPORTS
    MODULE-IDENTITY,OBJECT-TYPE,
    IpAddress, Unsigned32, Integer32        FROM SNMPv2-SMI
    rnd                                     FROM RADLAN-MIB
    dnsResConfigSbeltEntry                  FROM DNS-RESOLVER-MIB
    DnsName, DnsType                        FROM DNS-SERVER-MIB
    DisplayString, TEXTUAL-CONVENTION,
    TruthValue, RowStatus                   FROM SNMPv2-TC
    dns, DnsName, DnsNameAsIndex, DnsClass,
    DnsType, DnsQClass, DnsQType, DnsTime,
    DnsOpCode, DnsRespCode                  FROM DNS-SERVER-MIB
    InetAddress, InetAddressType            FROM INET-ADDRESS-MIB
    InterfaceIndex, ifIndex                 FROM IF-MIB;

-------------------------------------------------------------------------------
-- new MIBS definitions to support DHCPv6 --
-------------------------------------------------------------------------------

rlDnsCl MODULE-IDENTITY
      LAST-UPDATED "201304010000Z"  -- April 1, 2013
      ORGANIZATION "Marvell Semiconductor, Inc."
      CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
      DESCRIPTION
              "The MIB module describes the private MIB for DNS supported
               by Marvell MTS software and products."      
      REVISION     "201304010000Z"  -- April 1, 2013
      DESCRIPTION
              "Added MODULE-IDENTITY"
      ::= { rnd 93  }
      
      
-- domain name table
rlDnsClv2DomainNameTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlDnsClv2DomainNameEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
     "The domain names table for DNS client ver2."
    ::= { rlDnsCl 14 }

rlDnsClv2DomainNameEntry OBJECT-TYPE
    SYNTAX RlDnsClv2DomainNameEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
     "The row definition for this table."
    INDEX { rlDnsClv2DomainNameSource,
            rlDnsClv2DomainNameIfIndex,
            rlDnsClv2DomainNamePreference,
            rlDnsClv2DomainNameName }
    ::= { rlDnsClv2DomainNameTable 1 }

RlDnsClv2DomainNameEntry ::= SEQUENCE {
    rlDnsClv2DomainNameSource         INTEGER,
    rlDnsClv2DomainNameIfIndex        InterfaceIndex,
    rlDnsClv2DomainNamePreference     Integer32,
    rlDnsClv2DomainNameName           DnsNameAsIndex,
    rlDnsClv2DomainNameRowStatus      RowStatus
}

rlDnsClv2DomainNameSource OBJECT-TYPE
    SYNTAX INTEGER {
        static(1),
        dhcpv6(3),
        dhcpv4(4)
    }
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
       "The domain name source. 'static' if defined by user through CLI,
        'dhcpv6' or 'dhcpv4' if received by DHCP network protocol."
    DEFVAL  { static }
    ::=   { rlDnsClv2DomainNameEntry 1 }

rlDnsClv2DomainNameIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS  current
    DESCRIPTION
        "The IfIndex from which the domain-name configuration was received,
         for static entries, value will always be 1."
    DEFVAL { 1 }
    ::=   { rlDnsClv2DomainNameEntry 2 }

rlDnsClv2DomainNamePreference OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This value identifies the preference of domain-name,
         The lower the value, the more desirable the resolver considers this
         domain-name in domain-search-list."
    ::= { rlDnsClv2DomainNameEntry 3 }

rlDnsClv2DomainNameName OBJECT-TYPE
    SYNTAX DnsNameAsIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Domain-name name."
    ::=   { rlDnsClv2DomainNameEntry 4 }

rlDnsClv2DomainNameRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The row status variable, used according to
         row installation and removal conventions."
    ::= { rlDnsClv2DomainNameEntry 5 }
--------------------------------------------------------------------------------
-- DNS name-servers table
--------------------------------------------------------------------------------
rlDnsClv2ServersTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlDnsClv2ServersEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The DNS servers table for DNS client ver2."
    ::= { rlDnsCl 15 }

rlDnsClv2ServersEntry OBJECT-TYPE
    SYNTAX RlDnsClv2ServersEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The row definition for this table."
    INDEX { rlDnsClv2ServersSource,
            rlDnsClv2ServersIfIndex,
            rlDnsClv2ServersPreference,
            rlDnsClv2ServersAddrType ,
            rlDnsClv2ServersInetAddr,
            rlDnsClv2ServersSubTree,
            rlDnsClv2ServersClass }
    ::= { rlDnsClv2ServersTable 1 }

RlDnsClv2ServersEntry ::= SEQUENCE {
    rlDnsClv2ServersSource         INTEGER,
    rlDnsClv2ServersIfIndex        InterfaceIndex,
    rlDnsClv2ServersPreference     Integer32,
    rlDnsClv2ServersAddrType       InetAddressType,
    rlDnsClv2ServersInetAddr       InetAddress,
    rlDnsClv2ServersSubTree        DnsNameAsIndex,
    rlDnsClv2ServersClass          DnsClass,
    rlDnsClv2ServersRowStatus      RowStatus
}

rlDnsClv2ServersSource OBJECT-TYPE
    SYNTAX INTEGER {
        static(1),
        dhcpv6(3),
        dhcpv4(4)
    }
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The DNS servers source. Static if defined by user through CLI,
         dhcpv6 or dhcpv4 if received by network protocol DHCPv6 or DHCPv4."
    DEFVAL  { static }
    ::=   { rlDnsClv2ServersEntry 1 }

rlDnsClv2ServersIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS  current
    DESCRIPTION
        "The IfIndex from which the DNS-server configuration was received,
         for static entries, value will always be 1."
    DEFVAL { 1 }
    ::=   { rlDnsClv2ServersEntry 2 }

rlDnsClv2ServersPreference OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS not-accessible
    STATUS  current
    DESCRIPTION
        "This value identifies the preference for the name server
         identified in this row of the table.  The lower the
         value, the more desirable the resolver considers this
         server."
    ::=   { rlDnsClv2ServersEntry 3 }

    rlDnsClv2ServersAddrType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The address type of rlDnsClv2ServersInetAddr.  Only
         IPv4, IPv4z, IPv6, and IPv6z addresses are expected, or
         unknown(0) if datagrams for all local IP addresses are
         accepted."
   ::= { rlDnsClv2ServersEntry 4 }

rlDnsClv2ServersInetAddr OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP address of the name server identified by
         this row of the table."
    ::= { rlDnsClv2ServersEntry 5 }

rlDnsClv2ServersSubTree OBJECT-TYPE
    SYNTAX DnsNameAsIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Queries sent to the name server identified by this row
         of the table are limited to those for names in the name
         subtree identified by this variable.  If no such
         limitation applies, the value of this variable is the
         name of the root domain (a DNS name consisting of a
         single zero octet)."
    ::= { rlDnsClv2ServersEntry 6 }

rlDnsClv2ServersClass OBJECT-TYPE
    SYNTAX DnsClass
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The class of DNS queries that will be sent to the server
         identified by this row of the table."
    ::= { rlDnsClv2ServersEntry 7 }

rlDnsClv2ServersRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
    ::= { rlDnsClv2ServersEntry 8 }

--------------------------------------------------------------------------------
-- DNS fixed addresses table
--------------------------------------------------------------------------------
rlDnsClv2FixedTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlDnsClv2FixedEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Read-Only MIB for 'fixed' DNS names.
         when a DNS entry is fixed, a refresh operation is invoked periodically,
         to make sure the entry is kept 'warm' in the DNS cache.
         if the refresh operation fails, the DNSCL will enter a polling state,
         and will retry to resolve the entry again in constant intervals.
         polling-interval duration for unresolved entries is configurable
         by MIB scalar 'rlDnsClMinPollingInterval'."
    ::= { rlDnsCl 16}

rlDnsClv2FixedEntry OBJECT-TYPE
    SYNTAX RlDnsClv2FixedEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The row definition for this table."
    INDEX { rlDnsClv2FixedName,
            rlDnsClv2FixedType }
    ::= { rlDnsClv2FixedTable 1 }

RlDnsClv2FixedEntry ::= SEQUENCE {
    rlDnsClv2FixedName          DnsNameAsIndex,
    rlDnsClv2FixedType          DnsType,
    rlDnsClv2FixedPrettyName    DnsName,
    rlDnsClv2FixedState         INTEGER,
    rlDnsClv2FixedCounter       Integer32,
    rlDnsClv2FixedTTL           DnsTime,
    rlDnsClv2FixedTTRefresh     DnsTime,
    rlDnsClv2FixedTTPolling     DnsTime
}

rlDnsClv2FixedName OBJECT-TYPE
    SYNTAX DnsNameAsIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "DNS name of FIXED domain name"
    ::= { rlDnsClv2FixedEntry 1 }

rlDnsClv2FixedType OBJECT-TYPE
    SYNTAX DnsType
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "requested type of Resource Record
       for the current resolved fixed entry.
       for e.g - A (IPv4), AAAA (IPv6)"
    ::= { rlDnsClv2FixedEntry 2 }

rlDnsClv2FixedPrettyName OBJECT-TYPE
    SYNTAX DnsName
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "Name of the RR at this row in the table.  This is
       identical to the rlDnsClv2FixedName variable, except that
       character case is preserved in this variable, per DNS
       conventions."
   REFERENCE
       "RFC-1035 section 2.3.3."
    ::= { rlDnsClv2FixedEntry 3 }

rlDnsClv2FixedState OBJECT-TYPE
    SYNTAX INTEGER {
        init(1),
        ready(2),
        resolving(3),
        refreshing(4),
        polling(5)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "current state of fixed entry.
       unresolved entries are in 'polling' state."
    ::= { rlDnsClv2FixedEntry 4 }

rlDnsClv2FixedCounter OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "Number of 'fix' requests for this DNS name & type"
    ::= { rlDnsClv2FixedEntry 5 }

rlDnsClv2FixedTTL OBJECT-TYPE
    SYNTAX DnsTime
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "Remaining TTL of resolved fixed entry"
    ::= { rlDnsClv2FixedEntry 6 }

rlDnsClv2FixedTTRefresh OBJECT-TYPE
    SYNTAX DnsTime
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "Remaining time-to-refresh of resolved fixed entry"
    ::= { rlDnsClv2FixedEntry 7 }

rlDnsClv2FixedTTPolling OBJECT-TYPE
    SYNTAX DnsTime
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "Remaining polling-interval time of unresolved fixed entry"
    ::= { rlDnsClv2FixedEntry 8 }

--------------------------------------------------------------------------------
-- Clear DNS action MIB
--------------------------------------------------------------------------------
rlDnsClv2ClearCacheTable OBJECT-TYPE
    SYNTAX  INTEGER {
        staticOnly(1),
        dynamicOnly(2),
        all(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "action MIB for clearing DNS cache tables,
        'static' option will clear all statically configured hostname-to-IP mappings,
        'dynamic' option will clear both negative & positive cache from dynamic (DNS) entries,
        'all' will clear all entries (static & dynamic) in static, positive & negative cache."
    ::= { rlDnsCl 17 }

--------------------------------------------------------------------------------
-- DNS Read-Only Unified Cache Table
--------------------------------------------------------------------------------
rlDnsClv2UnifiedCacheTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlDnsClv2UnifiedCacheEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Unified DNS Cache Table (static,dynamic & fixed entries).
       This is a read-only MIB for presentation purposes."
    ::= { rlDnsCl 18 }

rlDnsClv2UnifiedCacheEntry OBJECT-TYPE
    SYNTAX RlDnsClv2UnifiedCacheEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The row definition for this table."
    INDEX { rlDnsClv2UnifiedCacheName,     -- Hostname
            rlDnsClv2UnifiedCacheSource,   -- Static/Dynamic/Fixed
            rlDnsClv2UnifiedCacheState,    -- OK/NE/??
            rlDnsClv2UnifiedCacheType,     -- NoResolution/IPv6/IPv4
            rlDnsClv2UnifiedCacheIndex }
    ::= { rlDnsClv2UnifiedCacheTable 1 }

RlDnsClv2UnifiedCacheEntry ::= SEQUENCE {
    -- keys
    rlDnsClv2UnifiedCacheName               DnsNameAsIndex,
    rlDnsClv2UnifiedCacheSource             INTEGER,   -- Static/Dynamic/Fixed
    rlDnsClv2UnifiedCacheState              INTEGER,   -- OK/NE/??
    rlDnsClv2UnifiedCacheType               INTEGER,
    rlDnsClv2UnifiedCacheIndex              Integer32,
    -- fields
    rlDnsClv2UnifiedCacheInetAddrType       InetAddressType,
    rlDnsClv2UnifiedCacheInetAddr           InetAddress,
    rlDnsClv2UnifiedCacheTTL                DnsTime,
    rlDnsClv2UnifiedCacheRemainingTTL       DnsTime,
    rlDnsClv2UnifiedCachePrettyName         DnsName
}

-- keys:
rlDnsClv2UnifiedCacheName OBJECT-TYPE
    SYNTAX DnsNameAsIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The requested domain name"
    ::= { rlDnsClv2UnifiedCacheEntry 1 }

rlDnsClv2UnifiedCacheSource OBJECT-TYPE
    SYNTAX INTEGER {
        static(1),
        dynamic(2),
        fixed(3)
    }
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The cache entry source (static/dynamic/fixed)."
    ::= { rlDnsClv2UnifiedCacheEntry 2 }

rlDnsClv2UnifiedCacheState OBJECT-TYPE
    SYNTAX INTEGER {
        ok(1), -- positive,
        ne(2), -- negative
        un(3)  -- unresolved
    }
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The state of the current cache entry"
    ::= { rlDnsClv2UnifiedCacheEntry 3 }

rlDnsClv2UnifiedCacheType OBJECT-TYPE
    SYNTAX INTEGER {
        ipv6(1),
        ipv4(2)
    }
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "IP address type of the Resource Record in the cache which is
       identified in this row of the table.
       for negative/unresolved entries the 'noResolution' value is returned."
    ::= { rlDnsClv2UnifiedCacheEntry 4 }

rlDnsClv2UnifiedCacheIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "A value which makes entries in the table unique when the
       other index values do not provide a unique index."
    ::= { rlDnsClv2UnifiedCacheEntry 5 }

-- fields :
rlDnsClv2UnifiedCacheInetAddrType OBJECT-TYPE
    SYNTAX InetAddressType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "The INET address type of rlDnsClv2UnifiedCacheInetAddr,
       for e.g IPv4, IPv6, IPv6z or UNKNOWN"
    ::= { rlDnsClv2UnifiedCacheEntry 6 }

rlDnsClv2UnifiedCacheInetAddr OBJECT-TYPE
    SYNTAX InetAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "Resolved IP Address of given Domain-Name"
    ::= { rlDnsClv2UnifiedCacheEntry 7 }

rlDnsClv2UnifiedCacheTTL OBJECT-TYPE
    SYNTAX DnsTime
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "Time-To-Live of RR in DNS cache.  This is the initial
       TTL value which was received with the RR when it was originally received.
       for unresolved entries, will return the polling interval instead of TTL"
    ::= { rlDnsClv2UnifiedCacheEntry 8 }

rlDnsClv2UnifiedCacheRemainingTTL OBJECT-TYPE
    SYNTAX DnsTime
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "Remaining TTL seconds since RR was received.
       For unresolved entries, will return remaining time till next retry"
    ::= { rlDnsClv2UnifiedCacheEntry 9 }

rlDnsClv2UnifiedCachePrettyName OBJECT-TYPE
   SYNTAX      DnsName
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "Name of the RR at this row in the table.  This is
           identical to the rlDnsClv2UnifiedCacheName variable, except that
           character case is preserved in this variable, per DNS
           conventions."
   REFERENCE
           "RFC-1035 section 2.3.3."
   ::= { rlDnsClv2UnifiedCacheEntry 10 }

-------------------------------------------------------------------------------
-- End of new MIBS definitions to support DHCPv6
-------------------------------------------------------------------------------

rlDnsClMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "MIB's version, the current version is 1."
::= { rlDnsCl 1 }

rlDnsClEnable OBJECT-TYPE
    SYNTAX INTEGER{
       enable(1),
       disable(2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
       "Enable or Disable the use of the DNS client feature."
    ::=  { rlDnsCl 2 }

rlDnsClDomainNameTable OBJECT-TYPE
   SYNTAX SEQUENCE OF RlDnsClDomainNameEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
    "The domain names table."
     ::= { rlDnsCl 3}

rlDnsClDomainNameEntry  OBJECT-TYPE
   SYNTAX RlDnsClDomainNameEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
     " The row definition for this table."
   INDEX { rlDnsClDomainNameName }
   ::= { rlDnsClDomainNameTable  1 }

RlDnsClDomainNameEntry  ::= SEQUENCE {
    rlDnsClDomainNameName           DnsNameAsIndex,
    rlDnsClDomainNameOwner          INTEGER,
    rlDnsClDomainNameRowStatus      RowStatus
}

rlDnsClDomainNameName OBJECT-TYPE
   SYNTAX DnsNameAsIndex
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
     "The domain name for this ifIndex."
     ::= { rlDnsClDomainNameEntry 1 }

rlDnsClDomainNameOwner OBJECT-TYPE
    SYNTAX  INTEGER{
           static(1),
           dhcp(2),
           dhcpv6(3)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The Domain Name owner. Static if Domain Name defined by user, dhcp
        if received by boot protocol like DHCP."
    DEFVAL  { static }
    ::=   { rlDnsClDomainNameEntry 2 }

rlDnsClDomainNameRowStatus  OBJECT-TYPE
    SYNTAX   RowStatus
    MAX-ACCESS   read-write
    STATUS   current
    DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
    ::= { rlDnsClDomainNameEntry 3 }

rlDnsClMaxNumOfRetransmissions OBJECT-TYPE
    SYNTAX      INTEGER (0..100)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The maximum number of retransmissions for each query."
    DEFVAL      { 1 }
::= { rlDnsCl 4 }

rlDnsClMinRetransmissionInterval OBJECT-TYPE
    SYNTAX      INTEGER (1..3600)
    MAX-ACCESS      read-write
    STATUS      current
    DESCRIPTION
        "The minimum number of seconds that must elapsed before
         retransmission for each query."
    DEFVAL      { 2 }
::= { rlDnsCl 5 }

rlDnsClNamesTable OBJECT-TYPE
   SYNTAX SEQUENCE OF RlDnsClNamesEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
    "The Names table."
     ::= { rlDnsCl 6}

rlDnsClNamesEntry  OBJECT-TYPE
   SYNTAX RlDnsClNamesEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
       " The row definition for this table."
   INDEX { rlDnsClNamesName,
           rlDnsClNamesOwner,
           rlDnsClNamesIndex }
   ::= { rlDnsClNamesTable 1 }

RlDnsClNamesEntry  ::= SEQUENCE {
  rlDnsClNamesName          DnsNameAsIndex,
  rlDnsClNamesOwner         INTEGER,
  rlDnsClNamesIndex         Integer32,
  rlDnsClNamesAddr          IpAddress,
  rlDnsClNamesRowStatus     RowStatus
}

rlDnsClNamesName OBJECT-TYPE
   SYNTAX     DnsNameAsIndex
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
       "The host name."
     ::= { rlDnsClNamesEntry 1 }

rlDnsClNamesOwner OBJECT-TYPE
    SYNTAX  INTEGER{
           static(1),
           dhcp(2),
           dhcpv6(3)
    }
    MAX-ACCESS not-accessible
    STATUS  current
    DESCRIPTION
       "The Host Name Entry owner. Static if  Host Name Entry defined by user, dhcp
        if received by boot protocol like DHCP."
    DEFVAL  { static }
    ::=   { rlDnsClNamesEntry 2 }

rlDnsClNamesIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A value which makes entries in the table unique when the
            other index values (rlDnsClNamesName) do not
            provide a unique index."
    ::= { rlDnsClNamesEntry 3 }

rlDnsClNamesAddr OBJECT-TYPE
   SYNTAX     IpAddress
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
       "The host IP address"
     ::=  { rlDnsClNamesEntry 4 }

rlDnsClNamesRowStatus  OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlDnsClNamesEntry 5 }


 -- rlDnsResConfigSbeltExtTable

rlDnsResConfigSbeltExtTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF RlDnsResConfigSbeltExtEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Augmenting rlDnsResConfigSbeltTable (dns resolver safety belt table)
         for added info"
    ::= {rlDnsCl 7 }

rlDnsResConfigSbeltExtEntry OBJECT-TYPE
    SYNTAX     RlDnsResConfigSbeltExtEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A row of the table rlDnsResConfigSbeltTable Extended
         by this definition."
    AUGMENTS { dnsResConfigSbeltEntry }
    ::= {rlDnsResConfigSbeltExtTable  1 }

RlDnsResConfigSbeltExtEntry  ::= SEQUENCE {
  rlDnsResConfigSbeltOwner         INTEGER
}

rlDnsResConfigSbeltOwner OBJECT-TYPE
    SYNTAX  INTEGER{
           static(1),
           dhcp(2),
           dhcpv6(3)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The DNS server Entry owner. Static if DNS server Entry defined by user, dhcp
        if received by boot protocol like DHCP."
    DEFVAL  { static }
    ::=   { rlDnsResConfigSbeltExtEntry 1 }


 -- rlDnsClNamesInetTable

rlDnsClNamesInetTable OBJECT-TYPE
   SYNTAX SEQUENCE OF RlDnsClNamesInetEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
    "The Names table."
     ::= { rlDnsCl 8}

rlDnsClNamesInetEntry  OBJECT-TYPE
   SYNTAX RlDnsClNamesInetEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
       " The row definition for this table."
   INDEX { rlDnsClNamesInetName,
           rlDnsClNamesInetOwner,
           rlDnsClNamesInetIndex,
           rlDnsClNamesInetRRType }
   ::= { rlDnsClNamesInetTable 1 }

RlDnsClNamesInetEntry  ::= SEQUENCE {
  rlDnsClNamesInetName          DnsNameAsIndex,
  rlDnsClNamesInetOwner         INTEGER,
  rlDnsClNamesInetIndex         Integer32,
  rlDnsClNamesInetRRType        DnsType,
  rlDnsClNamesInetAddrType      InetAddressType,
  rlDnsClNamesInetAddr          InetAddress,
  rlDnsClNamesInetRowStatus     RowStatus
}

rlDnsClNamesInetName OBJECT-TYPE
   SYNTAX     DnsNameAsIndex
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
       "The host name."
     ::= { rlDnsClNamesInetEntry 1 }

rlDnsClNamesInetOwner OBJECT-TYPE
    SYNTAX  INTEGER{
           static(1),
           dhcp(2),
           dhcpv6(3)
    }
    MAX-ACCESS not-accessible
    STATUS  current
    DESCRIPTION
       "The Host Name Entry owner. Static if  Host Name Entry defined by user, dhcp
        if received by boot protocol like DHCP."
    DEFVAL  { static }
    ::=   { rlDnsClNamesInetEntry 2 }

rlDnsClNamesInetIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A value which makes entries in the table unique when the
            other index values (rlDnsClNamesName) do not
            provide a unique index."
    ::= { rlDnsClNamesInetEntry 3 }

rlDnsClNamesInetRRType OBJECT-TYPE
       SYNTAX      DnsType
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "DNS type of the Resource Record in the cache which is
               identified in this row of the table. The user can configure 'a' or 'aaaa' types only."
       ::= { rlDnsClNamesInetEntry 4 }

rlDnsClNamesInetAddrType OBJECT-TYPE
       SYNTAX     InetAddressType
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
              "The address type of rlDnsResNCacheErrInetSource.  Only
               IPv4, IPv4z, IPv6, and IPv6z addresses are expected, or
               unknown(0) if datagrams for all local IP addresses are
               accepted."
       ::= { rlDnsClNamesInetEntry 5 }

rlDnsClNamesInetAddr OBJECT-TYPE
   SYNTAX     InetAddress
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
       "The host IP address"
     ::=  { rlDnsClNamesInetEntry 6 }

rlDnsClNamesInetRowStatus  OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlDnsClNamesInetEntry 7 }

-- DNS Resolver Safety Belt Inet Table

rlDnsResConfigSbeltInetTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF RlDnsResConfigSbeltInetEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "Table of safety belt information used by the resolver
           when it hasn't got any better idea of where to send a
           query, such as when the resolver is booting or is a stub
           resolver."
   ::= { rlDnsCl 9 }

rlDnsResConfigSbeltInetEntry OBJECT-TYPE
   SYNTAX      RlDnsResConfigSbeltInetEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "An entry in the resolver's Sbelt table.
           Rows may be created or deleted at any time by the DNS
           resolver and by SNMP SET requests.  Whether the values
           changed via SNMP are saved in stable storage across
           `reset' operations is implementation-specific."
   INDEX     { rlDnsResConfigSbeltInetAddrType ,
               rlDnsResConfigSbeltInetAddr,
               rlDnsResConfigSbeltInetSubTree,
               rlDnsResConfigSbeltInetClass }
   ::= { rlDnsResConfigSbeltInetTable 1 }

RlDnsResConfigSbeltInetEntry ::=
   SEQUENCE {
       rlDnsResConfigSbeltInetAddrType
           InetAddressType,
       rlDnsResConfigSbeltInetAddr
           InetAddress,
       rlDnsResConfigSbeltInetName
           DnsName,
       rlDnsResConfigSbeltInetRecursion
           INTEGER,
       rlDnsResConfigSbeltInetPref
           INTEGER,
       rlDnsResConfigSbeltInetSubTree
           DnsNameAsIndex,
       rlDnsResConfigSbeltInetClass
           DnsClass,
       rlDnsResConfigSbeltInetStatus
           RowStatus
   }

rlDnsResConfigSbeltInetAddrType OBJECT-TYPE
   SYNTAX     InetAddressType
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
          "The address type of rlDnsResConfigSbeltInetAddr.  Only
           IPv4, IPv4z, IPv6, and IPv6z addresses are expected, or
           unknown(0) if datagrams for all local IP addresses are
           accepted."
   ::= { rlDnsResConfigSbeltInetEntry 1 }

rlDnsResConfigSbeltInetAddr OBJECT-TYPE
   SYNTAX      InetAddress
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "The IP address of the Sbelt name server identified by
           this row of the table."
   ::= { rlDnsResConfigSbeltInetEntry 2 }

rlDnsResConfigSbeltInetName OBJECT-TYPE
   SYNTAX      DnsName
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
           "The DNS name of a Sbelt nameserver identified by this
           row of the table.  A zero-length string indicates that
           the name is not known by the resolver."
   ::= { rlDnsResConfigSbeltInetEntry 3 }

rlDnsResConfigSbeltInetRecursion OBJECT-TYPE
   SYNTAX      INTEGER { iterative(1),
                         recursive(2),
                         recursiveAndIterative(3) }
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
           "Kind of queries resolver will be sending to the name
           server identified in this row of the table:

           iterative(1) indicates that resolver will be directing
           iterative queries to this name server (RD bit turned
           off).

           recursive(2) indicates that resolver will be directing
           recursive queries to this name server (RD bit turned
           on).

           recursiveAndIterative(3) indicates that the resolver
           will be directing both recursive and iterative queries
           to the server identified in this row of the table."
    ::= { rlDnsResConfigSbeltInetEntry 4 }
rlDnsResConfigSbeltInetPref OBJECT-TYPE
   SYNTAX      INTEGER (0..2147483647)
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
           "This value identifies the preference for the name server
           identified in this row of the table.  The lower the
           value, the more desirable the resolver considers this
           server."
    ::= { rlDnsResConfigSbeltInetEntry 5 }

rlDnsResConfigSbeltInetSubTree OBJECT-TYPE
   SYNTAX      DnsNameAsIndex
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "Queries sent to the name server identified by this row
           of the table are limited to those for names in the name
           subtree identified by this variable.  If no such
           limitation applies, the value of this variable is the
           name of the root domain (a DNS name consisting of a
           single zero octet)."
   ::= { rlDnsResConfigSbeltInetEntry 6 }

rlDnsResConfigSbeltInetClass OBJECT-TYPE
   SYNTAX      DnsClass
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "The class of DNS queries that will be sent to the server
           identified by this row of the table."
   ::= { rlDnsResConfigSbeltInetEntry 7 }

rlDnsResConfigSbeltInetStatus OBJECT-TYPE
   SYNTAX      RowStatus
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
           "Row status column for this row of the Sbelt table."
   ::= { rlDnsResConfigSbeltInetEntry 8 }


-- Resolver Cache Inet Table

rlDnsResCacheRRInetTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF RlDnsResCacheRRInetEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "This table contains information about all the resource
           records currently in the resolver's cache."
   ::= { rlDnsCl 10 }

rlDnsResCacheRRInetEntry OBJECT-TYPE
   SYNTAX      RlDnsResCacheRRInetEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "An entry in the resolvers's cache.  Rows may be created
           only by the resolver.  SNMP SET requests may be used to
           delete rows."
   INDEX     { rlDnsResCacheRRInetName,
               rlDnsResCacheRRInetClass,
               rlDnsResCacheRRInetType,
               rlDnsResCacheRRInetIndex }
   ::= { rlDnsResCacheRRInetTable 1 }

RlDnsResCacheRRInetEntry ::=
   SEQUENCE {
       rlDnsResCacheRRInetName
           DnsNameAsIndex,
       rlDnsResCacheRRInetClass
           DnsClass,
       rlDnsResCacheRRInetType
           DnsType,
       rlDnsResCacheRRInetTTL
           DnsTime,
       rlDnsResCacheRRInetElapsedTTL
           DnsTime,
       rlDnsResCacheRRInetSourceAddrType
           InetAddressType,
       rlDnsResCacheRRInetSource
           InetAddress,
       rlDnsResCacheRRInetData
           OCTET STRING,
       rlDnsResCacheRRInetStatus
           RowStatus,
       rlDnsResCacheRRInetIndex
           Integer32,
       rlDnsResCacheRRInetPrettyName
           DnsName
   }

rlDnsResCacheRRInetName OBJECT-TYPE
   SYNTAX      DnsNameAsIndex
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "Owner name of the Resource Record in the cache which is
           identified in this row of the table.  As described in
           RFC-1034, the owner of the record is the domain name
           were the RR is found."
   REFERENCE
           "RFC-1034 section 3.6."
   ::= { rlDnsResCacheRRInetEntry 1 }

rlDnsResCacheRRInetClass OBJECT-TYPE
   SYNTAX      DnsClass
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "DNS class of the Resource Record in the cache which is
           identified in this row of the table."
   ::= { rlDnsResCacheRRInetEntry 2 }

rlDnsResCacheRRInetType OBJECT-TYPE
   SYNTAX      DnsType
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "DNS type of the Resource Record in the cache which is
           identified in this row of the table."
   ::= { rlDnsResCacheRRInetEntry 3 }

rlDnsResCacheRRInetTTL OBJECT-TYPE
   SYNTAX      DnsTime
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "Time-To-Live of RR in DNS cache.  This is the initial
           TTL value which was received with the RR when it was
           originally received."
   ::= { rlDnsResCacheRRInetEntry 4 }

rlDnsResCacheRRInetElapsedTTL OBJECT-TYPE
   SYNTAX      DnsTime
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "Elapsed seconds since RR was received."
   ::= { rlDnsResCacheRRInetEntry 5 }

rlDnsResCacheRRInetSourceAddrType OBJECT-TYPE
   SYNTAX     InetAddressType
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
          "The address type of rlDnsResCacheRRInetSource.  Only
           IPv4, IPv4z, IPv6, and IPv6z addresses are expected, or
           unknown(0) if datagrams for all local IP addresses are
           accepted."
   ::= { rlDnsResCacheRRInetEntry 6 }

rlDnsResCacheRRInetSource OBJECT-TYPE
   SYNTAX      InetAddress
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "Host from which RR was received, 0.0.0.0 if unknown."
   ::= { rlDnsResCacheRRInetEntry 7 }

rlDnsResCacheRRInetData OBJECT-TYPE
   SYNTAX      OCTET STRING
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "RDATA portion of a cached RR.  The value is in the
           format defined for the particular DNS class and type of
           the resource record."
   REFERENCE
           "RFC-1035 section 3.2.1."
   ::= { rlDnsResCacheRRInetEntry 8 }

rlDnsResCacheRRInetStatus OBJECT-TYPE
   SYNTAX      RowStatus
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
           "Status column for the resolver cache table.  Since only
           the agent (DNS resolver) creates rows in this table, the
           only values that a manager may write to this variable
           are active(1) and destroy(6)."
   ::= { rlDnsResCacheRRInetEntry 9 }

rlDnsResCacheRRInetIndex OBJECT-TYPE
   SYNTAX      Integer32
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "A value which makes entries in the table unique when the
           other index values (rlDnsResCacheRRName,
           rlDnsResCacheRRClass, and rlDnsResCacheRRType) do not
           provide a unique index."
   ::= { rlDnsResCacheRRInetEntry 10 }

rlDnsResCacheRRInetPrettyName OBJECT-TYPE
   SYNTAX      DnsName
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "Name of the RR at this row in the table.  This is
           identical to the rlDnsResCacheRRName variable, except that
           character case is preserved in this variable, per DNS
           conventions."
   REFERENCE
           "RFC-1035 section 2.3.3."
   ::= { rlDnsResCacheRRInetEntry 11 }


-- Resolver Negative Cache Inet Table

rlDnsResNCacheErrInetTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF RlDnsResNCacheErrInetEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "The resolver's negative response cache.  This table
           contains information about authoritative errors that
           have been cached by the resolver."
   ::= { rlDnsCl 11 }

rlDnsResNCacheErrInetEntry OBJECT-TYPE
   SYNTAX      RlDnsResNCacheErrInetEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "An entry in the resolver's negative response cache
           table.  Only the resolver can create rows.  SNMP SET
           requests may be used to delete rows."
   INDEX     { rlDnsResNCacheErrInetQName,
               rlDnsResNCacheErrInetQClass,
               rlDnsResNCacheErrInetQType,
               rlDnsResNCacheErrInetIndex }
   ::= { rlDnsResNCacheErrInetTable 1 }

RlDnsResNCacheErrInetEntry ::=
   SEQUENCE {
       rlDnsResNCacheErrInetQName
           DnsNameAsIndex,
       rlDnsResNCacheErrInetQClass
           DnsQClass,
       rlDnsResNCacheErrInetQType
           DnsQType,
       rlDnsResNCacheErrInetTTL
           DnsTime,
       rlDnsResNCacheErrInetElapsedTTL
           DnsTime,
       rlDnsResNCacheErrInetSourceAddrType
          InetAddressType,
      rlDnsResNCacheErrInetSource
           InetAddress,
       rlDnsResNCacheErrInetCode
           INTEGER,
       rlDnsResNCacheErrInetStatus
           RowStatus,
       rlDnsResNCacheErrInetIndex
           Integer32,
       rlDnsResNCacheErrInetPrettyName
           DnsName
   }

rlDnsResNCacheErrInetQName OBJECT-TYPE
   SYNTAX      DnsNameAsIndex
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "QNAME associated with a cached authoritative error."
   REFERENCE
           "RFC-1034 section 3.7.1."
   ::= { rlDnsResNCacheErrInetEntry 1 }

rlDnsResNCacheErrInetQClass OBJECT-TYPE
   SYNTAX      DnsQClass
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "DNS QCLASS associated with a cached authoritative
           error."
   ::= { rlDnsResNCacheErrInetEntry 2 }

rlDnsResNCacheErrInetQType OBJECT-TYPE
   SYNTAX      DnsQType
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "DNS QTYPE associated with a cached authoritative error."
   ::= { rlDnsResNCacheErrInetEntry 3 }

rlDnsResNCacheErrInetTTL OBJECT-TYPE
   SYNTAX      DnsTime
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "Time-To-Live of a cached authoritative error at the time
           of the error, it should not be decremented by the number
           of seconds since it was received.  This should be the
           TTL as copied from the MINIMUM field of the SOA that
           accompanied the authoritative error, or a smaller value
           if the resolver implements a ceiling on negative
           response cache TTLs."
   REFERENCE
           "RFC-1034 section 4.3.4."
   ::= { rlDnsResNCacheErrInetEntry 4 }

rlDnsResNCacheErrInetElapsedTTL OBJECT-TYPE
   SYNTAX      DnsTime
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "Elapsed seconds since authoritative error was received."
   ::= { rlDnsResNCacheErrInetEntry 5 }

rlDnsResNCacheErrInetSourceAddrType OBJECT-TYPE
   SYNTAX     InetAddressType
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
          "The address type of rlDnsResNCacheErrInetSource.  Only
           IPv4, IPv4z, IPv6, and IPv6z addresses are expected, or
           unknown(0) if datagrams for all local IP addresses are
           accepted."
   ::= { rlDnsResNCacheErrInetEntry 6 }

rlDnsResNCacheErrInetSource OBJECT-TYPE
   SYNTAX      InetAddress
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "Host which sent the authoritative error, 0.0.0.0 if
           unknown."
   ::= { rlDnsResNCacheErrInetEntry 7 }

rlDnsResNCacheErrInetCode OBJECT-TYPE
   SYNTAX      INTEGER { nonexistantName(1), noData(2), other(3), unresolved(4) }
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "The authoritative error that has been cached:

           nonexistantName(1) indicates an authoritative name error
           (RCODE = 3).

           noData(2) indicates an authoritative response with no
           error (RCODE = 0) and no relevant data.

           other(3) indicates some other cached authoritative
           error.  At present, no such errors are known to exist.

           unresolved(4) is used for 'fixed' entries that are currently unresolved."
   ::= { rlDnsResNCacheErrInetEntry 8 }

rlDnsResNCacheErrInetStatus OBJECT-TYPE
   SYNTAX      RowStatus
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
           "Status column for the resolver negative response cache
           table.  Since only the agent (DNS resolver) creates rows
           in this table, the only values that a manager may write
           to this variable are active(1) and destroy(6)."
   ::= { rlDnsResNCacheErrInetEntry 9 }

rlDnsResNCacheErrInetIndex OBJECT-TYPE
   SYNTAX      Integer32
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
           "A value which makes entries in the table unique when the
           other index values (rlDnsResNCacheErrQName,
           rlDnsResNCacheErrQClass, and rlDnsResNCacheErrQType) do not
           provide a unique index."
   ::= { rlDnsResNCacheErrInetEntry 10 }

rlDnsResNCacheErrInetPrettyName OBJECT-TYPE
   SYNTAX      DnsName
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "QNAME associated with this row in the table.  This is
           identical to the rlDnsResNCacheErrQName variable, except
           that character case is preserved in this variable, per
           DNS conventions."
   REFERENCE
           "RFC-1035 section 2.3.3."
   ::= { rlDnsResNCacheErrInetEntry 11 }

 -- rlDnsResConfigSbeltExtInetTable

rlDnsResConfigSbeltExtInetTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF RlDnsResConfigSbeltExtInetEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Augmenting rlDnsResConfigSbeltInetTable (dns resolver safety belt table)
         for added info"
    ::= {rlDnsCl 12 }

rlDnsResConfigSbeltExtInetEntry OBJECT-TYPE
    SYNTAX     RlDnsResConfigSbeltExtInetEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A row of the table rlDnsResConfigSbeltInetTable Extended
         by this definition."
    AUGMENTS { rlDnsResConfigSbeltInetEntry }
    ::= {rlDnsResConfigSbeltExtInetTable  1 }

RlDnsResConfigSbeltExtInetEntry  ::= SEQUENCE {
  rlDnsResConfigSbeltInetOwner         INTEGER
}


rlDnsResConfigSbeltInetOwner OBJECT-TYPE
    SYNTAX  INTEGER{
           static(1),
           dhcp(2),
           dhcpv6(3)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The DNS server Entry owner. Static if DNS server Entry defined by user, dhcp
        if received by boot protocol like DHCP."
    DEFVAL  { static }
    ::=   { rlDnsResConfigSbeltExtInetEntry 1 }

rlDnsClMinPollingInterval OBJECT-TYPE
    SYNTAX      INTEGER (0..3600)
    MAX-ACCESS      read-write
    STATUS      current
    DESCRIPTION
        "The minimum number of seconds that must elapsed between invocations
         of the resolving procedure for fixed DNS entries which are currently
         unresolved."
    DEFVAL      { 0 }
::= { rlDnsCl 13 }

END

