RADLAN-DIGITALKEYMANAGE-MIB DEFINITIONS ::= BEGIN

-- Title:                RADLAN ROS
--                       Private DIGITAL KEY MANAGE MIB
-- Version:              7.50
-- Date:                 26-Jan-2011

IMPORTS
    rnd                                                     FROM RADLAN-MIB
    OBJECT-TYPE, MODULE-IDENTITY                            FROM SNMPv2-SMI
    DisplayString, RowStatus, DateAndTime, TruthValue       FROM SNMPv2-TC;

rlDigitalKeyManage MODULE-IDENTITY
                LAST-UPDATED "200701020000Z"
                ORGANIZATION "Marvell Semiconductor, Inc."
                CONTACT-INFO
					"5488 Marvell Lane
					Santa Clara, CA 95054
					USA

					Website:  www.marvell.com"
                DESCRIPTION
                      "This private MIB module defines digital key manage private MIBs."
                REVISION "200701020000Z"
                DESCRIPTION
                      "Initial revision."
        ::= { rnd 86 }

rlMD5KeyChainTable OBJECT-TYPE
    SYNTAX  SEQUENCE  OF RlMD5KeyChainEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
       "Key-chains and keys"
    ::=   { rlDigitalKeyManage 1 }

rlMD5KeyChainEntry   OBJECT-TYPE
    SYNTAX  RlMD5KeyChainEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
            "Key-chain with key ID that belongs to this chain"
    INDEX  {rlMD5KeyChainName, rlMD5KeyChainKeyId}
    ::=  { rlMD5KeyChainTable 1 }

RlMD5KeyChainEntry ::= SEQUENCE {
    rlMD5KeyChainName                       DisplayString,
    rlMD5KeyChainKeyId                      INTEGER,
    rlMD5KeyChainKey                        DisplayString,
    rlMD5KeyChainKeyStartAccept             DateAndTime,
    rlMD5KeyChainKeyStartGenerate           DateAndTime,
    rlMD5KeyChainKeyStopGenerate            DateAndTime,
    rlMD5KeyChainKeyStopAccept              DateAndTime,
    rlMD5KeyChainKeyValidForAccept          TruthValue,
    rlMD5KeyChainKeyValidForGenerate        TruthValue,
    rlMD5KeyChainRowStatus                  RowStatus
}

rlMD5KeyChainName OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Name of the key-chain to which belongs
         the secret authentication key"
    ::= { rlMD5KeyChainEntry 1 }

rlMD5KeyChainKeyId OBJECT-TYPE
    SYNTAX  INTEGER  (1..255)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A 8-bit identifier for the secret authentication key.
         This identifier unique only for specific key chain"
    ::= { rlMD5KeyChainEntry 2 }

rlMD5KeyChainKey OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..16))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The 128-bit secret authentication key"
    ::= { rlMD5KeyChainEntry 3 }

rlMD5KeyChainKeyStartAccept OBJECT-TYPE
    SYNTAX  DateAndTime
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The time that the router will start accepting packets
          that have been created with the given key"
    DEFVAL   { '00000000'H }
    ::= { rlMD5KeyChainEntry 4 }

rlMD5KeyChainKeyStartGenerate OBJECT-TYPE
    SYNTAX  DateAndTime
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The time that the router will start using the key
         for packet generation"
    DEFVAL   { '00000000'H }
    ::= { rlMD5KeyChainEntry 5 }

rlMD5KeyChainKeyStopGenerate OBJECT-TYPE
    SYNTAX  DateAndTime
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The time that the router will stop using the key
         for packet generation"
    DEFVAL   { 'FFFFFFFF'H }
    ::= { rlMD5KeyChainEntry 6 }

rlMD5KeyChainKeyStopAccept OBJECT-TYPE
    SYNTAX  DateAndTime
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The time that the router will stop accepting packets
          that have been created with the given key"
    DEFVAL   { 'FFFFFFFF'H }
    ::= { rlMD5KeyChainEntry 7 }


rlMD5KeyChainKeyValidForAccept  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "A value of 'true' indicates that given key is valid for
             accepting packets"
    DEFVAL { false }
    ::= { rlMD5KeyChainEntry 8 }

rlMD5KeyChainKeyValidForGenerate  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "A value of 'true' indicates that given key is valid for
             packet generation"
    DEFVAL { false }
    ::= { rlMD5KeyChainEntry 9 }

rlMD5KeyChainRowStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "It is used to insert, update or delete an entry"
    ::= { rlMD5KeyChainEntry 10 }


END

