RADLAN-rlMacMulticast-MIB DEFINITIONS ::= BEGIN

-- Title:      RADLAN Multicast Bridge Configuration
-- Version:    7.46
-- Date:       15-Jan-2007
--

IMPORTS
    TruthValue,TEXTUAL-CONVENTION,
    RowStatus                                            FROM SNMPv2-TC
    VlanIndex,PortList                                   FROM Q-BRIDGE-MIB
    Unsigned32, IpAddress, NOTIFICATION-TYPE,
    OBJECT-TYPE                                          FROM SNMPv2-SMI
    rndErrorDesc, rndErrorSeverity                       FROM RADLAN-DEVICEPARAMS-MIB
    rnd, rlMacMulticast, rndNotifications                FROM RADLAN-MIB
    InetAddressType, InetAddress, InetVersion            FROM INET-ADDRESS-MIB;

-- IGMP Snooping and mac multicast moved here from appolo ,
-- under mac multicast because of historic reasons

rlMacMulticastEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable/Disable MAC Multicast bridging in the device."
    ::= { rlMacMulticast 1 }

rlIgmpSnoop  OBJECT IDENTIFIER ::= { rlMacMulticast 2 }

--
-- rlIgmpSnooping
--

 rlIgmpSnoopMibVersion OBJECT-TYPE
     SYNTAX      INTEGER
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
         "MIB's version, the current version is 3.
          IGMP Snooping supports IGMPv3."
     ::= { rlIgmpSnoop 1 }

rlIgmpSnoopEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable/Disable IGMP Snooping in the switch."
    ::= { rlIgmpSnoop 2 }

rlIgmpSnoopHostAgingTime OBJECT-TYPE
    SYNTAX      INTEGER (0 .. 2147483647 )
    UNITS   "seconds"
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The amount of time that should pass before aging out
         an entry in the rlIgmpSnoopGroupTable will be aged out."
    DEFVAL  {260}
    ::= { rlIgmpSnoop 3 }

rlIgmpSnoopRouterAgingTime OBJECT-TYPE
    SYNTAX      INTEGER (1 .. 2147483647 )
    UNITS   "seconds"
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
    "The amount of time that should pass before aging out
     an entry in the rlIgmpSnoopInterfaceTable will be aged out."
    DEFVAL  {300}
    ::= { rlIgmpSnoop 4 }
--   IgmpSnoopGroupTable - DEPRICATED

-- rlIgmpSnoopGroupTable OBJECT-TYPE
--     SYNTAX      SEQUENCE OF RlIgmpSnoopGroupEntry
--  MAX-ACCESS  not-accessible
--     STATUS      current
--     DESCRIPTION
--         "The (conceptual) table listing the IP multicast groups
--          for which there are members on a particular interface."
--     ::= { rlIgmpSnoop 5 }
--
-- rlIgmpSnoopGroupEntry OBJECT-TYPE
--     SYNTAX      RlIgmpSnoopGroupEntry
--     MAX-ACCESS  not-accessible
--     STATUS      current
--     DESCRIPTION
--         "An entry (conceptual row) in the rlIgmpSnoopGroupTable."
--     INDEX  { rlIgmpSnoopGroupTag, rlIgmpSnoopGroupAddress,
--              rlIgmpSnoopGroupPort}
--     ::= { rlIgmpSnoopGroupTable 1 }
--
-- RlIgmpSnoopGroupEntry ::= SEQUENCE {
--     rlIgmpSnoopGroupTag         INTEGER,
--     rlIgmpSnoopGroupAddress     MacAddress,
--     rlIgmpSnoopGroupPort        INTEGER,
--     rlIgmpSnoopGroupExpiryTime  INTEGER
-- }
--
-- rlIgmpSnoopGroupTag OBJECT-TYPE
--     SYNTAX      INTEGER
--     MAX-ACCESS  read-only
--     STATUS      current
--     DESCRIPTION
--         "The VLAN tag for which this entry contains
--          information for an IP multicast group address."
--     ::= { rlIgmpSnoopGroupEntry 1 }
--
-- rlIgmpSnoopGroupAddress OBJECT-TYPE
--     SYNTAX      MacAddress
--     MAX-ACCESS  read-only
--     STATUS      current
--     DESCRIPTION
--     "The MAC multicast group address for which this entry
--      contains information."
--     ::= { rlIgmpSnoopGroupEntry 2 }
--
-- rlIgmpSnoopGroupPort OBJECT-TYPE
--     SYNTAX      INTEGER
--     MAX-ACCESS  read-only
--     STATUS      current
--     DESCRIPTION
--         "The ifIndex value of the port for which this entry contains
--          information for an IP multicast group address."
--     ::= { rlIgmpSnoopGroupEntry 3 }
--
-- rlIgmpSnoopGroupExpiryTime OBJECT-TYPE
--     SYNTAX      INTEGER
--     MAX-ACCESS  read-only
--     STATUS      current
--     DESCRIPTION
--         "The minimum amount of time remaining before this entry will aged out."
--     ::= { rlIgmpSnoopGroupEntry 4 }

--   rlIgmpSnoopRouterTable - DEPRICATED
-- rlIgmpSnoopRouterTable OBJECT-TYPE
--     SYNTAX      SEQUENCE OF RlIgmpSnoopRouterEntry
--     MAX-ACCESS  not-accessible
--     STATUS      current
--     DESCRIPTION
--         "The (conceptual) table listing the ports for which there are
--          IP Multicast Routers."
--     ::= { rlIgmpSnoop 6 }
--
-- rlIgmpSnoopRouterEntry OBJECT-TYPE
--     SYNTAX      RlIgmpSnoopRouterEntry
--     MAX-ACCESS  not-accessible
--     STATUS      current
--     DESCRIPTION
--         "An entry (conceptual row) in the rlIgmpSnoopRouterTable."
--     INDEX  { rlIgmpSnoopRouterTag, rlIgmpSnoopRouterPort }
--     ::= { rlIgmpSnoopRouterTable 1 }
--
-- RlIgmpSnoopRouterEntry ::= SEQUENCE {
--     rlIgmpSnoopRouterTag        INTEGER,
--     rlIgmpSnoopRouterPort       INTEGER,
--     rlIgmpSnoopRouterExpiryTime INTEGER
-- }
--
-- rlIgmpSnoopRouterTag OBJECT-TYPE
--     SYNTAX      INTEGER
--     MAX-ACCESS  read-only
--     STATUS      current
--     DESCRIPTION
--         "The tag of the VLAN for which this entry contains
--          information for an IP Multicast Router."
--     ::= { rlIgmpSnoopRouterEntry 1 }
--
-- rlIgmpSnoopRouterPort OBJECT-TYPE
--     SYNTAX      INTEGER
--     MAX-ACCESS  read-only
--     STATUS      current
--     DESCRIPTION
--         "The interface for which this entry contains information for
--          an IP multicast Router."
--     ::= { rlIgmpSnoopRouterEntry 2 }
--
-- rlIgmpSnoopRouterExpiryTime OBJECT-TYPE
--     SYNTAX      INTEGER
--     MAX-ACCESS  read-only
--     STATUS      current
--     DESCRIPTION
--         "The minimum amount of time remaining before this entry will aged out."
--     ::= { rlIgmpSnoopRouterEntry 3 }

IgmpVersion ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "IGMP version."
    SYNTAX  INTEGER {
        none(0),
        v1(1),
        v2(2),
        v3(3)
}


-- rlIgmpSnoopVlanTable  changed to Inet type (November 2007)  DEPRICATED (See rlIgmpMldSnoopVlanTable)

 rlIgmpSnoopVlanTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF RlIgmpSnoopVlanEntry
     MAX-ACCESS  not-accessible
     STATUS      obsolete
     DESCRIPTION
         "The table listing the per vlan parameters : enable/disable ,
         aging-out timers , filter ports and permanent ports."
     ::= { rlIgmpSnoop 7 }

 rlIgmpSnoopVlanEntry OBJECT-TYPE
     SYNTAX      RlIgmpSnoopVlanEntry
     MAX-ACCESS  not-accessible
     STATUS      obsolete
     DESCRIPTION
         "An entry (conceptual row) in the rlIgmpSnoopVlanTable."
     INDEX  { rlIgmpSnoopVlanTag }
     ::= { rlIgmpSnoopVlanTable 1 }

RlIgmpSnoopVlanEntry ::= SEQUENCE {
     rlIgmpSnoopVlanTag                  INTEGER,
     rlIgmpSnoopVlanEnable               TruthValue,
     rlIgmpSnoopVlanRouterLearn          TruthValue,
     rlIgmpSnoopVlanHostTimeOut          INTEGER,
     rlIgmpSnoopVlanQuerierTimeOut       INTEGER,
     rlIgmpSnoopVlanRouterTimeOut        INTEGER,
     rlIgmpSnoopVlanLeaveTimeOut         INTEGER,
     rlIgmpSnoopVlanIgmpVersion          IgmpVersion,
     rlIgmpSnoopVlanRouterPortlist       PortList
 }

 rlIgmpSnoopVlanTag OBJECT-TYPE
     SYNTAX      INTEGER
     MAX-ACCESS  read-only
     STATUS      obsolete
     DESCRIPTION
         "The tag of the VLAN for which this entry contains
          information for an IP Multicast Router."
     ::= { rlIgmpSnoopVlanEntry 1 }


 rlIgmpSnoopVlanEnable OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
         "Enable/Disable IGMP Snooping in the vlan."
     ::= { rlIgmpSnoopVlanEntry 2 }

 rlIgmpSnoopVlanRouterLearn OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
         "Enable/Disable of Learning of routers in the vlan."
     ::= { rlIgmpSnoopVlanEntry 3 }

 rlIgmpSnoopVlanHostTimeOut OBJECT-TYPE
     SYNTAX      INTEGER (0 .. 2147483647 )
    UNITS   "seconds"
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
         "The amount of time that should pass before aging out
          an entry in the rlIgmpSnoopMembershipTable for this vlan."
     DEFVAL  {260}
     ::= { rlIgmpSnoopVlanEntry 4 }

 rlIgmpSnoopVlanQuerierTimeOut OBJECT-TYPE
     SYNTAX      INTEGER (1 .. 2147483647 )
    UNITS   "seconds"
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
         "The amount of time where no query is heard until
          querier is activated"
     DEFVAL  {260}
     ::= { rlIgmpSnoopVlanEntry 5 }

 rlIgmpSnoopVlanRouterTimeOut OBJECT-TYPE
     SYNTAX      INTEGER (1 .. 2147483647 )
     UNITS   "seconds"
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
         "The amount of time that should pass before aging out
          a port in the router ports dynamically learnt for
          this vlan."
     DEFVAL  {300}
     ::= { rlIgmpSnoopVlanEntry 6 }

 rlIgmpSnoopVlanLeaveTimeOut OBJECT-TYPE
     SYNTAX      INTEGER (0 .. 2147483647 )
     UNITS   "seconds"
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
         "The amount of time that should pass before aging out
          an entry in the rlIgmpSnoopMembershipTable for this vlan,
          after  recieving a leave/exclude message from the port of
          the entry."
     DEFVAL  {10}
     ::= { rlIgmpSnoopVlanEntry 7 }

rlIgmpSnoopVlanIgmpVersion OBJECT-TYPE
     SYNTAX      IgmpVersion
     MAX-ACCESS  read-only
     STATUS      obsolete
     DESCRIPTION
         "The current IGMP protocol version running on the VLAN."
     ::= { rlIgmpSnoopVlanEntry 8 }

 rlIgmpSnoopVlanRouterPortlist OBJECT-TYPE
     SYNTAX      PortList
     MAX-ACCESS  read-only
     STATUS      obsolete
     DESCRIPTION
         "List of router ports learned dynamically on this VLAN
          from PIM, DVMRP, MRDISC and IGMP Query messages "
     ::= { rlIgmpSnoopVlanEntry 9}

-- rlIgmpSnoopIGMP224ReportsHandle

rlIgmpSnoopIGMP224ReportsHandle OBJECT-TYPE
   SYNTAX  INTEGER {
        allow(1),
        ignore (2)
    }
    MAX-ACCESS   read-write
    STATUS   current
    DESCRIPTION
       "This varaiable indicates whether to allow IGMP reports for groups in the
        224.0.0.X range when the group address is already manually configured or to ignore."
    ::= {  rlIgmpSnoop 8 }

-- rlIgmpSnoopMrouterEnabled - DEPRICATED
-- rlIgmpSnoopMrouterEnabled OBJECT-TYPE
--     SYNTAX  TruthValue
--     MAX-ACCESS  read-only
--     STATUS  current
--     DESCRIPTION
--         "Indicates whether the device functions as a multicast router."
--     ::= {  rlIgmpSnoop 9 }

--  rlIgmpSnoopMulticastTvTable  converted to Inet  (See rlIgmpMldSnoopMulticastTvTable)

rlIgmpSnoopMulticastTvTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlIgmpSnoopMulticastTvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " multicast vlan used for this port"
    ::= { rlIgmpSnoop 10 }

rlIgmpSnoopMulticastTvEntry OBJECT-TYPE
   SYNTAX      RlIgmpSnoopMulticastTvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " entry of multicast ip"
    INDEX   { rlIgmpSnoopMulticastTvVID, rlIgmpSnoopMulticastTvGroup }
    ::= { rlIgmpSnoopMulticastTvTable 1 }

RlIgmpSnoopMulticastTvEntry ::= SEQUENCE {
        rlIgmpSnoopMulticastTvVID           VlanIndex,
        rlIgmpSnoopMulticastTvGroup         IpAddress,
        rlIgmpSnoopMulticastTvStatus        RowStatus,
        rlIgmpSnoopMulticastTvCount         INTEGER
    }

rlIgmpSnoopMulticastTvVID OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "Specify the multicast ip to be used."
    ::= { rlIgmpSnoopMulticastTvEntry  1 }

rlIgmpSnoopMulticastTvGroup OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "Specify the multicast ip to be used."
    ::= { rlIgmpSnoopMulticastTvEntry  2 }

rlIgmpSnoopMulticastTvStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "The row status variable, used according to
        row installation and removal conventions."
    ::= { rlIgmpSnoopMulticastTvEntry 3 }

 rlIgmpSnoopMulticastTvCount OBJECT-TYPE
     SYNTAX      INTEGER (1 .. 268435456 )
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
         "The number of addresses starting with rlIgmpSnoopMulticastTvGroup."
     DEFVAL  {1}
     ::= { rlIgmpSnoopMulticastTvEntry 4 }

--  rlIgmpSnoopMembershipTable  changed to Inet type (November 2007)   (See rlIgmpMldSnoopMembershipTable)

rlIgmpSnoopMembershipTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlIgmpSnoopMembershipEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table listing the IP multicast memberships."
    ::= { rlIgmpSnoop 11 }

rlIgmpSnoopMembershipEntry OBJECT-TYPE
    SYNTAX      RlIgmpSnoopMembershipEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlIgmpSnoopMembershipTable."
    INDEX  { rlIgmpSnoopMembershipVlanTag, rlIgmpSnoopMembershipGroupIpAddress, rlIgmpSnoopMembershipSourceIpAddress }
    ::= { rlIgmpSnoopMembershipTable 1 }

RlIgmpSnoopMembershipEntry ::= SEQUENCE {
    rlIgmpSnoopMembershipVlanTag            VlanIndex,
    rlIgmpSnoopMembershipGroupIpAddress     IpAddress,
    rlIgmpSnoopMembershipSourceIpAddress    IpAddress,
    rlIgmpSnoopMembershipIncPortlist        PortList,
    rlIgmpSnoopMembershipExcPortlist        PortList,
    rlIgmpSnoopMembershipExpiryTime         INTEGER,
    rlIgmpSnoopMembershipCompatibilityMode  IgmpVersion
}

rlIgmpSnoopMembershipVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The VLAN tag for which this entry contains multicast membership information."
    ::= { rlIgmpSnoopMembershipEntry 1}

rlIgmpSnoopMembershipGroupIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The multicast group address."
    ::= { rlIgmpSnoopMembershipEntry 2}

rlIgmpSnoopMembershipSourceIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The unicast source address."
    ::= { rlIgmpSnoopMembershipEntry 3}

rlIgmpSnoopMembershipIncPortlist OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Included ports, where a report message was heard for the group
         (IGMP version 2|1) or group and source address (IGMP version 3)."
    ::= { rlIgmpSnoopMembershipEntry 4}

rlIgmpSnoopMembershipExcPortlist OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Excluded ports where an exclude report message
         was heard for the group and source address (IGMP version 3). "
    ::= { rlIgmpSnoopMembershipEntry 5}

rlIgmpSnoopMembershipExpiryTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "Time till entry will expire."
    ::= { rlIgmpSnoopMembershipEntry 6}

rlIgmpSnoopMembershipCompatibilityMode OBJECT-TYPE
    SYNTAX      IgmpVersion
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IGMP group compatibility mode."
    ::= { rlIgmpSnoopMembershipEntry 7 }


-- rlIgmpSnoopQuerierVlanTable  changed to Inet type (November 2007)  See rlIgmpMldSnoopQuerierVlanTable

rlIgmpSnoopQuerierVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlIgmpSnoopQuerierVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A table that contains IGMP Snooping Querier information about
        every vlan. This is indexed by vlan tag."
    ::= { rlIgmpSnoop 12 }

rlIgmpSnoopQuerierVlanEntry OBJECT-TYPE
    SYNTAX      RlIgmpSnoopQuerierVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlIgmpSnoopQuerierVlanTable."
    INDEX  { rlIgmpSnoopQuerierVlanTag }
    ::= { rlIgmpSnoopQuerierVlanTable 1 }

RlIgmpSnoopQuerierVlanEntry ::= SEQUENCE {
    rlIgmpSnoopQuerierVlanTag                       VlanIndex,
    rlIgmpSnoopQuerierAdminEnable                   TruthValue,
    rlIgmpSnoopQuerierOperEnable                    TruthValue,
    rlIgmpSnoopQuerierAdminAddr                     IpAddress,
    rlIgmpSnoopQuerierOperAddr                      IpAddress,
    rlIgmpSnoopQuerierAdminVersionNumber            IgmpVersion,
    rlIgmpSnoopQuerierOperVersionNumber             IgmpVersion,
    rlIgmpSnoopQuerierElectionEnable                TruthValue
}

rlIgmpSnoopQuerierVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An IGMP Snoop Querier entry vlan tag."
    ::= { rlIgmpSnoopQuerierVlanEntry 1 }

rlIgmpSnoopQuerierAdminEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The desired administrative state of IGMP Snoop Querier on the vlan."
    ::= { rlIgmpSnoopQuerierVlanEntry 2 }

rlIgmpSnoopQuerierOperEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current operational state of IGMP Snoop Querier on the vlan."
    ::= { rlIgmpSnoopQuerierVlanEntry 3 }

rlIgmpSnoopQuerierAdminAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The desired IP address is being used in IGMP Snoop Querier messages on the vlan."
    ::= { rlIgmpSnoopQuerierVlanEntry 4 }

rlIgmpSnoopQuerierOperAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current operational IP address is being used in IGMP Snoop Querier messages on the vlan."
    ::= { rlIgmpSnoopQuerierVlanEntry 5 }

rlIgmpSnoopQuerierAdminVersionNumber OBJECT-TYPE
    SYNTAX      IgmpVersion
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The highest version number of IGMP Snoop Querier for the vlan."
    ::= { rlIgmpSnoopQuerierVlanEntry 6 }

rlIgmpSnoopQuerierOperVersionNumber OBJECT-TYPE
    SYNTAX      IgmpVersion
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current operational version number of IGMP Snoop Querier for the vlan."
    ::= { rlIgmpSnoopQuerierVlanEntry 7 }

rlIgmpSnoopQuerierElectionEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Whether or not to participate in querier election.
         When true, the snooping querier participates in querier election.
         When false, the snooping querier is the elected querier until a general
         query is heard from another router on the vlan (always lose)."
    ::= { rlIgmpSnoopQuerierVlanEntry 8 }


rlIgmpSnoopQuerierEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Globally enable/disable IGMP Snooping Querier in the switch."
    ::= { rlIgmpSnoop 13 }

--
--
--   rlMacMulticastMaxEntriesNum

rlMacMulticastMaxEntriesNum OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximum number of Mac Multicast entries the device supports."
    ::= { rlMacMulticast 3 }

rlMacMulticastFilter  OBJECT IDENTIFIER ::= { rlMacMulticast 4 }

-- rlMacMulticastUnregFilterEnable
rlMacMulticastUnregFilterEnable OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Each bit represent a port whether Unregistered Multicast Filtering enable "
 ::= { rlMacMulticastFilter  1 }


-- mld
rlMldSnoop  OBJECT IDENTIFIER ::= { rlMacMulticast 5 }
--

rlMldSnoopEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable/Disable Mld Snooping in the switch."
    ::= { rlMldSnoop 1 }

rlMldSnoopHostAgingTime OBJECT-TYPE
    SYNTAX      INTEGER (60 .. 2147483647 )
    UNITS   "seconds"
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The amount of time that should pass before aging out
         an entry in the rlMldSnoopGroupTable will be aged out."
    DEFVAL  {260}
    ::= { rlMldSnoop 2 }

rlMldSnoopRouterAgingTime OBJECT-TYPE
    SYNTAX      INTEGER (1 .. 2147483647 )
    UNITS   "seconds"
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
    "The amount of time that should pass before aging out
     an entry in the rlMldSnoopInterfaceTable will be aged out."
    DEFVAL  {300}
    ::= { rlMldSnoop 3 }

--rlIgmpMldSnoopMembershipTable (replaces rlIgmpSnoopMembershipTable)

rlIgmpMldSnoopMembershipTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlIgmpMldSnoopMembershipEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table listing the IP multicast memberships."
    ::= { rlMldSnoop 4 }

rlIgmpMldSnoopMembershipEntry OBJECT-TYPE
    SYNTAX      RlIgmpMldSnoopMembershipEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlIgmpMldSnoopMembershipTable."
    INDEX  { rlIgmpMldSnoopMembershipVlanTag,
             rlIgmpMldSnoopMembershipGroupIpAddressType,
             rlIgmpMldSnoopMembershipGroupIpAddress,
             rlIgmpMldSnoopMembershipSourceIpAddressType,
             rlIgmpMldSnoopMembershipSourceIpAddress }
    ::= { rlIgmpMldSnoopMembershipTable 1 }

RlIgmpMldSnoopMembershipEntry ::= SEQUENCE {
    rlIgmpMldSnoopMembershipVlanTag             VlanIndex,
    rlIgmpMldSnoopMembershipGroupIpAddressType  InetAddressType,
    rlIgmpMldSnoopMembershipGroupIpAddress      InetAddress,
    rlIgmpMldSnoopMembershipSourceIpAddressType InetAddressType,
    rlIgmpMldSnoopMembershipSourceIpAddress     InetAddress,
    rlIgmpMldSnoopMembershipIncPortlist         PortList,
    rlIgmpMldSnoopMembershipExcPortlist         PortList,
    rlIgmpMldSnoopMembershipExpiryTime          INTEGER,
    rlIgmpMldSnoopMembershipCompatibilityMode   IgmpVersion
}

rlIgmpMldSnoopMembershipVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The VLAN tag for which this entry contains multicast membership information."
    ::= { rlIgmpMldSnoopMembershipEntry 1}

rlIgmpMldSnoopMembershipGroupIpAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type IPv4/IPv6."
    ::= { rlIgmpMldSnoopMembershipEntry 2}

rlIgmpMldSnoopMembershipGroupIpAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The multicast group address."
    ::= { rlIgmpMldSnoopMembershipEntry 3}

rlIgmpMldSnoopMembershipSourceIpAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type IPv4/IPv6."
    ::= { rlIgmpMldSnoopMembershipEntry 4}

rlIgmpMldSnoopMembershipSourceIpAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The unicast source address."
    ::= { rlIgmpMldSnoopMembershipEntry 5}

rlIgmpMldSnoopMembershipIncPortlist OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Included ports, where a report message was heard for the group
         (IGMPv2/V1 or MLDv1) or group and source address (IGMPv3/MLDv2)."
    ::= { rlIgmpMldSnoopMembershipEntry 6}

rlIgmpMldSnoopMembershipExcPortlist OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "list of excluded ports to which an exclude report message
         was heard for the group and source address (IGMPv3/MLDv2 ). "
    ::= { rlIgmpMldSnoopMembershipEntry 7}

rlIgmpMldSnoopMembershipExpiryTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "Time till entry will expire."
    ::= { rlIgmpMldSnoopMembershipEntry 8}

rlIgmpMldSnoopMembershipCompatibilityMode OBJECT-TYPE
    SYNTAX      IgmpVersion
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IGMP/MLD group compatibility mode."
    ::= { rlIgmpMldSnoopMembershipEntry 9 }

-- rlIgmpMldSnoopVlanTable (replaces rlIgmpSnoopVlanTable)

rlIgmpMldSnoopVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlIgmpMldSnoopVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table lists the per vlan parameters : enable/disable ,
        aging-out timers , filter ports and permanent ports."
    ::= { rlMldSnoop 5 }

rlIgmpMldSnoopVlanEntry OBJECT-TYPE
    SYNTAX      RlIgmpMldSnoopVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlIgmpSnoopVlanTable."
    INDEX  { rlIgmpMldSnoopVlanInetAddressType, rlIgmpMldSnoopVlanTag }
    ::= { rlIgmpMldSnoopVlanTable 1 }

RlIgmpMldSnoopVlanEntry ::= SEQUENCE {
    rlIgmpMldSnoopVlanInetAddressType               InetAddressType,
    rlIgmpMldSnoopVlanTag                           INTEGER,
    rlIgmpMldSnoopVlanEnable                        TruthValue,
    rlIgmpMldSnoopVlanRouterLearn                   TruthValue,
    rlIgmpMldSnoopVlanHostTimeOut                   INTEGER,
    rlIgmpMldSnoopVlanQuerierTimeOut                INTEGER,
    rlIgmpMldSnoopVlanRouterTimeOut                 INTEGER,
    rlIgmpMldSnoopVlanLeaveTimeOut                  INTEGER,
    rlIgmpMldSnoopVlanIgmpVersion                   IgmpVersion,
    rlIgmpMldSnoopVlanRouterPortlist                PortList,
    rlIgmpMldSnoopVlanRouterStaticPortlist          PortList,
    rlIgmpMldSnoopVlanRouterForbiddenPortlist       PortList,
    rlIgmpMldSnoopVlanQueryOverride                 TruthValue,
    rlIgmpMldSnoopVlanOperRobustness                Unsigned32,
    rlIgmpMldSnoopVlanOperQueryInterval             Unsigned32,
    rlIgmpMldSnoopVlanOperQueryMaxResponseTime      Unsigned32,
    rlIgmpMldSnoopVlanOperLastMemberQueryInterval   Unsigned32,
    rlIgmpMldSnoopVlanOperLastMemberQueryCount      Unsigned32,
    rlIgmpMldSnoopVlanOperStartupQueryInterval      Unsigned32,
    rlIgmpMldSnoopVlanOperStartupQueryCount         Unsigned32,
    rlIgmpMldSnoopVlanOperHostTimeOut               Unsigned32,
    rlIgmpMldSnoopVlanOperRouterTimeOut             Unsigned32,
    rlIgmpMldSnoopVlanOperLeaveTimeOut              Unsigned32,
    rlIgmpMldSnoopVlanAdminRobustness               Unsigned32,
    rlIgmpMldSnoopVlanAdminQueryInterval            Unsigned32,
    rlIgmpMldSnoopVlanAdminQueryMaxResponseTime     Unsigned32,
    rlIgmpMldSnoopVlanAdminLastMemberQueryInterval  Unsigned32,
    rlIgmpMldSnoopVlanAdminLastMemberQueryCount     Unsigned32,
    rlIgmpMldSnoopVlanAdminStartupQueryInterval     Unsigned32,
    rlIgmpMldSnoopVlanAdminStartupQueryCount        Unsigned32,
    rlIgmpMldSnoopVlanAdminHostTimeOut              Unsigned32,
    rlIgmpMldSnoopVlanAdminRouterTimeOut            Unsigned32,
    rlIgmpMldSnoopVlanAdminLeaveTimeOut             Unsigned32,
    rlIgmpMldSnoopVlanIsImmediateLeave              TruthValue
}

rlIgmpMldSnoopVlanInetAddressType OBJECT-TYPE
     SYNTAX     InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type ipv6/ipv4."
    ::= { rlIgmpMldSnoopVlanEntry 1}

rlIgmpMldSnoopVlanTag OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The tag of the VLAN for which this entry contains
         information for an IP Multicast Router."
    ::= { rlIgmpMldSnoopVlanEntry 2 }


rlIgmpMldSnoopVlanEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable/Disable IGMP Snooping in the vlan."
    ::= { rlIgmpMldSnoopVlanEntry 3 }

rlIgmpMldSnoopVlanRouterLearn OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable/Disable of Learning of routers in the vlan."
    ::= { rlIgmpMldSnoopVlanEntry 4 }

rlIgmpMldSnoopVlanHostTimeOut OBJECT-TYPE
    SYNTAX      INTEGER (60 .. 2147483647 )
    UNITS   "seconds"
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The amount of time that should pass before aging out
         an entry in the rlIgmpSnoopMembershipTable for this vlan."
    DEFVAL  {260}
    ::= { rlIgmpMldSnoopVlanEntry 5 }

rlIgmpMldSnoopVlanQuerierTimeOut OBJECT-TYPE
    SYNTAX      INTEGER (1 .. 2147483647 )
    UNITS   "seconds"
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The amount of time where no query is heard until
         querier is activated"
    DEFVAL  {260}
    ::= { rlIgmpMldSnoopVlanEntry 6 }

rlIgmpMldSnoopVlanRouterTimeOut OBJECT-TYPE
    SYNTAX      INTEGER (1 .. 2147483647 )
    UNITS   "seconds"
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The amount of time that should pass before aging out
         a port in the router ports dynamically learnt for
         this vlan."
    DEFVAL  {300}
    ::= { rlIgmpMldSnoopVlanEntry 7 }

rlIgmpMldSnoopVlanLeaveTimeOut OBJECT-TYPE
    SYNTAX      INTEGER (0 .. 2147483647 )
    UNITS   "seconds"
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The amount of time that should pass before aging out
         an entry in the rlIgmpSnoopMembershipTable for this vlan,
         after  recieving a leave/exclude message from the port of
         the entry."
    DEFVAL  {10}
    ::= { rlIgmpMldSnoopVlanEntry 8 }


rlIgmpMldSnoopVlanIgmpVersion OBJECT-TYPE
    SYNTAX      IgmpVersion
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current IGMP protocol version running on the VLAN."
    ::= { rlIgmpMldSnoopVlanEntry 9 }

rlIgmpMldSnoopVlanRouterPortlist OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "List of router ports learned dynamically
         from PIM, DVMRP, MRDISC, MOSPF and IGMP/MLD Query messages on this VLAN "
    ::= { rlIgmpMldSnoopVlanEntry 10}

rlIgmpMldSnoopVlanRouterStaticPortlist OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "List of router ports configured statically on this VLAN."
    ::= { rlIgmpMldSnoopVlanEntry 11}

rlIgmpMldSnoopVlanRouterForbiddenPortlist OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "List of ports statically configured to NOT
         be router ports on this VLAN"
    ::= { rlIgmpMldSnoopVlanEntry 12}


rlIgmpMldSnoopVlanQueryOverride OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable/Disable overriding of Query values"
    ::= { rlIgmpMldSnoopVlanEntry 13 }

rlIgmpMldSnoopVlanOperRobustness OBJECT-TYPE
    SYNTAX     Unsigned32 (1..255)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The Robustness Variable allows tuning for the expected
            packet loss on a subnet.  If a subnet is expected to be
            lossy, the Robustness Variable may be increased.  IGMP and
            MLD are robust to (Robustness Variable-1) packet losses."
    DEFVAL     { 2 }
    ::= { rlIgmpMldSnoopVlanEntry 14 }

rlIgmpMldSnoopVlanOperQueryInterval OBJECT-TYPE
    SYNTAX     Unsigned32 (1000..31744000)
    UNITS      "milliseconds"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The frequency at which IGMP or MLD Host-Query packets are
            transmitted on this interface. This variable must be a
            non-zero value."
    DEFVAL     { 125000 }
    ::= { rlIgmpMldSnoopVlanEntry 15 }

rlIgmpMldSnoopVlanOperQueryMaxResponseTime OBJECT-TYPE
    SYNTAX     Unsigned32  (0..8387584)
    UNITS      "milliseconds"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The maximum query response interval advertised in MGMDv2
            or v3 queries on this interface."
    REFERENCE "RFC 3810 section 9.3"
    DEFVAL     { 10000 }
    ::= { rlIgmpMldSnoopVlanEntry 16 }

rlIgmpMldSnoopVlanOperLastMemberQueryInterval OBJECT-TYPE
    SYNTAX     Unsigned32  (0..8387584)
    UNITS      "milliseconds"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The Last Member Query Interval is the Max Query Response
            Interval inserted into group-specific queries sent in
            response to leave group messages, and is also the amount
            of time between group-specific query messages.  This value
            may be tuned to modify the leave latency of the network. A
            reduced value results in reduced time to detect the loss of
            the last member of a group.  The value of this object is
            irrelevant if mgmdRouterInterfaceVersion is 1."
    DEFVAL     { 1000 }
    ::= { rlIgmpMldSnoopVlanEntry 17 }

rlIgmpMldSnoopVlanOperLastMemberQueryCount OBJECT-TYPE
    SYNTAX     Unsigned32 (1..255)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "Represents the number of group-specific and
            group-and-source-specific queries sent by the router before
            it assumes there are no local members."
    DEFVAL  { 2 }
    ::= { rlIgmpMldSnoopVlanEntry 18 }

rlIgmpMldSnoopVlanOperStartupQueryInterval OBJECT-TYPE
    SYNTAX     Unsigned32 (0..31744000)
    UNITS      "milliseconds"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "This variable represents the interval between General
            Queries sent by a Querier on startup."
    DEFVAL {0}
    ::= { rlIgmpMldSnoopVlanEntry 19 }

rlIgmpMldSnoopVlanOperStartupQueryCount OBJECT-TYPE
    SYNTAX     Unsigned32 (1..255)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "Represents the number of Queries sent out on startup
            separated by the Startup Query Interval."
    DEFVAL {1}
    ::= { rlIgmpMldSnoopVlanEntry 20 }


rlIgmpMldSnoopVlanOperHostTimeOut OBJECT-TYPE
     SYNTAX      Unsigned32 (0 .. 2147483647 )
    UNITS   "milliseconds"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
         "The amount of time that should pass before aging out
          an entry in the rlIgmpSnoopMembershipTable for this vlan.
          DEFVAL  { rlIgmpMldSnoopVlanOperRobustness *
                    rlIgmpMldSnoopVlanOperQueryInterval +
                    rlIgmpMldSnoopVlanOperQueryMaxResponseTime }"
     ::= { rlIgmpMldSnoopVlanEntry 21 }

rlIgmpMldSnoopVlanOperRouterTimeOut OBJECT-TYPE
     SYNTAX      Unsigned32 (0 .. 2147483647 )
     UNITS   "milliseconds"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
         "The amount of time that should pass before aging out
          a port in the router ports dynamically learnt for
          this vlan.
          DEFVAL  { rlIgmpMldSnoopVlanOperRobustness *
                    rlIgmpMldSnoopVlanOperQueryInterval }"
     ::= { rlIgmpMldSnoopVlanEntry 22 }

rlIgmpMldSnoopVlanOperLeaveTimeOut OBJECT-TYPE
     SYNTAX      Unsigned32 (0 .. 2147483647 )
     UNITS   "milliseconds"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
         "The amount of time that should pass before aging out
          an entry in the rlIgmpSnoopMembershipTable for this vlan,
          after  recieving a leave/exclude message from the port of
          the entry.
          DEFVAL  { rlIgmpMldSnoopVlanOperLastMemberQueryCount *
                    rlIgmpMldSnoopVlanOperLastMemberQueryInterval }"
     ::= { rlIgmpMldSnoopVlanEntry 23 }


rlIgmpMldSnoopVlanAdminRobustness OBJECT-TYPE
    SYNTAX     Unsigned32 (1..7)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
            "The Robustness Variable allows tuning for the expected
            packet loss on a subnet.  If a subnet is expected to be
            lossy, the Robustness Variable may be increased.  IGMP and
            MLD are robust to (Robustness Variable-1) packet losses."
    DEFVAL     { 2 }
    ::= { rlIgmpMldSnoopVlanEntry 24 }

rlIgmpMldSnoopVlanAdminQueryInterval OBJECT-TYPE
    SYNTAX     Unsigned32 (1000..18000000)
    UNITS      "milliseconds"
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
            "The frequency at which IGMP or MLD Host-Query packets are
            transmitted on this interface. This variable must be a
            non-zero value."
    DEFVAL     { 125000 }
    ::= { rlIgmpMldSnoopVlanEntry 25 }

rlIgmpMldSnoopVlanAdminQueryMaxResponseTime OBJECT-TYPE
    SYNTAX     Unsigned32  (1000..20000)
    UNITS      "milliseconds"
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
            "The maximum query response interval advertised in MGMDv2
            or v3 queries on this interface."
    REFERENCE "RFC 3810 section 9.3"
    DEFVAL     { 10000 }
    ::= { rlIgmpMldSnoopVlanEntry 26 }

rlIgmpMldSnoopVlanAdminLastMemberQueryInterval OBJECT-TYPE
    SYNTAX     Unsigned32  (100..25500)
    UNITS      "milliseconds"
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
            "The Last Member Query Interval is the Max Query Response
            Interval inserted into group-specific queries sent in
            response to leave group messages, and is also the amount
            of time between group-specific query messages.  This value
            may be tuned to modify the leave latency of the network. A
            reduced value results in reduced time to detect the loss of
            the last member of a group.  The value of this object is
            irrelevant if mgmdRouterInterfaceVersion is 1."
    DEFVAL     { 1000 }
    ::= { rlIgmpMldSnoopVlanEntry 27 }

rlIgmpMldSnoopVlanAdminLastMemberQueryCount OBJECT-TYPE
    SYNTAX     Unsigned32 (0..7)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
            "Represents the number of group-specific and
            group-and-source-specific queries sent by the router before
            it assumes there are no local members. Value 0 is used to indicate 
             usage of default value. DEFVAL  { rlIgmpMldSnoopVlanAdminRobustness }"
    ::= { rlIgmpMldSnoopVlanEntry 28 }

rlIgmpMldSnoopVlanAdminStartupQueryInterval OBJECT-TYPE
    SYNTAX     Unsigned32 (0..4500000)
    UNITS      "milliseconds"
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
            "This variable represents the interval between General
            Queries sent by a Querier on startup."
    DEFVAL {0}
    ::= { rlIgmpMldSnoopVlanEntry 29 }

rlIgmpMldSnoopVlanAdminStartupQueryCount OBJECT-TYPE
    SYNTAX     Unsigned32 (1..255)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
            "Represents the number of Queries sent out on startup
            separated by the Startup Query Interval."
    DEFVAL {0}
    ::= { rlIgmpMldSnoopVlanEntry 30 }

rlIgmpMldSnoopVlanAdminHostTimeOut OBJECT-TYPE
     SYNTAX      Unsigned32 (0 .. 2147483647 )
     UNITS   "milliseconds"
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
         "The amount of time that should pass before aging out
          an entry in the rlIgmpSnoopMembershipTable for this vlan.
          DEFVAL  { rlIgmpMldSnoopVlanAdminRobustness *
                    rlIgmpMldSnoopVlanAdminQueryInterval +
                    rlIgmpMldSnoopVlanAdminQueryMaxResponseTime }"
     ::= { rlIgmpMldSnoopVlanEntry 31 }

rlIgmpMldSnoopVlanAdminRouterTimeOut OBJECT-TYPE
     SYNTAX      Unsigned32 (0 .. 2147483647 )
     UNITS   "milliseconds"
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
         "The amount of time that should pass before aging out
          a port in the router ports dynamically learnt for
          this vlan.
          DEFVAL  { rlIgmpMldSnoopVlanAdminRobustness *
                    rlIgmpMldSnoopVlanAdminQueryInterval }"
     ::= { rlIgmpMldSnoopVlanEntry 32 }

rlIgmpMldSnoopVlanAdminLeaveTimeOut OBJECT-TYPE
     SYNTAX      Unsigned32 (0 .. 2147483647 )
     UNITS   "milliseconds"
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
         "The amount of time that should pass before aging out
          an entry in the rlIgmpSnoopMembershipTable for this vlan,
          after  recieving a leave/exclude message from the port of
          the entry.
          DEFVAL  { rlIgmpMldSnoopVlanAdminLastMemberQueryCount *
                    rlIgmpMldSnoopVlanAdminLastMemberQueryInterval }"
     ::= { rlIgmpMldSnoopVlanEntry 33 }

rlIgmpMldSnoopVlanIsImmediateLeave OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        " Enable/Disable immediate leave on this Vlan"
    DEFVAL {false}
    ::= { rlIgmpMldSnoopVlanEntry 34 }


-- rlIgmpMldSnoopMulticastTvTable (replaces rlIgmpSnoopMulticastTvTable)

rlIgmpMldSnoopMulticastTvTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlIgmpMldSnoopMulticastTvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " multicast vlan used for this port"
    ::= { rlMldSnoop  6 }

rlIgmpMldSnoopMulticastTvEntry OBJECT-TYPE
    SYNTAX      RlIgmpMldSnoopMulticastTvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " entry of multicast ip"
    INDEX   { rlIgmpMldSnoopMulticastTvInetAddressType, rlIgmpMldSnoopMulticastTvVID, rlIgmpMldSnoopMulticastTvGroupAddressType, rlIgmpMldSnoopMulticastTvGroup }
    ::= { rlIgmpMldSnoopMulticastTvTable 1 }

RlIgmpMldSnoopMulticastTvEntry ::= SEQUENCE {
        rlIgmpMldSnoopMulticastTvInetAddressType   InetAddressType,
        rlIgmpMldSnoopMulticastTvVID               VlanIndex,
        rlIgmpMldSnoopMulticastTvGroupAddressType  InetAddressType,
        rlIgmpMldSnoopMulticastTvGroup             InetAddress,
        rlIgmpMldSnoopMulticastTvStatus            RowStatus
    }

rlIgmpMldSnoopMulticastTvInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type ipv6/ipv4."
    ::= { rlIgmpMldSnoopMulticastTvEntry 1}

rlIgmpMldSnoopMulticastTvVID OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "Specify the multicast ip to be used."
    ::= { rlIgmpMldSnoopMulticastTvEntry  2 }

rlIgmpMldSnoopMulticastTvGroupAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type ipv6/ipv4."
    ::= { rlIgmpMldSnoopMulticastTvEntry 3}

rlIgmpMldSnoopMulticastTvGroup OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "Specify the multicast ip to be used."
    ::= { rlIgmpMldSnoopMulticastTvEntry  4 }

rlIgmpMldSnoopMulticastTvStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "The row status variable, used according to
        row installation and removal conventions."
    ::= { rlIgmpMldSnoopMulticastTvEntry 5 }



MldVersion ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "MLD version."
    SYNTAX  INTEGER {
        none(0),
        v1(1),
        v2(2)
}



-- rlMldSnoopQuerierVlanTable

rlMldSnoopQuerierVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlMldSnoopQuerierVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A table that contains MLD Snooping Querier information about
        every vlan. This is indexed by vlan tag."
    ::= { rlMldSnoop 7 }

rlMldSnoopQuerierVlanEntry OBJECT-TYPE
    SYNTAX      RlMldSnoopQuerierVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlMldSnoopQuerierVlanTable."
    INDEX  { rlMldSnoopQuerierVlanTag }
    ::= { rlMldSnoopQuerierVlanTable 1 }

RlMldSnoopQuerierVlanEntry ::= SEQUENCE {
    rlMldSnoopQuerierVlanTag                       VlanIndex,
    rlMldSnoopQuerierAdminEnable                   TruthValue,
    rlMldSnoopQuerierOperEnable                    TruthValue,
    rlMldSnoopQuerierAdminAddrInetAddressType      InetAddressType,
    rlMldSnoopQuerierAdminAddr                     InetAddress,
    rlMldSnoopQuerierOperAddrInetAddressType       InetAddressType,
    rlMldSnoopQuerierOperAddr                      InetAddress,
    rlMldSnoopQuerierAdminVersionNumber            MldVersion,
    rlMldSnoopQuerierOperVersionNumber             MldVersion,
        rlMldSnoopQuerierElectionEnable                TruthValue
}

rlMldSnoopQuerierVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An MLD Snoop Querier entry vlan tag."
    ::= { rlMldSnoopQuerierVlanEntry 1 }

rlMldSnoopQuerierAdminEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The desired administrative state of MLD Snoop Querier on the vlan."
    ::= { rlMldSnoopQuerierVlanEntry 2 }

rlMldSnoopQuerierOperEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current operational state of MLD Snoop Querier on the vlan."
    ::= { rlMldSnoopQuerierVlanEntry 3 }

rlMldSnoopQuerierAdminAddrInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type IPv6/IPv4."
    ::= { rlMldSnoopQuerierVlanEntry 4}

rlMldSnoopQuerierAdminAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The desired IP address is being used in MLD Snoop Querier messages on the vlan."
    ::= { rlMldSnoopQuerierVlanEntry 5 }

rlMldSnoopQuerierOperAddrInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type IPv6/IPv4."
    ::= { rlMldSnoopQuerierVlanEntry 6}

rlMldSnoopQuerierOperAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current operational IP address is being used in MLD Snoop Querier messages on the vlan."
    ::= { rlMldSnoopQuerierVlanEntry 7 }

rlMldSnoopQuerierAdminVersionNumber OBJECT-TYPE
    SYNTAX      MldVersion
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The highest version number of MLD Snoop Querier for the vlan."
    ::= { rlMldSnoopQuerierVlanEntry 8 }

rlMldSnoopQuerierOperVersionNumber OBJECT-TYPE
    SYNTAX      MldVersion
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current operational version number of MLD Snoop Querier for the vlan."
    ::= { rlMldSnoopQuerierVlanEntry 9 }

rlMldSnoopQuerierElectionEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Whether or not to participate in querier election.
         When true, the snooping querier participates in querier election.
         When false, the snooping querier is the elected querier until a general
         query is heard from another router on the vlan (always lose)."
    ::= { rlMldSnoopQuerierVlanEntry 10 }
---

rlMldSnoopQuerierEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Globally enable/disable MLD Snooping Querier in the switch."
    ::= { rlMldSnoop 8 }


rlIgmpMldSnoopQuerierGlobalAddressTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlIgmpMldSnoopQuerierGlobalAddressEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A table that contains IGMP/MLD Snooping Querier global address."
    ::= { rlMldSnoop 9 }


rlIgmpMldSnoopQuerierGlobalAddressEntry OBJECT-TYPE
    SYNTAX      RlIgmpMldSnoopQuerierGlobalAddressEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlIgmpMldSnoopQuerierGlobalAddressTable."
    INDEX  { rlIgmpMldSnoopQuerierGlobalAddressIPVersion }
    ::= { rlIgmpMldSnoopQuerierGlobalAddressTable 1 }

RlIgmpMldSnoopQuerierGlobalAddressEntry ::= SEQUENCE {
    rlIgmpMldSnoopQuerierGlobalAddressIPVersion InetVersion,
    rlIgmpMldSnoopQuerierGlobalAddressType      InetAddressType,
    rlIgmpMldSnoopQuerierGlobalAddress          InetAddress
}

rlIgmpMldSnoopQuerierGlobalAddressIPVersion OBJECT-TYPE
    SYNTAX     InetVersion
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "The IP version of this PIM interface.  A physical interface
            may be configured in multiple modes concurrently, e.g., IPv4
            and IPv6; however, the traffic is considered to be logically
            separate."
    ::= { rlIgmpMldSnoopQuerierGlobalAddressEntry 1 }

rlIgmpMldSnoopQuerierGlobalAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type IPv6/IPv4."
    ::= { rlIgmpMldSnoopQuerierGlobalAddressEntry 2}

rlIgmpMldSnoopQuerierGlobalAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The desired address to used in IGMP/MLD Snoop Querier messages if
         such an address is not configured on the vlan."
    ::= { rlIgmpMldSnoopQuerierGlobalAddressEntry 3 }


---
--- TRAPS
---

rlMacMulticastUnregFilterFailed TRAP-TYPE
    ENTERPRISE  rnd
    VARIABLES   { rndErrorDesc, rndErrorSeverity }
    DESCRIPTION
        "Warning trap indicating - Setting Mac Unregistered Filtering on port is failed. The bound variable rndErrorDesc provides the interface number. "
    ::= 1

rlIgmpMldSnoopTriplePlayPort NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Informational trap indicating that a query was recieved on a triple play port."
    ::= { rndNotifications 208 }


rlbrgIgmpSnoopQrrDuplicateIP  NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Warning trap indicating that duplicate ip\ipv6 address 
         occured between two queries"
    ::= { rndNotifications 227 }


END


