RADLAN-rlBrgMcMngr-MIB DEFINITIONS ::= BEGIN


IMPORTS
    rnd                                         FROM RADLAN-MIB
    VlanIndex                                   FROM Q-BRIDGE-MIB
    MODULE-IDENTITY, OBJECT-TYPE                FROM SNMPv2-SMI
    InetAddressType                             FROM INET-ADDRESS-MIB;

rlBrgMcMngr MODULE-IDENTITY
              LAST-UPDATED "200602120000Z"
              ORGANIZATION "Marvell Semiconductor, Inc."
              CONTACT-INFO
					"5488 Marvell Lane
					Santa Clara, CA 95054
					USA

					Website:  www.marvell.com"
              DESCRIPTION
                      "The private MIB module definition for Multicast support in Radlan devices."
              REVISION "200602120000Z"
              DESCRIPTION
                       "Editorial changes to support new MIB compilers."
               REVISION "200404190000Z"
              DESCRIPTION
                      "Initial version of this MIB."
          ::= { rnd 117 }


rlBrgMulticastManagerTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlBrgMulticastManagerEntry
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
    "The table containing Multicast information for each VLAN."
    ::= { rlBrgMcMngr  1}

rlBrgMulticastManagerEntry OBJECT-TYPE
SYNTAX  RlBrgMulticastManagerEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
    "An entry (conceptual row) in the rlBrgMulticastManagerTable."
    INDEX  { rlBrgMulticastManagerVlanTag }
    ::= { rlBrgMulticastManagerTable 1 }

RlBrgMulticastManagerEntry ::=
SEQUENCE {
        rlBrgMulticastManagerVlanTag  VlanIndex,
        rlBrgMulticastManagerAdminVlanMode INTEGER,
        rlBrgMulticastManagerOperVlanMode  INTEGER
}
rlBrgMulticastManagerVlanTag OBJECT-TYPE
    SYNTAX  VlanIndex
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
    " The VLAN tag for which this entry is configured."
    ::= { rlBrgMulticastManagerEntry 1 }

rlBrgMulticastManagerAdminVlanMode OBJECT-TYPE
    SYNTAX  INTEGER {
        mac-group(1),
        ip-group(2),
        ip-src-group(3)
    }
    MAX-ACCESS   read-write
    STATUS   current
    DESCRIPTION
        "The Bridge Multicast Admin Lookup Mode."
    DEFVAL { mac-group }
    ::= { rlBrgMulticastManagerEntry 2 }

rlBrgMulticastManagerOperVlanMode OBJECT-TYPE
    SYNTAX  INTEGER {
        mac-group(1),
        ip-group(2),
        ip-src-group(3)
    }
    MAX-ACCESS  read-only
    STATUS   current
    DESCRIPTION
        "The Bridge Multicast Oper Lookup Mode."
    DEFVAL { mac-group }
    ::= { rlBrgMulticastManagerEntry 3 }

-- rlBrgMulticastInetManagerTable (replaced DEPRICATED rlBrgMulticastManagerTable)

rlBrgMulticastInetManagerTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlBrgMulticastInetManagerEntry
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
    "The table containing Multicast information for each VLAN."
    ::= { rlBrgMcMngr  2}

rlBrgMulticastInetManagerEntry OBJECT-TYPE
SYNTAX  RlBrgMulticastInetManagerEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
    "An entry (conceptual row) in the rlBrgMulticastInetManagerTable."
    INDEX  { rlBrgMulticastInetManagerIpType, rlBrgMulticastInetManagerVlanTag }
    ::= { rlBrgMulticastInetManagerTable 1 }

RlBrgMulticastInetManagerEntry ::=
SEQUENCE {
        rlBrgMulticastInetManagerIpType     INTEGER,
        rlBrgMulticastInetManagerVlanTag  VlanIndex,
        rlBrgMulticastInetManagerAdminVlanMode INTEGER,
        rlBrgMulticastInetManagerOperVlanMode  INTEGER
}

rlBrgMulticastInetManagerIpType OBJECT-TYPE
     SYNTAX      INTEGER {
                     unknown(0),
                     ipv4(1),    -- these named numbers are aligned
                     ipv6(2),    -- with AddressFamilyNumbers from
                     dns(16)     -- IANA-ADDRESS-FAMILY-NUMBERS-MIB
                 }
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
           "The address type of Vlan Mode."
    ::= { rlBrgMulticastInetManagerEntry  1 }

rlBrgMulticastInetManagerVlanTag OBJECT-TYPE
    SYNTAX  VlanIndex
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
    " The VLAN tag for which this entry is configured."
    ::= { rlBrgMulticastInetManagerEntry 2 }

rlBrgMulticastInetManagerAdminVlanMode OBJECT-TYPE
    SYNTAX  INTEGER {
        mac-group(1),
        ip-group(2),
        ip-src-group(3)
    }
    MAX-ACCESS   read-write
    STATUS   current
    DESCRIPTION
        "The Bridge Multicast Admin Lookup Mode."
    DEFVAL { mac-group }
    ::= { rlBrgMulticastInetManagerEntry 3 }

rlBrgMulticastInetManagerOperVlanMode OBJECT-TYPE
    SYNTAX  INTEGER {
        mac-group(1),
        ip-group(2),
        ip-src-group(3)
    }
    MAX-ACCESS  read-only
    STATUS   current
    DESCRIPTION
        "The Bridge Multicast Oper Lookup Mode."
    DEFVAL { mac-group }
    ::= { rlBrgMulticastInetManagerEntry 4 }


END





