RADLAN-rlBrgMulticast-MIB DEFINITIONS ::= BEGIN

-- Title:      RADLAN Multicast Bridge Configuration
-- Version:    7.46
-- Date:       15-Jan-2007
--

IMPORTS
    TEXTUAL-CONVENTION, RowStatus                        FROM SNMPv2-TC
    VlanIndex,PortList                                   FROM Q-BRIDGE-MIB
    Unsigned32, IpAddress, OBJECT-TYPE,
    MODULE-IDENTITY                                         FROM SNMPv2-SMI
    rnd                                                      FROM RADLAN-MIB
    InetAddressType, InetAddress                         FROM INET-ADDRESS-MIB;


rlBrgMulticast MODULE-IDENTITY
      LAST-UPDATED "201304010000Z"  -- April 1, 2013
      ORGANIZATION "Marvell Semiconductor, Inc."
      CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
      DESCRIPTION
              "The MIB module describes the private MIB for Multicast Bridge
               supported by Marvell MTS software and products."
      REVISION     "201304010000Z"  -- April 1, 2013
      DESCRIPTION
              "Added MODULE-IDENTITY"
      ::= { rnd 116  }


--  rlBrgMulticastMibVersion

rlBrgMulticastMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "MIB's version, the current version is 4.
         Snooping supports IGMPv1/v2/v3 and MLDv1/v2."
::= { rlBrgMulticast 1 }

-- rlBrgStaticIpMulticastTable   (replaced by rlBrgStaticInetMulticastTable)

rlBrgStaticIpMulticastTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlBrgStaticIpMulticastEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing filtering information for IP Multicast
         addresses for each VLAN."
    ::= { rlBrgMulticast 3}

rlBrgStaticIpMulticastEntry OBJECT-TYPE
    SYNTAX      RlBrgStaticIpMulticastEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Filtering information configured into the device.
         The set of ports to which frames containing this IP
         Multicast destination address and IP source address
         are allowed to be forwarded."
    INDEX { rlBrgStaticIpMulticastVlanTag,
            rlBrgStaticIpMulticastGroupAddress,
            rlBrgStaticIpMulticastSourceAddress }
    ::= { rlBrgStaticIpMulticastTable 1 }

RlBrgStaticIpMulticastEntry ::= SEQUENCE {
        rlBrgStaticIpMulticastVlanTag           VlanIndex,
        rlBrgStaticIpMulticastGroupAddress      IpAddress,
        rlBrgStaticIpMulticastSourceAddress     IpAddress,
        rlBrgStaticIpMulticastFrwPorts          PortList,
        rlBrgStaticIpMulticastForbiddenPorts    PortList,
        rlBrgStaticIpMulticastStatus            RowStatus
}

rlBrgStaticIpMulticastVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "The VLAN tag for which this entry is configured."
    ::= { rlBrgStaticIpMulticastEntry 1}

rlBrgStaticIpMulticastGroupAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "The multicast group address for which the filtering information applies "
    ::= { rlBrgStaticIpMulticastEntry 2}

rlBrgStaticIpMulticastSourceAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "The unicast group address for which the filtering information applies."
    ::= { rlBrgStaticIpMulticastEntry 3}

rlBrgStaticIpMulticastFrwPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "The ports the data should be forwarded to "
    ::= { rlBrgStaticIpMulticastEntry 4}

rlBrgStaticIpMulticastForbiddenPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "The ports that overrides dynamic configuration and
          prevents multicast data forwarding for the group or
          group and source to these ports."
    ::= { rlBrgStaticIpMulticastEntry 5}

rlBrgStaticIpMulticastStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The status of the table entry. It's used to add/delete an entry"
    ::= { rlBrgStaticIpMulticastEntry  6}

-- bridge ip multicast FDB
-- rlBrgIpMulticastTable  (See rlBrgInetMulticastTable)

rlBrgIpMulticastTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlBrgIpMulticastEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing all filtering information for IP
         Multicast addresses for each VLAN "
    ::= { rlBrgMulticast 4}

rlBrgIpMulticastEntry OBJECT-TYPE
    SYNTAX      RlBrgIpMulticastEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlBrgIpMulticastTable
         contains IP Multicast FDB data "
    INDEX { rlBrgIpMulticastVlanTag,
            rlBrgIpMulticastGroupAddress,
            rlBrgIpMulticastSourceAddress }
::= { rlBrgIpMulticastTable 1 }

RlBrgIpMulticastEntry ::= SEQUENCE {
    rlBrgIpMulticastVlanTag         VlanIndex,
    rlBrgIpMulticastGroupAddress    IpAddress,
    rlBrgIpMulticastSourceAddress   IpAddress,
    rlBrgIpMulticastEgressPorts     PortList,
    rlBrgIpMulticastLearntPorts     PortList
}

rlBrgIpMulticastVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The VLAN tag for which this entry is configured."
    ::= { rlBrgIpMulticastEntry 1}

rlBrgIpMulticastGroupAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "Multicast group address (destination address) of data frames "
    ::= { rlBrgIpMulticastEntry 2}

rlBrgIpMulticastSourceAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unicast source address of data frames."
    ::= { rlBrgIpMulticastEntry 3}

rlBrgIpMulticastEgressPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The complete set of ports, in this VLAN, to which frames
         destined for this Group IP address or Group and Source
         address are currently being explicitly forwarded.  This
         does not include ports for which this address is only implicitly
         forwarded, in the dot1qForwardAllPorts list."
    ::= { rlBrgIpMulticastEntry 4}

rlBrgIpMulticastLearntPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The subset of ports in rlBrgIpMulticastEgressPorts which
         were learnt by IGMP or some other dynamic mechanism,
         in this Filtering database.."
    ::= { rlBrgIpMulticastEntry 5}

-- static ipm inet bridge configuration
--  rlBrgStaticInetMulticastTable  IPM FDB

rlBrgStaticInetMulticastTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlBrgStaticInetMulticastEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing filtering information for INET (Pv4 and IPv6)
        Multicast addresses for each VLAN."
    ::= { rlBrgMulticast 5}

rlBrgStaticInetMulticastEntry OBJECT-TYPE
    SYNTAX      RlBrgStaticInetMulticastEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Filtering information configured into the device.
         The set of ports to which frames containing this IP
         Multicast destination address and IP source address
         are allowed to be forwarded."
    INDEX { rlBrgStaticInetMulticastVlanTag,
            rlBrgStaticInetMulticastGroupAddressType, rlBrgStaticInetMulticastGroupAddress,
            rlBrgStaticInetMulticastSourceAddressType, rlBrgStaticInetMulticastSourceAddress }
    ::= { rlBrgStaticInetMulticastTable 1 }

RlBrgStaticInetMulticastEntry ::= SEQUENCE {
        rlBrgStaticInetMulticastVlanTag           VlanIndex,
        rlBrgStaticInetMulticastGroupAddressType  InetAddressType,
        rlBrgStaticInetMulticastGroupAddress      InetAddress,
        rlBrgStaticInetMulticastSourceAddressType InetAddressType,
        rlBrgStaticInetMulticastSourceAddress     InetAddress,
        rlBrgStaticInetMulticastFrwPorts          PortList,
        rlBrgStaticInetMulticastForbiddenPorts    PortList,
        rlBrgStaticInetMulticastStatus            RowStatus
}

rlBrgStaticInetMulticastVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "The VLAN tag for which this entry is configured."
    ::= { rlBrgStaticInetMulticastEntry 1}

rlBrgStaticInetMulticastGroupAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type ipv6/ipv4."
    ::= { rlBrgStaticInetMulticastEntry 2}

rlBrgStaticInetMulticastGroupAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "The multicast group address for which the filtering information applies "
    ::= { rlBrgStaticInetMulticastEntry 3}

rlBrgStaticInetMulticastSourceAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type ipv6/ipv4."
    ::= { rlBrgStaticInetMulticastEntry 4}

rlBrgStaticInetMulticastSourceAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "The unicast group address for which the filtering information applies."
    ::= { rlBrgStaticInetMulticastEntry 5}

rlBrgStaticInetMulticastFrwPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "The ports the data should be forwarded to "
    ::= { rlBrgStaticInetMulticastEntry 6}

rlBrgStaticInetMulticastForbiddenPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "The ports that overrides dynamic configuration and
          prevents multicast data forwarding for the group or
          group and source to these ports."
    ::= { rlBrgStaticInetMulticastEntry 7}

rlBrgStaticInetMulticastStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The status of the table entry. It's used to add/delete an entry"
    ::= { rlBrgStaticInetMulticastEntry  8}

-- rlBrgInetMulticastTable  IPM FDB

rlBrgInetMulticastTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlBrgInetMulticastEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing all filtering information for IP
         Multicast addresses for each VLAN "
    ::= { rlBrgMulticast 6}

rlBrgInetMulticastEntry OBJECT-TYPE
    SYNTAX      RlBrgInetMulticastEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlBrgInetMulticastTable
         contains IP Multicast FDB data "
    INDEX { rlBrgInetMulticastVlanTag,
            rlBrgInetMulticastGroupAddressType, rlBrgInetMulticastGroupAddress,
            rlBrgInetMulticastSourceAddressType, rlBrgInetMulticastSourceAddress }
::= { rlBrgInetMulticastTable 1 }

RlBrgInetMulticastEntry ::= SEQUENCE {
    rlBrgInetMulticastVlanTag           VlanIndex,
    rlBrgInetMulticastGroupAddressType  InetAddressType,
    rlBrgInetMulticastGroupAddress      InetAddress,
    rlBrgInetMulticastSourceAddressType InetAddressType,
    rlBrgInetMulticastSourceAddress     InetAddress,
    rlBrgInetMulticastEgressPorts       PortList,
    rlBrgInetMulticastLearntPorts       PortList
}

rlBrgInetMulticastVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The VLAN tag for which this entry is configured."
    ::= { rlBrgInetMulticastEntry 1}

rlBrgInetMulticastGroupAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type IPv4/IPv6."
    ::= { rlBrgInetMulticastEntry 2}

rlBrgInetMulticastGroupAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "Multicast group address (destination address) of data frames "
    ::= { rlBrgInetMulticastEntry 3}

rlBrgInetMulticastSourceAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Inet type IPv4/IPv6."
    ::= { rlBrgInetMulticastEntry 4}

rlBrgInetMulticastSourceAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unicast source address of data frames."
    ::= { rlBrgInetMulticastEntry 5}

rlBrgInetMulticastEgressPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The complete set of ports, in this VLAN, to which frames
         destined for this Group IP address or Group and Source
         address are currently being explicitly forwarded.  This
         does not include ports for which this address is only implicitly
         forwarded, in the dot1qForwardAllPorts list."
    ::= { rlBrgInetMulticastEntry 6}

rlBrgInetMulticastLearntPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The subset of ports in rlBrgIpMulticastEgressPorts which
         were learnt by IGMP or some other dynamic mechanism,
         in this Filtering database.."
    ::= { rlBrgInetMulticastEntry 7}


-- IPM FDB overlapping Reference Table

rlBrgIpmFdbRefTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlBrgIpmFdbRefEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing all information stored in
         IPM FDB overlapping Reference Table "
    ::= { rlBrgMulticast 7}

rlBrgIpmFdbRefEntry OBJECT-TYPE
    SYNTAX      RlBrgIpmFdbRefEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlBrgIpmFdbRefTable
         contains overlapping Reference Table FDB data "
    INDEX { rlBrgIpmFdbRefVlanTag,
            rlBrgIpmFdbRefGroupAddressType, rlBrgIpmFdbRefGroupAddress,
            rlBrgIpmFdbRefSourceAddressType, rlBrgIpmFdbRefSourceAddress }
::= { rlBrgIpmFdbRefTable 1 }

RlBrgIpmFdbRefEntry ::= SEQUENCE {
    rlBrgIpmFdbRefVlanTag           VlanIndex,
    rlBrgIpmFdbRefGroupAddressType  InetAddressType,
    rlBrgIpmFdbRefGroupAddress      InetAddress,
    rlBrgIpmFdbRefSourceAddressType InetAddressType,
    rlBrgIpmFdbRefSourceAddress     InetAddress,
    rlBrgIpmFdbRefPorts             PortList
}

rlBrgIpmFdbRefVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The VLAN tag for which this entry is configured."
    ::= { rlBrgIpmFdbRefEntry 1}

rlBrgIpmFdbRefGroupAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "Multicast group address (destination address) of data frames "
    ::= { rlBrgIpmFdbRefEntry 2}

rlBrgIpmFdbRefGroupAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "Multicast group address (destination address) of data frames "
    ::= { rlBrgIpmFdbRefEntry 3}

rlBrgIpmFdbRefSourceAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unicast source address of data frames."
    ::= { rlBrgIpmFdbRefEntry 4}

rlBrgIpmFdbRefSourceAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unicast source address of data frames."
    ::= { rlBrgIpmFdbRefEntry 5}

rlBrgIpmFdbRefPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The list of ports represented in IPM FDB overlapping
            Reference Table"
    ::= { rlBrgIpmFdbRefEntry 6}


-- IPM FDB Dynamic command MIB
DynamicCmdType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "Type of Dynamic IPM FDB command:
         Create Entry, Delete Entry, Set ports Pset."
    SYNTAX  INTEGER {
        createEntry(0),
        deleteEntry(1),
        addPorts(2),
        deletePorts(3)
}

rlBrgDynamicCmdTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlBrgDynamicCmdEntry
    MAX-ACCESS   not-accessible
    STATUS   current
    DESCRIPTION
       "The (conceptual) table for Dynamic IPM FDB command. For debugging purposes
        only. This MIB is prohibited to be used with working IGMP/MLD snooping"
    ::= {  rlBrgMulticast 8 }

rlBrgDynamicCmdEntry OBJECT-TYPE
    SYNTAX      RlBrgDynamicCmdEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlBrgDynamicCmdTable."
    INDEX  { rlBrgDynamicCmdKey }
    ::= { rlBrgDynamicCmdTable 1 }

RlBrgDynamicCmdEntry ::= SEQUENCE {
    rlBrgDynamicCmdKey               INTEGER,
    rlBrgDynamicCmdVlanTag           VlanIndex,
    rlBrgDynamicCmdGroupAddressType  InetAddressType,
    rlBrgDynamicCmdGroupAddress      InetAddress,
    rlBrgDynamicCmdSourceAddressType InetAddressType,
    rlBrgDynamicCmdSourceAddress     InetAddress,
    rlBrgDynamicCmdPorts             PortList,
    rlBrgDynamicCmdType              DynamicCmdType
}

rlBrgDynamicCmdKey OBJECT-TYPE
    SYNTAX      INTEGER (1)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Key of the rlBrgDynamicCmdTable table"
    ::= { rlBrgDynamicCmdEntry 1 }

rlBrgDynamicCmdVlanTag OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The VLAN tag for which this entry is configured."
    ::= { rlBrgDynamicCmdEntry 2}

rlBrgDynamicCmdGroupAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "Multicast group address (destination address) of data frames "
    ::= { rlBrgDynamicCmdEntry 3}

rlBrgDynamicCmdGroupAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "Multicast group address (destination address) of data frames "
    ::= { rlBrgDynamicCmdEntry 4}

rlBrgDynamicCmdSourceAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Unicast source address of data frames."
    ::= { rlBrgDynamicCmdEntry 5}

rlBrgDynamicCmdSourceAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Unicast source address of data frames."
    ::= { rlBrgDynamicCmdEntry 6}

rlBrgDynamicCmdPorts OBJECT-TYPE
    SYNTAX      PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The list of ports for them the command is issued"
    ::= { rlBrgDynamicCmdEntry 7}

rlBrgDynamicCmdType OBJECT-TYPE
    SYNTAX      DynamicCmdType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Current type of command"
    ::= { rlBrgDynamicCmdEntry 8 }


-------------------------------------------------------------------
--rlUserAssignedVidx
-------------------------------------------------------------------

rlUserAssignedVidx  OBJECT IDENTIFIER ::= { rlBrgMulticast 9 }

VidxIndex ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "Values of Vidx. 0 means no free Vidx."
    SYNTAX  Unsigned32 (0|4096..32767)


--rlUserAssignedVidxTable

rlUserAssignedVidxConfigTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlUserAssignedVidxConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing entries of User Assigned Vidx configuration information"
    ::= { rlUserAssignedVidx 1 }

rlUserAssignedVidxConfigEntry       OBJECT-TYPE
    SYNTAX      RlUserAssignedVidxConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table entry of User Assigned Vidx information table"
    INDEX   { rlUserAssignedVidxConfigIndex }
    ::= { rlUserAssignedVidxConfigTable 1 }

RlUserAssignedVidxConfigEntry::= SEQUENCE {
        rlUserAssignedVidxConfigIndex       VidxIndex,
        rlUserAssignedVidxConfigPorts       PortList,
        rlUserAssignedVidxConfigRowStatus   RowStatus
}

rlUserAssignedVidxConfigIndex       OBJECT-TYPE
    SYNTAX      VidxIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Vidx index. Values from 4K to 32K"
    ::= { rlUserAssignedVidxConfigEntry 1 }

rlUserAssignedVidxConfigPorts       OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "List of ports that belong to the Vidx"
    ::= { rlUserAssignedVidxConfigEntry 2 }

rlUserAssignedVidxConfigRowStatus   OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the status of this entry."
    ::= { rlUserAssignedVidxConfigEntry 3 }

--rlUserAssignedVidxGetFreeIndex

rlUserAssignedVidxGetNextFreeIndex OBJECT-TYPE
    SYNTAX           VidxIndex
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Returns the next free Vidx index. Values from 4K to 32K"
    ::= { rlUserAssignedVidx 2 }

rlBrgMulticastCurrentNumberOfEntries OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Current number of multicast entries."
::= { rlBrgMulticast 10 }


END


