MARVELL-ProtectedPorts-MIB DEFINITIONS ::= BEGIN

-- Title:      Marvell Switch Interfaces Private
-- Version:    7.46
-- Date:       13 Apr 2008

IMPORTS
    ifIndex                                         FROM IF-MIB
    Unsigned32, MODULE-IDENTITY, OBJECT-TYPE        FROM SNMPv2-SMI
    RowStatus, TruthValue, TEXTUAL-CONVENTION       FROM SNMPv2-TC
    PortList                                        FROM Q-BRIDGE-MIB
    rnd                                             FROM RADLAN-MIB;


rlProtectedPorts MODULE-IDENTITY
        LAST-UPDATED "200805031234Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
            "<description>"
        REVISION "200805031234Z"
        DESCRIPTION
            "The private MIB module definition for Protected Ports MIB."
        ::= { rnd 132 }



-- rlProtectedPortsTable

rlProtectedPortsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlProtectedPortsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing entries of protected ports configuration information"
    ::= { rlProtectedPorts 1 }

rlProtectedPortsEntry OBJECT-TYPE
    SYNTAX      RlProtectedPortsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table entry of protected ports configuration information"
    INDEX   { ifIndex }
    ::= { rlProtectedPortsTable 1 }

RlProtectedPortsEntry ::= SEQUENCE {
        rlProtectedPortType             INTEGER,
        rlProtectedPortCommunity        INTEGER
    }

rlProtectedPortType OBJECT-TYPE
    SYNTAX INTEGER {
        not-protected(1),
        protected(2),
        isolated-group(100)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Set port protected mode: not-protected, protected, isolated-group
         protected ports filter layer 2 traffic from other protected ports"
    DEFVAL  { not-protected }
    ::= { rlProtectedPortsEntry 1 }

rlProtectedPortCommunity OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION

        "Associate protected port with community number which becoming active only when
         rlProtectedPortsStatus changed to protected
         protected community ports filter layer 2 traffic from protected ports
         and from other protected community ports, but do not filter layer 2
         traffic from same community ports.

         Associate isolated-group port with community number which becoming active only when
         rlProtectedPortsStatus changed to isolated-group.
         Isolated-group ports filter layer 2 traffic from isolated-group ports with the same number of community number,
         but do not filter layer 2 traffic isolated-group ports with other community number and
         unprotected ports.

         value of 0 disassociate port from its community.
         "
    DEFVAL  { 0 }
    ::= { rlProtectedPortsEntry 2 }

--------------------------------------------------------------------------------

-- rlProtectedPortsStatusTable

rlProtectedPortsStatusTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlProtectedPortsStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing entries of protected ports status"
    ::= { rlProtectedPorts 2 }

rlProtectedPortsStatusEntry OBJECT-TYPE
    SYNTAX      RlProtectedPortsStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table entry containing protected ports DB status information"
    INDEX   { ifIndex }
    ::= { rlProtectedPortsStatusTable 1 }

RlProtectedPortsStatusEntry ::= SEQUENCE {
        rlProtectedPortEgressPorts PortList
    }

rlProtectedPortEgressPorts OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "list of ports which are not filtered by protected port mechanism when traffic is forwarded from
         the specified ifIndex"
    ::= { rlProtectedPortsStatusEntry 1 }

--------------------------------------------------------------------------------

-- rlProtectedPortsGroup

rlProtectedPortsGlobalEnable  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "true  - set all system fast ethernet ports to protected state
         false - set all system fast ethernet ports to not protected state"
    DEFVAL { false }
    ::= { rlProtectedPorts 3 }

    
END


