MARVELL-POE-MIB DEFINITIONS ::= BEGIN

-- Title:               Marvell LOCALIZATION ROS
--                      This Private MIB is enhancement for rfc3621.txt - Power Ethernet Mib
-- Version:             7.50
-- Date:                28 Nov 2005

IMPORTS
    rnd                                         FROM RADLAN-MIB
    DisplayString, TruthValue                   FROM SNMPv2-TC
	InterfaceIndexOrZero, InterfaceIndex    	FROM IF-MIB
    OBJECT-TYPE, MODULE-IDENTITY, Unsigned32    FROM SNMPv2-SMI;


rlPoe    MODULE-IDENTITY
         LAST-UPDATED "200911260000Z"
         ORGANIZATION "Marvell Semiconductor, Inc."
         CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
         DESCRIPTION
                "Add a new field in the PoE MIB to indicate Max power allocation allowed"
         REVISION "201006020000Z"
         DESCRIPTION
                "The private MIB module definition for Power Over Ethernet."
         REVISION "200911260000Z"
         DESCRIPTION
                "Initial revision."
        ::= { rnd 108 }

RlPoeType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION "PoE types:
                1 - none: no PoE, unknown type;
                2 - PoE: Standard AF PoE
                3 - PoE Plus: Standard AT PoE
                4 - 60 W: 60W poe port "
     SYNTAX  INTEGER {
                    none(1),
                    poe(2),
                    poeplus(3),
                    poe60w(4)
                }

--rlPethPsePortTable

rlPethPsePortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPethPsePortEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        " The table listing additional information for Power Over Ethernet ports."
    ::= {rlPoe 1 }

rlPethPsePortEntry  OBJECT-TYPE
    SYNTAX      RlPethPsePortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " An entry in the rlPethPsePortTable."
    INDEX    { rlPethPsePortGroupIndex , rlPethPsePortIndex  }
    ::= {rlPethPsePortTable  1 }

RlPethPsePortEntry ::= SEQUENCE {
    rlPethPsePortGroupIndex             	INTEGER,
    rlPethPsePortIndex                  	INTEGER,
    rlPethPsePortOutputVoltage          	INTEGER,
    rlPethPsePortOutputCurrent          	INTEGER,
    rlPethPsePortOutputPower            	INTEGER,
    rlPethPsePortPowerLimit             	INTEGER,
    rlPethPsePortStatus                 	INTEGER,
    rlPethPsePortStatusDescription      	DisplayString,
    rlPethPsePortOperPowerLimit         	INTEGER,
    rlPethPsePortTimeRangeName          	DisplayString,
    rlPethPsePortOperStatus             	TruthValue,
    rlPethPsePortMaxPowerAllocAllowed   	INTEGER,
    rlPethPsePortSupportPoeType         	RlPoeType,
    rlPethPsePortLinkPartnerPoeType     	RlPoeType,
	rlPethPsePortFourPairForced     		INTEGER,
	rlPethPsePortFourPairEnabled     		INTEGER,
	rlPethPsePortNegotiationAllocatedPower	INTEGER,
	rlPethPsePortNegotiationProtocolOwner	INTEGER,
	rlPethPsePortLegacySupport				INTEGER,
	rlPethPsePortHighPowerModeEnable		INTEGER,
	rlPethPsePortMenagementMode				INTEGER,
	rlPethPsePortStaticPowerAllocation		INTEGER
}

rlPethPsePortGroupIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the group
         containing the port to which a power Ethernet PSE is
         connected.  Group means box in the stack, module in a
         rack and the value 1 MUST be used for non-modular devices.
         Furthermore, the same value MUST be used in this variable,
         pethMainPseGroupIndex, and pethNotificationControlGroupIndex
         to refer to a given box in a stack or module in the rack."
    ::= { rlPethPsePortEntry 1 }

rlPethPsePortIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the power Ethernet PSE
         port within group pethPsePortGroupIndex to which the
         power Ethernet PSE entry is connected."
    ::= { rlPethPsePortEntry 2 }

rlPethPsePortOutputVoltage OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates on the output voltage level in milli volts from rlPethPsePortIndex."
    ::= { rlPethPsePortEntry 3 }

rlPethPsePortOutputCurrent OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates on the output current level in milli amper from rlPethPsePortIndex."
    ::= { rlPethPsePortEntry 4 }

rlPethPsePortOutputPower OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates on the output power level in milli watts from rlPethPsePortIndex."
    ::= { rlPethPsePortEntry 5 }

rlPethPsePortPowerLimit OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable indicates on the user configured power level in milli watts which is available from rlPethPsePortIndex."
    ::= { rlPethPsePortEntry 6 }

rlPethPsePortStatus OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates on the hardware status of rlPethPsePortIndex."
    ::= { rlPethPsePortEntry 7 }

rlPethPsePortStatusDescription OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(0..120))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the description of the hardware status of rlPethPsePortIndex."
    ::= { rlPethPsePortEntry 8 }

rlPethPsePortOperPowerLimit OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the maximum power level in milli watts which is available from rlPethPsePortIndex."
    ::= { rlPethPsePortEntry 9 }

rlPethPsePortTimeRangeName OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable is used to bind PoE port to time range."
    ::= { rlPethPsePortEntry 10 }

rlPethPsePortOperStatus OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This Read-Only variable indicates PoE port current status affected by time range active/inactive and admin status."
    ::= { rlPethPsePortEntry 11 }

rlPethPsePortMaxPowerAllocAllowed OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the maximum power allocation allowed per port (including wire power loses) in milli-watts which is available from rlPethPsePortIndex."
    ::= { rlPethPsePortEntry 12 }

rlPethPsePortSupportPoeType OBJECT-TYPE
    SYNTAX  RlPoeType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the supported type of the PoE port"
    ::= { rlPethPsePortEntry 13 }

rlPethPsePortLinkPartnerPoeType OBJECT-TYPE
    SYNTAX  RlPoeType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the link partner PoE type."
    ::= { rlPethPsePortEntry 14 }

rlPethPsePortFourPairForced OBJECT-TYPE
    SYNTAX      INTEGER {
        forcedEnable(0),
        forcedDisable(1)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable enabled the spare pair ALT_B in 60W port to force 4 pair enable."
    ::= { rlPethPsePortEntry 15 }

rlPethPsePortFourPairEnabled OBJECT-TYPE
    SYNTAX      INTEGER {
        fourPairEnable(1),
        fourPairDisable(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates that spare pair ALT_B is enable."
    ::= { rlPethPsePortEntry 16 }
	
rlPethPsePortNegotiationAllocatedPower OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the power allocation in milli watts from power negotiation"
    ::= { rlPethPsePortEntry 17 }

rlPethPsePortNegotiationProtocolOwner OBJECT-TYPE
    SYNTAX      INTEGER {
        protocolOwnerNone(0),
        protocolOwnerCDP(1),
		protocolOwnerLLDP(2),
        protocolOwnerCDPExpired(3),
        protocolOwnerLLDPExpired(4)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the protocol owner on power management negotiation protocol"
    ::= { rlPethPsePortEntry 18 }
	
rlPethPsePortLegacySupport OBJECT-TYPE
    SYNTAX      INTEGER {
        not-relevant(0),
		enabled(1),
        disabled(2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies poe Legacy per port configuration mode"
    ::= { rlPethPsePortEntry 19 }

rlPethPsePortHighPowerModeEnable OBJECT-TYPE
    SYNTAX      INTEGER {
		not-relevant(0),
        enabled(1),
        disabled(2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies poe port high power configuration mode"
    ::= { rlPethPsePortEntry 20 }

rlPethPsePortMenagementMode OBJECT-TYPE
    SYNTAX      INTEGER {
		not-relevant(0),
        dynamic(1),
        static(2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies poe power management mode configuration mode"
    ::= { rlPethPsePortEntry 21 }

rlPethPsePortStaticPowerAllocation OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates PoE Static power allocation.
		Static power allocation can be configured by setting rlPethPsePortMenagementMode"
    ::= { rlPethPsePortEntry 22 }
	
--rlPethMainPseTable

rlPethMainPseTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPethMainPseEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        " The table listing additional read - only information for Power Over Ethernet."
    ::= {rlPoe 2 }

rlPethMainPseEntry  OBJECT-TYPE
    SYNTAX      RlPethMainPseEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " An entry in the rlPethMainPseTable."
    INDEX    { rlPethMainPseGroupIndex }
    ::= {rlPethMainPseTable  1 }

RlPethMainPseEntry ::= SEQUENCE {
    rlPethMainPseGroupIndex          INTEGER,
    rlPethMainPseSwVersion           DisplayString,
    rlPethMainPseHwVersion           DisplayString,
    rlPethMainPseHwType              INTEGER,
    rlPethMainPsePowerGuardBand      INTEGER
}

rlPethMainPseGroupIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the group
         containing the port to which a power Ethernet PSE is
         connected.  Group means box in the stack, module in a
         rack and the value 1 MUST be used for non-modular devices.
         Furthermore, the same value MUST be used in this variable,
         pethMainPseGroupIndex, and pethNotificationControlGroupIndex
         to refer to a given box in a stack or module in the rack."
    ::= { rlPethMainPseEntry 1 }

rlPethMainPseSwVersion OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(0..20))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable identifies the MCU SW version."
    ::= { rlPethMainPseEntry 2 }

rlPethMainPseHwVersion OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(0..20))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "This variable identifies the MCU HW version."
    ::= { rlPethMainPseEntry 3 }

rlPethMainPseHwType OBJECT-TYPE
    SYNTAX  INTEGER {
        enhanced(1),
        plus(2),
        auto(3),
        nonPoe(4),
        enhancedPlus(5),
        poe60w(6)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable identifies the MCU HW type (enhanced, plus, none)."
    ::= { rlPethMainPseEntry 4 }

rlPethMainPsePowerGuardBand OBJECT-TYPE
    SYNTAX      INTEGER (0..254)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies the guard band in [W] for not connecting
         additional ports."
    ::= { rlPethMainPseEntry 5 }

--rlPethPowerPseTable

rlPethPowerPseTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPethPowerPseEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        " The table listing additional read-write information for Power Over Ethernet - PSE side."
    ::= {rlPoe 3 }

rlPethPowerPseEntry  OBJECT-TYPE
    SYNTAX      RlPethPowerPseEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " An entry in the rlPethPowerPseTable."
    INDEX    { rlPethPowerPseGroupIndex }
    ::= {rlPethPowerPseTable  1 }

RlPethPowerPseEntry ::= SEQUENCE {
    rlPethPowerPseGroupIndex          INTEGER,
    rlPethPowerPsePower               INTEGER,
    rlPethPowerPseRpsPower            INTEGER,
    rlPethPowerPsePowerManagementMode INTEGER,
    rlPethPowerPsedisconnectMethod    INTEGER,
    rlPethPowerPseTemperatureSensor   INTEGER,
    rlPethPowerPseInrushTestEnabled   INTEGER,
    rlPethPowerPseLegacyDisabled      INTEGER
}

rlPethPowerPseGroupIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..8)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the group
         containing the port to which a power Ethernet PSE is
         connected.  Group means box in the stack, module in a
         rack and the value 1 MUST be used for non-modular devices.
         Furthermore, the same value MUST be used in this variable,
         PethPowerPseGroupIndex, and pethNotificationControlGroupIndex
         to refer to a given box in a stack or module in the rack."
    ::= { rlPethPowerPseEntry 1 }


-- depricated
rlPethPowerPsePower OBJECT-TYPE
    SYNTAX      INTEGER {
        none(0),
        ps1(1),
        ps2(2),
        ps3(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies the maximum power in [W] supplied by PSE."
    ::= { rlPethPowerPseEntry 2 }

-- depricated
rlPethPowerPseRpsPower OBJECT-TYPE
    SYNTAX      INTEGER {
        none(0),
        rps1(1),
        rps2(2),
        rps3(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies the maximum power in [W] supplied by PSE + RPS."
    ::= { rlPethPowerPseEntry 3 }

rlPethPowerPsePowerManagementMode OBJECT-TYPE
    SYNTAX      INTEGER {
        portlimit(0),
        classlimit(5),
        maxlimit(6)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies power management mode."
    ::= { rlPethPowerPseEntry 4 }

rlPethPowerPsedisconnectMethod OBJECT-TYPE
    SYNTAX      INTEGER {
        lowestpriority(0),
        nextport(1)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies disconnect method. "
    ::= { rlPethPowerPseEntry 5 }

rlPethPowerPseTemperatureSensor OBJECT-TYPE
    SYNTAX      INTEGER (-200..200)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable identifies the pd temperature sensor. "
    ::= { rlPethPowerPseEntry 6 }

rlPethPowerPseInrushTestEnabled OBJECT-TYPE
    SYNTAX      INTEGER {
        enabled(0),
        disabled(1)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies if HW inrush test will be disabled.
        by default HW inrush test is enabled."
    ::= { rlPethPowerPseEntry 7 }

rlPethPowerPseLegacyDisabled OBJECT-TYPE
    SYNTAX      INTEGER {
        enabled(0),
        disabled(1)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable identifies poe Legacy global configuration mode"
    ::= { rlPethPowerPseEntry 8 }


--rlPethPdPortTable

rlPethPdPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPethPdPortEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        " The table listing additional read-write information for Power Over Ethernet - PD side."
    ::= {rlPoe 4 }

rlPethPdPortEntry  OBJECT-TYPE
    SYNTAX      RlPethPdPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " An entry in the rlPethPdPortTable."
    INDEX    { rlPethPdPortIndex }
    ::= {rlPethPdPortTable  1}

RlPethPdPortEntry ::= SEQUENCE {
    rlPethPdPortIndex               		InterfaceIndex,
    rlPethPdPortSupportPoeType      		RlPoeType,
    rlPethPdPortOperPoeType         		RlPoeType,
    rlPethPdPortPowerRequest        		Unsigned32,
    rlPethPdPortPowerAvailable      		Unsigned32,
	rlPethPdPortForcedMode					RlPoeType,
	rlPethPdPortNegotiationProtocolOwner	INTEGER
}

rlPethPdPortIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the power Ethernet PD
         port within group rlPethPdPortGroupIndex to which the
         power Ethernet PSE entry is connected."
    ::= { rlPethPdPortEntry 1 }

rlPethPdPortSupportPoeType OBJECT-TYPE
    SYNTAX  RlPoeType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the PoE type of the PD port (AF/AT/60W)"
    ::= { rlPethPdPortEntry 2 }

rlPethPdPortOperPoeType OBJECT-TYPE
    SYNTAX  RlPoeType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the operational PoE status of the PD port"
    ::= { rlPethPdPortEntry 3 }

rlPethPdPortPowerRequest OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the requested power the PD port request from the PSE in mili-Watts"
    ::= { rlPethPdPortEntry 4 }

rlPethPdPortPowerAvailable OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the available power the PSE port offers to the PD port in mili-Watts"
    ::= { rlPethPdPortEntry 5 }

rlPethPdPortForcedMode OBJECT-TYPE
    SYNTAX      RlPoeType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable indicates the powered PD port forced mode"
    ::= { rlPethPdPortEntry 6 }	

rlPethPdPortNegotiationProtocolOwner OBJECT-TYPE
    SYNTAX      INTEGER {
        protocolOwnerNone(0),
        protocolOwnerCDP(1),
		protocolOwnerLLDP(2),
        protocolOwnerCDPExpired(3),
        protocolOwnerLLDPExpired(4)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable indicates the protocol owner on power management negotiation protocol"
    ::= { rlPethPdPortEntry 7 }	


--rlPethPseUnitTable
	
rlPethPseUnitTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPethPseUnitEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        " The table listing additional read-write information for Power Over Ethernet unit capabilities."
    ::= {rlPoe 5 }

rlPethPseUnitEntry  OBJECT-TYPE
    SYNTAX      RlPethPseUnitEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " An entry in the rlPethPseUnitTable."
    INDEX    { rlPethUnitIndex } 
    ::= {rlPethPseUnitTable  1 }

RlPethPseUnitEntry ::= SEQUENCE {
    rlPethUnitIndex          INTEGER,
    rlPethUnitType           INTEGER,
	rlPethUnitColor			 INTEGER
}

rlPethUnitIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..8)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the unit id.  
		 It means box in the stack, module in a
         rack and the value 1 MUST be used for non-modular devices.
         Furthermore, the same value MUST be used in this variable,
         PethPowerPseGroupIndex, and pethNotificationControlGroupIndex
         to refer to a given box in a stack or module in the rack."
    ::= { rlPethPseUnitEntry 1 }

rlPethUnitType OBJECT-TYPE
    SYNTAX      INTEGER {
        unitTypeNone(0),
        unitTypePSE(1),
        unitTypePD(2),
        unitTypePSEPD(3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable identifies the unit type (PSE/PD/Both/None)."
    ::= { rlPethPseUnitEntry 2 }	
	
rlPethUnitColor OBJECT-TYPE
    SYNTAX      INTEGER {
        unitColorNone(0),
        unitColorGreen(1),
        unitColorYellow(2),
        unitColorRed(3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable identifies the unit PSE status (color can be green,yellow,red)."
    ::= { rlPethPseUnitEntry 3 }	

--
-- Clear port counters Section
--

rlPethPseCountersClear OBJECT-TYPE
    SYNTAX  InterfaceIndexOrZero
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Clear poe port counter. By setting the MIB to 0x0FFFFFFF, all poe ports counters are set to zero. 
		by Setting to port index, all specific poe port counters are set to zero"
    ::= {rlPoe 6}

--rlPethHwRevisionPseTable

rlPethHwRevisionPseTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPethHwRevisionPseEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        " The table listing additional read - only information for Power Over Ethernet PSE chipset HW Revision."
    ::= {rlPoe 7 }

rlPethHwRevisionPseEntry  OBJECT-TYPE
    SYNTAX      RlPethHwRevisionPseEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " An entry in the rlPethHwRevisionPseTable."
    INDEX    { rlPethHwRevisionPseGroupIndex, rlPethHwRevisionPseDeviceIndex }
    ::= {rlPethHwRevisionPseTable  1 }

RlPethHwRevisionPseEntry ::= SEQUENCE {
    rlPethHwRevisionPseGroupIndex     INTEGER,
    rlPethHwRevisionPseDeviceIndex    INTEGER,
    rlPethHwRevisionPseValue          DisplayString,
    rlPethHwRevisionVopStatus         INTEGER  
}

rlPethHwRevisionPseGroupIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..8)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the group
         containing the port to which a power Ethernet PSE is
         connected.  Group means box in the stack, module in a
         rack and the value 1 MUST be used for non-modular devices."
    ::= { rlPethHwRevisionPseEntry 1 }

rlPethHwRevisionPseDeviceIndex OBJECT-TYPE
    SYNTAX      INTEGER (0..7)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the device within the group
         containing the port to which a power Ethernet PSE is connected."
    ::= { rlPethHwRevisionPseEntry 2 }

rlPethHwRevisionPseValue OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(0..20))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable identifies the MCU HW version."
    ::= { rlPethHwRevisionPseEntry 3 }
    
rlPethHwRevisionVopStatus OBJECT-TYPE
    SYNTAX      INTEGER {
        deviceOk(0),
        detectionError(1),
        classificationError(2),
        legacyError(3),
        undefinedState(4)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies status of VoP problem in PoE device"
    DEFVAL { 0 }
    ::= { rlPethHwRevisionPseEntry 4 }

rlPoeClassErrorDetectionStatus OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies if class detection error is enabled (true) or disabled (false)"
    DEFVAL { true }
    ::= { rlPoe 8 }

--rlPethPerPseTable

rlPethPerPseTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPethPerPseEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        " The table listing additional information for Power Over Ethernet ports per PSE device."
    ::= {rlPoe 9 }

rlPethPerPseEntry  OBJECT-TYPE
    SYNTAX      RlPethPerPseEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " An entry in the rlPethPerPseTable."
    INDEX    { rlPethPerPseGroupIndex, rlPethPerPseDeviceIndex }
    ::= {rlPethPerPseTable  1 }

RlPethPerPseEntry ::= SEQUENCE {    
    rlPethPerPseGroupIndex            INTEGER,
    rlPethPerPseDeviceIndex           INTEGER,
	rlPethPerPseTemperatureValue      INTEGER
}

rlPethPerPseGroupIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..8)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the group
         containing the port to which a power Ethernet PSE is
         connected.  Group means box in the stack, module in a
         rack and the value 1 MUST be used for non-modular devices."
    ::= { rlPethPerPseEntry 1 }

rlPethPerPseDeviceIndex OBJECT-TYPE
    SYNTAX      INTEGER (0..7)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This variable uniquely identifies the PSE device within the group."
    ::= { rlPethPerPseEntry 2 }

rlPethPerPseTemperatureValue OBJECT-TYPE
    SYNTAX      INTEGER (-200..200)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This variable represents temperature reported from PSE device."
    ::= { rlPethPerPseEntry 3 }

END

