RADLAN-rlFft DEFINITIONS ::= BEGIN

-- Title:      RADLAN FFT Private Extension
-- Version:    7.37.00.00
-- Date:       17 May 2004

IMPORTS
    rnd                                                     FROM RADLAN-MIB
    Unsigned32, IpAddress,
    MODULE-IDENTITY, OBJECT-TYPE                            FROM SNMPv2-SMI
    RowStatus, TruthValue, PhysAddress, DisplayString,
    TEXTUAL-CONVENTION                                      FROM SNMPv2-TC
    InetAddress, InetAddressType,
    InetAddressPrefixLength                                 FROM INET-ADDRESS-MIB;


    Percents ::= TEXTUAL-CONVENTION
                 STATUS  current
                 DESCRIPTION
                     "Specifies percents."
                 SYNTAX  INTEGER (0..100)

    NetNumber ::= TEXTUAL-CONVENTION
                 STATUS  current
                 DESCRIPTION
                     "Specifies the network identification."
                 SYNTAX OCTET STRING (SIZE(4))


---
---  rlIpFFT
---

rlFFT            MODULE-IDENTITY
                 LAST-UPDATED "200406010000Z"
                 ORGANIZATION "Marvell Semiconductor, Inc."
                 CONTACT-INFO
					"5488 Marvell Lane
					Santa Clara, CA 95054
					USA

					Website:  www.marvell.com"
                 DESCRIPTION
                      "The private MIB module definition for RND Fast Forwarding Tables."
                 REVISION "200406010000Z"
                 DESCRIPTION
                      "Initial version of this MIB."
                 ::= { rnd 47 }



rlIpFFT      OBJECT IDENTIFIER ::= { rlFFT 1 }

rlIpFftMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "MIB's version, the current version is 1."
    ::= { rlIpFFT 1 }

rlInetMaxFftNumber OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximum number of IP FFTs."
    ::= { rlIpFFT 2 }

rlInetFftDynamicSupported OBJECT-TYPE
    SYNTAX  INTEGER {
        supported (1),
        unsupported (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether dynamic IP FFTs are supported."
    ::= { rlIpFFT 3 }

rlInetFftSubnetSupported OBJECT-TYPE
    SYNTAX  INTEGER {
        supported (1),
        unsupported (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether subtable per IP subnet is supported."
    ::= { rlIpFFT 4 }

rlIpFftUnknownAddrMsgUsed OBJECT-TYPE
    SYNTAX  INTEGER {
        used (1),
        unused (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether the 3SW uses the unknown address message."
    ::= { rlIpFFT 5 }

rlInetFftAgingTimeSupported OBJECT-TYPE
    SYNTAX  INTEGER {
        supported (1),
        unsupported (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether aging time is supported."
    ::= { rlIpFFT 6 }

rlIpFftSrcAddrSupported OBJECT-TYPE
    SYNTAX  INTEGER {
        supported (1),
        unsupported (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether an IP subtable per station contains source IP address."
    ::= { rlIpFFT 7 }

rlInetFftAgingTimeout OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The aging timeout in seconds."
    ::= { rlIpFFT 8 }

rlIpFftRedBoundary OBJECT-TYPE
    SYNTAX  Percents
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The red boundary in percents."
    ::= { rlIpFFT 9 }

rlIpFftYellowBoundary OBJECT-TYPE
    SYNTAX  Percents
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The yellow boundary in percents."
    ::= { rlIpFFT 10 }

--rlIpFftPollingInterval OBJECT-TYPE
--    SYNTAX  INTEGER
--    MAX-ACCESS  read-write
--    STATUS    current
--    DESCRIPTION
--        "The polling interval for dynamic IP FFTs support in seconds."
--    ::= { rlIpFFT 11 }

--
-- The IP FFT Number Routers Table
--

rlInetFftNumTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlInetFftNumEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing routes' numbers of
         the IP SFFTs and IP NFFTs. "
    ::= { rlIpFFT 12 }

rlInetFftNumEntry OBJECT-TYPE
    SYNTAX  RlInetFftNumEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the containing routes' numbers
         of IP SFFT and IP NFFT "
    INDEX  { rlInetFftNumIndex, rlInetFftNumAddressType }
    ::= { rlInetFftNumTable 1 }

RlInetFftNumEntry ::= SEQUENCE {
    rlInetFftNumIndex             INTEGER,
    rlInetFftNumAddressType       InetAddressType,
    rlInetFftNumStnRoutesNumber   INTEGER,
    rlInetFftNumSubRoutesNumber   INTEGER,
    rlInetFftNumInetTomeRoutesNumber INTEGER
}

rlInetFftNumIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IP FFT. "
    ::= { rlInetFftNumEntry 1 }

rlInetFftNumAddressType OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The inet address type that are contained in the IP SFFT. "
    ::= { rlInetFftNumEntry 2 }

rlInetFftNumStnRoutesNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of routes that are contained in the IP SFFT. "
    ::= { rlInetFftNumEntry 3 }

rlInetFftNumSubRoutesNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of routes that are contained in the IP NFFT. "
    ::= { rlInetFftNumEntry 4 }

rlInetFftNumInetTomeRoutesNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of routes that are Inet To Me. "
    ::= { rlInetFftNumEntry 5 }


--
-- The IP Fast Forwarding Table per station
--

rlInetFftStnTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlInetFftStnEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table contains IP Fast Forwarding information
         per station for IP datagrams. "
    ::= { rlIpFFT 13 }

rlInetFftStnEntry OBJECT-TYPE
    SYNTAX  RlInetFftStnEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) contains the IP fast forwarding
          information for IP datagrams from a particular source and
          destination addresses."
    INDEX  { rlInetFftStnIndex, rlInetFftStnMrid, rlInetFftStnDstInetAddressType, rlInetFftStnDstInetAddress }
    ::= { rlInetFftStnTable 1 }

RlInetFftStnEntry ::= SEQUENCE {
    rlInetFftStnIndex          INTEGER,
    rlInetFftStnMrid           INTEGER,
    rlInetFftStnDstInetAddressType  InetAddressType,
    rlInetFftStnDstInetAddress      InetAddress,
    rlInetFftStnDstRouteInetPrefix  InetAddressPrefixLength,
    rlInetFftStnDstInetAddrType     INTEGER,
    rlInetFftStnDstMacAddress  PhysAddress,
    rlInetFftStnSrcMacAddress  PhysAddress,
    rlInetFftStnOutIfIndex     INTEGER,
    rlInetFftStnVid            INTEGER,
    rlInetFftStnTaggedMode     INTEGER,
    rlInetFftStnAge            INTEGER
}

rlInetFftStnIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IP FFT. "
    ::= { rlInetFftStnEntry 1 }

rlInetFftStnMrid OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The router's Instance Identifier in the SFFT. "
    ::= { rlInetFftStnEntry 2 }

rlInetFftStnDstInetAddressType OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Ip destination type for which this entry
         contains IP forwarding information."
    ::= { rlInetFftStnEntry 3 }

rlInetFftStnDstInetAddress OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP destination address for which this entry
         contains IP forwarding information."
    ::= { rlInetFftStnEntry 4 }

rlInetFftStnDstRouteInetPrefix OBJECT-TYPE
    SYNTAX  InetAddressPrefixLength
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "The IP destination prefix for which this entry
          contains IP forwarding information."
    ::= { rlInetFftStnEntry 5 }

rlInetFftStnDstInetAddrType OBJECT-TYPE
    SYNTAX  INTEGER {
        local (1),
        remote (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP destination address type. "
 ::= { rlInetFftStnEntry 6 }

rlInetFftStnDstMacAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC destination address."
    ::= { rlInetFftStnEntry 7}

rlInetFftStnSrcMacAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC source address."
    ::= { rlInetFftStnEntry 8 }

rlInetFftStnOutIfIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of ifIndex of output physical port."
    ::= { rlInetFftStnEntry 9 }

rlInetFftStnVid  OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The vid of the output port."
    ::= { rlInetFftStnEntry 10 }

rlInetFftStnTaggedMode OBJECT-TYPE
    SYNTAX  INTEGER {
        untagged  (1),
        tagged           (2),
        basedPortConfig  (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The tagged value of the port. When the Tagged field is not
         a part of the FFT table in the ASIC,
         the Tagged field gets the BasedPortConfig value "
    ::= { rlInetFftStnEntry 11 }

rlInetFftStnAge OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The age of the entry in seconds from the inserting."
    ::= { rlInetFftStnEntry 12 }

--
-- The IP Fast Forwarding Table per subnet
--

rlInetFftSubTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlInetFftSubEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing IP Fast Forwarding information
         per subnet for IP datagrams. "
    ::= { rlIpFFT 14 }

rlInetFftSubEntry OBJECT-TYPE
    SYNTAX  RlInetFftSubEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the IP fast forwarding
         information for IP datagrams from a particular source and
         destination addresses."
    INDEX  { rlInetFftSubMrid , rlInetFftSubDstInetSubnetType, rlInetFftSubDstInetSubnet, rlInetFftSubDstInetPrefix }

    ::= { rlInetFftSubTable 1 }

RlInetFftSubEntry ::= SEQUENCE {
    rlInetFftSubMrid                    INTEGER,
    rlInetFftSubDstInetSubnetType       InetAddressType,
    rlInetFftSubDstInetSubnet           InetAddress,
    rlInetFftSubDstInetPrefix           InetAddressPrefixLength,
    rlInetFftSubNextHopSetRefCount      INTEGER,
    rlInetFftSubNextHopCount            INTEGER,
    rlInetFftSubNextHopIfindex1         INTEGER,
    rlInetFftSubNextHopInetAddr1Type    InetAddressType,
    rlInetFftSubNextHopInetAddr1        InetAddress,
    rlInetFftSubNextHopIfindex2         INTEGER,
    rlInetFftSubNextHopInetAddr2Type    InetAddressType,
    rlInetFftSubNextHopInetAddr2        InetAddress,
    rlInetFftSubNextHopIfindex3         INTEGER,
    rlInetFftSubNextHopInetAddr3Type    InetAddressType,
    rlInetFftSubNextHopInetAddr3        InetAddress,
    rlInetFftSubNextHopIfindex4         INTEGER,
    rlInetFftSubNextHopInetAddr4Type    InetAddressType,
    rlInetFftSubNextHopInetAddr4        InetAddress,
    rlInetFftSubNextHopIfindex5         INTEGER,
    rlInetFftSubNextHopInetAddr5Type    InetAddressType,
    rlInetFftSubNextHopInetAddr5        InetAddress,
    rlInetFftSubNextHopIfindex6         INTEGER,
    rlInetFftSubNextHopInetAddr6Type    InetAddressType,
    rlInetFftSubNextHopInetAddr6        InetAddress,
    rlInetFftSubNextHopIfindex7         INTEGER,
    rlInetFftSubNextHopInetAddr7Type    InetAddressType,
    rlInetFftSubNextHopInetAddr7        InetAddress,
    rlInetFftSubNextHopIfindex8         INTEGER,
    rlInetFftSubNextHopInetAddr8Type    InetAddressType,
    rlInetFftSubNextHopInetAddr8        InetAddress,
    rlInetFftSubAge                     INTEGER
}

rlInetFftSubMrid OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The router's Instance Identifier in the NFFT. "
    ::= { rlInetFftSubEntry 1 }

rlInetFftSubDstInetSubnetType OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP destination subnet type for which this entry
         contains IP forwarding information."
    ::= { rlInetFftSubEntry 2 }

rlInetFftSubDstInetSubnet OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP destination subnet for which this entry
         contains IP forwarding information."
    ::= { rlInetFftSubEntry 3 }

rlInetFftSubDstInetPrefix OBJECT-TYPE
    SYNTAX  InetAddressPrefixLength
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP destination prefix for which this entry
         contains IP forwarding information."
    ::= { rlInetFftSubEntry 4 }

rlInetFftSubNextHopSetRefCount OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of NFFT entries that used the given NextHop set (ECMP path). "

    ::= { rlInetFftSubEntry 5 }

rlInetFftSubNextHopCount OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of used NextHops in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 6 }

rlInetFftSubNextHopIfindex1 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop Ifindex in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 7 }

rlInetFftSubNextHopInetAddr1Type OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop IP address type in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 8 }

rlInetFftSubNextHopInetAddr1 OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop IP address in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 9 }

rlInetFftSubNextHopIfindex2 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The second NextHop Ifindex in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 10 }

rlInetFftSubNextHopInetAddr2Type OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop IP address type in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 11 }

rlInetFftSubNextHopInetAddr2 OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The second NextHop IP address in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 12 }

rlInetFftSubNextHopIfindex3 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The third NextHop Ifindex in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 13 }

rlInetFftSubNextHopInetAddr3Type OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop IP address type in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 14 }

rlInetFftSubNextHopInetAddr3 OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The third NextHop IP address in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 15 }

rlInetFftSubNextHopIfindex4 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The fourth NextHop Ifindex in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 16 }

rlInetFftSubNextHopInetAddr4Type OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop IP address type in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 17 }

rlInetFftSubNextHopInetAddr4 OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The fourth NextHop IP address in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 18 }

rlInetFftSubNextHopIfindex5 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The fifth NextHop Ifindex in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 19 }

rlInetFftSubNextHopInetAddr5Type OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop IP address type in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 20 }

rlInetFftSubNextHopInetAddr5 OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The fifth NextHop IP address in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 21 }

rlInetFftSubNextHopIfindex6 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The six NextHop Ifindex in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 22 }

rlInetFftSubNextHopInetAddr6Type OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop IP address type in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 23 }

rlInetFftSubNextHopInetAddr6 OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The six NextHop IP address in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 24 }

rlInetFftSubNextHopIfindex7 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The seven NextHop Ifindex in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 25 }

rlInetFftSubNextHopInetAddr7Type OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop IP address type in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 26 }

rlInetFftSubNextHopInetAddr7 OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The seven NextHop IP address in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 27 }

rlInetFftSubNextHopIfindex8 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The eight NextHop Ifindex in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 28 }

rlInetFftSubNextHopInetAddr8Type OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The first NextHop IP address type in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 29 }

rlInetFftSubNextHopInetAddr8 OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The eight NextHop IP address in the given NextHop set (ECMP path) for the NFFT entry. "
    ::= { rlInetFftSubEntry 30 }

rlInetFftSubAge OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The age of the entry in seconds from the inserting."

    ::= { rlInetFftSubEntry 31 }

--
-- The IP FFT Counters Table
--

rlInetFftCountersTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlInetFftCountersEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing IP Counters information
         per one IP FFT."
    ::= { rlIpFFT 15 }

rlInetFftCountersEntry OBJECT-TYPE
    SYNTAX  RlInetFftCountersEntry
    MAX-ACCESS      not-accessible
    STATUS              current
    DESCRIPTION
        "An entry (conceptual row) containing the IP Counters
         information containing amount of IP datagrams passed
         by certain IP FFT."
    INDEX  { rlInetFftCountersIndex }
    ::= { rlInetFftCountersTable 1 }

RlInetFftCountersEntry ::= SEQUENCE {
    rlInetFftCountersIndex    INTEGER,
    rlInetFftInReceives       INTEGER,
    rlInetFftForwDatagrams    INTEGER,
    rlInetFftInDiscards       INTEGER
}

rlInetFftCountersIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IP FFT."
    ::= { rlInetFftCountersEntry 1 }

rlInetFftInReceives  OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The amount of received IP datagrams "
    ::= { rlInetFftCountersEntry 2 }

rlInetFftForwDatagrams OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The amount of forwarded IP datagrams "
    ::= { rlInetFftCountersEntry 3 }

rlInetFftInDiscards OBJECT-TYPE
    SYNTAX          INTEGER
    MAX-ACCESS          read-only
    STATUS              current
    DESCRIPTION
        "The amount of discarded IP datagrams "
    ::= { rlInetFftCountersEntry 4 }

--
-- The IP NextHop Table (used by NFFT and Remote SFFT)
--

rlInetFftNextHopTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlInetFftNextHopEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table contains NextHop information
         used for routing IP datagrams. "
    ::= { rlIpFFT 16 }

rlInetFftNextHopEntry OBJECT-TYPE
    SYNTAX  RlInetFftNextHopEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) contains the NextHop info
          information for routing IP datagrams."

    INDEX  { rlInetFftNextHopifindex, rlInetFftNextHopInetAddressType, rlInetFftNextHopInetAddress}
    ::= { rlInetFftNextHopTable 1 }

RlInetFftNextHopEntry ::= SEQUENCE {
    rlInetFftNextHopifindex        INTEGER,
    rlInetFftNextHopInetAddressType InetAddressType,
    rlInetFftNextHopInetAddress    InetAddress,
    rlInetFftNextHopValid          INTEGER,
    rlInetFftNextHopType           INTEGER,
    rlInetFftNextHopReferenceCount INTEGER,
    rlInetFftNextHopNetAddress     PhysAddress,
    rlInetFftNextHopVid            INTEGER,
    rlInetFftNextHopMacAddress     PhysAddress,
    rlInetFftNextHopOutIfIndex     INTEGER
}

rlInetFftNextHopifindex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the IP Interface index of the NextHop. "
    ::= { rlInetFftNextHopEntry 1 }

rlInetFftNextHopInetAddressType OBJECT-TYPE
    SYNTAX  InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP address type of a NextHop for which an entry contains
         IP forwarding information. "
    ::= { rlInetFftNextHopEntry 2 }


rlInetFftNextHopInetAddress OBJECT-TYPE
    SYNTAX  InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP address of a NextHop for which an entry contains
         IP forwarding information. "
    ::= { rlInetFftNextHopEntry 3 }

rlInetFftNextHopValid OBJECT-TYPE
    SYNTAX  INTEGER {
        valid (1),
        invalid (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The NextHop Valid bit. When L2 info is missing,
         a NextHop has Invalid value. "
 ::= { rlInetFftNextHopEntry 4 }

rlInetFftNextHopType OBJECT-TYPE
    SYNTAX  INTEGER {
        local  (1),
        remote (2),
        reject (3),
        drop   (4)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The NextHop type. "
 ::= { rlInetFftNextHopEntry 5 }

rlInetFftNextHopReferenceCount OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IF LPM is supported:
               If ecmp supported:
                 the field NextHop_ref_count used to save number
                 of NextHop SETs that use the NextHop.
               Otherwise, NextHop_ref_count used to save number of
                 NFFT entries that use the NextHop.
         IF LPM is NOT supported:
               NextHop_ref_count used to save number of
               Remote SFFT entries that use the NextHop. "
 ::= { rlInetFftNextHopEntry 6 }

rlInetFftNextHopNetAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The NextHop Physical Address."
 ::= { rlInetFftNextHopEntry 7 }

rlInetFftNextHopVid  OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The vid of the output port."
    ::= { rlInetFftNextHopEntry 8 }

rlInetFftNextHopMacAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC destination address."
    ::= { rlInetFftNextHopEntry 9}

rlInetFftNextHopOutIfIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of ifIndex of output physical port."
    ::= { rlInetFftNextHopEntry 10 }

--
-- The L2 info Table (used by NextHop and Direct SFFT)
--

rlInetFftL2InfoTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlInetFftL2InfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table contains L2 information
         used for routing IP datagrams. "
    ::= { rlIpFFT 17 }

rlInetFftL2InfoEntry OBJECT-TYPE
    SYNTAX  RlInetFftL2InfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) contains the L2 info
          information for routing IP datagrams."

    INDEX  { rlInetFftL2InfoIfindex, rlInetFftL2InfoDstMacAddress }
    ::= { rlInetFftL2InfoTable 1 }

RlInetFftL2InfoEntry ::= SEQUENCE {
    rlInetFftL2InfoIfindex        INTEGER,
    rlInetFftL2InfoDstMacAddress  PhysAddress,
    rlInetFftL2InfoValid          INTEGER,
    rlInetFftL2InfoType           INTEGER,
    rlInetFftL2InfoReferenceCount INTEGER,
    rlInetFftL2InfoVid            INTEGER,
    rlInetFftL2InfoSrcMacAddress  PhysAddress,
    rlInetFftL2InfoOutIfIndex     INTEGER,
    rlInetFftL2InfoTaggedMode     INTEGER
}

rlInetFftL2InfoIfindex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The VLAN Ifindex of the destination port. "
    ::= { rlInetFftL2InfoEntry 1 }

rlInetFftL2InfoDstMacAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC destination address."
    ::= { rlInetFftL2InfoEntry 2}

rlInetFftL2InfoValid OBJECT-TYPE
    SYNTAX  INTEGER {
        valid (1),
        invalid (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The L2 info entry valid bit. When L2 info is missing some information,
          an L2 info has Invalid value. "
 ::= { rlInetFftL2InfoEntry 3 }

rlInetFftL2InfoType OBJECT-TYPE
    SYNTAX  INTEGER {
        other (1),
        vlan  (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The L2 info type. With Enthernet media l2 info type is vlan.
        WIth Tunneling feature, l2 info type will be expanded. "
 ::= { rlInetFftL2InfoEntry 4 }

rlInetFftL2InfoReferenceCount OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
     "The reference count contains a number of
      NextHop entries that use this L2 info."
 ::= { rlInetFftL2InfoEntry 5 }

rlInetFftL2InfoVid OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The vid of the destination port. "
    ::= { rlInetFftL2InfoEntry 6 }

rlInetFftL2InfoSrcMacAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC source address placed to Ehernet Header of IP forwarded packet."
    ::= { rlInetFftL2InfoEntry 7}

rlInetFftL2InfoOutIfIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of ifIndex of output physical port the packet is forwarded through."
    ::= { rlInetFftL2InfoEntry 8 }

rlInetFftL2InfoTaggedMode OBJECT-TYPE
    SYNTAX  INTEGER {
        untagged  (1),
        tagged           (2),
        basedPortConfig  (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The tagged value of the port. When the Tagged field is not
         a part of the FFT table in the ASIC,
         the Tagged field get the BasedPortConfig value."
    ::= { rlInetFftL2InfoEntry 9 }

rlIpv6FftRedBoundary OBJECT-TYPE
    SYNTAX  Percents
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The red boundary in percents."
    ::= { rlIpFFT 18 }

rlIpv6FftYellowBoundary OBJECT-TYPE
    SYNTAX  Percents
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The yellow boundary in percents."
    ::= { rlIpFFT 19 }

---
--- rlIpxFFT
---

rlIpxFFT      OBJECT IDENTIFIER ::= { rlFFT 2 }

rlIpxFftMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "MIB's version, the current version is 1."
    ::= { rlIpxFFT 1 }

rlIpxMaxFftNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximun number of IPX FFTs. An IPX FFT gets a number
         from 1 until rlIpxMaxFftSetNumber."
    ::= { rlIpxFFT 2 }

rlIpxFftDynamicSupported OBJECT-TYPE
    SYNTAX  INTEGER {
        supported (1),
        unsupported (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether dynamic IPX FFTs are supported."
    ::= { rlIpxFFT 3 }

rlIpxFftNetworkSupported OBJECT-TYPE
    SYNTAX  INTEGER {
        supported (1),
        unsupported (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether subtable per IPX network is supported."
    ::= { rlIpxFFT 4 }

rlIpxFftUnknownAddrMsgUsed OBJECT-TYPE
    SYNTAX  INTEGER {
        used (1),
        unused (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether the 3SW uses the unknown address message."
    ::= { rlIpxFFT 5 }

rlIpxFftAgingTimeSupported OBJECT-TYPE
    SYNTAX  INTEGER {
        supported (1),
        unsupported (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether aging time is supported for subtable per station."
    ::= { rlIpxFFT 6 }

rlIpxFftSrcAddrSupported OBJECT-TYPE
    SYNTAX  INTEGER {
        supported (1),
        unsupported (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether an IPX subtable per station contains source
                       IPX address."
    ::= { rlIpxFFT 7 }

rlIpxFftAgingTimeout OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The aging timeout in seconds."
    ::= { rlIpxFFT 8 }

rlIpxFftRedBoundary OBJECT-TYPE
    SYNTAX  INTEGER (1..100)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The red boundary in percents."
    ::= { rlIpxFFT 9 }

rlIpxFftYellowBoundary OBJECT-TYPE
    SYNTAX  Percents
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The yellow boundary in percents."
    ::= { rlIpxFFT 10 }

--rlIpxFftPollingInterval OBJECT-TYPE
--    SYNTAX  INTEGER
--    MAX-ACCESS  read-write
--    STATUS    current
--    DESCRIPTION
--        "The polling interval for dynamic IPX FFTs support in seconds."
--    ::= { rlIpxFFT 11 }

--
-- The IPX FFT Number Routers Table
--

rlIpxFftNumTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlIpxFftNumEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing number routes of
         the IPX Fast Forwarding Table. "
    ::= { rlIpxFFT 12 }

rlIpxFftNumEntry OBJECT-TYPE
    SYNTAX  RlIpxFftNumEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the containing number routes of
         of IPX SFFT and IPX NFFT "
    INDEX  { rlIpxFftNumIndex }
    ::= { rlIpxFftNumTable 1 }

RlIpxFftNumEntry ::= SEQUENCE {
    rlIpxFftNumIndex            INTEGER,
    rlIpxFftNumStnRoutesNumber  INTEGER,
    rlIpxFftNumSubRoutesNumber  INTEGER
}

rlIpxFftNumIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The value of the index of the IPX FFT. "
    ::= { rlIpxFftNumEntry 1 }

rlIpxFftNumStnRoutesNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of routes containing in the IPX SFFT. "
    ::= { rlIpxFftNumEntry 2 }

rlIpxFftNumSubRoutesNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of routes containing in the IPX NFFT. "
::= { rlIpxFftNumEntry 3 }

--
-- The IPX Fast Forwarding Table per station
--

rlIpxFftStnTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlIpxFftStnEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing IPX Fast Forwarding information
         per station for IPX. "
    ::= { rlIpxFFT 13 }

rlIpxFftStnEntry OBJECT-TYPE
    SYNTAX  RlIpxFftStnEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the IP fast forwarding
         information for IP datagrams from a particular source and
         destination addresses."
    INDEX  { rlIpxFftStnIndex, rlIpxFftStnDstNetid, rlIpxFftStnDstNode,
             rlIpxFftStnSrcNetid, rlIpxFftStnSrcNode }
    ::= { rlIpxFftStnTable 1 }

RlIpxFftStnEntry ::= SEQUENCE {
    rlIpxFftStnIndex            INTEGER,
    rlIpxFftStnDstNetid         NetNumber,
    rlIpxFftStnDstNode          PhysAddress,
    rlIpxFftStnSrcNetid         NetNumber,
    rlIpxFftStnSrcNode          PhysAddress,
    rlIpxFftStnDstIpxAddrType   INTEGER,
    rlIpxFftStnEncapsulation    INTEGER,
    rlIpxFftStnDstMacAddress    PhysAddress,
    rlIpxFftStnSrcMacAddress    PhysAddress,
    rlIpxFftStnOutIfIndex       INTEGER,
    rlIpxFftStnTci              INTEGER,
    rlIpxFftStnFacsIndex        INTEGER,
    rlIpxFftStnAge              INTEGER
}

rlIpxFftStnIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IPX FFT. "
    ::= { rlIpxFftStnEntry 1 }

rlIpxFftStnDstNetid OBJECT-TYPE
    SYNTAX  NetNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination network for which this entry
         contains IPX forwarding information."
    ::= { rlIpxFftStnEntry 2 }

rlIpxFftStnDstNode OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination node for which this entry
         contains IPX forwarding information."
    ::= { rlIpxFftStnEntry 3 }

rlIpxFftStnSrcNetid OBJECT-TYPE
    SYNTAX  NetNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source network for which this entry
         contains IPX forwarding information."
    ::= { rlIpxFftStnEntry 4 }

rlIpxFftStnSrcNode OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination node for which this entry
         contains IPX forwarding information."
    ::= { rlIpxFftStnEntry 5 }

rlIpxFftStnDstIpxAddrType OBJECT-TYPE
    SYNTAX  INTEGER {
        local (1),
        remote (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination address type. "
    ::= { rlIpxFftStnEntry 6 }

rlIpxFftStnEncapsulation OBJECT-TYPE
    SYNTAX  INTEGER {
        novell(1),
        ethernet(2),
        llc(3),
        snap(4)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "The encapsulation method associated with this route."
    ::= { rlIpxFftStnEntry 7 }

rlIpxFftStnDstMacAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC destination address."
    ::= { rlIpxFftStnEntry 8 }

rlIpxFftStnSrcMacAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC source address."
    ::= { rlIpxFftStnEntry 9 }

rlIpxFftStnOutIfIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of ifIndex of output physical port."
    ::= { rlIpxFftStnEntry 10 }

rlIpxFftStnTci OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of TCI or 0."
    ::= { rlIpxFftStnEntry 11 }

rlIpxFftStnFacsIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of index of the FACS Table."
    ::= { rlIpxFftStnEntry 12 }

rlIpxFftStnAge OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The age of the entry in seconds."
    ::= { rlIpxFftStnEntry 13 }

--
-- The IPX Fast Forwarding Table per network
--

rlIpxFftSubTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlIpxFftSubEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing IPX Fast Forwarding information
         per network for IPX . "
    ::= { rlIpxFFT 14 }

rlIpxFftSubEntry OBJECT-TYPE
    SYNTAX  RlIpxFftSubEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the IP fast forwarding
         information for IP datagrams from a particular source and
         destination addresses."
    INDEX  { rlIpxFftSubIndex, rlIpxFftSubDstNetid }
    ::= { rlIpxFftSubTable 1 }

RlIpxFftSubEntry ::= SEQUENCE {
    rlIpxFftSubIndex            INTEGER,
    rlIpxFftSubDstNetid         NetNumber,
    rlIpxFftSubEncapsulation    INTEGER,
    rlIpxFftSubDstMacAddress    PhysAddress,
    rlIpxFftSubSrcMacAddress    PhysAddress,
    rlIpxFftSubOutIfIndex       INTEGER,
    rlIpxFftSubTci              INTEGER,
    rlIpxFftSubFacsIndex        INTEGER,
    rlIpxFftSubAge              INTEGER
}

rlIpxFftSubIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IPX FFT. "
    ::= { rlIpxFftSubEntry 1 }

rlIpxFftSubDstNetid OBJECT-TYPE
    SYNTAX  NetNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination network for which this entry
         contains IPX forwarding information."
    ::= { rlIpxFftSubEntry 2 }

rlIpxFftSubEncapsulation OBJECT-TYPE
    SYNTAX  INTEGER {
        novell(1),
        ethernet(2),
        llc(3),
        snap(4)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The encapsulation method associated with this route."
    ::= { rlIpxFftSubEntry 3 }

rlIpxFftSubDstMacAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC destination address."
    ::= { rlIpxFftSubEntry 4 }

rlIpxFftSubSrcMacAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC source address."
    ::= { rlIpxFftSubEntry 5 }

rlIpxFftSubOutIfIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of ifIndex of output physical port."
    ::= { rlIpxFftSubEntry 6 }

rlIpxFftSubTci OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of TCI or 0."
    ::= { rlIpxFftSubEntry 7 }

rlIpxFftSubFacsIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of index of the FACS Table."
    ::= { rlIpxFftSubEntry 8 }

rlIpxFftSubAge OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The age of the entry in seconds."
    ::= { rlIpxFftSubEntry 9 }

--
-- The IPX FFT Counters Table
--

rlIpxFftCountersTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlIpxFftCountersEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing IPX Counters information
         per one IPX FFT."
    ::= { rlIpxFFT 15 }

rlIpxFftCountersEntry OBJECT-TYPE
    SYNTAX  RlIpxFftCountersEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the IP Counters
         information containing amount of IPX datagrams passed
         by certain IPX FFT."
    INDEX  { rlIpxFftCountersIndex }
    ::= { rlIpxFftCountersTable 1 }

RlIpxFftCountersEntry ::= SEQUENCE {
    rlIpxFftCountersIndex   INTEGER,
    rlIpxFftInReceives      INTEGER,
    rlIpxFftForwDatagrams   INTEGER,
    rlIpxFftInDiscards      INTEGER
}

rlIpxFftCountersIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IPX FFT."
    ::= { rlIpxFftCountersEntry 1 }

rlIpxFftInReceives  OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The amount of received IPX datagrams "
    ::= { rlIpxFftCountersEntry 2 }

rlIpxFftForwDatagrams OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The amount of forwarded IPX datagrams "
    ::= { rlIpxFftCountersEntry 3 }

rlIpxFftInDiscards OBJECT-TYPE
    SYNTAX          INTEGER
    MAX-ACCESS          read-only
    STATUS              current
    DESCRIPTION
        "The amount of discarded IPX datagrams "
    ::= { rlIpxFftCountersEntry 4 }

---
--- rlIpmFFT
---

rlIpmFFT    OBJECT IDENTIFIER ::= { rlFFT 3 }

rlIpmFftMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "MIB's version, the current version is 1."
    ::= { rlIpmFFT 1 }

rlIpmMaxFftNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximun number of IPM FFTs. NT_IPM  gets a number
         from Host Parameters"
    ::= { rlIpmFFT 2 }

rlIpmFftDynamicSupported OBJECT-TYPE
    SYNTAX  INTEGER {
        supported   (1),
        unsupported (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether dynamic IPM FFTs are supported.
         An NT_IPM  gets a number  from Host Parameters"
    ::= { rlIpmFFT 3 }

rlIpmFftUnknownAddrMsgUsed OBJECT-TYPE
    SYNTAX  INTEGER {
        used   (1),
        unused (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether the 3SW uses the unknown address message.
         An NT_IPM  gets a number  from Host Parameters"
    ::= { rlIpmFFT 4 }

rlIpmFftUserAgingTimeout OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The aging timeout in seconds. SNMP user writes.
         There is a default value of aging timeout."
    ::= { rlIpmFFT 5 }

rlIpmFftRouterAgingTimeout OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The aging timeout in seconds. NT_IPM keeps value that
         Router level gave. This is high priority value for aging timeout."
    ::= { rlIpmFFT 6 }

--rlIpmFftPollingInterval OBJECT-TYPE
--    SYNTAX  INTEGER
--    MAX-ACCESS  read-only
--    STATUS    current
--    DESCRIPTION
--        "The polling interval  for dynamic IPM FFT's support in seconds."
--    ::= { rlIpmFFT 7 }


--
-- The IPM FFT Number Routers Table
--

rlIpmFftNumTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlIpmFftNumEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing number routes of
         the IPM Fast Forwarding Table. "
    ::= { rlIpmFFT 8 }

rlIpmFftNumEntry OBJECT-TYPE
    SYNTAX      RlIpmFftNumEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the containing number routes of
         an IPM FFT."
    INDEX  { rlIpmFftNumIndex }
  ::= { rlIpmFftNumTable 1 }

RlIpmFftNumEntry ::= SEQUENCE {
    rlIpmFftNumIndex            INTEGER,
    rlIpmFftNumRoutesNumber     INTEGER
}

rlIpmFftNumIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IPM FFT."
    ::= { rlIpmFftNumEntry 1 }

rlIpmFftNumRoutesNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of routes containing in the IPM FFT."
    ::= { rlIpmFftNumEntry 2 }

--
-- The IPM Fast Forwarding Table
--

rlIpmFftTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlIpmFftEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing IPM Fast Forwarding information
         for IPM datagrams."
    ::= { rlIpmFFT 9 }

rlIpmFftEntry OBJECT-TYPE
    SYNTAX  RlIpmFftEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the IPM fast forwarding
         information for IP datagrams from a particular source and
         destination addresses."
    INDEX  { rlIpmFftIndex, rlIpmFftSrcIpAddress, rlIpmFftDstIpAddress }
    ::= { rlIpmFftTable 1 }

RlIpmFftEntry ::= SEQUENCE {
    rlIpmFftIndex           INTEGER,
    rlIpmFftSrcIpAddress    IpAddress,
    rlIpmFftDstIpAddress    IpAddress,
    rlIpmFftSrcIpMask       IpAddress,
    rlIpmFftInputIfIndex    INTEGER,
    rlIpmFftInputVlanTag    INTEGER,
    rlIpmFftForwardAction   INTEGER,
    rlIpmFftInportAction    INTEGER,
    rlIpmFftAge             INTEGER
}

rlIpmFftIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IPM FFT. "
    ::= { rlIpmFftEntry 1 }

rlIpmFftSrcIpAddress OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP source address for which this entry
         contains IPM forwarding information."
    ::= { rlIpmFftEntry 2 }

rlIpmFftDstIpAddress OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IPM destination address for which this entry
         contains IPM forwarding information."
    ::= { rlIpmFftEntry 3 }

rlIpmFftSrcIpMask OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "The IP source mask for which this entry
          contains IP forwarding information."
    ::= { rlIpmFftEntry 4 }

rlIpmFftInputIfIndex    OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The input ifIndex for which this entry
         contains IPM forwarding information."
    ::= { rlIpmFftEntry 5 }

rlIpmFftInputVlanTag    OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The input Vlan tag together with input ifIndex defines
          pair (ifIndex, tag)"
    ::= { rlIpmFftEntry 6 }

rlIpmFftForwardAction   OBJECT-TYPE
    SYNTAX  INTEGER {
        forward(1),
        discard (2)
    }
    MAX-ACCESS          read-only
    STATUS              current
    DESCRIPTION
        "The IPM forward action."
    ::= { rlIpmFftEntry 7 }

rlIpmFftInportAction    OBJECT-TYPE
    SYNTAX  INTEGER {
        sentToCPU(1),
        discard (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IPM illegal input port action."
    ::= { rlIpmFftEntry 8 }

rlIpmFftAge OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The age of the entry in seconds from the moment of inserting. "
    ::= { rlIpmFftEntry 9 }

--
-- The IPM FFT Output Port and Tag Table
--

rlIpmFftPortTagTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlIpmFftPortTagEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing IPM FFT output port tag information
         for IPM datagrams."
    ::= { rlIpmFFT 10 }

rlIpmFftPortTagEntry OBJECT-TYPE
    SYNTAX  RlIpmFftPortTagEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the IPM FFT output port tag
         information for IP datagrams from a particular source and
         destination addresses."
    INDEX  { rlIpmFftPortIndex, rlIpmFftPortSrcIpAddress,
             rlIpmFftPortDstIpAddress, rlIpmFftPortOutputifIndex,
             rlIpmFftPortOutputTag }
    ::= { rlIpmFftPortTagTable 1 }

RlIpmFftPortTagEntry ::= SEQUENCE {
    rlIpmFftPortIndex           INTEGER,
    rlIpmFftPortSrcIpAddress    IpAddress,
    rlIpmFftPortDstIpAddress    IpAddress,
    rlIpmFftPortOutputifIndex   INTEGER,
    rlIpmFftPortOutputTag       INTEGER
}

rlIpmFftPortIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IPM FFT. "
    ::= { rlIpmFftPortTagEntry 1 }

rlIpmFftPortSrcIpAddress OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP source address for which this entry
         contains IPM output port tag information."
    ::= { rlIpmFftPortTagEntry 2 }

rlIpmFftPortDstIpAddress OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IPM destination address for which this entry
         contains IPM port tag information."
    ::= { rlIpmFftPortTagEntry 3 }

rlIpmFftPortOutputifIndex   OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The output ifIndex "
    ::= { rlIpmFftPortTagEntry 4 }

rlIpmFftPortOutputTag   OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The output Vlan tag together with output ifIndex defines
          pair (ifIndex, tag)"
    ::= { rlIpmFftPortTagEntry 5 }

--
-- The IPM FFT Counters Table
--

rlIpmFftCountersTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlIpmFftCountersEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table containing IPM Counters information
         per FFT number. "
    ::= { rlIpmFFT 11 }

rlIpmFftCountersEntry OBJECT-TYPE
    SYNTAX  RlIpmFftCountersEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) containing the IPM Counters
         information containing amount of IPM datagrams passed by certain FFT."
    INDEX  { rlIpmFftCountersIndex }
    ::= { rlIpmFftCountersTable 1 }

RlIpmFftCountersEntry ::= SEQUENCE {
    rlIpmFftCountersIndex       INTEGER,
    rlIpmFftInReceives          INTEGER,
    rlIpmFftForwDatagrams       INTEGER,
    rlIpmFftInDiscards          INTEGER
}

rlIpmFftCountersIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the index of the IPM FFT. "
    ::= { rlIpmFftCountersEntry 1 }

rlIpmFftInReceives  OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The amount of received IPM datagrams "
    ::= { rlIpmFftCountersEntry 2 }

rlIpmFftForwDatagrams OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The amount of forwarded IPM datagrams "
    ::= { rlIpmFftCountersEntry 3 }

rlIpmFftInDiscards OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The amount of discarded IPM datagrams "
    ::= { rlIpmFftCountersEntry 4 }

END

