RADLAN-rndApplications DEFINITIONS ::= BEGIN

-- Title:      RADLAN Application Private Extension
-- Version:    7.37.00.00
-- Date:       17 May 2004

IMPORTS
    rnd                                                     FROM RADLAN-MIB
    InterfaceIndexOrZero, InterfaceIndex, ifIndex           FROM IF-MIB
    TEXTUAL-CONVENTION,
    DisplayString, RowStatus, TruthValue                    FROM SNMPv2-TC
    Unsigned32, Counter32, IpAddress,
    MODULE-IDENTITY, OBJECT-TYPE                            FROM SNMPv2-SMI
    InetAddressType, InetAddress                            FROM INET-ADDRESS-MIB;

rndApplications  MODULE-IDENTITY
                 LAST-UPDATED "200406010000Z"
                 ORGANIZATION "Marvell Semiconductor, Inc."
                 CONTACT-INFO
					"5488 Marvell Lane
					Santa Clara, CA 95054
					USA

					Website:  www.marvell.com"
                 DESCRIPTION
                      "The private MIB module definition for RND applications MIB."
                 REVISION "200406010000Z"
                 DESCRIPTION
                      "Initial version of this MIB."
                 ::= { rnd 35 }


-- Obsolete
-- rsServerDispatcher  OBJECT IDENTIFIER ::= { rndApplications 1}

-- rndMidLevelManagement group contains variables which direct the mid-level
-- management stations how to monitor and manage their domains.

rndMidLevelManagement  OBJECT IDENTIFIER ::= { rndApplications 2} -- NEW Group

rndAlarmOptions  OBJECT IDENTIFIER ::= { rndMidLevelManagement 2}

rndAlarmEnabling OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates whether alarms should be issued to the high-level
         NMS "
     ::=  { rndAlarmOptions 1 }

rndAlarmInterval OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates the minimal period of time which must pass after issuing
         an alarm before issuing the same alarm again."
     ::=  { rndAlarmOptions 2 }

rndMonitoredElementsTable  OBJECT-TYPE
   SYNTAX SEQUENCE OF RndMonitoredElementEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
    "The table of monitored elements of the network"
    ::= {rndMidLevelManagement 3}

rndMonitoredElementEntry  OBJECT-TYPE
   SYNTAX RndMonitoredElementEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
       " The row definition for this table."
   INDEX { rndMonitoredElementAddress }
    ::= {rndMonitoredElementsTable 1}

RndMonitoredElementEntry ::= SEQUENCE {

rndMonitoredElementAddress    IpAddress,
rndMonitoredElementCommunity  DisplayString(SIZE(1..20)),
rndMonitoredElementLabel      DisplayString(SIZE(1..20)),
rndDefaultPollingInterval     INTEGER,
rndDefaultLogFile             DisplayString,
rndMonitoredElementStatus     RowStatus
}
rndMonitoredElementAddress OBJECT-TYPE
   SYNTAX IpAddress
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION
    "The IP address of the monitored element"
     ::=  {rndMonitoredElementEntry  1 }

rndMonitoredElementCommunity OBJECT-TYPE
   SYNTAX DisplayString(SIZE(1..20))
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The community of the monitored element"
     ::=  {rndMonitoredElementEntry 2  }

rndMonitoredElementLabel OBJECT-TYPE
   SYNTAX DisplayString(SIZE(1..20))
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The label assigned by the network manager to the monitored element"
     ::=  {rndMonitoredElementEntry 3}

rndDefaultPollingInterval OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The default period of time between two consecutive pollings of the
     monitored element for the value of an object instance. If no other polling
     interval is specifically assigned to the monitored object instance, this
     one will be used"
     ::=  {rndMonitoredElementEntry 4}

rndDefaultLogFile OBJECT-TYPE
   SYNTAX DisplayString
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The default file path of the log-file which will contain the polling
     results for the monitored element. If no other file path is specifically
     assigned to the monitored object instance, this log-file will be used."

     ::=  {rndMonitoredElementEntry  5}

rndMonitoredElementStatus OBJECT-TYPE
   SYNTAX RowStatus
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
         "It is used to manage the monitored elements table and indicates
          the current monitoring status of an element."
     ::=  {rndMonitoredElementEntry  6}

rndMonitoringTable  OBJECT-TYPE
   SYNTAX SEQUENCE OF RndMonitoringEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
    "The table of monitored object instances. Each monitored object instance
     belongs to a monitored element previously entered in the
     rndMonitoredElementsTable. "
    ::= {rndMidLevelManagement 4}

rndMonitoringEntry OBJECT-TYPE
   SYNTAX RndMonitoringEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
       " The row definition for this table."
   INDEX { rndMonitoredElement, IMPLIED rndMonitoredObjectInstanceLabel }
    ::= {rndMonitoringTable 1}

RndMonitoringEntry ::= SEQUENCE {

rndMonitoredElement             DisplayString(SIZE(1..20)),
rndMonitoredObjectInstanceLabel DisplayString,
rndMonitoredObjectName          DisplayString,
rndMonitoredObjectIdentifier    OBJECT IDENTIFIER,
rndMonitoredObjectInstance      OBJECT IDENTIFIER,
rndMonitoredObjectSyntax        INTEGER,
rndMonitoringInterval           INTEGER,
rndAlarmMaxTreshold             INTEGER,
rndAlarmMinTreshold             INTEGER,
rndMonitoringLogfile            DisplayString,
rndMonitoringEntryStatus        RowStatus,
rndMonitoredIntegerInstance     INTEGER
}

rndMonitoredElement OBJECT-TYPE
   SYNTAX DisplayString(SIZE(1..20))
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION
    "A label assigned by the network manager to a monitored element to
     which this monitored object instance belongs. This label must have
     been previously entered in an instance of rndMonitoredElementLabel"
    ::=  {rndMonitoringEntry  1}

rndMonitoredObjectInstanceLabel OBJECT-TYPE
   SYNTAX DisplayString(SIZE(1..20))
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION
    "The label assigned by the network manager to the monitored object instance"
    ::=  {rndMonitoringEntry  2}

rndMonitoredObjectName OBJECT-TYPE
   SYNTAX DisplayString(SIZE(0..20))
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The symbolic object type name of the object to which the monitored object
     instance belongs (as it appears the MIB module definition). In case of
     ambiguity the <MIB module name> : <object type name> format should be used.
     An instance of rndMonitoredObjectName need not be assigned any value, if
     the corresponding instance of rndMonitoredObjectIdentifier is assigned a
     value, since any one of these, together with the object instance
     identifier, suffices to unambigously identify the monitored object
     instance."

    ::=  {rndMonitoringEntry  3}

rndMonitoredObjectIdentifier OBJECT-TYPE
   SYNTAX OBJECT IDENTIFIER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The object identifier of the object to which the monitored object
     instance belongs.
     An instance of rndMonitoredObjectIdentifier need not be assigned any value, if
     the corresponding instance of rndMonitoredObjectName is assigned a value,
     since any one of these, together with the object instance identifier,
     suffices to unambigously identify the monitored object instance."

    ::=  {rndMonitoringEntry  4}

rndMonitoredObjectInstance OBJECT-TYPE
   SYNTAX OBJECT IDENTIFIER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
        "The instance identifier (key) of the monitored object instance."
    ::=  {rndMonitoringEntry  5}

rndMonitoredObjectSyntax OBJECT-TYPE
   SYNTAX INTEGER {
       integer(1),
       octet-string(2),
       ip-address(3),
       object-identifier(4)
     }

   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The syntax of the monitored object instance (i.e., the syntax of the object
     type of the object to which the monitored instance belongs).
     Need not be assigned any value if the corresponding instance of
     rndMonitoredObjectName has been assigned a value"
    ::=  {rndMonitoringEntry  6}

rndMonitoringInterval OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The period of time between two consecutive retrievals of the monitored
     object instance's value."
    ::=  {rndMonitoringEntry  7}


rndAlarmMaxTreshold OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The value of the monitored object instance, the exceeding of which
     will cause the generation of an alarm to the high-level management
     station."
    ::=  {rndMonitoringEntry 8}

rndAlarmMinTreshold OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "If the value of the monitored object instance falls below the value
     assigned to rndAlarmMinTreshold, an alarm to the high-level management
     station will be issued."
    ::=  {rndMonitoringEntry  9}


rndMonitoringLogfile OBJECT-TYPE
   SYNTAX DisplayString
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The entire path of the file in which the results of the monitoring
     of this object instance should be recorded."
    ::=  {rndMonitoringEntry  10}

rndMonitoringEntryStatus OBJECT-TYPE
   SYNTAX RowStatus
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
         "It is used to manage the monitored object instances table and
          indicates the current monitoring status of an object instance."
    ::=  {rndMonitoringEntry  11}

rndMonitoredIntegerInstance OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
         ""
    ::=  {rndMonitoringEntry  12}

rndMibFilesTable  OBJECT-TYPE
   SYNTAX SEQUENCE OF RndMibFileEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
    "The table of monitored object instances. Each monitored object instance
     belongs to a monitored element previously entered in the
     rndMonitoredElementsTable. "
    ::= {rndMidLevelManagement 5}

rndMibFileEntry OBJECT-TYPE
   SYNTAX RndMibFileEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
       " The row definition for this table."
   INDEX { rndMibFileIndex }
    ::= {rndMibFilesTable 1}

RndMibFileEntry ::= SEQUENCE {

rndMibFileIndex                 INTEGER,
rndMibFilePath                  DisplayString,
rndMibFileRefresh               INTEGER,
rndMibFileEntryStatus           RowStatus
}
rndMibFileIndex OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION
    "The number of the MIB file in the list MIB files supported by the
     Mid-Level management station. The order of the MIB files in this
     list must reflect the the IMPORT relation between the MIBS contained
     in the MIB files, i.e., if MIB A IMPORTS FROM MIB B, the file containing
     MIB A must have a lesser index in this table than the file containing
     MIB B."
    ::=  {rndMibFileEntry  1}


rndMibFilePath OBJECT-TYPE
   SYNTAX DisplayString
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The path of the MIB file in the MIB file server."
    ::=  {rndMibFileEntry  2}

rndMibFileRefresh OBJECT-TYPE
   SYNTAX INTEGER {
      no(1),
      yes(2)
   }
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "Indicates if the file should be fetched after setting this entry from the
     MIB file server."
    ::=  {rndMibFileEntry  3}

rndMibFileEntryStatus OBJECT-TYPE
   SYNTAX RowStatus
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
         "It is used to manage the MIB files table."
    ::=  {rndMibFileEntry  4}

rndHardwareConfiguration OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates whether the current SET SNMP PDU contains hardware
         configuration (i.e., normally read-only variables). SET of such
         variables in the Mid-level management station will be allowed only
         if this variable is included in the SNMP PDU and its value is true.
         Its value as returned in  a GET SNMP PDU will always be false."
    ::= {rndMidLevelManagement 6}

rndEraseSimulatedConfiguration OBJECT-TYPE
    SYNTAX INTEGER {
        eraseSimulatedConfiguration(1),
        simulatedConfigurationPresent(2),
        simulatedConfigurationErased(3)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "eraseSimulatedConfiguration instructs the MLNMS to erase all the
         simulated configuration from its configuration data-base (CDB). This
         the only accepted value for SNMP SET statements and will never be
         returned in SNMP GET statements.
         simulatedConfigurationPresent indicates that the MLNMS currently has
         a simulated configuration.
         simulatedConfigurationErased indicates that the MLNMS currently has
         no simulated configuration."
    ::= {rndMidLevelManagement 7}

rndDeleteValuesTable  OBJECT-TYPE
   SYNTAX SEQUENCE OF RndDeleteValuesEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
    "This table indicates which MIB variables are row status fields which
     control the status of the entry to which they belong. This table also
     indicates which (integer!) value of these MIB variables will cause, if
     present in a SNMP SET PDU, the deletion of the conceptual row instance
     to which the SET MIB variable instance belongs."
    ::= {rndMidLevelManagement 8}

rndDeleteValuesEntry  OBJECT-TYPE
   SYNTAX RndDeleteValuesEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
       " The row definition for the rndDeleteValuesTable table."
   INDEX { IMPLIED rndRowStatusVariableName }
    ::= {rndDeleteValuesTable 1}

RndDeleteValuesEntry ::= SEQUENCE {

rndRowStatusVariableName    DisplayString,
rndRowStatusObjectId        OBJECT IDENTIFIER,
rndRowDeleteValue           INTEGER,
rndDeleteValueEntryStatus   RowStatus
}

rndRowStatusVariableName OBJECT-TYPE
   SYNTAX DisplayString(SIZE(1..80))
--   MAX-ACCESS         read-only
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The name of the row status field. This name may not necessarily be any
     name which is present in the MIBs loaded into the MLNMS station."

     ::=  {rndDeleteValuesEntry 1}

rndRowStatusObjectId OBJECT-TYPE
   SYNTAX OBJECT IDENTIFIER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The object id of the row status field. If the rndRowStatusVariableName is
     a name present in the MIBs loaded into the MLNMS, this MIB
     variable is not required, but if given, it must match the object id known
     to the MLNMS.
     The variable identified by rndRowStatusVariableName and/or rndRowStatusObjectId
     must be a read-write MIB variable of type INTEGER which belongs to an
     entry (i.e, is a child of a MIB variable of type SEQUENCE)."

     ::=  {rndDeleteValuesEntry 2}

rndRowDeleteValue OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The value of the variable identified by rndRowStatusVariableName and/or
     rndRowStatusObjectId, which, if present in a SNMP SET PDU, will cause
     the deletion of the conceptual row instance which the SET MIB variable
     instance belongs."
     ::=  {rndDeleteValuesEntry 3}

rndDeleteValueEntryStatus  OBJECT-TYPE
   SYNTAX  RowStatus
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
         "It is used to delete an entry from this table."
     ::=  {rndDeleteValuesEntry 4}

snmpTesting  OBJECT IDENTIFIER ::= { rndMidLevelManagement 9}

rndSimulatedVariablesTable  OBJECT-TYPE
   SYNTAX SEQUENCE OF RndSimulatedVariablesEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
    "This table indicates which MIB variables are simulated."
    ::= {snmpTesting 1}

rndSimulatedVariablesEntry  OBJECT-TYPE
   SYNTAX RndSimulatedVariablesEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
       " The row definition for the rndSimulatedVariablesTable table."
   INDEX { rndSimulatedVariableEntryIndex }
    ::= {rndSimulatedVariablesTable 1}

RndSimulatedVariablesEntry ::= SEQUENCE {

rndSimulatedVariableEntryIndex  INTEGER,
rndSimulatedVariableObjectId    OBJECT IDENTIFIER,
rndNotSupportedField            INTEGER,
rndSimulatedVariableEntryStatus RowStatus
}

rndSimulatedVariableEntryIndex OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION
    "The index entry."

     ::=  {rndSimulatedVariablesEntry 1}

rndSimulatedVariableObjectId OBJECT-TYPE
   SYNTAX OBJECT IDENTIFIER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "The object id of the simulated variable. If the simulated variable belongs
     to a table entry, the entire entry is henceforth supported."

     ::=  {rndSimulatedVariablesEntry 2}

rndNotSupportedField OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION
    "Variable for not supported simulation."
     ::=  {rndSimulatedVariablesEntry 3}

rndSimulatedVariableEntryStatus  OBJECT-TYPE
   SYNTAX  RowStatus
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
         "It is used to delete an entry from this table."
     ::=  {rndSimulatedVariablesEntry 4}

rndSnmpTestPassword  OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "This variable enables the user supplying the correct code to use the
     SNMP test feature."
    ::= {snmpTesting 2}

rndSnmpTests  OBJECT-TYPE
   SYNTAX INTEGER {
                   noSimulation(1),
                   simulateSetFailure(2),
                   simulateAppGet(3),
                   simulateAppGetNext(4)
                  }
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "This variable enables the authorized user to test various SNMP features."
    ::= {snmpTesting 3}

rndSimulateUndo  OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "This variable enables the authorized user to test the SNMP UNDO feature."
    ::= {snmpTesting 4}

rlSnmpServTestRequest  OBJECT-TYPE
   SYNTAX INTEGER
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "This variable enables the authorized user to test the SNMP SERV package."
    ::= {snmpTesting 5}

rlSnmpServTestResponse  OBJECT-TYPE
   SYNTAX OCTET STRING
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION
    "This variable enables the authorized user to retrieve the results of
    a the SNMP SERV package test."
   ::= {snmpTesting 6}

rlSnmpServCreateTestPool  OBJECT-TYPE
   SYNTAX INTEGER { create(1), no-create(2) }
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
    "This variable enables the authorized user to indicate that after its reset
     the device should create a buffer pool for SNMPServ process PDU
     testing."
   ::= {snmpTesting 7}

rlSnmpServITCbindClients  OBJECT-TYPE
    SYNTAX OBJECT IDENTIFIER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This variable enables the authorized user to to indicate that after
         its reset the device should create ITC clients for SnmpServ data
         requests clients.
         The semantics of this variable is as follows:
            subidentifier 2*n indicates whether the client n is synchronous(1) or
            asynchronous(2)
            subidentifier 2*n+1 indicates the number of simulatneous requests
            expected by client n."
    ::= {snmpTesting 8}

rlSnmpTestSimulatedVariables  OBJECT IDENTIFIER ::= {snmpTesting 9}

rlTstBasicRateTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlTstBasicRateEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table for testing SNMP agent."
    ::= { snmpTesting 10 }

rlTstBasicRateEntry OBJECT-TYPE
    SYNTAX RlTstBasicRateEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the rlTstBasicRateTable."
    INDEX { ifIndex }
    ::= { rlTstBasicRateTable 1 }

RlTstBasicRateEntry ::= SEQUENCE {
    rlTstBasicRateIfType INTEGER,
    rlTstBasicRateLineTopology INTEGER,
    rlTstBasicRateIfMode INTEGER,
    rlTstBasicRateSignalMode INTEGER
    }

rlTstBasicRateIfType OBJECT-TYPE
    SYNTAX INTEGER {
        isdns(75),
        isdnu(76)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        ""
    ::= { rlTstBasicRateEntry 1 }

rlTstBasicRateLineTopology OBJECT-TYPE
    SYNTAX INTEGER {
        pointToPoint(1),
        pointToMultipoint(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        ""
    ::= { rlTstBasicRateEntry 2 }

rlTstBasicRateIfMode OBJECT-TYPE
    SYNTAX INTEGER {
        te(1),
        nt(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        ""
    ::= { rlTstBasicRateEntry 3 }

rlTstBasicRateSignalMode OBJECT-TYPE
    SYNTAX INTEGER {
        active(1),
        inactive(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        ""
    ::= { rlTstBasicRateEntry 4 }

rlMibTree OBJECT IDENTIFIER ::= {rndMidLevelManagement 10 }

rlMibTreeTable OBJECT-TYPE
   SYNTAX SEQUENCE OF RlMibTreeEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
    "This reflects the MIB tree of the device."
   ::= {rlMibTree 1 }


rlMibTreeEntry OBJECT-TYPE
   SYNTAX RlMibTreeEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
       " Each row shows a tree relationsship in the MIB."
   INDEX { rlMibTreeFather, rlMibTreeSonIndex }
   ::= {rlMibTreeTable 1 }

   RlMibTreeEntry ::= SEQUENCE {

     rlMibTreeFather                 DisplayString,
     rlMibTreeSonIndex               INTEGER,
     rlMibTreeSon                    DisplayString,
     rlMibTreeSonObjectId            OBJECT IDENTIFIER,
     rlMibTreeGrandFather            DisplayString
}


 rlMibTreeFather OBJECT-TYPE
     SYNTAX DisplayString
     MAX-ACCESS         not-accessible
     STATUS     current
     DESCRIPTION
       " The father in a tree relation ship."
     ::= {rlMibTreeEntry 1 }

 rlMibTreeSonIndex OBJECT-TYPE
     SYNTAX INTEGER
     MAX-ACCESS         not-accessible
     STATUS     current
     DESCRIPTION
       " Running index for this table."
     ::= {rlMibTreeEntry 2 }

 rlMibTreeSon OBJECT-TYPE
     SYNTAX DisplayString
     MAX-ACCESS         read-only
     STATUS     current
     DESCRIPTION
       " The son in a tree relation ship."
     ::= {rlMibTreeEntry 3 }

 rlMibTreeSonObjectId OBJECT-TYPE
     SYNTAX OBJECT IDENTIFIER
     MAX-ACCESS         read-only
     STATUS     current
     DESCRIPTION
       " The object identifier of the son in a tree relation ship."
     ::= {rlMibTreeEntry 4}

 rlMibTreeGrandFather OBJECT-TYPE
     SYNTAX DisplayString
     MAX-ACCESS         read-only
     STATUS     current
     DESCRIPTION
       " The grand father (i.e father's father) in a tree relation ship."
     ::= {rlMibTreeEntry 5 }


rlMibInstances OBJECT IDENTIFIER ::= {rndMidLevelManagement 11 }

rlMibTableInstancesInfoTable OBJECT-TYPE
   SYNTAX SEQUENCE OF RlMibTableInstancesInfoEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
    "A table for retreiving information on the current instances in a requested MIB table."
   ::= {rlMibInstances 1 }


rlMibTableInstancesInfoEntry OBJECT-TYPE
   SYNTAX RlMibTableInstancesInfoEntry
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION
       "A row with index rlMibTableInstancesInfoTableName = 'xTable' contains
        information on current instances in 'xTable'."
   INDEX { IMPLIED rlMibTableInstancesInfoTableName }
   ::= {rlMibTableInstancesInfoTable 1 }

   RlMibTableInstancesInfoEntry ::= SEQUENCE {

     rlMibTableInstancesInfoTableName       DisplayString,
     rlMibTableInstancesInfoNumOfInstances  INTEGER
}


rlMibTableInstancesInfoTableName OBJECT-TYPE
   SYNTAX DisplayString(SIZE(1..160))
   MAX-ACCESS     not-accessible
   STATUS         current
   DESCRIPTION
       "The name of the MIB table (for examle: snmpCommunityTable)"
     ::= {rlMibTableInstancesInfoEntry 1 }

rlMibTableInstancesInfoNumOfInstances OBJECT-TYPE
   SYNTAX         INTEGER
   MAX-ACCESS     read-only
   STATUS         current
   DESCRIPTION
       "Get operation on this object will retreive the current number of instances
        in the MIB table specified by the index rlMibTableInstancesInfoTableName."
     ::= {rlMibTableInstancesInfoEntry 2 }

-- Obsolete
-- rsIpZeroHopRouting  OBJECT IDENTIFIER ::= { rndApplications 3}


rsPingMIB OBJECT IDENTIFIER ::= { rndApplications 4} -- NEW Group

--------------------------------------------------------------------------------
-- rsPingTable
--------------------------------------------------------------------------------

--
-- Textual Conventions
--

PingCompletionStatus ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION  "If all the echo request packets in this sequence have been
                 responded by valid echo responses, this object is set to ok.
                 Otherwise this status indicates the problem. bad-reply-data indicates
                 that the reply data is not equal to the response data."
   SYNTAX INTEGER {
                 ok(1),
                 timeout(2),
                 net-unreachable(3),
                 host-unreachable(4),
                 protocol-unreachable(5),
                 time-to-live-exceeded(6),
                 reassembly-time-exceeded(7),
                 unable-to-send(8),
                 bad-reply-data(9),
                 incomplete(10),
                 -- Eltex starts here
                 message-too-long(25)
                 }

rsPingTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RsPingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of ping request entries."
    ::= { rsPingMIB 1 }

rsPingEntry OBJECT-TYPE
    SYNTAX RsPingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A ping request entry.

        A management station wishing to create an entry should
        first generate a pseudo-random serial number to be used
        as the index to this sparse table. It must also create in the same
        PDU the associated instance of the address object. It should also
        modify in the same PDU the default values for the other configuration
        objects if the defaults are not appropriate.

        Once the sequence completes, the management station should
        retrieve the values of the status objects of interest, and
        should then delete the entry.  In order to prevent old
        entries from clogging the table, entries will be aged out,
        but an entry will never be deleted within 5 minutes of
        completing."
    INDEX { rsPingAddress }
    ::= { rsPingTable 1 }

RsPingEntry ::= SEQUENCE {
    rsPingAddress          IpAddress,
    rsPingPacketCount      INTEGER,
    rsPingPacketSize       INTEGER,
    rsPingPacketTimeout    INTEGER,
    rsPingDelay            INTEGER,
    rsPingTrapOnCompletion TruthValue,
    rsPingSentPackets      Counter32,
    rsPingReceivedPackets  Counter32,
    rsPingMinReturnTime    INTEGER,
    rsPingAvgReturnTime    INTEGER,
    rsPingMaxReturnTime    INTEGER,
    rsPingCompletionStatus PingCompletionStatus,
    rsPingTimeStamp        DisplayString,
    rsPingEntryStatus      RowStatus
    }

rsPingAddress OBJECT-TYPE
    SYNTAX IpAddress
--    Rsyntax OCTET STRING
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The address of the device to be pinged.
         Once an instance of this object is created, its
         value can not be changed."
    ::= { rsPingEntry 1 }

rsPingPacketCount OBJECT-TYPE
    SYNTAX INTEGER(1..2147483647)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies the number of ping packets to send to the target
        in this sequence."
--    DEFVAL { 5 }
    ::= { rsPingEntry 2 }

 rsPingPacketSize OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies the size of ping packets to send to the target
        in this sequence.  The lower and upper boundaries of this
        object are implementation dependent."
--    DEFVAL { 100 }
    ::= { rsPingEntry 3 }

rsPingPacketTimeout OBJECT-TYPE
    SYNTAX INTEGER(0..3600000)
--  Units
--    milliseconds
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies the amount of time to wait for a response to a
        transmitted packet before declaring the packet 'dropped.'"
--    DEFVAL { 2000 }
    ::= { rsPingEntry 4 }

rsPingDelay OBJECT-TYPE
    SYNTAX INTEGER(0..3600000)
--  Units
--    milliseconds
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "Specifies the minimum amount of time to wait before sending
        the next packet in a sequence after receiving a response.
        The actual delay may be greater due to internal task scheduling."
--    DEFVAL { 0 }
    ::= { rsPingEntry 5 }

rsPingTrapOnCompletion OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies whether or not a rsPingCompletion trap should
         be issued on completion of the sequence of pings.  If such a
         trap is desired, the NMS should ensure that the community table
         contains an instance specified by the NMSs IP address with
         rndCommunityTrapsEnable = trapsEnable."
--  DEFVAL { false }
    ::= { rsPingEntry 6 }

rsPingSentPackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of ping packets that have been sent to the target
        in this sequence."
    ::= { rsPingEntry 7 }

rsPingReceivedPackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of ping packets that have been received from the
        target in this sequence."
    ::= { rsPingEntry 8 }

rsPingMinReturnTime OBJECT-TYPE
    SYNTAX INTEGER
--  Units
--    milliseconds
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The minimum round trip time of all the packets that have
         been sent in this sequence. The value returned to a GET request
         is meaningless if no ping response in a sequence has been received
         yet."
    ::= { rsPingEntry 9 }

rsPingAvgReturnTime OBJECT-TYPE
    SYNTAX INTEGER
--  Units
--    milliseconds
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The average round trip time of all the packets that have
         been sent in this sequence.The value returned to a GET request
         is meaningless if no ping response in a sequence has been received
         yet."
    ::= { rsPingEntry 10 }

rsPingMaxReturnTime OBJECT-TYPE
    SYNTAX INTEGER
--  Units
--    milliseconds
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximum round trip time of all the packets that have
         been sent in this sequence.The value returned to a GET request
         is meaningless if no ping response in a sequence has been received
         yet."
    ::= { rsPingEntry 11 }

rsPingCompletionStatus OBJECT-TYPE
    SYNTAX         PingCompletionStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "If all the echo request packets in this sequence have been
         responded by valid echo responses, this object is set to ok.
         Otherwise this status indicates the problem. bad-reply-data indicates
         that the reply data is not equal to the response data."
    ::= { rsPingEntry 12 }

rsPingTimeStamp OBJECT-TYPE
    SYNTAX DisplayString(SIZE(19))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time-stamp indicating the time and date of creation or last
         update of this request. The format of the time-stamp is
         dd/mm/yyyy hh:mm:ss"
    ::= { rsPingEntry 13 }


rsPingEntryStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The status of this table entry."
    ::= { rsPingEntry 14 }

--------------------------------------------------------------------------------
-- rsPingInetTable
--------------------------------------------------------------------------------

-- For IPv6 support
-- Must replace old rsPingTable MIB

rsPingInetTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RsPingInetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of ping request entries."
    ::= { rsPingMIB 2 }

rsPingInetEntry OBJECT-TYPE
    SYNTAX      RsPingInetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A ping request entry.

        A management station wishing to create an entry should
        first generate a pseudo-random serial number to be used
        as the index to this sparse table. It must also create in the same
        PDU the associated instance of the address object. It should also
        modify in the same PDU the default values for the other configuration
        objects if the defaults are not appropriate.

        Once the sequence completes, the management station should
        retrieve the values of the status objects of interest, and
        should then delete the entry.  In order to prevent old
        entries from clogging the table, entries will be aged out,
        but an entry will never be deleted within 5 minutes of
        completing."
    INDEX { rsPingInetAddressType, rsPingInetAddress }
    ::= { rsPingInetTable 1 }

RsPingInetEntry ::= SEQUENCE {
    rsPingInetAddressType      InetAddressType,
    rsPingInetAddress          InetAddress,
    rsPingInetPacketCount      INTEGER,
    rsPingInetPacketSize       INTEGER,
    rsPingInetPacketTimeout    INTEGER,
    rsPingInetDelay            INTEGER,
    rsPingInetTrapOnCompletion TruthValue,
    rsPingInetSentPackets      Counter32,
    rsPingInetReceivedPackets  Counter32,
    rsPingInetMinReturnTime    INTEGER,
    rsPingInetAvgReturnTime    INTEGER,
    rsPingInetMaxReturnTime    INTEGER,
    rsPingInetCompletionStatus PingCompletionStatus,
    rsPingInetTimeStamp        DisplayString,
    rsPingInetEntryStatus      RowStatus,
    rsPingInetSourceAddr       InetAddress
    }

rsPingInetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The address type of the device to be pinged.
                Once an instance of this object is created, its
                value can not be changed."
    ::= { rsPingInetEntry 1 }

rsPingInetAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The address of the device to be pinged.
                Once an instance of this object is created, its
                value can not be changed."
    ::= { rsPingInetEntry 2 }

rsPingInetPacketCount OBJECT-TYPE
    SYNTAX      INTEGER(1..2147483647)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the number of ping packets to send to the target
                in this sequence."
    ::= { rsPingInetEntry 3 }

 rsPingInetPacketSize OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the size of ping packets to send to the target
                in this sequence.  The lower and upper boundaries of this
                object are implementation dependent."
    ::= { rsPingInetEntry 4 }

rsPingInetPacketTimeout OBJECT-TYPE
    SYNTAX      INTEGER(0..3600000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the amount of time (in milliseconds) to wait for a response to a
                transmitted packet before declaring the packet 'dropped.'"
    ::= { rsPingInetEntry 5 }

rsPingInetDelay OBJECT-TYPE
    SYNTAX      INTEGER(0..3600000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies the minimum amount of time (in milliseconds) to wait before sending
                the next packet in a sequence after receiving a response.
                The actual delay may be greater due to internal task scheduling."
    ::= { rsPingInetEntry 6 }

rsPingInetTrapOnCompletion OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "Specifies whether or not a rsPingCompletion trap should
                 be issued on completion of the sequence of pings.  If such a
                 trap is desired, the NMS should ensure that the community table
                 contains an instance specified by the NMSs IP address with
                 rndCommunityTrapsEnable = trapsEnable."
    ::= { rsPingInetEntry 7 }

rsPingInetSentPackets OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of ping packets that have been sent to the target
                in this sequence."
    ::= { rsPingInetEntry 8 }

rsPingInetReceivedPackets OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The number of ping packets that have been received from the
                target in this sequence."
    ::= { rsPingInetEntry 9 }

rsPingInetMinReturnTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The minimum round trip time (in milliseconds) of all the packets that have
                been sent in this sequence. The value returned to a GET request
                is meaningless if no ping response in a sequence has been received yet."
    ::= { rsPingInetEntry 10 }

rsPingInetAvgReturnTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The average round trip time (in milliseconds) of all the packets that have
                been sent in this sequence.The value returned to a GET request
                is meaningless if no ping response in a sequence has been received yet."
    ::= { rsPingInetEntry 11 }

rsPingInetMaxReturnTime OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The maximum round trip time (in milliseconds) of all the packets that have
                been sent in this sequence.The value returned to a GET request
                is meaningless if no ping response in a sequence has been received yet."
    ::= { rsPingInetEntry 12 }

rsPingInetCompletionStatus OBJECT-TYPE
    SYNTAX      PingCompletionStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "If all the echo request packets in this sequence have been
                responded by valid echo responses, this object is set to ok.
                Otherwise this status indicates the problem. bad-reply-data indicates
                that the reply data is not equal to the response data."
    ::= { rsPingInetEntry 13 }

rsPingInetTimeStamp OBJECT-TYPE
    SYNTAX      DisplayString(SIZE(19))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "The time-stamp indicating the time and date of creation or last
                update of this request. The format of the time-stamp is
                dd/mm/yyyy hh:mm:ss"
    ::= { rsPingInetEntry 14 }

rsPingInetEntryStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The status of this table entry."
    ::= { rsPingInetEntry 15 }

rsPingInetSourceAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION "The status of this table entry."
    ::= { rsPingInetEntry 16 }

--------------------------------------------------------------------------------

rsPowerSupplyRedundacy OBJECT IDENTIFIER ::= { rndApplications 5} -- NEW Group
rsPowerSupplyRedundacyTable   OBJECT-TYPE
    SYNTAX SEQUENCE OF RsPowerSupplyRedundacyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The power supply redundancy table."
    ::=  { rsPowerSupplyRedundacy 1  }

rsPowerSupplyRedundacyEntry OBJECT-TYPE
    SYNTAX RsPowerSupplyRedundacyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The status of power supply redundancy for this table."
    INDEX { rsPowerSupplyRedundacyReNumber}
    ::= { rsPowerSupplyRedundacyTable 1}

RsPowerSupplyRedundacyEntry ::= SEQUENCE {
    rsPowerSupplyRedundacyReNumber       INTEGER,
    rsPowerSupplyRedundacyStatus         INTEGER
    }

rsPowerSupplyRedundacyReNumber OBJECT-TYPE
    SYNTAX INTEGER  (1..31)
    MAX-ACCESS          read-only
    STATUS      current
    DESCRIPTION
        "This number identifies the module backed up
         by power supply redundancy in the stack."
    ::= { rsPowerSupplyRedundacyEntry 1}

rsPowerSupplyRedundacyStatus OBJECT-TYPE
    SYNTAX INTEGER{
        notExist(1),
        existButNotWorking(2),
        bothWorking(3),
        internalOnlyWorking(4),
        externalOnlyWorking(5)
        }
    MAX-ACCESS          read-only
    STATUS      current
    DESCRIPTION
        "The status of a power supply redundancy of the entry."
    ::= { rsPowerSupplyRedundacyEntry 2}

rsNvram  OBJECT IDENTIFIER ::= { rndApplications 6 }
rsEraseNvramAfterReset OBJECT-TYPE
    SYNTAX DisplayString  (SIZE(0..20))
    MAX-ACCESS          read-write
    STATUS      current
    DESCRIPTION
        "The name of NVRAM application that will be erased
         after reset or ALL if all NVRAM should be erased."
    ::=  { rsNvram 1 }

rsNvramApplTable   OBJECT-TYPE
    SYNTAX SEQUENCE OF RsNvramApplEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The NVRAM application table."
    ::=  { rsNvram 2 }

rsNvramApplEntry OBJECT-TYPE
    SYNTAX RsNvramApplEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The status of NVRAM application table."
    INDEX { rsNvramApplIndex}
    ::= { rsNvramApplTable 1}

RsNvramApplEntry ::= SEQUENCE {
    rsNvramApplIndex       INTEGER,
    rsNvramApplName        DisplayString
    }

rsNvramApplIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS          read-only
    STATUS      current
    DESCRIPTION
        "The index of NVRAM application table."
    ::= { rsNvramApplEntry 1}

rsNvramApplName OBJECT-TYPE
    SYNTAX DisplayString  (SIZE(0..20))
    MAX-ACCESS          read-only
    STATUS      current
    DESCRIPTION
        "The name of application used NVRAM."
    ::= { rsNvramApplEntry 2}

END

