RADLAN-TRUNK-MIB DEFINITIONS ::= BEGIN

IMPORTS
    rnd                                     FROM RADLAN-MIB
    OBJECT-TYPE, IpAddress, Unsigned32,Counter32, TimeTicks,
    MODULE-IDENTITY                         FROM SNMPv2-SMI
    DisplayString, TEXTUAL-CONVENTION, TruthValue, RowStatus,
    PhysAddress
                                            FROM SNMPv2-TC
    dot3adAggIndex, dot3adAggPortIndex      FROM IEEE8023-LAG-MIB;


 rlDot3adAgg   MODULE-IDENTITY
          LAST-UPDATED "200612020000Z"
          ORGANIZATION "Marvell Semiconductor, Inc."
          CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
          DESCRIPTION
                  "The private MIB module definition for trunk support in Radlan devices."
          REVISION "200612020000Z"
          DESCRIPTION
                  "Initial version of this MIB."
          ::= { rnd 65 }

rlDot3adAggMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "MIB's version, the current version is 1."
    ::= { rlDot3adAgg 1 }

--
-- rlDot3adAggBalanceTable
--
rlDot3adAggBalanceTable  OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDot3adAggBalanceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of this table specifies a balancing criterion used
         for the corresponding dot3adAggIndex.

         A criterion configured in this table is used to distribute
         the traffic both over Link Aggregation Group members and
         multiple ECMP paths."
    ::= { rlDot3adAgg 2 }

rlDot3adAggBalanceEntry OBJECT-TYPE
    SYNTAX  RlDot3adAggBalanceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A list of information for each dot3adAggIndex."
    INDEX  { dot3adAggIndex, rlDot3adAggBalanceForwardType }
    ::= { rlDot3adAggBalanceTable 1 }

RlDot3adAggBalanceEntry ::= SEQUENCE {
    rlDot3adAggBalanceForwardType       INTEGER,
    rlDot3adAggBalanceLayer             INTEGER,
    rlDot3adAggBalanceUsedAddresses     INTEGER,
    rlDot3adAggBalanceBroadcastType     INTEGER
}

rlDot3adAggBalanceForwardType OBJECT-TYPE
    SYNTAX  INTEGER {
        bridging(1),
        routing(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A Forwarding type: Bridging or Routing."
    ::= { rlDot3adAggBalanceEntry 1 }

rlDot3adAggBalanceLayer OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A Network Layer Number, may have the following values: 2, 3 or 4.
         The default value is:
           Bridging: 2
           Routing:  3."
    ::= { rlDot3adAggBalanceEntry 2 }

rlDot3adAggBalanceUsedAddresses  OBJECT-TYPE
    SYNTAX  INTEGER {
        notApplied(0),
        dstAddr(1),
        srcAddr(2),
        dstAndSrcAddr(3),
        vlanId(4),
        ethType(5)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies the Network Layer addresses used for Balancing of
         unicast frames.
         The function sets the criterion (by layer and used address in it)."
    DEFVAL { dstAddr }
    ::= { rlDot3adAggBalanceEntry 3 }

rlDot3adAggBalanceBroadcastType  OBJECT-TYPE
    SYNTAX  INTEGER {
        common(0),
        dedicated(1)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies a balancing criterion used for L2 broadcast and unknown
         frames:
            common:
                a link allocated for broadcast and unknown frames is used
                for unicast frames too
            dedicated:
                a link allocated for broadcast and unknown frames is not used
                for unicast frames"
    DEFVAL { common }
    ::= { rlDot3adAggBalanceEntry 4 }

rlDot3adAggNumOfTrunks OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of trunks supported by the device."
    ::= { rlDot3adAgg 3 }

rlDot3adAggMaxPortsInTrunks OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximun number of ports in a trunk."
    ::= { rlDot3adAgg 4 }

rlDot3adAggTrunkCreationSupport OBJECT-TYPE
    SYNTAX  INTEGER {
        notSupported(0),
        supportsTrunkOrLacp(1)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies if there is support to rldot3adAggCreationTable,
         and the type of the support:
         supportedTrunkOrLacp - ports that are members in some trunk
         are belongs to it by manual configuration or by lacp,
         but not togther.
         notSupported - there is not support to rldot3adAggCreationTable."
    ::= { rlDot3adAgg 5 }

--
-- rlDot3adAggCreationTable
--
rlDot3adAggCreationTable  OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDot3adAggCreationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of this table is for creation of an aggregator
         for the corresponding dot3adAggIndex, when the value of the
         rlDot3adAggCreationSupport is diffrent from notSupported."
    ::= { rlDot3adAgg 6 }

rlDot3adAggCreationEntry OBJECT-TYPE
    SYNTAX  RlDot3adAggCreationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An information for each dot3adAggIndex."
    INDEX  { dot3adAggIndex }
    ::= { rlDot3adAggCreationTable 1 }

RlDot3adAggCreationEntry ::= SEQUENCE {
    rlDot3adAggCreationTrunk       TruthValue,
    rlDot3adAggCreationLacp        TruthValue
}

rlDot3adAggCreationTrunk OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The aggregator can aggregate ports in manual configuration."
    ::= { rlDot3adAggCreationEntry 1 }

rlDot3adAggCreationLacp OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The aggregator can aggregate ports by lacp."
    ::= { rlDot3adAggCreationEntry 2 }

rlDot3adAggLoadBalancingPerTrunk OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies if load balancing is defined per trunk
         or per device."
    ::= { rlDot3adAgg 7 }

--
-- rlDot3adAggPortLacpTable
--
rlDot3adAggPortLacpTable  OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDot3adAggPortLacpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of this table specifies lacp protocol state and
         statistics for the corresponding dot3adAggPortIndex."
    ::= { rlDot3adAgg 8 }

rlDot3adAggPortLacpEntry OBJECT-TYPE
    SYNTAX  RlDot3adAggPortLacpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A list of information for each dot3adAggPortIndex."
    INDEX  { dot3adAggPortIndex }
    ::= { rlDot3adAggPortLacpTable 1 }

RlDot3adAggPortLacpEntry ::= SEQUENCE {
    rlDot3adAggPortLacpPdusRx               Counter32,
    rlDot3adAggPortLacpPDUsTx               Counter32,
    rlDot3adAggPortLacpRxState              INTEGER,
    rlDot3adAggPortLacpMuxState             INTEGER,
    rlDot3adAggPortLacpPeriodicState        INTEGER,
    rlDot3adAggPortLacpSelected             INTEGER,
    rlDot3adAggPortLacpReady                TruthValue,
    rlDot3adAggPortLacpPortMoved            TruthValue,
    rlDot3adAggPortLacpNNT                  TruthValue,
    rlDot3adAggPortLacpPeriodicTxTimer      INTEGER,
    rlDot3adAggPortLacpCurrentWhileTimer    INTEGER,
    rlDot3adAggPortLacpWaitWhileTimer       INTEGER
}

rlDot3adAggPortLacpPdusRx OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of valid LACPDUs received on this
         Aggregation Port. This value is read-only."
    ::= { rlDot3adAggPortLacpEntry 1 }

rlDot3adAggPortLacpPDUsTx OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of LACPDUs transmitted on this
         Aggregation Port. This value is read-only."
    ::= { rlDot3adAggPortLacpEntry 2 }

rlDot3adAggPortLacpRxState OBJECT-TYPE
    SYNTAX INTEGER {
        current(1),
        expired(2),
        defaulted(3),
        initialize(4),
        portDisabled(5),
        lacpDisabled(6)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This attribute holds the value 'current' if the Receive
         state machine for the Aggregation Port is in the
         CURRENT state, 'expired' if the Receive state machine
         is in the EXPIRED state, 'defaulted' if the Receive state
         machine is in the DEFAULTED state, 'initialize' if the
         Receive state machine is in the INITIALIZE state,
         'portDisabled' if the Receive state machine is in the
         PORT_DISABLED state, or 'lacpDisabled' if the Receive state
         machine is in the LACP_DISABLED state.
         This value is read-only."
    ::= { rlDot3adAggPortLacpEntry 3 }

rlDot3adAggPortLacpMuxState OBJECT-TYPE
    SYNTAX INTEGER {
        detached(1),
        waiting(2),
        attached(3),
        collecting(4),
        distributing(5),
        collectingDistributing(6)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This attribute holds the value 'detached' if the Mux
         state machine for the Aggregation Port is
         in the DETACHED state, 'waiting' if the Mux state machine
         is in the WAITING state, 'attached' if the Mux state
         machine for the Aggregation Port is in the ATTACHED
         state, 'collecting' if the Mux state machine for the
         Aggregation Port is in the COLLECTING state, 'distributing'
         if the Mux state machine for the Aggregation Port is
         in the DISTRIBUTING state, and 'collecting_ distributing'
         if the Mux state machine for the Aggregation Port is in
         the COLLECTING_DISTRIBUTING state.
         This value is read-only."
    ::= { rlDot3adAggPortLacpEntry 4 }

rlDot3adAggPortLacpPeriodicState OBJECT-TYPE
    SYNTAX INTEGER {
        noPeriodic(1),
        fastPeriodic(2),
        slowPeriodic(3),
        periodicTx(4)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This attribute holds the value 'noPeriodic' if the Periodic
         state machine for the Aggregation Port is
         in the NO_PERIODIC state, 'fastPeriodic' if the Mux state machine
         is in the FAST_PERIODIC state, 'slowPeriodic' if the Mux state
         machine for the Aggregation Port is in the SLOW_PERIODIC
         state, or 'periodicTx' if the Periodic state machine
         for the Aggregation Port is in the PERIODIC_TX state.
         This value is read-only."
    ::= { rlDot3adAggPortLacpEntry 5 }

rlDot3adAggPortLacpSelected OBJECT-TYPE
    SYNTAX INTEGER {
        unselected(1),
        selected(2),
        waiting(3)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "This attribute holds the value 'unselected' if the Selected variable
         for the Aggregation Port is set to UNSELECTED, 'selected' if the
         Selected variable for the Aggregation Port is set to SELECTED,
         or 'waiting' if the Selected variable for the Aggregation Port
         is set to WAITING.
         This value is read-only."
    ::= { rlDot3adAggPortLacpEntry 6 }

rlDot3adAggPortLacpReady OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A read-only Boolean value indicating whether the
         Aggregation Port is in the WAITING state in the Mux state machine
         and its wait_while_timer has expired ('TRUE').
         otherwise, its valus is 'FALSE'."
    ::= { rlDot3adAggPortLacpEntry 7 }

rlDot3adAggPortLacpPortMoved OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A read-only Boolean value indicating whether the
         Partner_Oper_System or Partner_Oper_Port_Number in use by the
         Aggregation Port has been changed in an incoming LACPDU ('TRUE').
         otherwise, its valus is 'FALSE'."
    ::= { rlDot3adAggPortLacpEntry 8 }

rlDot3adAggPortLacpNNT OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "A read-only Boolean value indicating whether there is a new protocol
         information that should be transmitted on the link, or that the Partner
         needs to be reminded of the old information.
         otherwise, its valus is 'FALSE'."
    ::= { rlDot3adAggPortLacpEntry 9 }

rlDot3adAggPortLacpPeriodicTxTimer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The amount of time in seconds remaining before the Periodeic Tx timer
         will expire.
         This value is read-only."
    ::= { rlDot3adAggPortLacpEntry 10 }

rlDot3adAggPortLacpCurrentWhileTimer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The amount of time in seconds remaining before the Current While timer
         will expire.
         This value is read-only."
    ::= { rlDot3adAggPortLacpEntry 11 }

rlDot3adAggPortLacpWaitWhileTimer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The amount of time in seconds remaining before the Wait While timer
         will expire.
         This value is read-only."
    ::= { rlDot3adAggPortLacpEntry 12 }

rlDot3adAggLacpMembershipRestrictionsSupport OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies if there is support to
         rlDot3adAggLacpMembershipRestrictionsTable."
    ::= { rlDot3adAgg 9 }

--
-- rlDot3adAggLacpMembershipRestrictionsTable
--
rlDot3adAggLacpMembershipRestrictionsTable  OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDot3adAggLacpMembershipRestrictionsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of this table specifies membership restrictions
         for ports that lacp is enbaled on them, and try to attach to
         the corresponding dot3adAggIndex."
    ::= { rlDot3adAgg 10 }

rlDot3adAggLacpMembershipRestrictionsEntry OBJECT-TYPE
    SYNTAX  RlDot3adAggLacpMembershipRestrictionsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A list of information for each dot3adAggIndex."
    INDEX  { dot3adAggIndex }
    ::= { rlDot3adAggLacpMembershipRestrictionsTable 1 }

RlDot3adAggLacpMembershipRestrictionsEntry ::= SEQUENCE {
    rlDot3adAggLacpMembershipRestrictionsPartnerAdminKey            Unsigned32,
    rlDot3adAggLacpMembershipRestrictionsSpeedAdminMode             Unsigned32,
    rlDot3adAggLacpMembershipRestrictionsPartnerAdminSystemId       PhysAddress,
    rlDot3adAggLacpMembershipRestrictionsPartnerAdminSystemPriority Unsigned32,
    rlDot3adAggLacpMembershipRestrictionsIndividualAggregator       TruthValue
}

rlDot3adAggLacpMembershipRestrictionsPartnerAdminKey OBJECT-TYPE
    SYNTAX Unsigned32 (0.. 65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This variable specifies the administrative key
         of the remote LACP aggregator.
         A value of 0 is returned if the value of the variable
         hasn't been set."
    DEFVAL { 0 }
    ::= { rlDot3adAggLacpMembershipRestrictionsEntry 1 }

rlDot3adAggLacpMembershipRestrictionsSpeedAdminMode OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This variable specifies the required speed of the LACP aggregator
         in bits per second.
         A value of 10 is returned for 10G.
         A value of 0 is returned if the value of the variable
         hasn't been set."
    DEFVAL { 0 }
    ::= { rlDot3adAggLacpMembershipRestrictionsEntry 2 }

rlDot3adAggLacpMembershipRestrictionsPartnerAdminSystemId OBJECT-TYPE
    SYNTAX PhysAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This variable specifies the administrative MAC Address
         of the remote LACP aggregator.
         A null mac address is returned if the value of the variable
         hasn't been set."
    ::= { rlDot3adAggLacpMembershipRestrictionsEntry 3 }

rlDot3adAggLacpMembershipRestrictionsPartnerAdminSystemPriority OBJECT-TYPE
    SYNTAX Unsigned32 (0.. 65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This variable specifies the administrative System Priority
         of the remote LACP aggregator.
         A value of 0 is returned if the value of the variable
         hasn't been set."
    DEFVAL { 0 }
    ::= { rlDot3adAggLacpMembershipRestrictionsEntry 4 }

rlDot3adAggLacpMembershipRestrictionsIndividualAggregator OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This variable specifies if the lacp aggregator represents an
         Aggregate ('FALSE') or an Individual link ('TRUE')."
    DEFVAL { false }
    ::= { rlDot3adAggLacpMembershipRestrictionsEntry 5 }

rlDot3adAggLacpSystemPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "indicates the system priority value of ports and trunk in LACP."
    ::= { rlDot3adAgg 11 }

END


