RADLAN-IPV6FHS-MIB DEFINITIONS ::= BEGIN

-- Title:      RADLAN IPv6 First Hop Security Configuration
-- Version:    7.60
-- Date:       12-Dec-2012
--

IMPORTS
    DisplayString,TruthValue,TEXTUAL-CONVENTION,
    RowStatus,MacAddress                                 FROM SNMPv2-TC
    VlanIndex,PortList                                   FROM Q-BRIDGE-MIB
    Unsigned32, IpAddress, NOTIFICATION-TYPE,
    Integer32, Counter32, OBJECT-TYPE                    FROM SNMPv2-SMI
    rndErrorDesc, rndErrorSeverity                       FROM RADLAN-DEVICEPARAMS-MIB
    rnd, rlMacMulticast, rndNotifications                FROM RADLAN-MIB
    InetAddressType,InetAddress,InetAddressPrefixLength  FROM INET-ADDRESS-MIB
    InterfaceIndex, InterfaceIndexOrZero                 FROM IF-MIB
    VlanId                                               FROM Q-BRIDGE-MIB
    VlanList1, VlanList2, VlanList3, VlanList4           FROM RADLAN-BRIDGEMIBOBJECTS-MIB;


rlIpv6Fhs MODULE-IDENTITY
        LAST-UPDATED "201212120000Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO 
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
                "The private MIB module definition for IPv6 First Hop Security."
        REVISION "201212120000Z"
        DESCRIPTION
                "Initial version of this MIB."
        ::= { rnd  215}

  --------------------------------------------------------------
  -- Textual Conventions
  --------------------------------------------------------------

 RlIpv6FhsSettingStatusType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The setting status type."
    SYNTAX      INTEGER {
                    unspecified(-1),
                    enabled(1),
                    disabled(2)
                }

 RlIpv6FhsSettingType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The setting type."
    SYNTAX      INTEGER {
                    default(1),
                    global(2),
                    vlan(3),
                    port(4)
                }



 --------------------------------------------------------------
 -- groups in the IPV6FHS MIB
 --------------------------------------------------------------

 rlFirstHopSec         OBJECT IDENTIFIER ::= { rlIpv6Fhs 1 }
 rlNdInspection        OBJECT IDENTIFIER ::= { rlIpv6Fhs 2 }
 rlRaGuard             OBJECT IDENTIFIER ::= { rlIpv6Fhs 3 }
 rlNbrBindingIntegrity OBJECT IDENTIFIER ::= { rlIpv6Fhs 4 }
 rlDhcpGuard           OBJECT IDENTIFIER ::= { rlIpv6Fhs 5 }
 rlSourceGuard         OBJECT IDENTIFIER ::= { rlIpv6Fhs 6 }

 --------------------------------------------------------------
 -- The First Hop Security
 --------------------------------------------------------------

 --------------------------------------------------------------
 -- The First Hop Security Policy Configuration Table
 --------------------------------------------------------------

 rlFirstHopSecPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlFirstHopSecPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies first hop security
                 per policy configurations."
    ::= { rlFirstHopSec 1 }

 rlFirstHopSecPolicyEntry OBJECT-TYPE
    SYNTAX  RlFirstHopSecPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlFirstHopSecPolicyName }
    ::= { rlFirstHopSecPolicyTable 1 }

 RlFirstHopSecPolicyEntry ::= SEQUENCE {
    rlFirstHopSecPolicyName               DisplayString,
    rlFirstHopSecPolicyLogDrop            RlIpv6FhsSettingStatusType,
    rlFirstHopSecPolicyRowStatus          RowStatus
    }

 rlFirstHopSecPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The first hop security policy name"
    ::= { rlFirstHopSecPolicyEntry 1 }

 rlFirstHopSecPolicyLogDrop OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Enable/disable of the logging of dropped packets."
    DEFVAL  { unspecified }
    ::= { rlFirstHopSecPolicyEntry 2 }

 rlFirstHopSecPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
    ::= { rlFirstHopSecPolicyEntry 3 }

 --------------------------------------------------------------
 -- The First Hop Security Policy Attachment Table - Port
 --------------------------------------------------------------

 rlFirstHopSecPortPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlFirstHopSecPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies first hop security policy
                 attachment for ports."
    ::= { rlFirstHopSec 2 }

 rlFirstHopSecPortPolicyEntry OBJECT-TYPE
    SYNTAX  RlFirstHopSecPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlFirstHopSecPortPolicyIfIndex,
            IMPLIED rlFirstHopSecPortPolicyName }
    ::= { rlFirstHopSecPortPolicyTable 1 }

 RlFirstHopSecPortPolicyEntry ::= SEQUENCE {
    rlFirstHopSecPortPolicyIfIndex            InterfaceIndex,
    rlFirstHopSecPortPolicyName               DisplayString,
    rlFirstHopSecPortPolicyVlan1to1024        OCTET STRING,
    rlFirstHopSecPortPolicyVlan1025to2048     OCTET STRING,
    rlFirstHopSecPortPolicyVlan2049to3072     OCTET STRING,
    rlFirstHopSecPortPolicyVlan3073to4094     OCTET STRING,
    rlFirstHopSecPortPolicyRowStatus          RowStatus
    }

 rlFirstHopSecPortPolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlFirstHopSecPortPolicyEntry 1 }

 rlFirstHopSecPortPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The first hop security policy name"
    ::= { rlFirstHopSecPortPolicyEntry 2 }

 rlFirstHopSecPortPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlFirstHopSecPortPolicyEntry 3 }

 rlFirstHopSecPortPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlFirstHopSecPortPolicyEntry 4 }

 rlFirstHopSecPortPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlFirstHopSecPortPolicyEntry 5 }

 rlFirstHopSecPortPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlFirstHopSecPortPolicyEntry 6 }

 rlFirstHopSecPortPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlFirstHopSecPortPolicyEntry 7 }

 --------------------------------------------------------------
 -- The First Hop Security Policy Attachment Table - Port (Read Only)
 --------------------------------------------------------------

 rlFirstHopSecPolicyPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlFirstHopSecPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies first hop security policy
                 attachment for ports."
    ::= { rlFirstHopSec 3 }

 rlFirstHopSecPolicyPortEntry OBJECT-TYPE
    SYNTAX  RlFirstHopSecPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlFirstHopSecPolicyPortName,
            rlFirstHopSecPolicyPortIfIndex }
    ::= { rlFirstHopSecPolicyPortTable 1 }

 RlFirstHopSecPolicyPortEntry ::= SEQUENCE {
    rlFirstHopSecPolicyPortName               DisplayString,
    rlFirstHopSecPolicyPortIfIndex            InterfaceIndex,
    rlFirstHopSecPolicyPortVlan1to1024        OCTET STRING,
    rlFirstHopSecPolicyPortVlan1025to2048     OCTET STRING,
    rlFirstHopSecPolicyPortVlan2049to3072     OCTET STRING,
    rlFirstHopSecPolicyPortVlan3073to4094     OCTET STRING
    }

 rlFirstHopSecPolicyPortName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The first hop security policy name"
    ::= { rlFirstHopSecPolicyPortEntry 1 }

 rlFirstHopSecPolicyPortIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlFirstHopSecPolicyPortEntry 2 }

 rlFirstHopSecPolicyPortVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlFirstHopSecPolicyPortEntry 3 }

 rlFirstHopSecPolicyPortVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlFirstHopSecPolicyPortEntry 4 }

 rlFirstHopSecPolicyPortVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlFirstHopSecPolicyPortEntry 5 }

 rlFirstHopSecPolicyPortVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlFirstHopSecPolicyPortEntry 6 }

 --------------------------------------------------------------
 -- The First Hop Security Policy Attachment Table - Vlan
 --------------------------------------------------------------

 rlFirstHopSecVlanPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlFirstHopSecVlanPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies first hop security policy
                 attachment for vlans."
    ::= { rlFirstHopSec 4 }

 rlFirstHopSecVlanPolicyEntry OBJECT-TYPE
    SYNTAX  RlFirstHopSecVlanPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlFirstHopSecVlanPolicyVlanTag }
    ::= { rlFirstHopSecVlanPolicyTable 1 }

 RlFirstHopSecVlanPolicyEntry ::= SEQUENCE {
    rlFirstHopSecVlanPolicyVlanTag            VlanId,
    rlFirstHopSecVlanPolicyName               DisplayString,
    rlFirstHopSecVlanPolicyRowStatus          RowStatus
 }

 rlFirstHopSecVlanPolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { rlFirstHopSecVlanPolicyEntry 1 }

 rlFirstHopSecVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "The first hop security policy name"
    ::= { rlFirstHopSecVlanPolicyEntry 2 }

 rlFirstHopSecVlanPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlFirstHopSecVlanPolicyEntry 3 }
 --------------------------------------------------------------
 -- The First Hop Security Policy Attachment Table - Vlan
 --------------------------------------------------------------

 rlFirstHopSecPolicyVlanTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlFirstHopSecPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies first hop security policy
                 attachment for vlans."
    ::= { rlFirstHopSec 5 }

 rlFirstHopSecPolicyVlanEntry OBJECT-TYPE
    SYNTAX  RlFirstHopSecPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlFirstHopSecPolicyVlanPolicyName }
    ::= { rlFirstHopSecPolicyVlanTable 1 }

 RlFirstHopSecPolicyVlanEntry ::= SEQUENCE {
    rlFirstHopSecPolicyVlanPolicyName    DisplayString,
    rlFirstHopSecPolicyVlan1to1024       OCTET STRING,
    rlFirstHopSecPolicyVlan1025to2048    OCTET STRING,
    rlFirstHopSecPolicyVlan2049to3072    OCTET STRING,
    rlFirstHopSecPolicyVlan3073to4094    OCTET STRING

 }

 rlFirstHopSecPolicyVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION
        "The first hop security policy name"
    ::= { rlFirstHopSecPolicyVlanEntry 1 }

 rlFirstHopSecPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1 to 1024."
    DEFVAL {'00'H}
    ::= { rlFirstHopSecPolicyVlanEntry 2 }

 rlFirstHopSecPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1025 to 2048."
    DEFVAL {'00'H}
    ::= { rlFirstHopSecPolicyVlanEntry 3 }

 rlFirstHopSecPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 2049 to 3072."
    DEFVAL {'00'H}
    ::= { rlFirstHopSecPolicyVlanEntry 4 }

 rlFirstHopSecPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 3073 to 4094."
    DEFVAL {'00'H}
    ::= { rlFirstHopSecPolicyVlanEntry 5 }

 --------------------------------------------------------------
 -- The First Hop Security Policy Enable Table
 --------------------------------------------------------------

rlFirstHopSecEnableVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlFirstHopSecEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table contains only one entry of a static vlan list."
    ::= { rlFirstHopSec 6 }

rlFirstHopSecEnableVlanEntry OBJECT-TYPE
    SYNTAX      RlFirstHopSecEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Statically created by local or network management vlan list"
    INDEX   {rlFirstHopSecEnableVlanIndex}
    ::= { rlFirstHopSecEnableVlanTable 1 }

RlFirstHopSecEnableVlanEntry ::=SEQUENCE {
    rlFirstHopSecEnableVlanIndex         INTEGER,
    rlFirstHopSecEnableVlan1to1024       OCTET STRING,
    rlFirstHopSecEnableVlan1025to2048    OCTET STRING,
    rlFirstHopSecEnableVlan2049to3072    OCTET STRING,
    rlFirstHopSecEnableVlan3073to4094    OCTET STRING

}

rlFirstHopSecEnableVlanIndex  OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
     "The table contains only one static entry."

   ::= { rlFirstHopSecEnableVlanEntry 1 }

rlFirstHopSecEnableVlan1to1024 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1 to 1024."
   DEFVAL {'00'H}
   ::= { rlFirstHopSecEnableVlanEntry 2 }

rlFirstHopSecEnableVlan1025to2048 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1025 to 2048."
   DEFVAL {'00'H}
   ::= { rlFirstHopSecEnableVlanEntry 3 }

rlFirstHopSecEnableVlan2049to3072 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 2049 to 3072."
   DEFVAL {'00'H}
   ::= { rlFirstHopSecEnableVlanEntry 4 }

rlFirstHopSecEnableVlan3073to4094 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 3073 to 4094."
   DEFVAL {'00'H}
   ::= { rlFirstHopSecEnableVlanEntry 5 }

 --------------------------------------------------------------
 -- The First Hop Security Active Policy Table (Read Only)
 --------------------------------------------------------------

 rlFirstHopSecActivePolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlFirstHopSecActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies first hop security
                 per policy configurations."
    ::= { rlFirstHopSec 7 }

 rlFirstHopSecActivePolicyEntry OBJECT-TYPE
    SYNTAX  RlFirstHopSecActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlFirstHopSecActivePolicyIfIndex,
            rlFirstHopSecActivePolicyVlanTag }
    ::= { rlFirstHopSecActivePolicyTable 1 }

 RlFirstHopSecActivePolicyEntry ::= SEQUENCE {
    rlFirstHopSecActivePolicyIfIndex            InterfaceIndex,
    rlFirstHopSecActivePolicyVlanTag            VlanId,
    rlFirstHopSecActivePolicyNamePort           DisplayString,
    rlFirstHopSecActivePolicyNameVlan           DisplayString,
    rlFirstHopSecActivePolicyLogDrop            RlIpv6FhsSettingStatusType,
    rlFirstHopSecActivePolicyLogDropType        RlIpv6FhsSettingType
    }

 rlFirstHopSecActivePolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlFirstHopSecActivePolicyEntry 1 }

 rlFirstHopSecActivePolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { rlFirstHopSecActivePolicyEntry 2 }

 rlFirstHopSecActivePolicyNamePort OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The first hop security policy name attached to given interface."
    ::= { rlFirstHopSecActivePolicyEntry 3 }

 rlFirstHopSecActivePolicyNameVlan OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The first hop security policy name attached to given vlan."
    ::= { rlFirstHopSecActivePolicyEntry 4 }

 rlFirstHopSecActivePolicyLogDrop OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Enable/disable of the logging of dropped packets."
    ::= { rlFirstHopSecActivePolicyEntry 5 }

 rlFirstHopSecActivePolicyLogDropType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlFirstHopSecActivePolicyLogDrop setting type."
    ::= { rlFirstHopSecActivePolicyEntry 6 }


 --------------------------------------------------------------
 -- First Hop Security Counters Table (Read Only)
 --------------------------------------------------------------

 rlFirstHopSecCountersTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlFirstHopSecCountersEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table displays first hop security counters"
    ::= { rlFirstHopSec 8 }

 rlFirstHopSecCountersEntry OBJECT-TYPE
    SYNTAX  RlFirstHopSecCountersEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlFirstHopSecCountersIfIndex }
    ::= { rlFirstHopSecCountersTable 1 }

 RlFirstHopSecCountersEntry ::= SEQUENCE {
    rlFirstHopSecCountersIfIndex                                      InterfaceIndex,
    rlFirstHopSecCountersRxNdpRA                                      Counter32,
    rlFirstHopSecCountersDropNdpRA                                    Counter32,
    rlFirstHopSecCountersRxNdpRS                                      Counter32,
    rlFirstHopSecCountersDropNdpRS                                    Counter32,
    rlFirstHopSecCountersRxNdpNA                                      Counter32,
    rlFirstHopSecCountersDropNdpNA                                    Counter32,
    rlFirstHopSecCountersRxNdpNS                                      Counter32,
    rlFirstHopSecCountersDropNdpNS                                    Counter32,
    rlFirstHopSecCountersRxNdpRedirect                                Counter32,
    rlFirstHopSecCountersDropNdpRedirect                              Counter32,
    rlFirstHopSecCountersRxDhcpAdverise                               Counter32,
    rlFirstHopSecCountersDropDhcpAdverise                             Counter32,
    rlFirstHopSecCountersRxDhcpReply                                  Counter32,
    rlFirstHopSecCountersDropDhcpReply                                Counter32,
    rlFirstHopSecCountersRxDhcpReconfigure                            Counter32,
    rlFirstHopSecCountersDropDhcpReconfigure                          Counter32,
    rlFirstHopSecCountersRxDhcpRelayReply                             Counter32,
    rlFirstHopSecCountersDropDhcpRelayReply                           Counter32,
    rlFirstHopSecCountersRxDhcpLeasequeryReply                        Counter32,
    rlFirstHopSecCountersDropDhcpLeasequeryReply                      Counter32,
    rlFirstHopSecCountersDropRaGuardUnauthorizedMessage               Counter32,
    rlFirstHopSecCountersDropRaGuardUnauthorizedHopLimit              Counter32,
    rlFirstHopSecCountersDropRaGuardUnauthorizedManagedConfigFlag     Counter32,
    rlFirstHopSecCountersDropRaGuardUnauthorizedOtherConfigFlag       Counter32,
    rlFirstHopSecCountersDropRaGuardUnauthorizedRouterPreference      Counter32,
    rlFirstHopSecCountersDropRaGuardUnauthorizedAdvertisedPrefix      Counter32,
    rlFirstHopSecCountersDropRaGuardUnauthorizedSourceAddress         Counter32,
    rlFirstHopSecCountersDropNdInspectionInvalidSourceMac             Counter32,
    rlFirstHopSecCountersDropNdInspectionUnsecureMessage              Counter32,
    rlFirstHopSecCountersDropNdInspectionUnauthorizedSecLevel         Counter32,
    rlFirstHopSecCountersDropDhcpGuardUnauthorizedMessage             Counter32,
    rlFirstHopSecCountersDropDhcpGuardUnauthorizedSourceAddress       Counter32,
    rlFirstHopSecCountersDropDhcpGuardUnauthorizedServerPreference    Counter32,
    rlFirstHopSecCountersDropDhcpGuardUnauthorizedAssignedAddress     Counter32,
    rlFirstHopSecCountersDropSourceGuardNoBinding                     Counter32,
    rlFirstHopSecCountersDropNbrBindingIntegrityIllegalIcmpv6         Counter32,
    rlFirstHopSecCountersDropNbrBindingIntegrityIllegalDhcpv6         Counter32,
    rlFirstHopSecCountersRxDhcpRelease                                Counter32,
    rlFirstHopSecCountersDropDhcpRelease                              Counter32,
    rlFirstHopSecCountersRxDhcpDecline                                Counter32,
    rlFirstHopSecCountersDropDhcpDecline                              Counter32
    }

 rlFirstHopSecCountersIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
          "Interface index"
    ::= { rlFirstHopSecCountersEntry 1 }

 rlFirstHopSecCountersRxNdpRA OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Router Advertisement messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 2 }

 rlFirstHopSecCountersDropNdpRA OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Router Advertisement messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 3 }

 rlFirstHopSecCountersRxNdpRS OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Router Solicitation messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 4 }

 rlFirstHopSecCountersDropNdpRS OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Router Solicitation messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 5 }

 rlFirstHopSecCountersRxNdpNA OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Neighbor Advertisement messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 6 }

 rlFirstHopSecCountersDropNdpNA OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Neighbor Advertisement messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 7 }

 rlFirstHopSecCountersRxNdpNS OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Neighbor Solicitation messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 8 }

 rlFirstHopSecCountersDropNdpNS OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Neighbor Solicitation messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 9 }

 rlFirstHopSecCountersRxNdpRedirect OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Redirect messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 10 }

 rlFirstHopSecCountersDropNdpRedirect OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of NDP Redirect messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 11 }

 rlFirstHopSecCountersRxDhcpAdverise OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 ADVERTISE messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 12 }

 rlFirstHopSecCountersDropDhcpAdverise OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 ADVERTISE messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 13 }

 rlFirstHopSecCountersRxDhcpReply OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 REPLY messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 14 }

 rlFirstHopSecCountersDropDhcpReply OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 REPLY messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 15 }

 rlFirstHopSecCountersRxDhcpReconfigure OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 RECONFIGURE messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 16 }

 rlFirstHopSecCountersDropDhcpReconfigure OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 RECONFIGURE messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 17 }

 rlFirstHopSecCountersRxDhcpRelayReply OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 RELAY-REPLY messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 18 }

 rlFirstHopSecCountersDropDhcpRelayReply OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 RELAY-REPLY messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 19 }

 rlFirstHopSecCountersRxDhcpLeasequeryReply OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 LEASEQUERY-REPLY messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 20 }

 rlFirstHopSecCountersDropDhcpLeasequeryReply OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 LEASEQUERY-REPLY messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 21 }

 rlFirstHopSecCountersDropRaGuardUnauthorizedMessage OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped router messages received on host interface."
    ::= { rlFirstHopSecCountersEntry 22 }

 rlFirstHopSecCountersDropRaGuardUnauthorizedHopLimit OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped RA messages due to unauthorized Cur-Hop-Limit."
    ::= { rlFirstHopSecCountersEntry 23 }

 rlFirstHopSecCountersDropRaGuardUnauthorizedManagedConfigFlag OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped RA messages due to unauthorized Managed config flag."
    ::= { rlFirstHopSecCountersEntry 24 }

 rlFirstHopSecCountersDropRaGuardUnauthorizedOtherConfigFlag OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped RA messages due to unauthorized Other config flag."
    ::= { rlFirstHopSecCountersEntry 25 }

 rlFirstHopSecCountersDropRaGuardUnauthorizedRouterPreference OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped RA messages due to unauthorized router preference."
    ::= { rlFirstHopSecCountersEntry 26 }

 rlFirstHopSecCountersDropRaGuardUnauthorizedAdvertisedPrefix OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped RA messages due to unauthorized advertised prefix."
    ::= { rlFirstHopSecCountersEntry 27 }

 rlFirstHopSecCountersDropRaGuardUnauthorizedSourceAddress OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped RA messages due to unauthorized source address."
    ::= { rlFirstHopSecCountersEntry 28 }

 rlFirstHopSecCountersDropNdInspectionInvalidSourceMac OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped NDP messages due to invalid source MAC address."
    ::= { rlFirstHopSecCountersEntry 29 }

 rlFirstHopSecCountersDropNdInspectionUnsecureMessage OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped NDP messages due to being unsecure."
    ::= { rlFirstHopSecCountersEntry 30 }

 rlFirstHopSecCountersDropNdInspectionUnauthorizedSecLevel OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped NDP messages due to unauthorized CGA sec-level."
    ::= { rlFirstHopSecCountersEntry 31 }

 rlFirstHopSecCountersDropDhcpGuardUnauthorizedMessage OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped DHCPv6 server messages on client interface."
    ::= { rlFirstHopSecCountersEntry 32 }

 rlFirstHopSecCountersDropDhcpGuardUnauthorizedSourceAddress OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped DHCPv6 server messages due to unauthorized source address."
    ::= { rlFirstHopSecCountersEntry 33 }

 rlFirstHopSecCountersDropDhcpGuardUnauthorizedServerPreference OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped DHCPv6 server messages due to unauthorized server preference."
    ::= { rlFirstHopSecCountersEntry 34 }

 rlFirstHopSecCountersDropDhcpGuardUnauthorizedAssignedAddress OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped DHCPv6 server messages due to unauthorized address in IA_ADDR."
    ::= { rlFirstHopSecCountersEntry 35 }

 rlFirstHopSecCountersDropSourceGuardNoBinding OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of frame dropped by IPv6 Source Guard due to lack of binding in Neighbor Binding Table."
    ::= { rlFirstHopSecCountersEntry 36 }

 rlFirstHopSecCountersDropNbrBindingIntegrityIllegalIcmpv6 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped ICMPv6 messages due to one of the following reasons:
      invalid source address, invalid destination address, invalid Hop-Limit,
      invalid ICMP code, invalid ICMP length, invalid ICMP checksum,
      invalid target address, invalid flag, invalid option."
    ::= { rlFirstHopSecCountersEntry 37 }

 rlFirstHopSecCountersDropNbrBindingIntegrityIllegalDhcpv6 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of dropped DHCPv6 messages due to one of the following reasons:
      invalid source address, invalid destination address, invalid Hop-Limit,
      invalid ICMP code, invalid ICMP length, invalid ICMP checksum,
      invalid target address, invalid flag, invalid option."
    ::= { rlFirstHopSecCountersEntry 38 }

 rlFirstHopSecCountersRxDhcpRelease OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 RELEASE messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 39 }

 rlFirstHopSecCountersDropDhcpRelease OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 RELEASE messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 40 }

 rlFirstHopSecCountersRxDhcpDecline OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 DECLINE messages received on the interface."
    ::= { rlFirstHopSecCountersEntry 41 }

 rlFirstHopSecCountersDropDhcpDecline OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of DHCPv6 DECLINE messages dropped on the interface."
    ::= { rlFirstHopSecCountersEntry 42 }

 --------------------------------------------------------------
 -- The First Hop Security Global Configurations
 --------------------------------------------------------------

 rlFirstHopSecLogDrop OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Enable/disable of the logging of dropped packets."
    DEFVAL { disabled }
    ::= { rlFirstHopSec 9 }

 --------------------------------------------------------------
 -- First Hop Security Clear Counters (Action Only)
 --------------------------------------------------------------
 rlFirstHopSecClearCounters OBJECT-TYPE
    SYNTAX InterfaceIndexOrZero
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "When this object is set to zero IPv6 First Hop Security Counters
           are cleared on all interfaces.
           When this object is set to a valid interface index then IPv6 First
           Hop Security counters are cleared on this interface.
           Reading this object has no effect."
    ::= { rlFirstHopSec 10 }

--------------------------------------------------------------
 -- First Hop Security Error Counters Table (Read Only)
 --------------------------------------------------------------

 rlFirstHopSecErrorCountersTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlFirstHopSecErrorCountersEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table displays first hop security error counters"
    ::= { rlFirstHopSec 11 }

 rlFirstHopSecErrorCountersEntry OBJECT-TYPE
    SYNTAX  RlFirstHopSecErrorCountersEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "Static row for this table."
    INDEX { rlFirstHopSecErrorCountersIndex }
    ::= { rlFirstHopSecErrorCountersTable 1 }

 RlFirstHopSecErrorCountersEntry ::= SEQUENCE {
    rlFirstHopSecErrorCountersIndex              INTEGER,
    rlFirstHopSecErrorCountersNBTOverflow        Counter32,
    rlFirstHopSecErrorCountersNPTOverflow        Counter32,
    rlFirstHopSecErrorCountersTcamOverflow       Counter32
}

 rlFirstHopSecErrorCountersIndex  OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
     "The table contains only one static entry."
   ::= { rlFirstHopSecErrorCountersEntry 1 }

 rlFirstHopSecErrorCountersNBTOverflow OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Neighbor Binding Table overflow"
    ::= { rlFirstHopSecErrorCountersEntry 2 }

 rlFirstHopSecErrorCountersNPTOverflow OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Neighbor Prefix Table overflow"
    ::= { rlFirstHopSecErrorCountersEntry 3 }

rlFirstHopSecErrorCountersTcamOverflow OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts TCAM overflow"
    ::= { rlFirstHopSecErrorCountersEntry 4 }

 --------------------------------------------------------------
 -- First Hop Security Clear Error Counters (Action Only)
 --------------------------------------------------------------
 rlFirstHopSecClearErrorCounters OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "When this object is set to true IPv6 First Hop Security Error Counters
           are cleared.
           Setting this object to false or reading this object has no effect."
    ::= { rlFirstHopSec 12 }


 --------------------------------------------------------------
 -- The ND Inspection
 --------------------------------------------------------------

 --------------------------------------------------------------
 -- The ND Inspection Policy Configuration Table
 --------------------------------------------------------------

 rlNdInspectionPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNdInspectionPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies ND inspection
                 per policy configurations."
    ::= { rlNdInspection 1 }

 rlNdInspectionPolicyEntry OBJECT-TYPE
    SYNTAX  RlNdInspectionPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlNdInspectionPolicyName }
    ::= { rlNdInspectionPolicyTable 1 }

 RlNdInspectionPolicyEntry ::= SEQUENCE {
    rlNdInspectionPolicyName               DisplayString,
    rlNdInspectionPolicyDeviceRole         INTEGER,
    rlNdInspectionPolicyDropUnsecured      RlIpv6FhsSettingStatusType,
    rlNdInspectionPolicySecLevelMin        Integer32,
    rlNdInspectionPolicyValidateSrcMac     RlIpv6FhsSettingStatusType,
    rlNdInspectionPolicyRowStatus          RowStatus
    }

 rlNdInspectionPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The ND inspection policy name"
    ::= { rlNdInspectionPolicyEntry 1 }

 rlNdInspectionPolicyDeviceRole OBJECT-TYPE
   SYNTAX      INTEGER {
        unspecified(-1),
        host(1),
        router(2)
   }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Specify the role of the device attached."
    DEFVAL  { unspecified }
    ::= { rlNdInspectionPolicyEntry 2 }

 rlNdInspectionPolicyDropUnsecured OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Enable/disable of dropping unsecured messages."
    DEFVAL  { unspecified }
    ::= { rlNdInspectionPolicyEntry 3 }

 rlNdInspectionPolicySecLevelMin OBJECT-TYPE
    SYNTAX      Integer32 (-2 | -1 | 0..7)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "The minimum security level parameter value when
           Cryptographically Generated Address (CGA) options are used.
           The value of -1 indicates unspecified value.
           The value of -2 indicates verification of security level is disabled."
    DEFVAL  { -1 }
    ::= { rlNdInspectionPolicyEntry 4 }

 rlNdInspectionPolicyValidateSrcMac OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Enable/disable validating of the source media access control (MAC)
           address against the link-layer address."
    DEFVAL  { unspecified }
    ::= { rlNdInspectionPolicyEntry 5 }

 rlNdInspectionPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
    ::= { rlNdInspectionPolicyEntry 6 }

 --------------------------------------------------------------
 -- The ND Inspection Policy Attachment Table - Port
 --------------------------------------------------------------

 rlNdInspectionPortPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNdInspectionPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies ND inspection policy
                 attachment for ports."
    ::= { rlNdInspection 2 }

 rlNdInspectionPortPolicyEntry OBJECT-TYPE
    SYNTAX  RlNdInspectionPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlNdInspectionPortPolicyIfIndex,
            IMPLIED rlNdInspectionPortPolicyName }
    ::= { rlNdInspectionPortPolicyTable 1 }

 RlNdInspectionPortPolicyEntry ::= SEQUENCE {
    rlNdInspectionPortPolicyIfIndex            InterfaceIndex,
    rlNdInspectionPortPolicyName               DisplayString,
    rlNdInspectionPortPolicyVlan1to1024        OCTET STRING,
    rlNdInspectionPortPolicyVlan1025to2048     OCTET STRING,
    rlNdInspectionPortPolicyVlan2049to3072     OCTET STRING,
    rlNdInspectionPortPolicyVlan3073to4094     OCTET STRING,
    rlNdInspectionPortPolicyRowStatus          RowStatus
    }

 rlNdInspectionPortPolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlNdInspectionPortPolicyEntry 1 }

 rlNdInspectionPortPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The ND inspection policy name"
    ::= { rlNdInspectionPortPolicyEntry 2 }

 rlNdInspectionPortPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlNdInspectionPortPolicyEntry 3 }

 rlNdInspectionPortPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlNdInspectionPortPolicyEntry 4 }

 rlNdInspectionPortPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlNdInspectionPortPolicyEntry 5 }

 rlNdInspectionPortPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlNdInspectionPortPolicyEntry 6 }

 rlNdInspectionPortPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlNdInspectionPortPolicyEntry 7 }

 --------------------------------------------------------------
 -- The ND Inspection Policy Attachment Table - Port (Read Only)
 --------------------------------------------------------------

 rlNdInspectionPolicyPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNdInspectionPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies ND inspection policy
                 attachment for ports."
    ::= { rlNdInspection 3 }

 rlNdInspectionPolicyPortEntry OBJECT-TYPE
    SYNTAX  RlNdInspectionPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlNdInspectionPolicyPortName,
            rlNdInspectionPolicyPortIfIndex }
    ::= { rlNdInspectionPolicyPortTable 1 }

 RlNdInspectionPolicyPortEntry ::= SEQUENCE {
    rlNdInspectionPolicyPortName               DisplayString,
    rlNdInspectionPolicyPortIfIndex            InterfaceIndex,
    rlNdInspectionPolicyPortVlan1to1024        OCTET STRING,
    rlNdInspectionPolicyPortVlan1025to2048     OCTET STRING,
    rlNdInspectionPolicyPortVlan2049to3072     OCTET STRING,
    rlNdInspectionPolicyPortVlan3073to4094     OCTET STRING
    }

 rlNdInspectionPolicyPortName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The ND inspection policy name"
    ::= { rlNdInspectionPolicyPortEntry 1 }

 rlNdInspectionPolicyPortIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlNdInspectionPolicyPortEntry 2 }

 rlNdInspectionPolicyPortVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlNdInspectionPolicyPortEntry 3 }

 rlNdInspectionPolicyPortVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlNdInspectionPolicyPortEntry 4 }

 rlNdInspectionPolicyPortVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlNdInspectionPolicyPortEntry 5 }

 rlNdInspectionPolicyPortVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlNdInspectionPolicyPortEntry 6 }

 --------------------------------------------------------------
 -- The ND Inspection Policy Attachment Table - Vlan
 --------------------------------------------------------------

 rlNdInspectionVlanPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNdInspectionVlanPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies ND inspection policy
                 attachment for vlans."
    ::= { rlNdInspection 4 }

 rlNdInspectionVlanPolicyEntry OBJECT-TYPE
    SYNTAX  RlNdInspectionVlanPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlNdInspectionVlanPolicyVlanTag }
    ::= { rlNdInspectionVlanPolicyTable 1 }

 RlNdInspectionVlanPolicyEntry ::= SEQUENCE {
    rlNdInspectionVlanPolicyVlanTag            VlanId,
    rlNdInspectionVlanPolicyName               DisplayString,
    rlNdInspectionVlanPolicyRowStatus          RowStatus
 }

 rlNdInspectionVlanPolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { rlNdInspectionVlanPolicyEntry 1 }

 rlNdInspectionVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "The ND inspection policy name"
    ::= { rlNdInspectionVlanPolicyEntry 2 }

 rlNdInspectionVlanPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlNdInspectionVlanPolicyEntry 3 }
 --------------------------------------------------------------
 -- The ND Inspection Policy Attachment Table - Vlan
 --------------------------------------------------------------

 rlNdInspectionPolicyVlanTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNdInspectionPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies ND inspection policy
                 attachment for vlans."
    ::= { rlNdInspection 5 }

 rlNdInspectionPolicyVlanEntry OBJECT-TYPE
    SYNTAX  RlNdInspectionPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlNdInspectionPolicyVlanPolicyName }
    ::= { rlNdInspectionPolicyVlanTable 1 }

 RlNdInspectionPolicyVlanEntry ::= SEQUENCE {
    rlNdInspectionPolicyVlanPolicyName    DisplayString,
    rlNdInspectionPolicyVlan1to1024       OCTET STRING,
    rlNdInspectionPolicyVlan1025to2048    OCTET STRING,
    rlNdInspectionPolicyVlan2049to3072    OCTET STRING,
    rlNdInspectionPolicyVlan3073to4094    OCTET STRING

 }

 rlNdInspectionPolicyVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION
        "The ND inspection policy name"
    ::= { rlNdInspectionPolicyVlanEntry 1 }

 rlNdInspectionPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1 to 1024."
    DEFVAL {'00'H}
    ::= { rlNdInspectionPolicyVlanEntry 2 }

 rlNdInspectionPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1025 to 2048."
    DEFVAL {'00'H}
    ::= { rlNdInspectionPolicyVlanEntry 3 }

 rlNdInspectionPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 2049 to 3072."
    DEFVAL {'00'H}
    ::= { rlNdInspectionPolicyVlanEntry 4 }

 rlNdInspectionPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 3073 to 4094."
    DEFVAL {'00'H}
    ::= { rlNdInspectionPolicyVlanEntry 5 }

 --------------------------------------------------------------
 -- The ND Inspection Policy Enable Table
 --------------------------------------------------------------

rlNdInspectionEnableVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlNdInspectionEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table contains only one entry of a static vlan list."
    ::= { rlNdInspection 6 }

rlNdInspectionEnableVlanEntry OBJECT-TYPE
    SYNTAX      RlNdInspectionEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Statically created by local or network management vlan list"
    INDEX   {rlNdInspectionEnableVlanIndex}
    ::= { rlNdInspectionEnableVlanTable 1 }

RlNdInspectionEnableVlanEntry ::=SEQUENCE {
    rlNdInspectionEnableVlanIndex         INTEGER,
    rlNdInspectionEnableVlan1to1024       OCTET STRING,
    rlNdInspectionEnableVlan1025to2048    OCTET STRING,
    rlNdInspectionEnableVlan2049to3072    OCTET STRING,
    rlNdInspectionEnableVlan3073to4094    OCTET STRING

}

rlNdInspectionEnableVlanIndex  OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
     "The table contains only one static entry."

   ::= { rlNdInspectionEnableVlanEntry 1 }

rlNdInspectionEnableVlan1to1024 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1 to 1024."
    DEFVAL {'00'H}
   ::= { rlNdInspectionEnableVlanEntry 2 }

rlNdInspectionEnableVlan1025to2048 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1025 to 2048."
   DEFVAL {'00'H}
   ::= { rlNdInspectionEnableVlanEntry 3 }

rlNdInspectionEnableVlan2049to3072 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 2049 to 3072."
   DEFVAL {'00'H}
   ::= { rlNdInspectionEnableVlanEntry 4 }

rlNdInspectionEnableVlan3073to4094 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 3073 to 4094."
   DEFVAL {'00'H}
   ::= { rlNdInspectionEnableVlanEntry 5 }

 --------------------------------------------------------------
 -- The ND Inspection Active Policy Table (Read Only)
 --------------------------------------------------------------

 rlNdInspectionActivePolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNdInspectionActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies ND inspection
                 per policy configurations."
    ::= { rlNdInspection 7 }

 rlNdInspectionActivePolicyEntry OBJECT-TYPE
    SYNTAX  RlNdInspectionActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlNdInspectionActivePolicyIfIndex,
            rlNdInspectionActivePolicyVlanTag }
    ::= { rlNdInspectionActivePolicyTable 1 }

 RlNdInspectionActivePolicyEntry ::= SEQUENCE {
    rlNdInspectionActivePolicyIfIndex            InterfaceIndex,
    rlNdInspectionActivePolicyVlanTag            VlanId,
    rlNdInspectionActivePolicyNamePort           DisplayString,
    rlNdInspectionActivePolicyNameVlan           DisplayString,
    rlNdInspectionActivePolicyDeviceRole         INTEGER,
    rlNdInspectionActivePolicyDeviceRoleType     RlIpv6FhsSettingType,
    rlNdInspectionActivePolicyDropUnsecured      RlIpv6FhsSettingStatusType,
    rlNdInspectionActivePolicyDropUnsecuredType  RlIpv6FhsSettingType,
    rlNdInspectionActivePolicySecLevelMin        Integer32,
    rlNdInspectionActivePolicySecLevelMinType    RlIpv6FhsSettingType,
    rlNdInspectionActivePolicyValidateSrcMac     RlIpv6FhsSettingStatusType,
    rlNdInspectionActivePolicyValidateSrcMacType RlIpv6FhsSettingType
    }

 rlNdInspectionActivePolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlNdInspectionActivePolicyEntry 1 }

 rlNdInspectionActivePolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { rlNdInspectionActivePolicyEntry 2 }

 rlNdInspectionActivePolicyNamePort OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The ND inspection policy name attached to given interface."
    ::= { rlNdInspectionActivePolicyEntry 3 }

 rlNdInspectionActivePolicyNameVlan OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The ND inspection policy name attached to given vlan."
    ::= { rlNdInspectionActivePolicyEntry 4 }

 rlNdInspectionActivePolicyDeviceRole OBJECT-TYPE
   SYNTAX      INTEGER {
        host(1),
        router(2)
   }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Specify the role of the device attached."
    ::= { rlNdInspectionActivePolicyEntry 5 }

 rlNdInspectionActivePolicyDeviceRoleType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlNdInspectionActivePolicyDeviceRole setting type."
    ::= { rlNdInspectionActivePolicyEntry 6 }

 rlNdInspectionActivePolicyDropUnsecured OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Enable/disable of dropping unsecured messages."
    ::= { rlNdInspectionActivePolicyEntry 7 }

 rlNdInspectionActivePolicyDropUnsecuredType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlNdInspectionActivePolicyDropUnsecured setting type."
    ::= { rlNdInspectionActivePolicyEntry 8 }

 rlNdInspectionActivePolicySecLevelMin OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..7)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "The minimum security level parameter value when
           Cryptographically Generated Address (CGA) options are used.
           The value of -2 indicates verification of security level is disabled."
    ::= { rlNdInspectionActivePolicyEntry 9 }

 rlNdInspectionActivePolicySecLevelMinType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlNdInspectionActivePolicySecLevelMin setting type."
    ::= { rlNdInspectionActivePolicyEntry 10 }

 rlNdInspectionActivePolicyValidateSrcMac OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Enable/disable validating of the source media access control (MAC)
           address against the link-layer address."
    ::= { rlNdInspectionActivePolicyEntry 11 }

    rlNdInspectionActivePolicyValidateSrcMacType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlNdInspectionActivePolicyValidateSrcMac setting type."
    ::= { rlNdInspectionActivePolicyEntry 12 }



 --------------------------------------------------------------
 -- The ND Inspection Global Configurations
 --------------------------------------------------------------

 rlNdInspectionValidateSrcMac OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Enable/disable validating of the source media access control (MAC)
           address against the link-layer address."
    DEFVAL { disabled }
    ::= { rlNdInspection 8 }

 rlNdInspectionDropUnsecured OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Global configuration of dropping unsecured messages.
           Unsecure messages are neighbor discovery messages with no or invalid
           CGA and RSA Signature options.
           The value true(1) means that unsecured messages are dropped; the
           value false(2) means that they are not."
    DEFVAL  { false }
    ::= { rlNdInspection 9 }

 rlNdInspectionSecLevelMin OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..7)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "The minimum security level parameter value when
           Cryptographically Generated Address (CGA) options are used.
           The value -2 indicates verification of security level is disabled."
    DEFVAL  { -2 }
    ::= { rlNdInspection 10 }

 --------------------------------------------------------------
 -- The ND Inspection Traps
 --------------------------------------------------------------
 rlNdInspectionMessageDropTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Warning trap indicating that IPv6 ND Inspection has dropped a message."
    ::=  { rndNotifications 228 }

 --------------------------------------------------------------
 -- The RA Guard
 --------------------------------------------------------------

 --------------------------------------------------------------
 -- The RA Guard Policy Configuration Table
 --------------------------------------------------------------

 rlRaGuardPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlRaGuardPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies RA guard
                 per policy configurations."
    ::= { rlRaGuard 1 }

 rlRaGuardPolicyEntry OBJECT-TYPE
    SYNTAX  RlRaGuardPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlRaGuardPolicyName }
    ::= { rlRaGuardPolicyTable 1 }

 RlRaGuardPolicyEntry ::= SEQUENCE {
    rlRaGuardPolicyName                     DisplayString,
    rlRaGuardPolicyDeviceRole               INTEGER,
    rlRaGuardPolicyHopLimitMin              Integer32,
    rlRaGuardPolicyHopLimitMax              Integer32,
    rlRaGuardPolicyManagedConfigFlag        INTEGER,
    rlRaGuardPolicyMatchRaAddrSpecified     TruthValue,
    rlRaGuardPolicyMatchRaAddr              DisplayString,
    rlRaGuardPolicyMatchRaPrefixesSpecified TruthValue,
    rlRaGuardPolicyMatchRaPrefixes          DisplayString,
    rlRaGuardPolicyOtherConfigFlag          INTEGER,
    rlRaGuardPolicyRouterPrefMin            INTEGER,
    rlRaGuardPolicyRouterPrefMax            INTEGER,
    rlRaGuardPolicyRowStatus                RowStatus
    }

 rlRaGuardPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The RA Guard policy name."
    ::= { rlRaGuardPolicyEntry 1 }

 rlRaGuardPolicyDeviceRole OBJECT-TYPE
   SYNTAX      INTEGER {
        unspecified(-1),
        host(1),
        router(2)
   }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Specify the role of the device attached."
    DEFVAL  { unspecified }
    ::= { rlRaGuardPolicyEntry 2 }

 rlRaGuardPolicyHopLimitMin OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0 | 1..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Minimum hop-count limit.
           A value of -1 indicates unspecified value.
           A value of 0 indicates validation is disabled."
    DEFVAL  { -1 }
    ::= { rlRaGuardPolicyEntry 3 }

 rlRaGuardPolicyHopLimitMax OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0 | 1..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Maximum hop-count limit.
           A value of -1 indicates unspecified value.
           A value of 0 indicates validation is disabled."
    DEFVAL  { -1 }
    ::= { rlRaGuardPolicyEntry 4 }

 rlRaGuardPolicyManagedConfigFlag OBJECT-TYPE
    SYNTAX INTEGER {
        unspecified(-1),
        disabled(0),
        enabled-off(1),
        enabled-on(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Configuration of -Managed address configuration- flag
          verification."
    DEFVAL  { unspecified }
    ::= { rlRaGuardPolicyEntry 5 }

 rlRaGuardPolicyMatchRaAddrSpecified OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates whether the rlRaGuardPolicyMatchRaAddr is specified"
    DEFVAL { false }
    ::= { rlRaGuardPolicyEntry 6 }

 rlRaGuardPolicyMatchRaAddr OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..64))
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "The IPv6 prefix list to be matched for router's source IPv6 address.
        Relevant only when rlRaGuardPolicyMatchRaAddrSpecified is true.
        The empty string means this validation is disabled."
    DEFVAL { "" }
    ::= { rlRaGuardPolicyEntry 7 }

 rlRaGuardPolicyMatchRaPrefixesSpecified OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates whether the rlRaGuardPolicyMatchRaPrefixes is specified"
    DEFVAL { false }
    ::= { rlRaGuardPolicyEntry 8 }

 rlRaGuardPolicyMatchRaPrefixes OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..64))
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "The IPv6 prefix list to be matched for advertised prefixes.
        Relevant only when rlRaGuardPolicyMatchRaPrefixesSpecified is true.
        The empty string means this validation is disabled."
    DEFVAL { "" }
    ::= { rlRaGuardPolicyEntry 9 }

 rlRaGuardPolicyOtherConfigFlag OBJECT-TYPE
    SYNTAX INTEGER {
        unspecified(-1),
        disabled(0),
        enabled-off(1),
        enabled-on(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Configuration of -Other configuration- flag verification."
    DEFVAL  { unspecified }
    ::= { rlRaGuardPolicyEntry 10 }

 rlRaGuardPolicyRouterPrefMin OBJECT-TYPE
    SYNTAX INTEGER {
        unspecified(-1),
        disabled(0),
        low(1),
        medium(2),
        high(3)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Minimum advertised preference limit."
    DEFVAL  { unspecified }
    ::= { rlRaGuardPolicyEntry 11 }

 rlRaGuardPolicyRouterPrefMax OBJECT-TYPE
    SYNTAX INTEGER {
        unspecified(-1),
        disabled(0),
        low(1),
        medium(2),
        high(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Maximum advertised preference limit. "
    DEFVAL  { unspecified }
    ::= { rlRaGuardPolicyEntry 12 }

 rlRaGuardPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
    ::= { rlRaGuardPolicyEntry 13 }

 --------------------------------------------------------------
 -- The RA Guard Policy Attachment Table - Port
 --------------------------------------------------------------

 rlRaGuardPortPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlRaGuardPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies RA guard policy
                 attachment for ports."
    ::= { rlRaGuard 2 }

 rlRaGuardPortPolicyEntry OBJECT-TYPE
    SYNTAX  RlRaGuardPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlRaGuardPortPolicyIfIndex,
            IMPLIED rlRaGuardPortPolicyName }
    ::= { rlRaGuardPortPolicyTable 1 }

 RlRaGuardPortPolicyEntry ::= SEQUENCE {
    rlRaGuardPortPolicyIfIndex            InterfaceIndex,
    rlRaGuardPortPolicyName               DisplayString,
    rlRaGuardPortPolicyVlan1to1024        OCTET STRING,
    rlRaGuardPortPolicyVlan1025to2048     OCTET STRING,
    rlRaGuardPortPolicyVlan2049to3072     OCTET STRING,
    rlRaGuardPortPolicyVlan3073to4094     OCTET STRING,
    rlRaGuardPortPolicyRowStatus          RowStatus
    }

 rlRaGuardPortPolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlRaGuardPortPolicyEntry 1 }

 rlRaGuardPortPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The RA Guard policy name."
    ::= { rlRaGuardPortPolicyEntry 2 }

 rlRaGuardPortPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlRaGuardPortPolicyEntry 3 }

 rlRaGuardPortPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlRaGuardPortPolicyEntry 4 }

 rlRaGuardPortPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlRaGuardPortPolicyEntry 5 }

 rlRaGuardPortPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlRaGuardPortPolicyEntry 6 }

 rlRaGuardPortPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlRaGuardPortPolicyEntry 7 }

 --------------------------------------------------------------
 -- The RA Guard Policy Attachment Table - Port (Read Only)
 --------------------------------------------------------------

 rlRaGuardPolicyPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlRaGuardPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies RA guard policy
                 attachment for ports."
    ::= { rlRaGuard 3 }

 rlRaGuardPolicyPortEntry OBJECT-TYPE
    SYNTAX  RlRaGuardPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlRaGuardPolicyPortName,
            rlRaGuardPolicyPortIfIndex }
    ::= { rlRaGuardPolicyPortTable 1 }

 RlRaGuardPolicyPortEntry ::= SEQUENCE {
    rlRaGuardPolicyPortName               DisplayString,
    rlRaGuardPolicyPortIfIndex            InterfaceIndex,
    rlRaGuardPolicyPortVlan1to1024        OCTET STRING,
    rlRaGuardPolicyPortVlan1025to2048     OCTET STRING,
    rlRaGuardPolicyPortVlan2049to3072     OCTET STRING,
    rlRaGuardPolicyPortVlan3073to4094     OCTET STRING
    }

 rlRaGuardPolicyPortName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The RA Guard policy name"
    ::= { rlRaGuardPolicyPortEntry 1 }

 rlRaGuardPolicyPortIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlRaGuardPolicyPortEntry 2 }

 rlRaGuardPolicyPortVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlRaGuardPolicyPortEntry 3 }

 rlRaGuardPolicyPortVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlRaGuardPolicyPortEntry 4 }

 rlRaGuardPolicyPortVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlRaGuardPolicyPortEntry 5 }

 rlRaGuardPolicyPortVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlRaGuardPolicyPortEntry 6 }

 --------------------------------------------------------------
 -- The RA Guard Policy Attachment Table - Vlan
 --------------------------------------------------------------

rlRaGuardVlanPolicyTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlRaGuardVlanPolicyEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION  "The table specifies RA guard policy
                attachment for vlans."
   ::= { rlRaGuard 4 }

rlRaGuardVlanPolicyEntry OBJECT-TYPE
   SYNTAX  RlRaGuardVlanPolicyEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION   "The row definition for this table."
   INDEX { rlRaGuardVlanPolicyVlanTag }
   ::= { rlRaGuardVlanPolicyTable 1 }

RlRaGuardVlanPolicyEntry ::= SEQUENCE {
   rlRaGuardVlanPolicyVlanTag            VlanId,
   rlRaGuardVlanPolicyName               DisplayString,
   rlRaGuardVlanPolicyRowStatus          RowStatus
}

rlRaGuardVlanPolicyVlanTag OBJECT-TYPE
   SYNTAX VlanId
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
       "The VLAN identifier."
   ::= { rlRaGuardVlanPolicyEntry 1 }

rlRaGuardVlanPolicyName OBJECT-TYPE
   SYNTAX DisplayString (SIZE(1..32))
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "The RA Guard policy name."
   ::= { rlRaGuardVlanPolicyEntry 2 }

rlRaGuardVlanPolicyRowStatus OBJECT-TYPE
   SYNTAX RowStatus
   MAX-ACCESS read-create
   STATUS current
   DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
   ::= { rlRaGuardVlanPolicyEntry 3 }
 --------------------------------------------------------------
 -- The RA Guard Policy Attachment Table - Vlan
 --------------------------------------------------------------

 rlRaGuardPolicyVlanTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlRaGuardPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies RA guard policy
                 attachment for vlans."
    ::= { rlRaGuard 5 }

 rlRaGuardPolicyVlanEntry OBJECT-TYPE
    SYNTAX  RlRaGuardPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlRaGuardPolicyVlanPolicyName }
    ::= { rlRaGuardPolicyVlanTable 1 }

 RlRaGuardPolicyVlanEntry ::= SEQUENCE {
    rlRaGuardPolicyVlanPolicyName    DisplayString,
    rlRaGuardPolicyVlan1to1024       OCTET STRING,
    rlRaGuardPolicyVlan1025to2048    OCTET STRING,
    rlRaGuardPolicyVlan2049to3072    OCTET STRING,
    rlRaGuardPolicyVlan3073to4094    OCTET STRING

 }

 rlRaGuardPolicyVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION
        "The RA Guard policy name"
    ::= { rlRaGuardPolicyVlanEntry 1 }

 rlRaGuardPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1 to 1024."
   DEFVAL {'00'H}
    ::= { rlRaGuardPolicyVlanEntry 2 }

 rlRaGuardPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1025 to 2048."
   DEFVAL {'00'H}
    ::= { rlRaGuardPolicyVlanEntry 3 }

 rlRaGuardPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 2049 to 3072."
   DEFVAL {'00'H}
    ::= { rlRaGuardPolicyVlanEntry 4 }

 rlRaGuardPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 3073 to 4094."
   DEFVAL {'00'H}
    ::= { rlRaGuardPolicyVlanEntry 5 }

 --------------------------------------------------------------
 -- The RA Guard Policy Enable Table
 --------------------------------------------------------------

 rlRaGuardEnableVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlRaGuardEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table contains only one entry of a static vlan list."
    ::= { rlRaGuard 6 }

 rlRaGuardEnableVlanEntry OBJECT-TYPE
    SYNTAX      RlRaGuardEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Statically created by local or network management vlan list"
    INDEX   {rlRaGuardEnableVlanIndex}
    ::= { rlRaGuardEnableVlanTable 1 }

 RlRaGuardEnableVlanEntry ::=SEQUENCE {
    rlRaGuardEnableVlanIndex         INTEGER,
    rlRaGuardEnableVlan1to1024       OCTET STRING,
    rlRaGuardEnableVlan1025to2048    OCTET STRING,
    rlRaGuardEnableVlan2049to3072    OCTET STRING,
    rlRaGuardEnableVlan3073to4094    OCTET STRING

 }

rlRaGuardEnableVlanIndex  OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
     "The table contains only one static entry."

   ::= { rlRaGuardEnableVlanEntry 1 }

rlRaGuardEnableVlan1to1024 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1 to 1024."
   DEFVAL {'00'H}
   ::= { rlRaGuardEnableVlanEntry 2 }

rlRaGuardEnableVlan1025to2048 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1025 to 2048."
   DEFVAL {'00'H}
   ::= { rlRaGuardEnableVlanEntry 3 }

rlRaGuardEnableVlan2049to3072 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 2049 to 3072."
   DEFVAL {'00'H}
   ::= { rlRaGuardEnableVlanEntry 4 }

rlRaGuardEnableVlan3073to4094 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 3073 to 4094."
   DEFVAL {'00'H}
   ::= { rlRaGuardEnableVlanEntry 5 }
 --------------------------------------------------------------
 -- The RA Guard Active Policy Table (Read Only)
 --------------------------------------------------------------

 rlRaGuardActivePolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlRaGuardActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies RA Guard
                 per policy configurations."
    ::= { rlRaGuard 7 }

 rlRaGuardActivePolicyEntry OBJECT-TYPE
    SYNTAX  RlRaGuardActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlRaGuardActivePolicyIfIndex,
            rlRaGuardActivePolicyVlanTag }
    ::= { rlRaGuardActivePolicyTable 1 }

 RlRaGuardActivePolicyEntry ::= SEQUENCE {
    rlRaGuardActivePolicyIfIndex                  InterfaceIndex,
    rlRaGuardActivePolicyVlanTag                  VlanId,
    rlRaGuardActivePolicyNamePort                 DisplayString,
    rlRaGuardActivePolicyNameVlan                 DisplayString,
    rlRaGuardActivePolicyDeviceRole               INTEGER,
    rlRaGuardActivePolicyDeviceRoleType           RlIpv6FhsSettingType,
    rlRaGuardActivePolicyHopLimitMin              Integer32,
    rlRaGuardActivePolicyHopLimitMinType          RlIpv6FhsSettingType,
    rlRaGuardActivePolicyHopLimitMax              Integer32,
    rlRaGuardActivePolicyHopLimitMaxType          RlIpv6FhsSettingType,
    rlRaGuardActivePolicyManagedConfigFlag        INTEGER,
    rlRaGuardActivePolicyManagedConfigFlagType    RlIpv6FhsSettingType,
    rlRaGuardActivePolicyMatchRaAddr              DisplayString,
    rlRaGuardActivePolicyMatchRaAddrType          RlIpv6FhsSettingType,
    rlRaGuardActivePolicyMatchRaPrefixes          DisplayString,
    rlRaGuardActivePolicyMatchRaPrefixesType      RlIpv6FhsSettingType,
    rlRaGuardActivePolicyOtherConfigFlag          INTEGER,
    rlRaGuardActivePolicyOtherConfigFlagType      RlIpv6FhsSettingType,
    rlRaGuardActivePolicyRouterPrefMin            INTEGER,
    rlRaGuardActivePolicyRouterPrefMinType        RlIpv6FhsSettingType,
    rlRaGuardActivePolicyRouterPrefMax            INTEGER,
    rlRaGuardActivePolicyRouterPrefMaxType        RlIpv6FhsSettingType
    }

 rlRaGuardActivePolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlRaGuardActivePolicyEntry 1 }

 rlRaGuardActivePolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { rlRaGuardActivePolicyEntry 2 }

 rlRaGuardActivePolicyNamePort OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The RA Guard policy name attached to given interface."
    ::= { rlRaGuardActivePolicyEntry 3 }

 rlRaGuardActivePolicyNameVlan OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The RA Guard policy name attached to given vlan."
    ::= { rlRaGuardActivePolicyEntry 4 }

 rlRaGuardActivePolicyDeviceRole OBJECT-TYPE
   SYNTAX      INTEGER {
        host(1),
        router(2)
   }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Specify the role of the device attached."
    ::= { rlRaGuardActivePolicyEntry 5 }

 rlRaGuardActivePolicyDeviceRoleType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlRaGuardActivePolicyDeviceRole setting type."
    ::= { rlRaGuardActivePolicyEntry 6 }

 rlRaGuardActivePolicyHopLimitMin OBJECT-TYPE
    SYNTAX      Integer32 (0 | 1..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Minimum hop-count limit.
           A value of 0 indicates validation is disabled."
    ::= { rlRaGuardActivePolicyEntry 7 }

 rlRaGuardActivePolicyHopLimitMinType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlRaGuardActivePolicyHopLimitMin setting type."
    ::= { rlRaGuardActivePolicyEntry 8 }

 rlRaGuardActivePolicyHopLimitMax OBJECT-TYPE
    SYNTAX      Integer32 ( 0 | 1..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Maximum hop-count limit.
           A value of 0 indicates validation is disabled."
    ::= { rlRaGuardActivePolicyEntry 9 }

 rlRaGuardActivePolicyHopLimitMaxType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlRaGuardActivePolicyHopLimitMax setting type."
    ::= { rlRaGuardActivePolicyEntry 10 }

 rlRaGuardActivePolicyManagedConfigFlag OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(0),
        enabled-off(1),
        enabled-on(2)
        }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Configuration of -Managed address configuration- flag
          verification."
    ::= { rlRaGuardActivePolicyEntry 11 }

 rlRaGuardActivePolicyManagedConfigFlagType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlRaGuardActivePolicyManagedConfigFlag setting type."
    ::= { rlRaGuardActivePolicyEntry 12 }

 rlRaGuardActivePolicyMatchRaAddr OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..64))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The IPv6 prefix list to be matched for router's source IPv6 address.
        The empty string means this validation is disabled."
    ::= { rlRaGuardActivePolicyEntry 13 }

 rlRaGuardActivePolicyMatchRaAddrType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "rlRaGuardActivePolicyMatchRaAddr setting type."
    ::= { rlRaGuardActivePolicyEntry 14 }

 rlRaGuardActivePolicyMatchRaPrefixes OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..64))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The IPv6 prefix list to be matched for advertised prefixes.
        The empty string means this validation is disabled."
    ::= { rlRaGuardActivePolicyEntry 15 }

 rlRaGuardActivePolicyMatchRaPrefixesType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "rlRaGuardActivePolicyMatchRaPrefixes setting type."
    ::= { rlRaGuardActivePolicyEntry 16 }

 rlRaGuardActivePolicyOtherConfigFlag OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(0),
        enabled-off(1),
        enabled-on(2)
        }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Configuration of -Other configuration- flag verification."
    ::= { rlRaGuardActivePolicyEntry 17 }

 rlRaGuardActivePolicyOtherConfigFlagType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlRaGuardActivePolicyOtherConfigFlag setting type."
    ::= { rlRaGuardActivePolicyEntry 18 }

 rlRaGuardActivePolicyRouterPrefMin OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(0),
        low(1),
        medium(2),
        high(3)
        }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Minimum advertised preference limit."
    ::= { rlRaGuardActivePolicyEntry 19 }

 rlRaGuardActivePolicyRouterPrefMinType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlRaGuardActivePolicyRouterPrefMin setting type."
    ::= { rlRaGuardActivePolicyEntry 20 }

 rlRaGuardActivePolicyRouterPrefMax OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(0),
        low(1),
        medium(2),
        high(3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Maximum advertised preference limit. "
    ::= { rlRaGuardActivePolicyEntry 21 }

 rlRaGuardActivePolicyRouterPrefMaxType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlRaGuardActivePolicyRouterPrefMax setting type. "
    ::= { rlRaGuardActivePolicyEntry 22 }

 --------------------------------------------------------------
 -- The RA Guard Global Configurations
 --------------------------------------------------------------

 rlRaGuardHopLimitMin OBJECT-TYPE
    SYNTAX      Integer32 (0 | 1..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Minimum hop-count limit.
          A value of zero indicates that hop-count limit is not verified."
    DEFVAL  { 0 }
    ::= { rlRaGuard 8 }

 rlRaGuardHopLimitMax OBJECT-TYPE
    SYNTAX      Integer32 (0 | 1..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Maximum hop-count limit.
          A value of zero indicates that hop-count limit is not verified."
    DEFVAL  { 0 }
    ::= { rlRaGuard 9 }

 rlRaGuardManagedConfigFlag OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(0),
        enabled-off(1),
        enabled-on(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Global configuration of -Managed address configuration- flag
          verification."
    DEFVAL  { 0 }
    ::= { rlRaGuard 10 }

 rlRaGuardOtherConfigFlag OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(0),
        enabled-off(1),
        enabled-on(2)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Global configuration of -Other configuration- flag
          verification."
    DEFVAL  { 0 }
    ::= { rlRaGuard 11 }

 rlRaGuardRouterPrefMin OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(0),
        low(1),
        medium(2),
        high(3)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Minimum advertised preference limit."
    DEFVAL  { disabled }
    ::= { rlRaGuard 12 }

 rlRaGuardRouterPrefMax OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(0),
        low(1),
        medium(2),
        high(3)
        }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Maximum advertised preference limit."
    DEFVAL  { disabled }
    ::= { rlRaGuard 13 }

 --------------------------------------------------------------
 -- The RA Guard Traps
 --------------------------------------------------------------
 rlRaGuardMessageDropTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Warning trap indicating that IPv6 Ra Guard has dropped a message."
    ::=  { rndNotifications 229 }

 --------------------------------------------------------------
 -- Neighbor Binding Integrity
 --------------------------------------------------------------

 --------------------------------------------------------------
 -- Neighbor Binding Integrity Policy Configuration Table
 --------------------------------------------------------------

 rlNbrBindingIntegrityPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNbrBindingIntegrityPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Neighbor Binding Integrity
                 per policy configurations."
    ::= { rlNbrBindingIntegrity 1 }

 rlNbrBindingIntegrityPolicyEntry OBJECT-TYPE
    SYNTAX  RlNbrBindingIntegrityPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlNbrBindingIntegrityPolicyName }
    ::= { rlNbrBindingIntegrityPolicyTable 1 }

 RlNbrBindingIntegrityPolicyEntry ::= SEQUENCE {
    rlNbrBindingIntegrityPolicyName                     DisplayString,
    rlNbrBindingIntegrityPolicyDeviceRole               INTEGER,
    rlNbrBindingIntegrityPolicyLogBinding               RlIpv6FhsSettingStatusType,
    rlNbrBindingIntegrityPolicyMaxEntriesVlanLimit      Integer32,
    rlNbrBindingIntegrityPolicyMaxEntriesInterfaceLimit Integer32,
    rlNbrBindingIntegrityPolicyMaxEntriesMacLimit       Integer32,
    rlNbrBindingIntegrityPolicyRowStatus                RowStatus,
    rlNbrBindingIntegrityPolicyPrefixValidation         RlIpv6FhsSettingStatusType,
    rlNbrBindingIntegrityPolicyAddressConfig            INTEGER
    }

 rlNbrBindingIntegrityPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Neighbor Binding Integrity policy name."
    ::= { rlNbrBindingIntegrityPolicyEntry 1 }

 rlNbrBindingIntegrityPolicyDeviceRole OBJECT-TYPE
   SYNTAX      INTEGER {
        unspecified(-1),
        perimeter(1),
        internal(2)
   }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Specify the role of the device attached."
    DEFVAL  { unspecified }
    ::= { rlNbrBindingIntegrityPolicyEntry 2 }

 rlNbrBindingIntegrityPolicyLogBinding OBJECT-TYPE
    SYNTAX RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Enable/disable logging of Neighbor Binding Table events"
    DEFVAL  { unspecified }
    ::= { rlNbrBindingIntegrityPolicyEntry 3 }

 rlNbrBindingIntegrityPolicyMaxEntriesVlanLimit OBJECT-TYPE
    SYNTAX      Integer32 (-2 | -1 | 0..65535)
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates how many entries can be added to Neighbor Binding Table
         with the same VLAN tag.
         The value of -1 indicates unspecified value.
         The value of -2 indicates there is no limit."
    DEFVAL { -1 }
    ::= { rlNbrBindingIntegrityPolicyEntry 4 }

 rlNbrBindingIntegrityPolicyMaxEntriesInterfaceLimit OBJECT-TYPE
    SYNTAX      Integer32 (-2 | -1 | 0..65535)
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates how many entries can be added to Neighbor Binding Table
         with the same interface identifier.
         The value of -1 indicates unspecified value.
         The value of -2 indicates there is no limit."
    DEFVAL { -1 }
    ::= { rlNbrBindingIntegrityPolicyEntry 5 }

 rlNbrBindingIntegrityPolicyMaxEntriesMacLimit OBJECT-TYPE
    SYNTAX      Integer32 (-2 | -1 | 0..65535)
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates how many entries can be added to Neighbor Binding Table
         with the same MAC address.
         The value of -1 indicates unspecified value.
         The value of -2 indicates there is no limit."
    DEFVAL { -1 }
    ::= { rlNbrBindingIntegrityPolicyEntry 6 }

 rlNbrBindingIntegrityPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
    ::= { rlNbrBindingIntegrityPolicyEntry 7 }

 rlNbrBindingIntegrityPolicyPrefixValidation OBJECT-TYPE
    SYNTAX RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Enable/disable address prefix validation using Neighbor Prefix Table."
    DEFVAL  { unspecified }
    ::= { rlNbrBindingIntegrityPolicyEntry 8 }

 rlNbrBindingIntegrityPolicyAddressConfig OBJECT-TYPE
   SYNTAX      INTEGER {
        unspecified(-1),
        autoconfig(1),
        autoconfigAndManual(3),
        dhcp(4),
        autoconfigAndDhcp(5),
        autoconfigManualAndDhcp(7)
   }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Specify the allowed methods for address binding in Neighbor Binding Table.
          autoconfig(1) refers to stateless address autoconfiguration.
          autoconfigAndManual(3) allows manual and stateless address autoconfiguration.
          dhcp(4) permits binding only from DHCP.
          autoconfigAndDhcp(5) binds from DHCP and stateless address autoconfiguration.
          autoconfigManualAndDhcp(7) binds from Manual, DHCP and stateless address autoconfiguration."
    DEFVAL  { unspecified }
    ::= { rlNbrBindingIntegrityPolicyEntry 9 }

 --------------------------------------------------------------
 -- Neighbor Binding Integrity Policy Attachment Table - Port
 --------------------------------------------------------------

 rlNbrBindingIntegrityPortPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNbrBindingIntegrityPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Neighbor Binding Integrity policy
                 attachment for ports."
    ::= { rlNbrBindingIntegrity 2 }

 rlNbrBindingIntegrityPortPolicyEntry OBJECT-TYPE
    SYNTAX  RlNbrBindingIntegrityPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlNbrBindingIntegrityPortPolicyIfIndex,
            IMPLIED rlNbrBindingIntegrityPortPolicyName }
    ::= { rlNbrBindingIntegrityPortPolicyTable 1 }

 RlNbrBindingIntegrityPortPolicyEntry ::= SEQUENCE {
    rlNbrBindingIntegrityPortPolicyIfIndex            InterfaceIndex,
    rlNbrBindingIntegrityPortPolicyName               DisplayString,
    rlNbrBindingIntegrityPortPolicyVlan1to1024        OCTET STRING,
    rlNbrBindingIntegrityPortPolicyVlan1025to2048     OCTET STRING,
    rlNbrBindingIntegrityPortPolicyVlan2049to3072     OCTET STRING,
    rlNbrBindingIntegrityPortPolicyVlan3073to4094     OCTET STRING,
    rlNbrBindingIntegrityPortPolicyRowStatus          RowStatus
    }

 rlNbrBindingIntegrityPortPolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlNbrBindingIntegrityPortPolicyEntry 1 }

 rlNbrBindingIntegrityPortPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The Neighbor Binding Integrity policy name."
    ::= { rlNbrBindingIntegrityPortPolicyEntry 2 }

 rlNbrBindingIntegrityPortPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlNbrBindingIntegrityPortPolicyEntry 3 }

 rlNbrBindingIntegrityPortPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlNbrBindingIntegrityPortPolicyEntry 4 }

 rlNbrBindingIntegrityPortPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlNbrBindingIntegrityPortPolicyEntry 5 }

 rlNbrBindingIntegrityPortPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlNbrBindingIntegrityPortPolicyEntry 6 }

 rlNbrBindingIntegrityPortPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlNbrBindingIntegrityPortPolicyEntry 7 }

 ------------------------------------------------------------------------
 -- Neighbor Binding Integrity Policy Attachment Table - Port (Read Only)
 ------------------------------------------------------------------------

 rlNbrBindingIntegrityPolicyPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNbrBindingIntegrityPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Neighbor Binding Integrity policy
                 attachment for ports."
    ::= { rlNbrBindingIntegrity 3 }

 rlNbrBindingIntegrityPolicyPortEntry OBJECT-TYPE
    SYNTAX  RlNbrBindingIntegrityPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlNbrBindingIntegrityPolicyPortName,
            rlNbrBindingIntegrityPolicyPortIfIndex }
    ::= { rlNbrBindingIntegrityPolicyPortTable 1 }

 RlNbrBindingIntegrityPolicyPortEntry ::= SEQUENCE {
    rlNbrBindingIntegrityPolicyPortName               DisplayString,
    rlNbrBindingIntegrityPolicyPortIfIndex            InterfaceIndex,
    rlNbrBindingIntegrityPolicyPortVlan1to1024        OCTET STRING,
    rlNbrBindingIntegrityPolicyPortVlan1025to2048     OCTET STRING,
    rlNbrBindingIntegrityPolicyPortVlan2049to3072     OCTET STRING,
    rlNbrBindingIntegrityPolicyPortVlan3073to4094     OCTET STRING
    }

 rlNbrBindingIntegrityPolicyPortName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The Neighbor Binding Integrity policy name"
    ::= { rlNbrBindingIntegrityPolicyPortEntry 1 }

 rlNbrBindingIntegrityPolicyPortIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlNbrBindingIntegrityPolicyPortEntry 2 }

 rlNbrBindingIntegrityPolicyPortVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlNbrBindingIntegrityPolicyPortEntry 3 }

 rlNbrBindingIntegrityPolicyPortVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlNbrBindingIntegrityPolicyPortEntry 4 }

 rlNbrBindingIntegrityPolicyPortVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlNbrBindingIntegrityPolicyPortEntry 5 }

 rlNbrBindingIntegrityPolicyPortVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlNbrBindingIntegrityPolicyPortEntry 6 }

 --------------------------------------------------------------
 -- Neighbor Binding Integrity Policy Attachment Table - Vlan
 --------------------------------------------------------------

rlNbrBindingIntegrityVlanPolicyTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlNbrBindingIntegrityVlanPolicyEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION  "The table specifies Neighbor Binding Integrity policy
                attachment for vlans."
   ::= { rlNbrBindingIntegrity 4 }

rlNbrBindingIntegrityVlanPolicyEntry OBJECT-TYPE
   SYNTAX  RlNbrBindingIntegrityVlanPolicyEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION   "The row definition for this table."
   INDEX { rlNbrBindingIntegrityVlanPolicyVlanTag }
   ::= { rlNbrBindingIntegrityVlanPolicyTable 1 }

RlNbrBindingIntegrityVlanPolicyEntry ::= SEQUENCE {
   rlNbrBindingIntegrityVlanPolicyVlanTag            VlanId,
   rlNbrBindingIntegrityVlanPolicyName               DisplayString,
   rlNbrBindingIntegrityVlanPolicyRowStatus          RowStatus
}

rlNbrBindingIntegrityVlanPolicyVlanTag OBJECT-TYPE
   SYNTAX VlanId
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
       "The VLAN identifier."
   ::= { rlNbrBindingIntegrityVlanPolicyEntry 1 }

rlNbrBindingIntegrityVlanPolicyName OBJECT-TYPE
   SYNTAX DisplayString (SIZE(1..32))
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "The Neighbor Binding Integrity policy name."
   ::= { rlNbrBindingIntegrityVlanPolicyEntry 2 }

rlNbrBindingIntegrityVlanPolicyRowStatus OBJECT-TYPE
   SYNTAX RowStatus
   MAX-ACCESS read-create
   STATUS current
   DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
   ::= { rlNbrBindingIntegrityVlanPolicyEntry 3 }
 --------------------------------------------------------------
 -- Neighbor Binding Integrity Policy Attachment Table - Vlan
 --------------------------------------------------------------

 rlNbrBindingIntegrityPolicyVlanTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNbrBindingIntegrityPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Neighbor Binding Integrity policy
                 attachment for vlans."
    ::= { rlNbrBindingIntegrity 5 }

 rlNbrBindingIntegrityPolicyVlanEntry OBJECT-TYPE
    SYNTAX  RlNbrBindingIntegrityPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlNbrBindingIntegrityPolicyVlanPolicyName }
    ::= { rlNbrBindingIntegrityPolicyVlanTable 1 }

 RlNbrBindingIntegrityPolicyVlanEntry ::= SEQUENCE {
    rlNbrBindingIntegrityPolicyVlanPolicyName    DisplayString,
    rlNbrBindingIntegrityPolicyVlan1to1024       OCTET STRING,
    rlNbrBindingIntegrityPolicyVlan1025to2048    OCTET STRING,
    rlNbrBindingIntegrityPolicyVlan2049to3072    OCTET STRING,
    rlNbrBindingIntegrityPolicyVlan3073to4094    OCTET STRING
 }

 rlNbrBindingIntegrityPolicyVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION
        "The Neighbor Binding Integrity policy name"
    ::= { rlNbrBindingIntegrityPolicyVlanEntry 1 }

 rlNbrBindingIntegrityPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1 to 1024."
    DEFVAL {'00'H}
    ::= { rlNbrBindingIntegrityPolicyVlanEntry 2 }

 rlNbrBindingIntegrityPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1025 to 2048."
    DEFVAL {'00'H}
    ::= { rlNbrBindingIntegrityPolicyVlanEntry 3 }

 rlNbrBindingIntegrityPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 2049 to 3072."
    DEFVAL {'00'H}
    ::= { rlNbrBindingIntegrityPolicyVlanEntry 4 }

 rlNbrBindingIntegrityPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 3073 to 4094."
    DEFVAL {'00'H}
    ::= { rlNbrBindingIntegrityPolicyVlanEntry 5 }

 --------------------------------------------------------------
 -- Neighbor Binding Integrity Policy Enable Table
 --------------------------------------------------------------

 rlNbrBindingIntegrityEnableVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlNbrBindingIntegrityEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table contains only one entry of a static vlan list."
    ::= { rlNbrBindingIntegrity 6 }

 rlNbrBindingIntegrityEnableVlanEntry OBJECT-TYPE
    SYNTAX      RlNbrBindingIntegrityEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Statically created by local or network management vlan list"
    INDEX   {rlNbrBindingIntegrityEnableVlanIndex}
    ::= { rlNbrBindingIntegrityEnableVlanTable 1 }

 RlNbrBindingIntegrityEnableVlanEntry ::=SEQUENCE {
    rlNbrBindingIntegrityEnableVlanIndex         INTEGER,
    rlNbrBindingIntegrityEnableVlan1to1024       OCTET STRING,
    rlNbrBindingIntegrityEnableVlan1025to2048    OCTET STRING,
    rlNbrBindingIntegrityEnableVlan2049to3072    OCTET STRING,
    rlNbrBindingIntegrityEnableVlan3073to4094    OCTET STRING
 }

rlNbrBindingIntegrityEnableVlanIndex  OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
     "The table contains only one static entry."

   ::= { rlNbrBindingIntegrityEnableVlanEntry 1 }

rlNbrBindingIntegrityEnableVlan1to1024 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1 to 1024."
   DEFVAL {'00'H}
   ::= { rlNbrBindingIntegrityEnableVlanEntry 2 }

rlNbrBindingIntegrityEnableVlan1025to2048 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1025 to 2048."
   DEFVAL {'00'H}
   ::= { rlNbrBindingIntegrityEnableVlanEntry 3 }

rlNbrBindingIntegrityEnableVlan2049to3072 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 2049 to 3072."
   DEFVAL {'00'H}
   ::= { rlNbrBindingIntegrityEnableVlanEntry 4 }

rlNbrBindingIntegrityEnableVlan3073to4094 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 3073 to 4094."
   DEFVAL {'00'H}
   ::= { rlNbrBindingIntegrityEnableVlanEntry 5 }


 -------------------------------------------
 -- Neighbor Binding Integrity Binding Table
 -------------------------------------------

rlNbrBindingIntegrityBindingTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlNbrBindingIntegrityBindingEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION  "The table specifies Neighbor Binding Integrity binding table."
   ::= { rlNbrBindingIntegrity 7 }

rlNbrBindingIntegrityBindingEntry OBJECT-TYPE
   SYNTAX  RlNbrBindingIntegrityBindingEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION   "The row definition for this table."
   INDEX { rlNbrBindingIntegrityBindingVlanTag,
           rlNbrBindingIntegrityBindingSourceAddressType,
           rlNbrBindingIntegrityBindingSourceAddress  }
   ::= { rlNbrBindingIntegrityBindingTable 1 }

RlNbrBindingIntegrityBindingEntry ::= SEQUENCE {
   rlNbrBindingIntegrityBindingVlanTag            VlanId,
   rlNbrBindingIntegrityBindingSourceAddressType  InetAddressType,
   rlNbrBindingIntegrityBindingSourceAddress      InetAddress,
   rlNbrBindingIntegrityBindingIfIndex            InterfaceIndex,
   rlNbrBindingIntegrityBindingMacAddress         MacAddress,
   rlNbrBindingIntegrityBindingOrigin             INTEGER,
   rlNbrBindingIntegrityBindingState              INTEGER,
   rlNbrBindingIntegrityBindingExpiryTime         Unsigned32,
   rlNbrBindingIntegrityBindingRowStatus          RowStatus,
   rlNbrBindingIntegrityBindingTCAMOverflow       TruthValue
}

rlNbrBindingIntegrityBindingVlanTag OBJECT-TYPE
   SYNTAX VlanId
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
       "The binding entry's VLAN tag."
   ::= { rlNbrBindingIntegrityBindingEntry 1 }

rlNbrBindingIntegrityBindingSourceAddressType OBJECT-TYPE
   SYNTAX  InetAddressType
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION
        "The binding entry's INET address type of the source.
         The only inet type that is supported is ipv6."
   ::= { rlNbrBindingIntegrityBindingEntry 2 }

rlNbrBindingIntegrityBindingSourceAddress OBJECT-TYPE
   SYNTAX  InetAddress
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION
        "The binding entry's INET address of the source."
   ::= { rlNbrBindingIntegrityBindingEntry 3 }

rlNbrBindingIntegrityBindingIfIndex OBJECT-TYPE
   SYNTAX  InterfaceIndex
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "The binding entry's anchor interface."
   ::= { rlNbrBindingIntegrityBindingEntry 4 }

rlNbrBindingIntegrityBindingMacAddress OBJECT-TYPE
   SYNTAX  MacAddress
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "The binding entry's anchor MAC Address."
   ::= { rlNbrBindingIntegrityBindingEntry 5 }

rlNbrBindingIntegrityBindingOrigin OBJECT-TYPE
   SYNTAX INTEGER {
        static(1),
        ndp(2),
        dhcp(3)
        }
   MAX-ACCESS  read-only
   STATUS current
   DESCRIPTION
        "The binding entry's origin: local, static, ndp, dhcp."
   ::= { rlNbrBindingIntegrityBindingEntry 6 }

rlNbrBindingIntegrityBindingState OBJECT-TYPE
   SYNTAX INTEGER {
        valid(0),
        tentative(1)
        }
   MAX-ACCESS  read-only
   STATUS current
   DESCRIPTION
        "The binding entry's state: valid, tentative."
   ::= { rlNbrBindingIntegrityBindingEntry 7 }

rlNbrBindingIntegrityBindingExpiryTime OBJECT-TYPE
   SYNTAX Unsigned32
   MAX-ACCESS  read-only
   STATUS current
   DESCRIPTION
        "The time in seconds until the entry is expired.
         A value of 4294967295 denotes infinite lifetime."
   ::= { rlNbrBindingIntegrityBindingEntry 8 }

rlNbrBindingIntegrityBindingRowStatus OBJECT-TYPE
   SYNTAX RowStatus
   MAX-ACCESS read-create
   STATUS current
   DESCRIPTION
      "The row status variable, used according to row
      installation and removal conventions."
   ::= { rlNbrBindingIntegrityBindingEntry 9 }

rlNbrBindingIntegrityBindingTCAMOverflow OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Signs if entry is configured in TCAM"
    DEFVAL  { false }
    ::= { rlNbrBindingIntegrityBindingEntry 10 }


 -------------------------------------------
 -- Neighbor Binding Integrity Clear Table (Action only)
 -------------------------------------------

 rlNbrBindingIntegrityClearTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlNbrBindingIntegrityClearEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION  "The table clears Neighbor Binding Integrity binding table
                 according to configured filters."
   ::= { rlNbrBindingIntegrity 8 }


 rlNbrBindingIntegrityClearEntry OBJECT-TYPE
   SYNTAX  RlNbrBindingIntegrityClearEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION   "The row definition for this table."
   INDEX { rlNbrBindingIntegrityClearIndex  }
   ::= { rlNbrBindingIntegrityClearTable 1 }

 RlNbrBindingIntegrityClearEntry ::= SEQUENCE {
   rlNbrBindingIntegrityClearIndex              INTEGER,
   rlNbrBindingIntegrityClearVlanTag            VlanId,
   rlNbrBindingIntegrityClearSourceAddressType  InetAddressType,
   rlNbrBindingIntegrityClearSourceAddress      InetAddress,
   rlNbrBindingIntegrityClearIfIndex            InterfaceIndex,
   rlNbrBindingIntegrityClearMacAddress         MacAddress,
   rlNbrBindingIntegrityClearRowStatus          RowStatus,
   rlNbrBindingIntegrityClearBindMethod         INTEGER
 }

 rlNbrBindingIntegrityClearIndex OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION
        "The row index in the table."
   ::= { rlNbrBindingIntegrityClearEntry 1 }

 rlNbrBindingIntegrityClearVlanTag OBJECT-TYPE
   SYNTAX VlanId
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
       "Clear binding entries with this VLAN tag."
   ::= { rlNbrBindingIntegrityClearEntry 2 }

 rlNbrBindingIntegrityClearSourceAddressType OBJECT-TYPE
   SYNTAX  InetAddressType
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
       "Clear binding entries with this source address type.
        The only inet type that is supported is ipv6."
   ::= { rlNbrBindingIntegrityClearEntry 3 }

 rlNbrBindingIntegrityClearSourceAddress OBJECT-TYPE
   SYNTAX  InetAddress
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "Clear binding entries with this source address."
   ::= { rlNbrBindingIntegrityClearEntry 4 }

 rlNbrBindingIntegrityClearIfIndex OBJECT-TYPE
   SYNTAX  InterfaceIndex
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "cClear binding entries with this anchor interface."
   ::= { rlNbrBindingIntegrityClearEntry 5 }

 rlNbrBindingIntegrityClearMacAddress OBJECT-TYPE
   SYNTAX  MacAddress
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "clear binding entries with this anchor MAC Address."
   ::= { rlNbrBindingIntegrityClearEntry 6 }

 rlNbrBindingIntegrityClearRowStatus OBJECT-TYPE
   SYNTAX RowStatus
   MAX-ACCESS read-create
   STATUS current
   DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
   ::= { rlNbrBindingIntegrityClearEntry 7 }

 rlNbrBindingIntegrityClearBindMethod OBJECT-TYPE
   SYNTAX      INTEGER {
        ndp(1),
        dhcp(2)
   }
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "clear dynamic entries bound using the specified method."
   ::= { rlNbrBindingIntegrityClearEntry 8 }


 --------------------------------------------------
 -- Neighbor Binding Integrity Binding Prefix Table
 --------------------------------------------------

rlNbrBindingIntegrityBindingPrefixTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlNbrBindingIntegrityBindingPrefixEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION  "The table specifies Neighbor Binding Integrity binding table."
   ::= { rlNbrBindingIntegrity 18 }

rlNbrBindingIntegrityBindingPrefixEntry OBJECT-TYPE
   SYNTAX  RlNbrBindingIntegrityBindingPrefixEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION   "The row definition for this table."
   INDEX { rlNbrBindingIntegrityBindingPrefixVlanTag,
           rlNbrBindingIntegrityBindingPrefixAddressType,
           rlNbrBindingIntegrityBindingPrefixAddress,
           rlNbrBindingIntegrityBindingPrefixLength  }
   ::= { rlNbrBindingIntegrityBindingPrefixTable 1 }

RlNbrBindingIntegrityBindingPrefixEntry ::= SEQUENCE {
   rlNbrBindingIntegrityBindingPrefixVlanTag            VlanId,
   rlNbrBindingIntegrityBindingPrefixAddressType        InetAddressType,
   rlNbrBindingIntegrityBindingPrefixAddress            InetAddress,
   rlNbrBindingIntegrityBindingPrefixLength             InetAddressPrefixLength,
   rlNbrBindingIntegrityBindingPrefixOrigin             INTEGER,
   rlNbrBindingIntegrityBindingPrefixAllowAutoconfig    TruthValue,
   rlNbrBindingIntegrityBindingPrefixExpiryTime         Unsigned32,
   rlNbrBindingIntegrityBindingPrefixRowStatus          RowStatus
}

rlNbrBindingIntegrityBindingPrefixVlanTag OBJECT-TYPE
   SYNTAX VlanId
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
       "The binding prefix entry's VLAN tag."
   ::= { rlNbrBindingIntegrityBindingPrefixEntry 1 }

rlNbrBindingIntegrityBindingPrefixAddressType OBJECT-TYPE
   SYNTAX  InetAddressType
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION
        "The binding prefix entry's INET address type.
         The only inet type that is supported is ipv6."
   ::= { rlNbrBindingIntegrityBindingPrefixEntry 2 }

rlNbrBindingIntegrityBindingPrefixAddress OBJECT-TYPE
   SYNTAX  InetAddress
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION
        "The binding prefix entry's address."
   ::= { rlNbrBindingIntegrityBindingPrefixEntry 3 }

rlNbrBindingIntegrityBindingPrefixLength OBJECT-TYPE
   SYNTAX  InetAddressPrefixLength
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION
        "Indicates the number of leading one bits that form the
        mask to be logical-ANDed with the inet address
        before being compared to the value in the
        rlNbrBindingIntegrityBindingPrefixAddress field."
   ::= { rlNbrBindingIntegrityBindingPrefixEntry 4 }

rlNbrBindingIntegrityBindingPrefixOrigin OBJECT-TYPE
   SYNTAX INTEGER {
        static(1),
        dynamic(2)
        }
   MAX-ACCESS  read-only
   STATUS current
   DESCRIPTION
        "The binding prefix entry's origin: static or dynamic"
   ::= { rlNbrBindingIntegrityBindingPrefixEntry 5 }

rlNbrBindingIntegrityBindingPrefixAllowAutoconfig OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "Indicates whether the prefix can be used for
         stateless address auto-configuration."
   ::= { rlNbrBindingIntegrityBindingPrefixEntry 6 }

rlNbrBindingIntegrityBindingPrefixExpiryTime OBJECT-TYPE
   SYNTAX Unsigned32
   MAX-ACCESS  read-only
   STATUS current
   DESCRIPTION
        "The time in seconds until the entry is expired.
         A value of 4294967295 denotes infinite lifetime."
   ::= { rlNbrBindingIntegrityBindingPrefixEntry 7 }

rlNbrBindingIntegrityBindingPrefixRowStatus OBJECT-TYPE
   SYNTAX RowStatus
   MAX-ACCESS read-create
   STATUS current
   DESCRIPTION
      "The row status variable, used according to row
      installation and removal conventions."
   ::= { rlNbrBindingIntegrityBindingPrefixEntry 8 }

 --------------------------------------------------------------
 -- Neighbor Binding Integrity Clear Prefix Table (Action only)
 --------------------------------------------------------------

 rlNbrBindingIntegrityClearPrefixTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlNbrBindingIntegrityClearPrefixEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION  "The table clears Neighbor Binding Integrity Binding Prefix table
                 according to configured filters."
   ::= { rlNbrBindingIntegrity 19 }


 rlNbrBindingIntegrityClearPrefixEntry OBJECT-TYPE
   SYNTAX  RlNbrBindingIntegrityClearPrefixEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION   "The row definition for this table."
   INDEX { rlNbrBindingIntegrityClearPrefixIndex  }
   ::= { rlNbrBindingIntegrityClearPrefixTable 1 }

 RlNbrBindingIntegrityClearPrefixEntry ::= SEQUENCE {
   rlNbrBindingIntegrityClearPrefixIndex        INTEGER,
   rlNbrBindingIntegrityClearPrefixVlanTag      VlanId,
   rlNbrBindingIntegrityClearPrefixAddressType  InetAddressType,
   rlNbrBindingIntegrityClearPrefixAddress      InetAddress,
   rlNbrBindingIntegrityClearPrefixLength       InetAddressPrefixLength,
   rlNbrBindingIntegrityClearPrefixRowStatus    RowStatus
 }

 rlNbrBindingIntegrityClearPrefixIndex OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION
        "The row index in the table."
   ::= { rlNbrBindingIntegrityClearPrefixEntry 1 }

 rlNbrBindingIntegrityClearPrefixVlanTag OBJECT-TYPE
   SYNTAX VlanId
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
       "Clear binding prefix entries with this VLAN tag."
   ::= { rlNbrBindingIntegrityClearPrefixEntry 2 }

 rlNbrBindingIntegrityClearPrefixAddressType OBJECT-TYPE
   SYNTAX  InetAddressType
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
       "Clear binding prefix entries with this address type.
        The only inet type that is supported is ipv6."
   ::= { rlNbrBindingIntegrityClearPrefixEntry 3 }

 rlNbrBindingIntegrityClearPrefixAddress OBJECT-TYPE
   SYNTAX  InetAddress
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "Clear binding prefix entries with this address prefix."
   ::= { rlNbrBindingIntegrityClearPrefixEntry 4 }

 rlNbrBindingIntegrityClearPrefixLength OBJECT-TYPE
   SYNTAX  InetAddressPrefixLength
   MAX-ACCESS  read-write
   STATUS current
   DESCRIPTION
        "Indicates the number of leading one bits that form the
        mask to be logical-ANDed with the inet address
        before being compared to the value in the
        rlNbrBindingIntegrityClearPrefixAddress field."
   ::= { rlNbrBindingIntegrityClearPrefixEntry 5 }

 rlNbrBindingIntegrityClearPrefixRowStatus OBJECT-TYPE
   SYNTAX RowStatus
   MAX-ACCESS read-create
   STATUS current
   DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
   ::= { rlNbrBindingIntegrityClearPrefixEntry 6 }

 --------------------------------------------------------------
 -- Neighbor Binding Integrity Active Policy Table (Read Only)
 --------------------------------------------------------------

 rlNbrBindingIntegrityActivePolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlNbrBindingIntegrityActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Neighbor Binding Integrity
                 per policy configurations."
    ::= { rlNbrBindingIntegrity 9 }

 rlNbrBindingIntegrityActivePolicyEntry OBJECT-TYPE
    SYNTAX  RlNbrBindingIntegrityActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlNbrBindingIntegrityActivePolicyIfIndex,
            rlNbrBindingIntegrityActivePolicyVlanTag }
    ::= { rlNbrBindingIntegrityActivePolicyTable 1 }

 RlNbrBindingIntegrityActivePolicyEntry ::= SEQUENCE {
    rlNbrBindingIntegrityActivePolicyIfIndex                  InterfaceIndex,
    rlNbrBindingIntegrityActivePolicyVlanTag                  VlanId,
    rlNbrBindingIntegrityActivePolicyNamePort                 DisplayString,
    rlNbrBindingIntegrityActivePolicyNameVlan                 DisplayString,
    rlNbrBindingIntegrityActivePolicyDeviceRole               INTEGER,
    rlNbrBindingIntegrityActivePolicyDeviceRoleType           RlIpv6FhsSettingType,
    rlNbrBindingIntegrityActivePolicyLogBinding               RlIpv6FhsSettingStatusType,
    rlNbrBindingIntegrityActivePolicyLogBindingType           RlIpv6FhsSettingType,
    rlNbrBindingIntegrityActivePolicyMaxEntriesVlanLimit      Integer32,
    rlNbrBindingIntegrityActivePolicyMaxEntriesVlanLimitType  RlIpv6FhsSettingType,
    rlNbrBindingIntegrityActivePolicyMaxEntriesInterfaceLimit Integer32,
    rlNbrBindingIntegrityActivePolicyMaxEntriesInterfaceLimitType RlIpv6FhsSettingType,
    rlNbrBindingIntegrityActivePolicyMaxEntriesMacLimit       Integer32,
    rlNbrBindingIntegrityActivePolicyMaxEntriesMacLimitType   RlIpv6FhsSettingType,
    rlNbrBindingIntegrityActivePolicyBindingLifetime          Integer32,
    rlNbrBindingIntegrityActivePolicyBindingLifetimeType      RlIpv6FhsSettingType,
    rlNbrBindingIntegrityActivePolicyPrefixValidation         RlIpv6FhsSettingStatusType,
    rlNbrBindingIntegrityActivePolicyPrefixValidationType     RlIpv6FhsSettingType,
    rlNbrBindingIntegrityActivePolicyAddressConfig            INTEGER,
    rlNbrBindingIntegrityActivePolicyAddressConfigType        RlIpv6FhsSettingType
    }

 rlNbrBindingIntegrityActivePolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 1 }

 rlNbrBindingIntegrityActivePolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 2 }

 rlNbrBindingIntegrityActivePolicyNamePort OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The Neighbor Binding Integrity policy name attached to given interface."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 3 }

 rlNbrBindingIntegrityActivePolicyNameVlan OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The Neighbor Binding Integrity policy name attached to given vlan."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 4 }

 rlNbrBindingIntegrityActivePolicyDeviceRole OBJECT-TYPE
   SYNTAX      INTEGER {
        perimeter(1),
        internal(2)
   }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Specify the role of the device attached."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 5 }

 rlNbrBindingIntegrityActivePolicyDeviceRoleType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlNbrBindingIntegrityActivePolicyDeviceRole setting type."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 6 }

 rlNbrBindingIntegrityActivePolicyLogBinding OBJECT-TYPE
    SYNTAX RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Enable/disable logging of Neighbor Binding Table events."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 7 }

 rlNbrBindingIntegrityActivePolicyLogBindingType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlNbrBindingIntegrityActivePolicyLogBinding setting type."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 8 }

 rlNbrBindingIntegrityActivePolicyMaxEntriesVlanLimit OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..65535)
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "Indicates how many entries can be added to Neighbor Binding Table
         with the same VLAN tag.
         The value of -2 indicates there is no limit."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 9 }

 rlNbrBindingIntegrityActivePolicyMaxEntriesVlanLimitType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "rlNbrBindingIntegrityActivePolicyMaxEntriesVlanLimit setting type."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 10 }

 rlNbrBindingIntegrityActivePolicyMaxEntriesInterfaceLimit OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..65535)
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "Indicates how many entries can be added to Neighbor Binding Table
         with the same interface identifier.
         The value of -2 indicates there is no limit."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 11 }

 rlNbrBindingIntegrityActivePolicyMaxEntriesInterfaceLimitType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "rlNbrBindingIntegrityActivePolicyMaxEntriesInterfaceLimit setting type."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 12 }

 rlNbrBindingIntegrityActivePolicyMaxEntriesMacLimit OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..65535)
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "Indicates how many entries can be added to Neighbor Binding Table
         with the same MAC address.
         The value of -2 indicates there is no limit."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 13 }

 rlNbrBindingIntegrityActivePolicyMaxEntriesMacLimitType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "rlNbrBindingIntegrityActivePolicyMaxEntriesMacLimit setting type."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 14 }

 rlNbrBindingIntegrityActivePolicyBindingLifetime OBJECT-TYPE
    SYNTAX      Integer32 (60..3600)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Neighbor Binding entry's default lifetime in seconds."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 15 }

 rlNbrBindingIntegrityActivePolicyBindingLifetimeType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlNbrBindingIntegrityActivePolicyBindingLifetime setting type."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 16 }

 rlNbrBindingIntegrityActivePolicyPrefixValidation OBJECT-TYPE
    SYNTAX RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Enable/disable address prefix validation using Neighbor Prefix Table."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 17 }

 rlNbrBindingIntegrityActivePolicyPrefixValidationType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "rlNbrBindingIntegrityActivePolicyPrefixValidation setting type."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 18 }

 rlNbrBindingIntegrityActivePolicyAddressConfig OBJECT-TYPE
   SYNTAX      INTEGER {
        autoconfig(1),
        autoconfigAndManual(3),
        dhcp(4),
        autoconfigAndDhcp(5),
        autoconfigManualAndDhcp(7)
   }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Specify the allowed methods for address binding in Neighbor Binding Table.
          autoconfig(1) refers to stateless address autoconfiguration.
          autoconfigAndManual(3) allows manual and stateless address autoconfiguration.
          dhcp(4) permits binding only from DHCP.
          autoconfigAndDhcp(5) binds from DHCP and stateless address autoconfiguration.
          autoconfigManualAndDhcp(7) binds from Manual, DHCP and stateless address autoconfiguration."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 19 }

 rlNbrBindingIntegrityActivePolicyAddressConfigType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "rlNbrBindingIntegrityActivePolicyAddressConfig setting type."
    ::= { rlNbrBindingIntegrityActivePolicyEntry 20 }


 --------------------------------------------------------------
 -- Neighbor Binding Integrity Global Configurations
 --------------------------------------------------------------

 rlNbrBindingIntegrityBindingLifetime OBJECT-TYPE
    SYNTAX      Integer32 (60..3600)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Neighbor Binding entry's default lifetime in seconds."
    DEFVAL  { 300 }
    ::= { rlNbrBindingIntegrity 10 }

 rlNbrBindingIntegrityLogBinding OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Enable/disable logging of Neighbor Binding Table events"
    DEFVAL  { false }
    ::= { rlNbrBindingIntegrity 11 }

 rlNbrBindingIntegrityMaxEntriesVlanLimit OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..65535)
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates how many entries can be added to Neighbor Binding Table
         with the same VLAN tag.
         The value of -2 indicates there is no limit."
    DEFVAL { -2 }
    ::= { rlNbrBindingIntegrity 12 }

 rlNbrBindingIntegrityMaxEntriesInterfaceLimit OBJECT-TYPE
    SYNTAX      Integer32 (-2 |0..65535)
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates how many entries can be added to Neighbor Binding Table
         with the same interface identifier.
         The value of -2 indicates there is no limit."
    DEFVAL { -2 }
    ::= { rlNbrBindingIntegrity 13 }

 rlNbrBindingIntegrityMaxEntriesMacLimit OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..65535)
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates how many entries can be added to Neighbor Binding Table
         with the same MAC address.
         The value of -2 indicates there is no limit."
    DEFVAL { -2 }
    ::= { rlNbrBindingIntegrity 14 }

 rlNbrBindingIntegrityEntriesNum OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "Number of entries in Neighbor Binding Table."

    ::= { rlNbrBindingIntegrity 15 }

 rlNbrBindingIntegrityPrefixValidation OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Enable/disable address prefix validation using Neighbor Prefix Table."
    DEFVAL  { false }
    ::= { rlNbrBindingIntegrity 16 }

 rlNbrBindingIntegrityAddressConfig OBJECT-TYPE
   SYNTAX      INTEGER {
        autoconfig(1),
        autoconfigAndManual(3),
        dhcp(4),
        autoconfigAndDhcp(5),
        autoconfigManualAndDhcp(7)
   }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Specify the allowed methods for address binding in Neighbor Binding Table.
          autoconfig(1) refers to stateless address autoconfiguration.
          autoconfigAndManual(3) allows manual and stateless address autoconfiguration.
          dhcp(4) permits binding only from DHCP.
          autoconfigAndDhcp(5) binds from DHCP and stateless address autoconfiguration.
          autoconfigManualAndDhcp(7) binds from Manual, DHCP and stateless address autoconfiguration."
    DEFVAL  { autoconfigAndManual }
    ::= { rlNbrBindingIntegrity 17 }

 rlNbrBindingIntegrityPrefixEntriesNum OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "Number of entries in Neighbor Prefix Table."
    ::= { rlNbrBindingIntegrity 21 }

 --------------------------------------------------------------------
 -- Neighbor Binding Integrity Clear DHCP Recovery File (Action Only)
 --------------------------------------------------------------------

 rlNbrBindingIntegrityClearDhcpRecoveryFile OBJECT-TYPE
    SYNTAX      Integer32 (0..4094)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Clear neighbor binding integrity's DHCP recovery file.
           Setting a value of zero clears the information for all VLANs.
           Setting a non-zero value clears the information for a specific VLAN.
           Reading this object has not effect."
    ::= { rlNbrBindingIntegrity 20 }


 --------------------------------------------------------------
 -- Neighbor Binding Integrity Traps
 --------------------------------------------------------------

 rlNbrBindingIntegrityEntryAddedTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Information trap indicating that new binding entry was added to
         Neighbor Binding Table."
    ::=  { rndNotifications 230 }

 rlNbrBindingIntegrityEntryStateChangeTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Information trap indicating that binding entry state was changed."
    ::=  { rndNotifications 231 }

 rlNbrBindingIntegrityEntryAnchorChangeTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Information trap indicating that binding entry anchor was changed."
    ::=  { rndNotifications 232 }

 rlNbrBindingIntegrityEntryDeletedTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Information trap indicating that binding entry was deleted."
    ::=  { rndNotifications 233 }

 rlNbrBindingIntegrityEntryLimitReachTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Warning trap indicating that a new entry was not inserted into
         Neighbor Binding table because of maximum limit has been reached."
    ::=  { rndNotifications 234 }

 rlNbrBindingIntegrityOverflowTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Warning trap indicating that a new entry was not inserted into
         Neighbor Binding table because of the Neighbor Binding table overflow."
    ::=  { rndNotifications 235 }

 rlSrcGuardTCAMOverflowTrap
 NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Warning trap indicating that a new Source Guard entry was not inserted into
         TCAM because of the lack of resources."
    ::=  { rndNotifications 238 }

 rlNbrBindingIntegrityPrefixOverflowTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Warning trap indicating that a new entry was not inserted into
         Neighbor Prefix table because of the Neighbor Prefix table overflow."
    ::=  { rndNotifications 239 }

 --------------------------------------------------------------
 -- The DHCPv6 Guard
 --------------------------------------------------------------

 --------------------------------------------------------------
 -- The DHCPv6 Guard Policy Configuration Table
 --------------------------------------------------------------

 rlDhcpGuardPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDhcpGuardPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies DHCPv6 guard
                 per policy configurations."
    ::= { rlDhcpGuard 1 }

 rlDhcpGuardPolicyEntry OBJECT-TYPE
    SYNTAX  RlDhcpGuardPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlDhcpGuardPolicyName }
    ::= { rlDhcpGuardPolicyTable 1 }

 RlDhcpGuardPolicyEntry ::= SEQUENCE {
    rlDhcpGuardPolicyName                      DisplayString,
    rlDhcpGuardPolicyDeviceRole                INTEGER,
    rlDhcpGuardPolicyMatchServerAddrSpecified  TruthValue,
    rlDhcpGuardPolicyMatchServerAddr           DisplayString,
    rlDhcpGuardPolicyMatchReplyAddrSpecified   TruthValue,
    rlDhcpGuardPolicyMatchReplyAddr            DisplayString,
    rlDhcpGuardPolicyPrefMin                   Integer32,
    rlDhcpGuardPolicyPrefMax                   Integer32,
    rlDhcpGuardPolicyRowStatus                 RowStatus
    }

 rlDhcpGuardPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The DHCPv6 guard policy name"
    ::= { rlDhcpGuardPolicyEntry 1 }

 rlDhcpGuardPolicyDeviceRole OBJECT-TYPE
   SYNTAX      INTEGER {
        unspecified(-1),
        client(1),
        server(2)
   }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Specify the role of the device attached."
    DEFVAL  { unspecified }
    ::= { rlDhcpGuardPolicyEntry 2 }

 rlDhcpGuardPolicyMatchServerAddrSpecified OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates whether the rlDhcpGuardPolicyMatchServerAddr is specified."
    DEFVAL { false }
    ::= { rlDhcpGuardPolicyEntry 3 }

 rlDhcpGuardPolicyMatchServerAddr OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..64))
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "The IPv6 prefix list to be matched for IPv6 address in messages sent by DHCPv6 servers.
        Relevant only when rlDhcpGuardPolicyMatchServerAddrSpecified is true.
        The empty string means this validation is disabled."
    DEFVAL { "" }
    ::= { rlDhcpGuardPolicyEntry 4 }

rlDhcpGuardPolicyMatchReplyAddrSpecified OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates whether the rlDhcpGuardPolicyMatchReplyAddr is specified."
    DEFVAL { false }
    ::= { rlDhcpGuardPolicyEntry 5 }

 rlDhcpGuardPolicyMatchReplyAddr OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..64))
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "The IPv6 prefix list to be matched for assigned IPv6 addressed by DHCPv6 servers.
        Relevant only when rlDhcpGuardPolicyMatchReplyAddrSpecified is true.
        The empty string means this validation is disabled."
    DEFVAL { "" }
    ::= { rlDhcpGuardPolicyEntry 6 }

 rlDhcpGuardPolicyPrefMin OBJECT-TYPE
    SYNTAX      Integer32 (-2 | -1 | 0..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Minimum preference value limit.
           A value of -1 indicates unspecified value.
           A value of -2 indicates validation is disabled."
    DEFVAL  { -1 }
    ::= { rlDhcpGuardPolicyEntry 7 }

 rlDhcpGuardPolicyPrefMax OBJECT-TYPE
    SYNTAX      Integer32 (-2 | -1 | 0..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Maximum preference value limit.
           A value of -1 indicates unspecified value.
           A value of -2 indicates validation is disabled."
    DEFVAL  { -1 }
    ::= { rlDhcpGuardPolicyEntry 8 }

 rlDhcpGuardPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
    ::= { rlDhcpGuardPolicyEntry 9 }

 --------------------------------------------------------------
 -- The DHCPv6 Guard Policy Attachment Table - Port
 --------------------------------------------------------------

 rlDhcpGuardPortPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDhcpGuardPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies DHCPv6 guard policy
                 attachment for ports."
    ::= { rlDhcpGuard 2 }

 rlDhcpGuardPortPolicyEntry OBJECT-TYPE
    SYNTAX  RlDhcpGuardPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlDhcpGuardPortPolicyIfIndex,
            IMPLIED rlDhcpGuardPortPolicyName }
    ::= { rlDhcpGuardPortPolicyTable 1 }

 RlDhcpGuardPortPolicyEntry ::= SEQUENCE {
    rlDhcpGuardPortPolicyIfIndex            InterfaceIndex,
    rlDhcpGuardPortPolicyName               DisplayString,
    rlDhcpGuardPortPolicyVlan1to1024        OCTET STRING,
    rlDhcpGuardPortPolicyVlan1025to2048     OCTET STRING,
    rlDhcpGuardPortPolicyVlan2049to3072     OCTET STRING,
    rlDhcpGuardPortPolicyVlan3073to4094     OCTET STRING,
    rlDhcpGuardPortPolicyRowStatus          RowStatus
    }

 rlDhcpGuardPortPolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlDhcpGuardPortPolicyEntry 1 }

 rlDhcpGuardPortPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The DHCPv6 guard policy name"
    ::= { rlDhcpGuardPortPolicyEntry 2 }

 rlDhcpGuardPortPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlDhcpGuardPortPolicyEntry 3 }

 rlDhcpGuardPortPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlDhcpGuardPortPolicyEntry 4 }

 rlDhcpGuardPortPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlDhcpGuardPortPolicyEntry 5 }

 rlDhcpGuardPortPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlDhcpGuardPortPolicyEntry 6 }

 rlDhcpGuardPortPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlDhcpGuardPortPolicyEntry 7 }

 --------------------------------------------------------------
 -- The DHCPv6 Guard Policy Attachment Table - Port (Read Only)
 --------------------------------------------------------------

 rlDhcpGuardPolicyPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDhcpGuardPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies DHCPv6 guard policy
                 attachment for ports."
    ::= { rlDhcpGuard 3 }

 rlDhcpGuardPolicyPortEntry OBJECT-TYPE
    SYNTAX  RlDhcpGuardPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlDhcpGuardPolicyPortName,
            rlDhcpGuardPolicyPortIfIndex }
    ::= { rlDhcpGuardPolicyPortTable 1 }

 RlDhcpGuardPolicyPortEntry ::= SEQUENCE {
    rlDhcpGuardPolicyPortName               DisplayString,
    rlDhcpGuardPolicyPortIfIndex            InterfaceIndex,
    rlDhcpGuardPolicyPortVlan1to1024        OCTET STRING,
    rlDhcpGuardPolicyPortVlan1025to2048     OCTET STRING,
    rlDhcpGuardPolicyPortVlan2049to3072     OCTET STRING,
    rlDhcpGuardPolicyPortVlan3073to4094     OCTET STRING
    }

 rlDhcpGuardPolicyPortName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The DHCPv6 guard policy name"
    ::= { rlDhcpGuardPolicyPortEntry 1 }

 rlDhcpGuardPolicyPortIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlDhcpGuardPolicyPortEntry 2 }

 rlDhcpGuardPolicyPortVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlDhcpGuardPolicyPortEntry 3 }

 rlDhcpGuardPolicyPortVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlDhcpGuardPolicyPortEntry 4 }

 rlDhcpGuardPolicyPortVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlDhcpGuardPolicyPortEntry 5 }

 rlDhcpGuardPolicyPortVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlDhcpGuardPolicyPortEntry 6 }

 --------------------------------------------------------------
 -- The DHCPv6 Guard Policy Attachment Table - Vlan
 --------------------------------------------------------------

 rlDhcpGuardVlanPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDhcpGuardVlanPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies DHCPv6 guard policy
                 attachment for vlans."
    ::= { rlDhcpGuard 4 }

 rlDhcpGuardVlanPolicyEntry OBJECT-TYPE
    SYNTAX  RlDhcpGuardVlanPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlDhcpGuardVlanPolicyVlanTag }
    ::= { rlDhcpGuardVlanPolicyTable 1 }

 RlDhcpGuardVlanPolicyEntry ::= SEQUENCE {
    rlDhcpGuardVlanPolicyVlanTag            VlanId,
    rlDhcpGuardVlanPolicyName               DisplayString,
    rlDhcpGuardVlanPolicyRowStatus          RowStatus
 }

 rlDhcpGuardVlanPolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlDhcpGuardVlanPolicyEntry 1 }

 rlDhcpGuardVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "The DHCPv6 guard policy name"
    ::= { rlDhcpGuardVlanPolicyEntry 2 }

 rlDhcpGuardVlanPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlDhcpGuardVlanPolicyEntry 3 }
 --------------------------------------------------------------
 -- The DHCPv6 Guard Policy Attachment Table - Vlan
 --------------------------------------------------------------

 rlDhcpGuardPolicyVlanTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDhcpGuardPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies DHCPv6 guard policy
                 attachment for vlans."
    ::= { rlDhcpGuard 5 }

 rlDhcpGuardPolicyVlanEntry OBJECT-TYPE
    SYNTAX  RlDhcpGuardPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlDhcpGuardPolicyVlanPolicyName }
    ::= { rlDhcpGuardPolicyVlanTable 1 }

 RlDhcpGuardPolicyVlanEntry ::= SEQUENCE {
    rlDhcpGuardPolicyVlanPolicyName    DisplayString,
    rlDhcpGuardPolicyVlan1to1024       OCTET STRING,
    rlDhcpGuardPolicyVlan1025to2048    OCTET STRING,
    rlDhcpGuardPolicyVlan2049to3072    OCTET STRING,
    rlDhcpGuardPolicyVlan3073to4094    OCTET STRING

 }

 rlDhcpGuardPolicyVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION
        "The DHCPv6 guard policy name"
    ::= { rlDhcpGuardPolicyVlanEntry 1 }

 rlDhcpGuardPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1 to 1024."
    DEFVAL {'00'H}
    ::= { rlDhcpGuardPolicyVlanEntry 2 }

 rlDhcpGuardPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1025 to 2048."
    DEFVAL {'00'H}
    ::= { rlDhcpGuardPolicyVlanEntry 3 }

 rlDhcpGuardPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 2049 to 3072."
    DEFVAL {'00'H}
    ::= { rlDhcpGuardPolicyVlanEntry 4 }


 rlDhcpGuardPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 3073 to 4094."
    DEFVAL {'00'H}
    ::= { rlDhcpGuardPolicyVlanEntry 5 }

 --------------------------------------------------------------
 -- The DHCPv6 Guard Policy Enable Table
 --------------------------------------------------------------

rlDhcpGuardEnableVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlDhcpGuardEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table contains only one entry of a static vlan list."
    ::= { rlDhcpGuard 6 }

rlDhcpGuardEnableVlanEntry OBJECT-TYPE
    SYNTAX      RlDhcpGuardEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Statically created by local or network management vlan list"
    INDEX   {rlDhcpGuardEnableVlanIndex}
    ::= { rlDhcpGuardEnableVlanTable 1 }

RlDhcpGuardEnableVlanEntry ::=SEQUENCE {
    rlDhcpGuardEnableVlanIndex         INTEGER,
    rlDhcpGuardEnableVlan1to1024       OCTET STRING,
    rlDhcpGuardEnableVlan1025to2048    OCTET STRING,
    rlDhcpGuardEnableVlan2049to3072    OCTET STRING,
    rlDhcpGuardEnableVlan3073to4094    OCTET STRING

}

rlDhcpGuardEnableVlanIndex  OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
     "The table contains only one static entry."

   ::= { rlDhcpGuardEnableVlanEntry 1 }

rlDhcpGuardEnableVlan1to1024 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1 to 1024."
   DEFVAL {'00'H}
   ::= { rlDhcpGuardEnableVlanEntry 2 }

rlDhcpGuardEnableVlan1025to2048 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1025 to 2048."
   DEFVAL {'00'H}
   ::= { rlDhcpGuardEnableVlanEntry 3 }

rlDhcpGuardEnableVlan2049to3072 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 2049 to 3072."
   DEFVAL {'00'H}
   ::= { rlDhcpGuardEnableVlanEntry 4 }

rlDhcpGuardEnableVlan3073to4094 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 3073 to 4094."
   DEFVAL {'00'H}
   ::= { rlDhcpGuardEnableVlanEntry 5 }

 --------------------------------------------------------------
 -- The DHCPv6 Guard Active Policy Table (Read Only)
 --------------------------------------------------------------

 rlDhcpGuardActivePolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDhcpGuardActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies DHCPv6 guard
                 per policy configurations."
    ::= { rlDhcpGuard 7 }

 rlDhcpGuardActivePolicyEntry OBJECT-TYPE
    SYNTAX  RlDhcpGuardActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlDhcpGuardActivePolicyIfIndex,
            rlDhcpGuardActivePolicyVlanTag }
    ::= { rlDhcpGuardActivePolicyTable 1 }

 RlDhcpGuardActivePolicyEntry ::= SEQUENCE {
    rlDhcpGuardActivePolicyIfIndex              InterfaceIndex,
    rlDhcpGuardActivePolicyVlanTag              VlanId,
    rlDhcpGuardActivePolicyNamePort             DisplayString,
    rlDhcpGuardActivePolicyNameVlan             DisplayString,
    rlDhcpGuardActivePolicyDeviceRole           INTEGER,
    rlDhcpGuardActivePolicyDeviceRoleType       RlIpv6FhsSettingType,
    rlDhcpGuardActivePolicyMatchServerAddr      DisplayString,
    rlDhcpGuardActivePolicyMatchServerAddrType  RlIpv6FhsSettingType,
    rlDhcpGuardActivePolicyMatchReplyAddr       DisplayString,
    rlDhcpGuardActivePolicyMatchReplyAddrType   RlIpv6FhsSettingType,
    rlDhcpGuardActivePolicyPrefMin              Integer32,
    rlDhcpGuardActivePolicyPrefMinType          RlIpv6FhsSettingType,
    rlDhcpGuardActivePolicyPrefMax              Integer32,
    rlDhcpGuardActivePolicyPrefMaxType          RlIpv6FhsSettingType
    }

 rlDhcpGuardActivePolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlDhcpGuardActivePolicyEntry 1 }

 rlDhcpGuardActivePolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { rlDhcpGuardActivePolicyEntry 2 }

 rlDhcpGuardActivePolicyNamePort OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The DHCPv6 guard policy name attached to given interface."
    ::= { rlDhcpGuardActivePolicyEntry 3 }

 rlDhcpGuardActivePolicyNameVlan OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The DHCPv6 guard policy name attached to given vlan."
    ::= { rlDhcpGuardActivePolicyEntry 4 }

 rlDhcpGuardActivePolicyDeviceRole OBJECT-TYPE
   SYNTAX      INTEGER {
        client(1),
        server(2)
   }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Specify the role of the device attached."
    ::= { rlDhcpGuardActivePolicyEntry 5 }

 rlDhcpGuardActivePolicyDeviceRoleType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlDhcpGuardActivePolicyDeviceRole setting type."
    ::= { rlDhcpGuardActivePolicyEntry 6 }

 rlDhcpGuardActivePolicyMatchServerAddr OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..64))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The IPv6 prefix list to be matched for IPv6 address in messages sent by DHCPv6 servers.
        The empty string means this validation is disabled."
    ::= { rlDhcpGuardActivePolicyEntry 7 }

 rlDhcpGuardActivePolicyMatchServerAddrType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "rlDhcpGuardActivePolicyMatchServerAddr setting type."
    ::= { rlDhcpGuardActivePolicyEntry 8 }

 rlDhcpGuardActivePolicyMatchReplyAddr OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..64))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The IPv6 prefix list to be matched for assigned IPv6 addressed by DHCPv6 servers.
        The empty string means this validation is disabled."
    ::= { rlDhcpGuardActivePolicyEntry 9 }


 rlDhcpGuardActivePolicyMatchReplyAddrType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "rlDhcpGuardActivePolicyMatchReplyAddr setting type."
    ::= { rlDhcpGuardActivePolicyEntry 10 }

 rlDhcpGuardActivePolicyPrefMin OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Minimum preference value limit.
           A value of -2 indicates validation is disabled."
    ::= { rlDhcpGuardActivePolicyEntry 11 }

 rlDhcpGuardActivePolicyPrefMinType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlDhcpGuardActivePolicyPrefMin setting type."
    ::= { rlDhcpGuardActivePolicyEntry 12 }

 rlDhcpGuardActivePolicyPrefMax OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "Maximum preference value limit.
           A value of -2 indicates validation is disabled."
    ::= { rlDhcpGuardActivePolicyEntry 13 }

 rlDhcpGuardActivePolicyPrefMaxType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlDhcpGuardActivePolicyPrefMax setting type."
    ::= { rlDhcpGuardActivePolicyEntry 14 }



 --------------------------------------------------------------
 -- The DHCPv6 Guard Global Configurations
 --------------------------------------------------------------

 rlDhcpGuardPrefMin OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Minimum preference value limit.
           A value of -2 indicates validation is disabled."
    DEFVAL  { -2 }
    ::= { rlDhcpGuard 8 }

 rlDhcpGuardPrefMax OBJECT-TYPE
    SYNTAX      Integer32 (-2 | 0..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
          "Maximum preference value limit.
           A value of -2 indicates validation is disabled."
    DEFVAL  { -2 }
    ::= { rlDhcpGuard 9 }

 --------------------------------------------------------------
 -- The DHCPv6 Guard Traps
 --------------------------------------------------------------
 rlDhcpGuardMessageDropTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Warning trap indicating that IPv6 DHCP Guard has dropped a message."
    ::=  { rndNotifications 236 }

 --------------------------------------------------------------
 -- The Source Guard
 --------------------------------------------------------------
 --------------------------------------------------------------
 -- The Source Guard Policy Configuration Table
 --------------------------------------------------------------

rlSourceGuardPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSourceGuardPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Source Guard
                 per policy configurations."
    ::= { rlSourceGuard 1 }

rlSourceGuardPolicyEntry OBJECT-TYPE
    SYNTAX  RlSourceGuardPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlSourceGuardPolicyName }
    ::= { rlSourceGuardPolicyTable 1 }

RlSourceGuardPolicyEntry ::= SEQUENCE {
    rlSourceGuardPolicyName                 DisplayString,
    rlSourceGuardPolicyTrusted              RlIpv6FhsSettingStatusType,
    rlSourceGuardPolicyRowStatus            RowStatus
    }

rlSourceGuardPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The Source Guard policy name."
    ::= { rlSourceGuardPolicyEntry 1 }

rlSourceGuardPolicyTrusted OBJECT-TYPE
    SYNTAX  RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Indicates whether policy defines trusted functionality"
    DEFVAL { unspecified }
    ::= { rlSourceGuardPolicyEntry 2 }

rlSourceGuardPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
    ::= { rlSourceGuardPolicyEntry 3 }


 --------------------------------------------------------------
 -- The Source Guard Policy Attachment Table - Port
 --------------------------------------------------------------

 rlSourceGuardPortPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSourceGuardPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Source Guard policy
                 attachment for ports."
    ::= { rlSourceGuard 2 }

 rlSourceGuardPortPolicyEntry OBJECT-TYPE
    SYNTAX  RlSourceGuardPortPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlSourceGuardPortPolicyIfIndex,
            IMPLIED rlSourceGuardPortPolicyName }
    ::= { rlSourceGuardPortPolicyTable 1 }

 RlSourceGuardPortPolicyEntry ::= SEQUENCE {
    rlSourceGuardPortPolicyIfIndex          InterfaceIndex,
    rlSourceGuardPortPolicyName             DisplayString,
    rlSourceGuardPortPolicyVlan1to1024      OCTET STRING,
    rlSourceGuardPortPolicyVlan1025to2048   OCTET STRING,
    rlSourceGuardPortPolicyVlan2049to3072   OCTET STRING,
    rlSourceGuardPortPolicyVlan3073to4094   OCTET STRING,
    rlSourceGuardPortPolicyRowStatus        RowStatus
    }

 rlSourceGuardPortPolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlSourceGuardPortPolicyEntry 1 }

 rlSourceGuardPortPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The Source guard policy name"
    ::= { rlSourceGuardPortPolicyEntry 2 }

 rlSourceGuardPortPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlSourceGuardPortPolicyEntry 3 }

 rlSourceGuardPortPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlSourceGuardPortPolicyEntry 4 }

 rlSourceGuardPortPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlSourceGuardPortPolicyEntry 5 }

 rlSourceGuardPortPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlSourceGuardPortPolicyEntry 6 }

 rlSourceGuardPortPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlSourceGuardPortPolicyEntry 7 }

 --------------------------------------------------------------
 -- The Source Guard Policy Attachment Table - Port (Read Only)
 --------------------------------------------------------------

 rlSourceGuardPolicyPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSourceGuardPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Source guard policy
                 attachment for ports."
    ::= { rlSourceGuard 3 }

 rlSourceGuardPolicyPortEntry OBJECT-TYPE
    SYNTAX  RlSourceGuardPolicyPortEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlSourceGuardPolicyPortName,
            rlSourceGuardPolicyPortIfIndex }
    ::= { rlSourceGuardPolicyPortTable 1 }

 RlSourceGuardPolicyPortEntry ::= SEQUENCE {
    rlSourceGuardPolicyPortName             DisplayString,
    rlSourceGuardPolicyPortIfIndex          InterfaceIndex,
    rlSourceGuardPolicyPortVlan1to1024      OCTET STRING,
    rlSourceGuardPolicyPortVlan1025to2048   OCTET STRING,
    rlSourceGuardPolicyPortVlan2049to3072   OCTET STRING,
    rlSourceGuardPolicyPortVlan3073to4094   OCTET STRING
    }

 rlSourceGuardPolicyPortName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The Source guard policy name"
    ::= { rlSourceGuardPolicyPortEntry 1 }

 rlSourceGuardPolicyPortIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlSourceGuardPolicyPortEntry 2 }

 rlSourceGuardPolicyPortVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1 to 1024."
    ::= { rlSourceGuardPolicyPortEntry 3 }

 rlSourceGuardPolicyPortVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 1025 to 2048."
    ::= { rlSourceGuardPolicyPortEntry 4 }

 rlSourceGuardPolicyPortVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 2049 to 3072."
    ::= { rlSourceGuardPolicyPortEntry 5 }

 rlSourceGuardPolicyPortVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A list of vlans from 3073 to 4094."
    ::= { rlSourceGuardPolicyPortEntry 6 }


 --------------------------------------------------------------
 -- The Source Guard Policy Attachment Table - Vlan
 --------------------------------------------------------------

 rlSourceGuardVlanPolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSourceGuardVlanPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Source Guard policy
                 attachment for vlans."
    ::= { rlSourceGuard 4 }

 rlSourceGuardVlanPolicyEntry OBJECT-TYPE
    SYNTAX  RlSourceGuardVlanPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlSourceGuardVlanPolicyVlanTag }
    ::= { rlSourceGuardVlanPolicyTable 1 }

 RlSourceGuardVlanPolicyEntry ::= SEQUENCE {
    rlSourceGuardVlanPolicyVlanTag            VlanId,
    rlSourceGuardVlanPolicyName               DisplayString,
    rlSourceGuardVlanPolicyRowStatus          RowStatus
 }

 rlSourceGuardVlanPolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlSourceGuardVlanPolicyEntry 1 }

 rlSourceGuardVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "The Source guard policy name"
    ::= { rlSourceGuardVlanPolicyEntry 2 }

 rlSourceGuardVlanPolicyRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlSourceGuardVlanPolicyEntry 3 }

 --------------------------------------------------------------
 -- The Source Guard Policy Table - Vlan
 --------------------------------------------------------------

 rlSourceGuardPolicyVlanTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSourceGuardPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Source Guard policy
                 attachment for vlans."
    ::= { rlSourceGuard 5 }

 rlSourceGuardPolicyVlanEntry OBJECT-TYPE
    SYNTAX  RlSourceGuardPolicyVlanEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { IMPLIED rlSourceGuardPolicyVlanPolicyName }
    ::= { rlSourceGuardPolicyVlanTable 1 }

 RlSourceGuardPolicyVlanEntry ::= SEQUENCE {
    rlSourceGuardPolicyVlanPolicyName    DisplayString,
    rlSourceGuardPolicyVlan1to1024       OCTET STRING,
    rlSourceGuardPolicyVlan1025to2048    OCTET STRING,
    rlSourceGuardPolicyVlan2049to3072    OCTET STRING,
    rlSourceGuardPolicyVlan3073to4094    OCTET STRING

 }

 rlSourceGuardPolicyVlanPolicyName OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION
        "The Source guard policy name"
    ::= { rlSourceGuardPolicyVlanEntry 1 }

 rlSourceGuardPolicyVlan1to1024 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1 to 1024."
    DEFVAL {'00'H}
    ::= { rlSourceGuardPolicyVlanEntry 2 }

 rlSourceGuardPolicyVlan1025to2048 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 1025 to 2048."
    DEFVAL {'00'H}
    ::= { rlSourceGuardPolicyVlanEntry 3 }

 rlSourceGuardPolicyVlan2049to3072 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 2049 to 3072."
    DEFVAL {'00'H}
    ::= { rlSourceGuardPolicyVlanEntry 4 }


 rlSourceGuardPolicyVlan3073to4094 OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "A list of vlans from 3073 to 4094."
    DEFVAL {'00'H}
    ::= { rlSourceGuardPolicyVlanEntry 5 }

 --------------------------------------------------------------
 -- The Source Guard Enable Table
 --------------------------------------------------------------

rlSourceGuardEnableVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlSourceGuardEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table contains only one entry of a static vlan list. The Source Guard enabled VLANs are set to 1s."
    ::= { rlSourceGuard 6 }

rlSourceGuardEnableVlanEntry OBJECT-TYPE
    SYNTAX      RlSourceGuardEnableVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Statically created by local or network management vlan list"
    INDEX   {rlSourceGuardEnableVlanIndex}
    ::= { rlSourceGuardEnableVlanTable 1 }

RlSourceGuardEnableVlanEntry ::=SEQUENCE {
    rlSourceGuardEnableVlanIndex         INTEGER,
    rlSourceGuardEnableVlan1to1024       OCTET STRING,
    rlSourceGuardEnableVlan1025to2048    OCTET STRING,
    rlSourceGuardEnableVlan2049to3072    OCTET STRING,
    rlSourceGuardEnableVlan3073to4094    OCTET STRING

}

rlSourceGuardEnableVlanIndex  OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
     "The table contains only one static entry."

   ::= { rlSourceGuardEnableVlanEntry 1 }

rlSourceGuardEnableVlan1to1024 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1 to 1024."
   DEFVAL {'00'H}
   ::= { rlSourceGuardEnableVlanEntry 2 }

rlSourceGuardEnableVlan1025to2048 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 1025 to 2048."
   DEFVAL {'00'H}
   ::= { rlSourceGuardEnableVlanEntry 3 }

rlSourceGuardEnableVlan2049to3072 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 2049 to 3072."
   DEFVAL {'00'H}
   ::= { rlSourceGuardEnableVlanEntry 4 }

rlSourceGuardEnableVlan3073to4094 OBJECT-TYPE
   SYNTAX      OCTET STRING(SIZE(0..128))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
     "A list of vlans from 3073 to 4094."
   DEFVAL {'00'H}
   ::= { rlSourceGuardEnableVlanEntry 5 }

 --------------------------------------------------------------
 -- The Source Guard Active Policy Table (Read Only)
 --------------------------------------------------------------

 rlSourceGuardActivePolicyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSourceGuardActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table specifies Source Guard Active Policy
                 per port and VLAN."
    ::= { rlSourceGuard 7 }

 rlSourceGuardActivePolicyEntry OBJECT-TYPE
    SYNTAX  RlSourceGuardActivePolicyEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "The row definition for this table."
    INDEX { rlSourceGuardActivePolicyIfIndex,
            rlSourceGuardActivePolicyVlanTag}
    ::= { rlSourceGuardActivePolicyTable 1 }

 RlSourceGuardActivePolicyEntry ::= SEQUENCE {
    rlSourceGuardActivePolicyIfIndex              InterfaceIndex,
    rlSourceGuardActivePolicyVlanTag              VlanId,
    rlSourceGuardActivePolicyNamePort             DisplayString,
    rlSourceGuardActivePolicyNameVlan             DisplayString,
    rlSourceGuardActivePolicyTrusted              RlIpv6FhsSettingStatusType,
    rlSourceGuardActivePolicyTrustedType          RlIpv6FhsSettingType
}

 rlSourceGuardActivePolicyIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The port's interface index."
    ::= { rlSourceGuardActivePolicyEntry 1 }

 rlSourceGuardActivePolicyVlanTag OBJECT-TYPE
    SYNTAX VlanId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { rlSourceGuardActivePolicyEntry 2 }

 rlSourceGuardActivePolicyNamePort OBJECT-TYPE
    SYNTAX DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The Source guard policy name attached to given interface."
    ::= { rlSourceGuardActivePolicyEntry 3 }

 rlSourceGuardActivePolicyNameVlan OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The Source Guard policy name attached to given vlan."
    ::= { rlSourceGuardActivePolicyEntry 4 }

 rlSourceGuardActivePolicyTrusted OBJECT-TYPE
    SYNTAX  RlIpv6FhsSettingStatusType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether policy defines trusted functionality"
    ::= { rlSourceGuardActivePolicyEntry 5 }

 rlSourceGuardActivePolicyTrustedType OBJECT-TYPE
    SYNTAX      RlIpv6FhsSettingType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
          "rlSourceGuardActivePolicyNamePort setting type."
    ::= { rlSourceGuardActivePolicyEntry 6 }

 --------------------------------------------------------------
 -- The Source Guard Traps
 --------------------------------------------------------------

 rlSrcGuardMessageDropTrap NOTIFICATION-TYPE
    OBJECTS   { rndErrorDesc, rndErrorSeverity }
    STATUS  current
    DESCRIPTION
        "Warning trap indicating that IPv6 Source Guard has dropped a message."
    ::=  { rndNotifications 237 }

END
