RADLAN-POLICY-MIB DEFINITIONS ::= BEGIN

-- Title:      RADLAN POLICY MIB
-- Version:    7.46
-- Date:       04 Jan 2007
--
-- 07-Oct-2003 Added to RlPolicyQosMode service
-- 07-Oct-2003 Added rlPolicyRulesDownloadMarker
-- 07-Oct-2003 Added rlPolicyDscpVptTable
-- 27-Jan-2005 Added cos-dscp to RlPolicyTrustTypes
-- 07-Feb-2005 Added rlPolicyFlowClassificationOffsetsGroupUseVPTId and
--                   rlPolicyFlowClassificationOffsetsGroupUseEtherTypeId To
--                   rlPolicyFlowClassificationOffsetsTable
--            Added rlPolicyClassifierVPTID And
--                  rlPolicyClassifierEtherTypeID To
--                  rlPolicyClassifierTable
--            Added Vpt and Ethertype support to rlPolicyClassifierAdditionalCriteriaSupported
-- 14-Mar-2005 Added  rlPolicyPortCfgPortRateLimitStatus,rlPolicyPortCfgCirPortRateLimit
--                      rlPolicyPortCfgCbsPortRateLimit to rlPolicyPortConfigurationTable
-- 14-Apr-2005 Added rlPolicyDefaultForwardingProtocol to rlPolicyDefaultForwardingTable
-- 17-Apr-2005 Added rlPolicyDscpToDpTable
-- 29-May-2005 Changed default value of rlPolicyClassifierEtherTypeID to 1501 (=minimum etherType value)
-- 08-Apr-2006 Added branch rlPolicyStatistics and following tables:
-- 20-May-2006 Added branch rlPolicyClassifierUtilization
-- 08-May-2006 Added rlPolicyFlowClassificationOffsetsGroupUseInnerVlanId To rlPolicyFlowClassificationOffsetsTable
--             Added rlPolicyClassifierInnerVID To rlPolicyClassifierTable
--            Added Inner vlan id support to rlPolicyClassifierAdditionalCriteriaSupported
-- 05-Jul-2006 Added rlPolicyVlanConfigurationTable
-- 18-Sep-2006 Added rlPolicyIsTCAvailable scalar
-- 04-Jan-2007 Added the new fields rlPolicyRulesTimeRange1 and rlPolicyRulesTimeRange2
--             Added subnote rlPolicyTimeBasedAcl
-- 23-Apr-2007 Added IPv6 ACL support
-- 09-Jul-2008 Change range of rlPolicyClassifierEtherTypeID to support virtual
--             IPv4 and IPv6 ethertypes (originated from IP/IPv6 ACL rule of
--             "permit/deny any any any" and not from ethertype field in MAC ACL)
-- 18-Jan-2008 Add rlPolicyClassifierUtilizationRulesNumber  to rlPolicyClassifierUtilizationEntry
-- 01-Jun-2009 Added the new fields rlPolicyRulesSrcPortRangeStart, rlPolicyRulesSrcPortRangeEnd,
--             rlPolicyRulesDestPortRangeStart, rlPolicyRulesDestPortRangeEnd
-- 18-Aug-2009 Removed Time Based Tables : code moved to general TimeBasedInfrastrucure
-- 19-Jan-2011 Removed 3rd party mentions

IMPORTS
    OBJECT-TYPE, IpAddress, Unsigned32,Counter32, zeroDotZero,
    MODULE-IDENTITY,Counter64                   FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue, RowStatus,
    RowPointer, DisplayString                   FROM SNMPv2-TC
    InterfaceIndexOrZero, InterfaceIndex        FROM IF-MIB
    diffServClassifierEntry                     FROM DIFF-SERV-MIB
    Percents, VlanPriority, rnd                 FROM RADLAN-MIB
    PortList, VlanId                            FROM Q-BRIDGE-MIB
    VlanList1, VlanList2, VlanList3, VlanList4  FROM RADLAN-BRIDGEMIBOBJECTS-MIB;


InterfaceType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "Interface type."
    SYNTAX  INTEGER {
        vlan(1),
        port(2)
}
StatisticsCntrNumOfBitsType  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "The counter can be of different sizes - 32 bit, 48 bit, 64 bit. Maximum is 64."
   SYNTAX INTEGER {
      uint32(32),
      uint48(48),
      uint64(64)


}

StatisticsDPType  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "Drop preceedence type."
   SYNTAX INTEGER {
      green(1),
      yellow(2),
      red(3)
}

StatisticsClearActionType  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "Clear action, value for clear scalar."
   SYNTAX INTEGER {
      noaction(1),
      action(2)
}

StatisticsCntrType  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "The counter can be of different types, depends on actions adhered to
                    rules that the counter is working on."
   SYNTAX INTEGER {
      statisticsCntrTypeSetDSCP(1),
      statisticsCntrTypeDeny(2)
}

 rlPolicy MODULE-IDENTITY
          LAST-UPDATED "200606260000Z"
          ORGANIZATION "Marvell Semiconductor, Inc."
          CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
          DESCRIPTION
                  "The private MIB module definition generic traffic policy in Radlan devices."
          REVISION "200503140000Z"
          DESCRIPTION
                  "Initial V2 version of this MIB."
          REVISION "200502070000Z"
          DESCRIPTION
                  "Added  rlPolicyPortCfgPortRateLimitStatus,rlPolicyPortCfgCirPortRateLimit
                   rlPolicyPortCfgCbsPortRateLimit to rlPolicyPortConfigurationTable"
          REVISION "200501270000Z"
          DESCRIPTION
                  "Added rlPolicyFlowClassificationOffsetsGroupUseVPTId and
                         rlPolicyFlowClassificationOffsetsGroupUseEtherTypeId To
                         rlPolicyFlowClassificationOffsetsTable
                   Added rlPolicyClassifierVPTID And
                         rlPolicyClassifierEtherTypeID To
                         rlPolicyClassifierTable
                   Added Vpt and Ethertype support to rlPolicyClassifierAdditionalCriteriaSupported
                   Added rlPolicyFlowClassificationOffsetsGroupUseInnerVlanId To
                         rlPolicyFlowClassificationOffsetsTable
                   Added rlPolicyClassifierInnerVID To
                         rlPolicyClassifierTable
                   Added Inner vlan id support to rlPolicyClassifierAdditionalCriteriaSupported"
          REVISION "200310070000Z"
          DESCRIPTION
                  "Added cos-dscp to RlPolicyTrustTypes."
          REVISION "200309220000Z"
          DESCRIPTION
                  "Add to RlPolicyQosMode service ,Add rlPolicyRulesDownloadMarker,Added rlPolicyDscpVptTable  ."
          REVISION "200504140000Z"
          DESCRIPTION
                  "Added rlPolicyDefaultForwardingProtocol to rlPolicyDefaultForwardingTable"
          REVISION "200504170000Z"
          DESCRIPTION
                  "Added rlPolicyDscpToDpTable"
          REVISION "200604080000Z"
          DESCRIPTION
                  "Added branch rlPolicyStatistics"
          REVISION "200605200000Z"
          DESCRIPTION
                  "Added branch rlPolicyClassifierUtilization"
          REVISION "200606260000Z"
          DESCRIPTION
                  "Added rlPolicyVlanConfigurationTable"
          ::= { rnd 59 }


RlPolicyGroupType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of 3 classifier types for which offset bytes can
         be specified. For Ip and Ipx, the offsets indicated are relative
         to the beginning of the L3 data (IP options field is skipped).  For
         the Bridged type, the offsets are relative to L2 (and any 802.1D tag
         is skipped).
         A value of notUsed is applied, if the classifier uses one set of
         offsets for bridge, IP and IPX"
    SYNTAX  INTEGER {
        bridged(1),
        routedIp(2),
        routedIpx(3),
        notUsed(4)
}

RlPolicyClassifierDiffservIfType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies port's type to which a classifier is applied. It is
         only used for the DiffServ mode. For the non-DiffServ mode
         the normal value may be used."
    SYNTAX  INTEGER {
        normal(1),
        allBoundaryPorts(2),
        allInteriorPorts(3)
}


RlPolicyTrustTypes ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Configure the port trust state
        cos     - Classifies ingress packets with the packet CoS values.
                  For untagged packets, the port default CoS is used.
        dscp    - Classifies ingress packets with the packet DSCP values.
                  For non-ip tagged packets, the packet CoS value is used
                  with the Cos-to-DSCP table .For non-IP untagged packets,
                  the default port CoS is used with the Cos-to-DSCP table
        tcp-udp - v750 deprecated.
                  port to dscp - Classifies ingress packets with the packet
                  destination port values. For non-ip tagged packets, the packet CoS
                  value is used with the Cos-to-DSCP table. For non-IP untagged packets,
                  the default port CoS is used with the Cos-to-DSCP table.
        none    - v750 deprecated.
                  802.1p is disabled for this port and the packet gets best effort queue.
        cos-dscp- Classifies ingress packets with the packet DSCP values.
                  For non-ip tagged packets, the packet CoS value is used
                  with the Cos-to-Queue table .For non-IP untagged packets,
                  the default port CoS is used with the Cos-to-Queue table
        "
    SYNTAX  INTEGER {
        cos(1),
        dscp(2),
--v750 deprecated        tcp-udp(3),
--v750 deprecatd - implemented by "disable mode" in globalQosMode        none(4),
        cos-dscp(3)

}

RlPolicyQosMode ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "The user can set the system to operate either in the Basic mode or in the Advanced mode.
          The setting of the mode applies to all ports in the system.
          configuring the system to work in the advanced mode,
          all setting for the basic mode are not in affect.
          For example, 802.1p is not available when operating in the advanced mode.
          When changing from basic mode to advanced mode and then back to basic mode,
          the user assignments in the basic mode are restored.
          Same for moving from advanced to basic and back again to advanced mode,
          here again the user assignments are kept.
          The different modes are mutually exclusive, i.e., only one can be
          active at a given time. For example, when configuring the system to work
          in the advanced mode, all setting for the basic mode are not in affect.
          This means that 802.1p is not available when operating in the advanced mode.
          When changing between modes (Basic, Advanced, Service, none), some of
          the user settings are reset to their default values. Specifically:
          1. When changing from the advanced mode to any other mode,
             the CCL definitions are lost.
          2. When changing from any mode to any other mode, the interface assignments:
             associated Policy map, trust mode of the Basic mode, shaper and scheduler
             settings are lost.
          3. When changing from service mode to any other mode, all service mode
             settings are lost.
          4. When changing to service mode, ACL are lost. The user is prompted if
             he wants to whether to import his active ACLs to the service mode.
          5. All other user configurations are kept.
          When the system is configured to the Basic mode and the user changes the
          trust mode, the CCL assignment per port and the shaper settings are reset
          to their default values."


    SYNTAX  INTEGER {
        disable(1),
        basic(2),
        advanced(3)
}


L4ProtType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
         "specify to Layer 4 protocol type for which the port number will refer
          at the rlPolicyTcpUdpPortDscpTable."

    SYNTAX  INTEGER {
        tcp(1),
        udp(2)
}



RlPolicyTimeBasedAclWeekPeriodicList  ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION  "Bitmap that includes days of week.
                 Each bit in the bitmap associated with corresponding day of the week."
    SYNTAX      BITS {
            monday(0),
            tuesday(1),
            wednesday(2),
            thursday(3),
            friday(4),
            saturday(5),
            sunday(6)
}

RlPolicyRulesActionDropType  ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION    "The Action Drop Type."
   SYNTAX INTEGER {
      hardDrop(1),
      softDrop(2)
}

RlPolicyMarkVlanAction  ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
    "Specifies the mark vlan action type in the class map table.
      1 - noMark - No vlan marking
      2 - mark  - mark vlan tagged.
      3 - markNestedVlan - add vlan tag to the packet. "
    SYNTAX  INTEGER {
        noMark(1),
        mark(2),
        markNestedVlan(3)
    }
RlPolicyRedirectAction  ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
    "Specifies the packet redirection options.
     Redirection is applied only on permitted packets.
      1 - disabled  - no redirect
      2 - trap - trap to local_host (CPU)
      3 - redirectToInterface - redirect to a output interface (port, trunk or vlan)
      4 - redirectToAllPorts - redirect to all ports, exept the ingress port.
      5 - mirror - forward the packet and sent a copy to local_host (CPU)
      6 - analyzerPort - forward the packet and sent a copy to egress port.
      7 - loopback - redirect the packet the the port it was recieved.
      8 - redirectToPortGroup - send to group of ports, defined in rlUserAssignedVidxTable table.
      9 - mirror_and_redirectToInterface - send the packet to interface and send a copy to local_host(CPU)
      10 -mirror_and_redirectToInterfacesGroup - send the packet to group of ports and send a copy to local_host(CPU)  "
    SYNTAX  INTEGER {
        disabled(1),
        trap(2),
        redirectToInterface(3),
        redirectToAllPorts(4),
        mirror(5),
        analyzerPort(6),
        loopback(7),
        redirectToPortGroup(8),
        mirrorAndRedirectToInterface(9),
        mirrorAndRedirectToInterfacesGroup(10)
    }

rlPolicyMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "MIB's version, the current version is 14
         1 - original version
         2 - two new fields
                rlPolicyActionChangeDscpNonConform
                rlPolicyActionNewDscpNonConform
             were added.
         3 - added support new policy features
                QoS modes: basic and advanced
                support for trusted mode  operations
                mapping tables for trusted ports
                dscp, tcpUdp, mutation, remarking.
         4 - I) added support to service mode.
             II)DSCP to VPT mapping table
             III) download marker
         5 - Added cos-Dscp to RlPolicyTrustTypes
         6 - Added rlPolicyFlowClassificationOffsetsGroupUseVPTId and
                   rlPolicyFlowClassificationOffsetsGroupUseEtherTypeId To
                   rlPolicyFlowClassificationOffsetsTable
             Added rlPolicyClassifierVPTID And
                   rlPolicyClassifierEtherTypeID To
                   rlPolicyClassifierTable
             Added Vpt and Ethertype support to rlPolicyClassifierAdditionalCriteriaSupported
         7 - Added  rlPolicyPortCfgPortRateLimitStatus,rlPolicyPortCfgCirPortRateLimit
                    rlPolicyPortCfgCbsPortRateLimit to rlPolicyPortConfigurationTable
         8 - Added  rlPolicyDefaultForwardingProtocol to rlPolicyDefaultForwardingTable
             Added rlPolicyDscpToDpTable
         9 - Add statistics
         10 - Add classifier utilization
         11 -Added rlPolicyFlowClassificationOffsetsGroupUseInnerVlanId To
                 rlPolicyFlowClassificationOffsetsTable
             Added rlPolicyClassifierInnerVID To
                 rlPolicyClassifierTable
             Added Inner vlan id support to rlPolicyClassifierAdditionalCriteriaSupported
         12 - Added rlPolicyVlanConfigurationTable
         13 - Added rlPolicyIsTCAvailable scalar
         14 - Added rlPolicyCPUSafeGuardEnable"
    ::= { rlPolicy 1 }

-- Groups:
--      rlPolicyClassifier
--      rlPolicyRules
--      rlPolicyMeterClass
--      rlPolicyAction
--      rlPolicyServiceClass
--      rlPolicyDiffServ
--      rlPolicyMapping
--      rlPolicyGlobalParams
--      rlPolicyMapping
--      rlPolicyDefaultForwardingTable
--      rlPolicyStatistics
--      rlPolicyClassifierUtilization
--------------
-- Classifier
--
rlPolicyClassifier OBJECT IDENTIFIER ::= { rlPolicy 2 }

--
-- Platform parameters variables
--
rlPolicyClassifierPlatDependParams OBJECT IDENTIFIER ::= { rlPolicyClassifier 1 }

rlPolicyFlowClassificationOffsetsGroupScheme OBJECT-TYPE
    SYNTAX INTEGER {
        allOffsetsPermitted(1),
        singleFlowClassificationOffsetGroupsForIpIpxBridge(2)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Some platforms allow Policy statements to examine all packet
         offsets(Opal); other platforms require specification of specific
         byte offsets for routedIp packets, another set of offsets for
         routedIpx, a third set for bridge."
    ::= { rlPolicyClassifierPlatDependParams 1 }

rlPolicyNumberOfOffsetsPerFlowClassificationOffsetGroup OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS obsolete
    DESCRIPTION
        "For platforms which require an FCOG, indicates the maximum
         number of byte offsets specifiable for each offset group."
    ::= { rlPolicyClassifierPlatDependParams 2 }

rlPolicyFlowClassificationOffsetGroupMaximumOffset OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the maximum value of a byte offset in a
         Flow Classification Offset Group. If 0, there is no limit."
    ::= { rlPolicyClassifierPlatDependParams 3 }

rlPolicyNumberOfOffsetsPerOmpcGroup OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "indicates the maximum number of byte offsets
         specifiable for each Ompc offset group."
    ::= { rlPolicyClassifierPlatDependParams 4 }

rlPolicyOmpcMaximumOffset OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the maximum value of a byte offset in a
         Ompc Group. If 0, there is no limit."
    ::= { rlPolicyClassifierPlatDependParams 5 }

rlPolicyOMPCPermittedOperators OBJECT-TYPE
    SYNTAX OCTET STRING (SIZE(1))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "A bit mask indicating which operators are permissable in an OMPC:
          ----------
          |87654321|
          ----------
          1 - equal operator permitted
          2 - not-equal operator permitted
          3 - greater-than operator permitted
          4 - less-than operator permitted"
    ::= { rlPolicyClassifierPlatDependParams 6 }

rlPolicyMaxOMPCLengthForBiggerSmallerOperation OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the maximal permissible length of an OMPC using
         bigger' or 'smaller' condition. If 0, there is no limit."
    ::= { rlPolicyClassifierPlatDependParams 7 }

rlPolicyClassifierAdditionalCriteriaSupported OBJECT-TYPE
    SYNTAX OCTET STRING (SIZE(1))
    MAX-ACCESS read-only
    STATUS obsolete
    DESCRIPTION
      "A bit mask indicating which additional Criteria may be supported
       by the classifier:
          ----------
          |87654321|
          ----------
          1 - input port supported
          2 - output port supported
          3 - VLAN ID for bridging supported
          4 - VPT ID for bridging supported
          5 - EtherType ID for bridging supported
          6 - Inner VLAN ID for bridging supported"
    ::= { rlPolicyClassifierPlatDependParams 8 }

rlPolicyClassifierAdditionalCriteriaUsedInOffsetCount OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  obsolete
    DESCRIPTION
        "Indicates whether the additional FCOG or Classifier criteria
         (ie. inPort, outPort VID count towards the maximum number of offsets
         ie. whether using inPort in the FCOG reduces the maximum number of
         offsets available."
    ::= { rlPolicyClassifierPlatDependParams 9 }

rlPolicyClassifierPermittedOffsetTypes OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  obsolete
    DESCRIPTION
        "A bit mask indicating which offset types are supported by the
         platform for FCOG and OMPC definitions:
            ----------
            |87654321|
            ----------
            1 - L2 offsets supported
            2 - L3 offsets supported"
    ::= { rlPolicyClassifierPlatDependParams 10 }

rlPolicyClassifierOMPCActions OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A bit mask indicating which operation could be performed with OPMC
            ----------
            |87654321|
            ----------
            1 - equal,
            2 - notEqual,
            3 - bigger,
            4 - smaller."
    ::= { rlPolicyClassifierPlatDependParams 11 }

--
--Flow Classification Offsets Table
--
rlPolicyFlowClassificationOffsetsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyFlowClassificationOffsetsGroupEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Specifies the byte offsets that the platform can use for
         policy decisions.  This table is used for platforms
         which impose limitations on choosing the OMPCs for classification.
         If the platform does not impose any limitations, the value of
         rlPolicyFlowClassificationOffsetsGroupScheme is allOffsetsPermitted.
         Each entry in the table specifies a combination of byte offsets
         which can be used to specify flow classification.  A rule may
         use a subset of the bytes of its Offset Group.
         The maximum value for each offset is given by
         rlPolicyFlowClassificationOffsetGroupMaximumOffset.
         The maximum number of offsets per Offset Group is given by
         rlPolicyNumberOfOffsetsPerFlowClassificationOffsetGroup."
    ::= { rlPolicyClassifier 2 }

rlPolicyFlowClassificationOffsetsGroupEntry OBJECT-TYPE
    SYNTAX RlPolicyFlowClassificationOffsetsGroupEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The flow classification offset table entry includes the
         following parameters"
    INDEX { rlPolicyFlowClassificationOffsetsGroupType }
    ::= { rlPolicyFlowClassificationOffsetsTable 1 }

RlPolicyFlowClassificationOffsetsGroupEntry ::= SEQUENCE {
    rlPolicyFlowClassificationOffsetsGroupType                  RlPolicyGroupType,
    rlPolicyFlowClassificationOffsetsGroupOffset                OBJECT IDENTIFIER,
    rlPolicyFlowClassificationOffsetsGroupOffsetType            OBJECT IDENTIFIER,
    rlPolicyFlowClassificationOffsetsGroupMask                  OCTET STRING,
    rlPolicyFlowClassificationOffsetsGroupUseInputInterface     TruthValue,
    rlPolicyFlowClassificationOffsetsGroupUseOutputInterface    TruthValue,
    rlPolicyFlowClassificationOffsetsGroupUseVlanId             TruthValue,
    rlPolicyFlowClassificationOffsetsGroupStatus                RowStatus,
    rlPolicyFlowClassificationOffsetsGroupUseVPTId              TruthValue,
    rlPolicyFlowClassificationOffsetsGroupUseEtherTypeId        TruthValue,
    rlPolicyFlowClassificationOffsetsGroupUseInnerVlanId        TruthValue
}

rlPolicyFlowClassificationOffsetsGroupType OBJECT-TYPE
    SYNTAX RlPolicyGroupType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Specifies a classifier type for which offset bytes can be specified."
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 1 }

rlPolicyFlowClassificationOffsetsGroupOffset OBJECT-TYPE
    SYNTAX  OBJECT IDENTIFIER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The list of offsets to be included in the Flow Classification Offset
         Group are specified as subidentifiers in the OID(after the first 2
         bytes which must be 1.1). The maximal number of permissible offsets
         is given by rlPolicyNumberOfOffsetsPerFlowClassificationOffsetGroup.
         The maximal value that an offset can have is
         rlPolicyFlowClassificationOffsetGroupMaximumOffset."
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 2 }

rlPolicyFlowClassificationOffsetsGroupOffsetType OBJECT-TYPE
    SYNTAX  OBJECT IDENTIFIER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates whether the corresponding byte denotes an offset from beginning
         of L2, from the beginning of L3 IPv4 packet data or from the beginning
         of L3 IPv6 packet data.
         Each byte in the OID contains either:
            (1) - L2 offset
            (2) - L3 Offset
            (3) - L3 IPv6 Offset"
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 3 }

rlPolicyFlowClassificationOffsetsGroupMask OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The list of masks corresponding to the offsets to be included in the
         Flow Classification Offset Group are specified as bytes in the
         OID(after the first 2 bytes which must be 1.1)."
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 4 }

rlPolicyFlowClassificationOffsetsGroupUseInputInterface OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates whether or not the Input Interface Index is usable
         in Policy Rule definitions."
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 5 }

rlPolicyFlowClassificationOffsetsGroupUseOutputInterface OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates whether or not the Output Interface Index(ie.
         routing/bridging decision) is usable in Policy Rule definitions"
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 6 }

rlPolicyFlowClassificationOffsetsGroupUseVlanId OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates whether or not the VlanId is usable in Policy Rule
         definitions for bridged packets"
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 7 }

rlPolicyFlowClassificationOffsetsGroupStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of a table entry.
         It is used to delete an entry from this table."
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 8 }

rlPolicyFlowClassificationOffsetsGroupUseVPTId OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates whether or not the VPT is usable in Policy Rule
         definitions for bridged packets"
    DEFVAL{ false }
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 9 }

rlPolicyFlowClassificationOffsetsGroupUseEtherTypeId OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates whether or not the EtherType is usable in Policy Rule
         definitions for bridged packets"
    DEFVAL{ false }
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 10 }

rlPolicyFlowClassificationOffsetsGroupUseInnerVlanId OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates whether or not the inner VlanId is usable in Policy Rule
         definitions for bridged packets"
    DEFVAL{ false }
    ::= { rlPolicyFlowClassificationOffsetsGroupEntry 11 }


--
--  Ompc Table
--
rlPolicyOMPCTable OBJECT-TYPE
  SYNTAX  SEQUENCE OF RlPolicyOMPCEntry
  MAX-ACCESS  not-accessible
  STATUS  current
  DESCRIPTION
         "The table of OMPC statements."
  ::= { rlPolicyClassifier 3 }

rlPolicyOMPCEntry OBJECT-TYPE
    SYNTAX  RlPolicyOMPCEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Each classification statement consists of the following parameters"
    INDEX  { rlPolicyOMPCGroupType, rlPolicyOMPCIndex }
    ::= { rlPolicyOMPCTable 1 }

RlPolicyOMPCEntry ::= SEQUENCE {
    rlPolicyOMPCGroupType       RlPolicyGroupType,
    rlPolicyOMPCIndex           INTEGER,
    rlPolicyOMPCOffset          INTEGER,
    rlPolicyOMPCOffsetType      INTEGER,
    rlPolicyOMPCMask            OCTET STRING,
    rlPolicyOMPCPattern         OCTET STRING,
    rlPolicyOMPCCondition       INTEGER,
    rlPolicyOMPCDescription     DisplayString,
    rlPolicyOMPCStatus          RowStatus
}

rlPolicyOMPCGroupType OBJECT-TYPE
    SYNTAX RlPolicyGroupType
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies a classifier type for which offset bytes can be specified."
    ::= { rlPolicyOMPCEntry 1 }

rlPolicyOMPCIndex OBJECT-TYPE
    SYNTAX  INTEGER(1..2147483647)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Index into the OMPC  Table. "
    ::= { rlPolicyOMPCEntry 2 }

rlPolicyOMPCOffset OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies the offset within the frame (in bytes) from the layer
         according to rlPolicyGroupType. The limitation of this field is
         according to the rlPolicyFlowClassificationOffsetGroupMaximumOffset
         parameter if this OMPC is used by an entry in the
         rlPolicyClassifierTable whose rlPolicyClassifierType is a protocol
         for which predefined offsets in rlPolicyFlowClassificationOffsetsTable
         are required.
         rlPolicyRequiredOffsetGroups indicates for which protocols there is
         such a requirement."
    ::= { rlPolicyOMPCEntry 3 }

rlPolicyOMPCOffsetType OBJECT-TYPE
    SYNTAX INTEGER {
        l2(1),
        l3(2),
        l3-ipv6(3)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates whether the offset should be interpreted as relative to the
         beginning of L2 or the beginning of L3"
    ::= { rlPolicyOMPCEntry 4 }

rlPolicyOMPCMask OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies which bits  of the rlPolicyOMPCPattern field are
         significant for packet comparison. The length of the mask,
         in case of 'bigger' or 'smaller' rlPolicyOMPCCondition,
         is limited by rlPolicyMaxOMPCLengthForBiggerSmallerOperation."
    ::= { rlPolicyOMPCEntry 5 }

rlPolicyOMPCPattern OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Describes the mask field. The length of this object must be equal
        to the length of rlPolicyOMPCMask."
    ::= { rlPolicyOMPCEntry 6 }

rlPolicyOMPCCondition OBJECT-TYPE
    SYNTAX INTEGER {
       equal(1),
       notEqual(2),
       bigger(3),
       smaller(4)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "These define the operation carried out on the two 'operands'
        (frame and pattern), i.e. Bigger means that frame bits should be
        bigger than pattern bits. The permitted values are according to
        rlPolicyOMPCPermittedOperators parameter, if this OMPC is used by
        an entry in the rlPolicyClassifierTable whose rlPolicyClassifierType
        is a protocol for which predefined offsets in
        rlPolicyFlowClassificationOffsetsTable are required.
        rlPolicyRequiredOffsetGroups indicates for which protocols there is
        such a requirement."
    DEFVAL{ equal }
    ::= { rlPolicyOMPCEntry 7 }

rlPolicyOMPCDescription OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..20))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
      "Free text specifing the nature of this OMPC."
    ::= { rlPolicyOMPCEntry 8 }

rlPolicyOMPCStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete an entry from this table."
    ::= { rlPolicyOMPCEntry 9 }

--
--  Classifier Table
--
rlPolicyClassifierTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlPolicyClassifierEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of Classifier statement."
    ::= { rlPolicyClassifier 4 }

rlPolicyClassifierEntry OBJECT-TYPE
    SYNTAX  RlPolicyClassifierEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Classifiers can be of the ingress, egress, or post-routing phase
         varieties.
         Each multifield classification statement consists of the
         following parameters."
    INDEX  { rlPolicyClassifierType, rlPolicyClassifierListIndex, rlPolicyClassifierSubListIndex, rlPolicyClassifierIndex }
    ::= { rlPolicyClassifierTable 1 }

RlPolicyClassifierEntry ::= SEQUENCE {
    rlPolicyClassifierType              RlPolicyGroupType,
    rlPolicyClassifierListIndex         INTEGER,
    rlPolicyClassifierSubListIndex      INTEGER,
    rlPolicyClassifierIndex             INTEGER,
    rlPolicyClassifierOmpcList          OBJECT IDENTIFIER,
    rlPolicyClassifierInIfIndex         InterfaceIndexOrZero,
    rlPolicyClassifierOutIfIndex        InterfaceIndexOrZero,
    rlPolicyClassifierVID               INTEGER,
    rlPolicyClassifierDiffservInIfType  RlPolicyClassifierDiffservIfType,
    rlPolicyClassifierDiffservOutIfType RlPolicyClassifierDiffservIfType,
    rlPolicyClassifierStatus            RowStatus,
    rlPolicyClassifierInIfIndexList     PortList,
    rlPolicyClassifierOutIfIndexList    PortList,
    rlPolicyClassifierVPTID             INTEGER,
    rlPolicyClassifierVPTIDMask         INTEGER,
    rlPolicyClassifierEtherTypeID       INTEGER,
    rlPolicyClassifierInnerVID          INTEGER
}

rlPolicyClassifierType OBJECT-TYPE
    SYNTAX  RlPolicyGroupType
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies a classifier type for which offset bytes can be specified."
    ::= { rlPolicyClassifierEntry 1 }

rlPolicyClassifierListIndex OBJECT-TYPE
    SYNTAX  INTEGER(1..2147483647)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
      "List Index into the Classifier Table."
    ::= { rlPolicyClassifierEntry 2 }

rlPolicyClassifierSubListIndex OBJECT-TYPE
    SYNTAX  INTEGER(1..2147483647)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
      "SubList Index into the Classifier Table."
    ::= { rlPolicyClassifierEntry 3 }

rlPolicyClassifierIndex OBJECT-TYPE
    SYNTAX  INTEGER(1..2147483647)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
      "Index into the Classifier Table."
    ::= { rlPolicyClassifierEntry 4 }

rlPolicyClassifierOmpcList OBJECT-TYPE
    SYNTAX  OBJECT IDENTIFIER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The list of OMPCs to check with this Classifier. Each
         subidentifier together with rlPolicyClassifierType specify one OMPC."
    ::= { rlPolicyClassifierEntry 5 }

rlPolicyClassifierInIfIndex OBJECT-TYPE
    SYNTAX  InterfaceIndexOrZero
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Input interface index to be compared with received packet,
         a value of 0 denotes that the classifier is applied to all ports."
    DEFVAL{ 0 }
    ::= { rlPolicyClassifierEntry 6 }

rlPolicyClassifierOutIfIndex OBJECT-TYPE
    SYNTAX  InterfaceIndexOrZero
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Output interface index to be compared with sent packet,
         a value of 0 denotes that the classifier is applied to all ports."
    DEFVAL { 0 }
    ::= { rlPolicyClassifierEntry 7 }

rlPolicyClassifierVID OBJECT-TYPE
    SYNTAX  INTEGER (0..4095)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
      "VLAN ID, used only for bridged traffic. "
    DEFVAL{ 0 }
    ::= { rlPolicyClassifierEntry 8 }

rlPolicyClassifierDiffservInIfType OBJECT-TYPE
    SYNTAX  RlPolicyClassifierDiffservIfType
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "For a classifier used by the Diffserv Rules table.  Enables
         specification of a classifier that should apply to all
         Diffserv boundary ports or all Diffserv Interior ports.
         If normal is specified, the rlPolicyClassifierInIfIndex field
         is used as it is in the non-diffserv case.  If allBoundary or
         allInterior is selected, rlPolicyClassifierInIfIndex is ignored"
        DEFVAL { normal }
    ::= { rlPolicyClassifierEntry 9 }

rlPolicyClassifierDiffservOutIfType OBJECT-TYPE
    SYNTAX  RlPolicyClassifierDiffservIfType
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "For a classifier used by the Diffserv Rules table.  Enables
         specification of a classifier that should apply to outbound
         traffic on all Diffserv boundary ports or all Diffserv Interior
         ports.
         If normal is specified, the rlPolicyClassifierOutIfIndex field
         is used as it is in the non-diffserv case.  If allBoundary or
         allInterior is selected, rlPolicyClassifierOutIfIndex is ignored"
    DEFVAL { normal }
    ::= { rlPolicyClassifierEntry 10 }

rlPolicyClassifierStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of a table entry.
         It is used to delete an entry from this table."
    ::= { rlPolicyClassifierEntry 11 }


rlPolicyClassifierInIfIndexList OBJECT-TYPE
    SYNTAX  PortList
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "allow to define list of ports for the specific classifier
         for ingress classification. if rlPolicyClassifierInIfIndex equal to zero
         then the following list should be reffered , if the list is empty we refer
         to ALL Ports"
    ::= { rlPolicyClassifierEntry 12 }

rlPolicyClassifierOutIfIndexList OBJECT-TYPE
    SYNTAX  PortList
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "allow to define list of ports for the specific classifier
         for egress classification. if rlPolicyClassifierOutIfIndex equal to zero
         then the following list should be reffered , if the list is empty we refer
         to ALL Ports"
    ::= { rlPolicyClassifierEntry 13 }


    rlPolicyClassifierVPTID OBJECT-TYPE
    SYNTAX  INTEGER (0..8)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
      "VPT ID - user priority tag to be compared with .
      8 is used to indicate not used value for this classifier"
    DEFVAL{ 8 }
    ::= { rlPolicyClassifierEntry 14 }


    rlPolicyClassifierVPTIDMask OBJECT-TYPE
    SYNTAX  INTEGER (0..7)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
      "VPT ID Mask ,mask the user priority field .
      0 is the default indicate Mask all compared with any VPT value"
    DEFVAL{ 0 }
    ::= { rlPolicyClassifierEntry 15 }

    rlPolicyClassifierEtherTypeID OBJECT-TYPE
    SYNTAX  INTEGER (1499..65536)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
      "EtherType ID, to be compared with.
      65535 is used to indicate not used value for this classifier
      1499 is uded to indicate IPv4 ethertype that is originated from IPv4 ACL with permit/deny any any any
      1500 is uded to indicate IPv6 ethertype that is originated from IPv6 ACL with permit/deny any any any"
    DEFVAL{ 65536 }
    ::= { rlPolicyClassifierEntry 16}

rlPolicyClassifierInnerVID OBJECT-TYPE
    SYNTAX  INTEGER (0..4095)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
      "INNER VLAN ID, used only for double tagged traffic. "
    DEFVAL{ 0 }
    ::= { rlPolicyClassifierEntry 17 }
----------------------------
--  Rules Class
--
rlPolicyRules OBJECT IDENTIFIER ::= { rlPolicy 3 }

rlPolicyRulesPlatDependParams OBJECT IDENTIFIER ::= { rlPolicyRules 1 }

rlPolicyDroppedPacketCountSupported OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates whether the dropped packets counter in the
         rlPolicyRulesTable is supported."
    ::= { rlPolicyRulesPlatDependParams 1 }

rlPolicyFilterActionOptions OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A bit mask indicating which operation could be perform
            ----------
            |87654321|
            ----------
            1 - block,
            2 - blockAndTrap,
            3 - permitAndTrap,
            4 - permit."
    ::= { rlPolicyRulesPlatDependParams 2 }

rlPolicyIngressMeteringSupported OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies whether the platform supports metering in inbound packet
         rules."
    ::= { rlPolicyRulesPlatDependParams 3 }

rlPolicyEgressMeteringSupported OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies whether the platform supports metering on outbound packet
         rules (for Diffserv)."
    ::= { rlPolicyRulesPlatDependParams 4 }

--------------
-- Rules Table
--
rlPolicyRulesTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlPolicyRulesEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of rules and Rules statements applied to all incoming traffic
         at the post-routing phase - ie. both the inPort and outPort are
         available for classification
         When Diffserv is not in effect(ie. IPX, bridging, or IP when the global option
         for Diffserv is off), certain table parameters are not available(see
         below). The DiffServ option is enabled or disabled by setting
         rlDiffservModeEnabled."
    ::= { rlPolicyRules 2 }

rlPolicyRulesEntry OBJECT-TYPE
    SYNTAX  RlPolicyRulesEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Each multifield classification statement consists of the following
         parameters."
    INDEX  { rlPolicyRulesTableType,
             rlPolicyRulesInterfaceDirection,
             rlPolicyRulesListIndex,
             rlPolicyRulesSubListIndex,
             rlPolicyRulesIndex }
    ::= { rlPolicyRulesTable 1 }

RlPolicyRulesEntry ::= SEQUENCE  {
    rlPolicyRulesTableType              RlPolicyGroupType,
    rlPolicyRulesInterfaceDirection     INTEGER,
    rlPolicyRulesListIndex              INTEGER,
    rlPolicyRulesSubListIndex           INTEGER,
    rlPolicyRulesIndex                  INTEGER,
    rlPolicyRulesFilteringAction        INTEGER,
    rlPolicyRulesDroppedPackets         Counter32,
    rlPolicyRulesFurtherRefPointer      INTEGER,
    rlPolicyRulesDescription            DisplayString,
    rlPolicyRulesStatus                 RowStatus,
    rlPolicyRulesCounterIdx             INTEGER,
    rlPolicyRulesCounter                Counter32,
    rlPolicyRulesActionPointer          INTEGER,
    rlPolicyRulesTimeRange1             INTEGER,
    rlPolicyRulesTimeRange2             INTEGER,
    rlPolicyRulesSrcPortRangeStart      INTEGER,
    rlPolicyRulesSrcPortRangeEnd        INTEGER,
    rlPolicyRulesDestPortRangeStart     INTEGER,
    rlPolicyRulesDestPortRangeEnd       INTEGER,
    rlPolicyRulesActionDropType         RlPolicyRulesActionDropType


}

rlPolicyRulesTableType OBJECT-TYPE
    SYNTAX  RlPolicyGroupType
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies a classifier type for which offset bytes can be specified."
    ::= { rlPolicyRulesEntry 1 }

rlPolicyRulesInterfaceDirection OBJECT-TYPE
    SYNTAX  INTEGER {
        inbound(1),     -- ingress interface / ingress metering support
        outbound(2),    -- egress interface / egress metering support
        none(3)         -- no Metering support
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies the direction for this entry on the
         interface. 'inbound' traffic is operated on during
         receipt, while 'outbound' traffic is operated on prior
         to transmission.
         Based on the metering support:
         inbound available while the ingress metering supported,
         outbound available while egress metering supported,
         and none while no metering supported."
    ::= { rlPolicyRulesEntry 2 }

rlPolicyRulesListIndex OBJECT-TYPE
    SYNTAX   INTEGER (1..2147483647)
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "Enumerates the rule list entry."
    ::= { rlPolicyRulesEntry 3 }

rlPolicyRulesSubListIndex OBJECT-TYPE
    SYNTAX   INTEGER (1..2147483647)
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "Enumerates the rule sub-list entry."
    ::= { rlPolicyRulesEntry 4 }

rlPolicyRulesIndex OBJECT-TYPE
    SYNTAX   INTEGER (1..2147483647)
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "Enumerates the rule index entry."
    ::= { rlPolicyRulesEntry 5 }


rlPolicyRulesFilteringAction OBJECT-TYPE
    SYNTAX  INTEGER  {
        block(1),
        blockAndTrap(2),
        permitAndTrap(3),
        permit(4),
        blockAndDisablePort(5),
        blockTrapAndDisablePort(6),
        blockAndLogInput(7),
        permitAndLogInput(8)
  }
    MAX-ACCESS   read-write
    STATUS   current
    DESCRIPTION
        "Specifies the action for the filter.
         Values 1-10 reserved for the System filtering implemetation;
         Values starting from 11 may be used for user definition about
         future application."
    DEFVAL { permit }
    ::= { rlPolicyRulesEntry 6}

rlPolicyRulesDroppedPackets OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of packets blocked by this filtering rule."
    ::= { rlPolicyRulesEntry 7 }

rlPolicyRulesFurtherRefPointer OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "This further reference indicate on the entry at the metering or
                 action table, based on the supported features. The
                 rlPolicyRulesFurtherRefPointer points on the metering table if the
                 metering feature is supported, if not this fields points on the
                 Action table"
    ::= { rlPolicyRulesEntry 8 }

rlPolicyRulesDescription OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..20))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
      "Free text specifing the nature of this Rule."
    ::= { rlPolicyRulesEntry 9 }

rlPolicyRulesStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Row status of the Rules entry."
    ::= { rlPolicyRulesEntry 10 }

rlPolicyRulesCounterIdx OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If not zero, perform counting of matched packets ."
    DEFVAL { 0 }
    ::= { rlPolicyRulesEntry 11 }

rlPolicyRulesCounter OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of packets that matched this filtering rule."
    ::= { rlPolicyRulesEntry 12 }

rlPolicyRulesActionPointer  OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "This further reference indicate on the entry at the
             action table, The rlPolicyRulesActionPointer points on the action
             table if the aggregate metering feature is supported,or
             if meter is not belong to data path. "
    ::= { rlPolicyRulesEntry 13 }


rlPolicyRulesTimeRange1 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "Time range of the first ACL. "
    DEFVAL { 0 }
    ::= { rlPolicyRulesEntry 14 }

rlPolicyRulesTimeRange2 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "Time range of the second ACL. "
    DEFVAL { 0 }
    ::= { rlPolicyRulesEntry 15 }

rlPolicyRulesSrcPortRangeStart OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "Start port of port range for source port. "
    DEFVAL { 0 }
    ::= { rlPolicyRulesEntry 16 }

rlPolicyRulesSrcPortRangeEnd OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "End port of port range for source port. "
    DEFVAL { 0 }
    ::= { rlPolicyRulesEntry 17 }

rlPolicyRulesDestPortRangeStart OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "Start port of port range for destination port. "
    DEFVAL { 0 }
    ::= { rlPolicyRulesEntry 18 }

rlPolicyRulesDestPortRangeEnd OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "End port of port range for destination port. "
    DEFVAL { 0 }
    ::= { rlPolicyRulesEntry 19 }

rlPolicyRulesActionDropType OBJECT-TYPE
    SYNTAX RlPolicyRulesActionDropType
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This field is valid only if rlPolicyRulesFilteringAction is
        not permit. Used to distinguish between Hard and Soft drop."
    DEFVAL { hardDrop }
    ::= { rlPolicyRulesEntry 20 }



------------------------
-- Rules download marker
--
rlPolicyRulesDownloadMarker OBJECT-TYPE
    SYNTAX  INTEGER {
        start(1),
        finish(2),
        finishCombined(3),
        undo(4),
        deleteStart(5),
        deleteFinish(6)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates when rules download or removing starts and terminates."
    ::= { rlPolicyRules 3 }



------------------
--  Metering Class
--
rlPolicyMeterClass OBJECT IDENTIFIER ::= { rlPolicy 4 }

rlPolicyMeterPlatDependParams OBJECT IDENTIFIER ::= { rlPolicyMeterClass 1 }

rlPolicyMeterDepth OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates how many meters can be chained in succession (ie. so
         that if the first meter fails, the second can be examined).
         The final meter in a sequence is always 'always-conform', so if
         the value of this parameter is 2, the platform that supports a
         single meter and then a second marking/action for meter failure."
    ::= { rlPolicyMeterPlatDependParams 1 }

------------
--  Metering Class Table
--
rlPolicyMeterClassTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlPolicyMeteringClassEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This table defines the Metering classes for the system."
    ::= { rlPolicyMeterClass 2 }

rlPolicyMeteringClassEntry OBJECT-TYPE
    SYNTAX  RlPolicyMeteringClassEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Each statement consists of the following parameters"
    INDEX  { rlPolicyMeteringClassIndex }
    ::= { rlPolicyMeterClassTable 1 }

RlPolicyMeteringClassEntry ::= SEQUENCE  {
    rlPolicyMeteringClassIndex                      INTEGER,
    rlPolicyMeteringClassAlwaysConform              TruthValue,
    rlPolicyMeteringClassAggregateMeterRate         INTEGER,
    rlPolicyMeteringClassAggregateMeterBurstSize    INTEGER,
    rlPolicyMeteringClassPerSessionMeteringRate     INTEGER,
    rlPolicyMeteringClassMaxSessionLimit            INTEGER,
    rlPolicyMeteringClassActionPointer              INTEGER,
    rlPolicyMeteringClassFailMeterPointer           INTEGER,
    rlPolicyMeteringClassStatus                     RowStatus,
    rlPolicyMeteringCounterEnable                   TruthValue,
    rlPolicyMeteringClassInProfileCounter           Counter32,
    rlPolicyMeteringClassOutProfileCounter          Counter32
}

rlPolicyMeteringClassIndex OBJECT-TYPE
    SYNTAX  INTEGER(1..2147483647)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This enumerates the table entry."
    ::= { rlPolicyMeteringClassEntry 1 }

rlPolicyMeteringClassAlwaysConform OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If true, the meter always accepts all traffic; its
         rate is effectively infinite. In such a case, the token
         bucket defined by the MeterRate and Burst-Size
         parameters is ignored.
         also used when there isn't metering support."
    DEFVAL { true }
    ::= { rlPolicyMeteringClassEntry 2 }

rlPolicyMeteringClassAggregateMeterRate OBJECT-TYPE
    SYNTAX  INTEGER
    UNITS   "kbps"
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The rate in kilobytes/second of traffic considered within the
         bandwidth allocated for this policy entry."
    DEFVAL { 0 }
    ::= { rlPolicyMeteringClassEntry 3 }

rlPolicyMeteringClassAggregateMeterBurstSize OBJECT-TYPE
    SYNTAX  INTEGER
    UNITS   "bytes"
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The Burst Size parameter for the aggregate meter leaky bucket.  A
         value of 0 means that the device should choose the Burst Size
         that it thinks is most suitable for the rule.
         The interval can be derived from (burstSizex8/Rate)."
    DEFVAL { 0 }
    ::= { rlPolicyMeteringClassEntry 4 }

rlPolicyMeteringClassPerSessionMeteringRate OBJECT-TYPE
    SYNTAX  INTEGER
    UNITS   "kbps"
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "A Quantitative Appliction policy rule where each individual
         session requires a guaranteed minimum bandwidth.
         Specifies the Ingress traffic flow meter per session
         indicate a bandwidth limit to be applied to each individual session
         Value 0 at rlPolicyMeteringClassPerSessionMetering
         and rlPolicyMeteringClassMaxSessionLimit
         is interpreted to mean no sepecific requarment and
         the aggregate metering will be done by the system decision.
         The rate in kilobytes/second"
     DEFVAL { 0 }
    ::= { rlPolicyMeteringClassEntry 5 }

rlPolicyMeteringClassMaxSessionLimit OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "indicate a the maximum number of session for a sepecific rule
         to guarante minimum bandwidth.
         Value 0 at rlPolicyMeteringClassPerSessionMetering
         and rlPolicyMeteringClassMaxSessionLimit
         is interpreted to mean no sepecific requarment and
         the aggregate metering will be done by the system decision."
    DEFVAL { 0 }
    ::= { rlPolicyMeteringClassEntry 6 }

rlPolicyMeteringClassActionPointer OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies the index in the rlPolicyActionTable to be
         accessed for packets that are in-profile.
         Value 0 is interpreted to mean no action.
         A non-zero value may be specified only for RoutedIp
         packets in Diffserv mode."
    ::= { rlPolicyMeteringClassEntry 7 }

rlPolicyMeteringClassFailMeterPointer OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies an index in the rlPolicyMeterClassTable. This
         is the meter that is to be used if the packet is out-of-profile
         relative to the current meter.
         If non-Diffserv mode, this field is not used.
         If the current meter is AlwaysConform, this field is not used."
    DEFVAL { 0 }
    ::= { rlPolicyMeteringClassEntry 8 }

rlPolicyMeteringClassStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of a table entry.
         It is used to delete an entry from this table."
    ::= { rlPolicyMeteringClassEntry 9 }


rlPolicyMeteringCounterEnable  OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable metering counter for the meter entry."
    DEFVAL { false }
    ::= { rlPolicyMeteringClassEntry 10 }

rlPolicyMeteringClassInProfileCounter OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "meter counter for packets that are in profile ."
    ::= { rlPolicyMeteringClassEntry 11 }

rlPolicyMeteringClassOutProfileCounter OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "meter counter for packets that are out of profile"
    ::= { rlPolicyMeteringClassEntry 12 }



------------
-- Action
---
rlPolicyAction OBJECT IDENTIFIER ::= { rlPolicy 5 }

rlPolicyActionPlatDependParams OBJECT IDENTIFIER ::= { rlPolicyAction 1 }

rlPolicyActionMREDSupported OBJECT-TYPE
    SYNTAX INTEGER {
        supported(1),
        notSupported(2)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates whether the platform supports setting MRED characteristics
         in the packet action"
    ::= { rlPolicyActionPlatDependParams 1 }

rlPolicyActionDroppedPacketCountSupported OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates whether the platform can maintain a count of
         packets Marked for drop by a particular action."
    ::= { rlPolicyActionPlatDependParams 2 }

rlPolicyActionDroppedDropPrecedenceSupported OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates whether the platform support at drop precedence."
    ::= { rlPolicyActionPlatDependParams 3 }

rlPolicyActionInProfileDropPrecedence OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A bit mask indicating which drop precedence supported
            ----------
            |87654321|
            ----------
            1 - low,
            2 - medium,
            3 - high,
            4 - drop"
    ::= { rlPolicyActionPlatDependParams 4 }

rlPolicyActionOutProfileDropPrecedence OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A bit mask indicating which drop precedence supported
            ----------
            |87654321|
            ----------
            1 - low,
            2 - medium,
            3 - high,
            4 - drop"
    ::= { rlPolicyActionPlatDependParams 5 }

rlPolicyActionDscpSupport OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-only
    STATUS  obsolete
    DESCRIPTION
        "Indicates whether the platform support at DSCP filed modification."
    ::= { rlPolicyActionPlatDependParams 6 }

rlPolicyActionDsQueueManagmentSupported OBJECT-TYPE
    SYNTAX INTEGER {
        supported(1),
        notSupported(2)
    }
    MAX-ACCESS read-only
    STATUS obsolete
    DESCRIPTION
        "Indicates whether the platform supports at Q managment for implementation,
        mred, randomDrop used by the min/max threshold"
    ::= { rlPolicyActionPlatDependParams 7 }

--
--  Action Table
--
rlPolicyActionTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlPolicyActionEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This table defines the Actions for packets that pass the meter table
         ie. the characteristics that are assigned to packets before they
         reach the scheduler.
         When Diffserv is not in effect(ie. IPX, bridging, or IP when the global option
         for Diffserv is off), certain table parameters are not available(see
         below). The DiffServ option is enabled or disabled by setting
         rlDiffservModeEnabled."
    ::= { rlPolicyAction 2 }

rlPolicyActionEntry OBJECT-TYPE
    SYNTAX  RlPolicyActionEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Each multifield classification statement consists of the following
         parameters"
    INDEX  { rlPolicyActionIndex }
    ::= { rlPolicyActionTable 1 }

RlPolicyActionEntry ::=  SEQUENCE  {
    rlPolicyActionIndex                         INTEGER,
    rlPolicyActionNewDscp                       INTEGER,
    rlPolicyActionChangeDscp                    TruthValue,
    rlPolicyActionMinThreshold                  INTEGER,
    rlPolicyActionMaxThreshold                  INTEGER,
    rlPolicyActionDropPolicy                    INTEGER,
    rlPolicyActionDroppedPackets                Counter32,
    rlPolicyActionNonDsInProfileDropPrecedence  INTEGER,
    rlPolicyActionNonDsOutProfileDropPrecedence INTEGER,
    rlPolicyActionChangeVpt                     TruthValue,
    rlPolicyActionNewVpt                        INTEGER,
    rlPolicyActionServiceClassPointer           INTEGER,
    rlPolicyActionStatus                        RowStatus,
    rlPolicyActionChangeDscpNonConform          TruthValue,
    rlPolicyActionChangeNewDscpNonConform       INTEGER,
    rlPolicyActionAdvancedTrustMode             TruthValue,
    rlPolicyActionNewIpPrecedence               INTEGER,
    rlPolicyActionChangeIpPrecedence            TruthValue,
    rlPolicyActionReDirect                      RlPolicyRedirectAction,
    rlPolicyActionNewInterface                  InterfaceIndexOrZero,
    rlPolicyActionChangeVidAction               RlPolicyMarkVlanAction,
    rlPolicyActionNewVid                        INTEGER,
    rlPolicyActionTrapTypeId                    INTEGER,
    rlPolicyActionAddTunnel                     Unsigned32
}

rlPolicyActionIndex OBJECT-TYPE
    SYNTAX  INTEGER(1..2147483647)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This enumerates the Action entry."
    ::= { rlPolicyActionEntry 1 }

rlPolicyActionNewDscp OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates the new DSCP with which the packet should
         be marked"
    DEFVAL{ 0 }
    ::= { rlPolicyActionEntry 2 }

rlPolicyActionChangeDscp OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If true, the packet is re-marked with the value indicated by
         newDscp above. If false, the packet's DSCP value is not changed"
    DEFVAL{ false }
    ::= { rlPolicyActionEntry 3 }

rlPolicyActionMinThreshold OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The min-threshold is the queue depth that a random
         drop process will seek to manage the queue's depth to.
         This object is in the action table rather than the
         queue table because Differentiated Services PHBs, such
         as the Assured Service, permit differently classified
         traffic to have different drop parameters even though
         they occupy the same queue."
    DEFVAL{ 0 }
    ::= { rlPolicyActionEntry 4 }

rlPolicyActionMaxThreshold OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The max-threshold is the maximum permissible queue
         depth. In tail drop scenarios, the queue will drop if a
         packet is presented to it and it is instantaneously
         full by this measure. In random drop scenarios, the
         queue will drop if a packet is presented to it and the
         average queue depth exceeds the max-threshold.
         This object is in the action table rather than the
         queue table because Differentiated Services PHBs, such
         as the Assured Service, permit differently classified
         traffic to have different drop parameters even though
         they occupy the same queue."
    DEFVAL { 0 }
    ::= { rlPolicyActionEntry 5 }

rlPolicyActionDropPolicy OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        alwaysDrop (2), -- Disallowed traffic
        tailDrop(3),    -- Fixed Queue Size
        randomDrop(4)   -- MRED w/thresholds per class
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        ""
    DEFVAL{ other }
    ::= { rlPolicyActionEntry 6 }

rlPolicyActionDroppedPackets OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of packets dropped by this action"
    ::= { rlPolicyActionEntry 7 }

rlPolicyActionNonDsInProfileDropPrecedence OBJECT-TYPE
    SYNTAX  INTEGER {
        low(1),
        medium(2),
        high(3),
        drop(4)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This paramer is used at non diffserv mode to attached the drop precedence
         for packet InProfile (metering), only if there is a support for drop precedence
         and with what level."
    DEFVAL{ low }
    ::= { rlPolicyActionEntry 8}

rlPolicyActionNonDsOutProfileDropPrecedence OBJECT-TYPE
    SYNTAX  INTEGER {
        low(1),
        medium(2),
        high(3),
        drop(4)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This paramer is used at non diffserv mode to attached the drop precedence
         for packet OutProfile (metering), only if there is a support for drop precedence
         and with what level."
    DEFVAL{ low }
    ::= { rlPolicyActionEntry 9}

rlPolicyActionChangeVpt OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Routed packets that run through the Rules receive VPT as define at the
              service class they attached to, bridge packets receive through the
              802.1p operation unless we define to change the VPT for those packets."
           DEFVAL { false }
    ::= { rlPolicyActionEntry 10 }

rlPolicyActionNewVpt OBJECT-TYPE
    SYNTAX  INTEGER (0 .. 7)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Priority Tag that will be written to packets ."
     DEFVAL { 0 }
    ::= { rlPolicyActionEntry 11 }

rlPolicyActionServiceClassPointer OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies the index in rlPolicyServiceClassTable denoting
         the service class to which the packet should be assigned
         after the action specified in this entry is carried out.
         A value of 0 means that no Service class is assigned.  A
         value of 0 is legal only for routedIp packets in Diffserv
         mode on Inbound processing."
    ::= { rlPolicyActionEntry 12}

rlPolicyActionStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of the table entry"
    ::= { rlPolicyActionEntry 13}

rlPolicyActionChangeDscpNonConform OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If true, the packet is re-marked with the value indicated by
         newDscp for non conforming packets.
         If false, the packet's DSCP value is not changed"
    DEFVAL{ false }
    ::= { rlPolicyActionEntry 14 }

rlPolicyActionChangeNewDscpNonConform OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates the new DSCP with which the packet should
         be marked"
    DEFVAL{ 0 }
    ::= { rlPolicyActionEntry 15 }

rlPolicyActionAdvancedTrustMode OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates if egress queue is assigned for packets match
        rule according to global trust mode or note."
    DEFVAL{ false }
    ::= { rlPolicyActionEntry 16 }

rlPolicyActionNewIpPrecedence OBJECT-TYPE
    SYNTAX  INTEGER(0..7)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates the new Ip- Precedence with which the packet should
         be marked"
    DEFVAL{ 0 }
    ::= { rlPolicyActionEntry 17 }

rlPolicyActionChangeIpPrecedence OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If true, the packet is re-marked with the value indicated by
         newIpPrecedence above. If false, the packet's DSCP value is not changed"
    DEFVAL{ false }
    ::= { rlPolicyActionEntry 18 }


rlPolicyActionReDirect OBJECT-TYPE
    SYNTAX  RlPolicyRedirectAction
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specified the redirection action/"
    DEFVAL{ disabled }
    ::= { rlPolicyActionEntry 19 }

rlPolicyActionNewInterface OBJECT-TYPE
    SYNTAX  InterfaceIndexOrZero
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Relevant if rlQosClassMapRedirect is either
        'redirectToInterface' or 'analyzerPort'.
        Specified the output interface the packet is redireted to or
        the port that gets copy of the packet in addition to the port
        it was farwarded. "
    DEFVAL{ 0 }
    ::= { rlPolicyActionEntry 20 }

rlPolicyActionChangeVidAction OBJECT-TYPE
    SYNTAX  RlPolicyMarkVlanAction
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If 'mark', than the classified
         traffic will be remarked with new VLAN id.
         If 'disabled' VLAN id is not changed.
         If markNestedVlan, if the egress interface defined as
         VLAN tagged member then a new VLAN tag is added  to the packet."
    DEFVAL{ noMark }
    ::= { rlPolicyActionEntry 21 }

rlPolicyActionNewVid OBJECT-TYPE
    SYNTAX  INTEGER(0..4095)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If rlPolicyActionChangeVid is true,
         specify the new Vlan id to assigned to the packet"
    DEFVAL{ 0 }
    ::= { rlPolicyActionEntry 22 }

rlPolicyActionTrapTypeId OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
     "If now zero, Indicates the trap type id the matched packets arrives with,
      relevant when RedirectAction is trap or mirror."
    DEFVAL{ 0}
    ::= { rlPolicyActionEntry 23 }

rlPolicyActionAddTunnel OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If not zero - Tunnel is added to matched packets."
    DEFVAL{ 0 }
    ::= { rlPolicyActionEntry 24 }

-------------------
-- Service Class
-------------------
rlPolicyServiceClass OBJECT IDENTIFIER ::= { rlPolicy 6 }

rlPolicyServiceClassPlatDependParams OBJECT IDENTIFIER ::= { rlPolicyServiceClass 1 }

rlPolicyNumberOfServiceClassesSupported OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates the number of service classes supported on each
         port of the platform.  Service classes can be neither
         created nor destroyed."
    ::= { rlPolicyServiceClassPlatDependParams 1 }

rlPolicyBoundedPriorityQueueSupport OBJECT-TYPE
    SYNTAX INTEGER {
        supported(1),
        notSupported(2)
    }
    MAX-ACCESS read-only
    STATUS obsolete
    DESCRIPTION
        "Indicates whether the platform supports setting an upper limit
         to the bandwidth of traffic transmitted on queues operating in
         Strict Priority mode."
    ::= { rlPolicyServiceClassPlatDependParams 2 }

rlPolicyDefaultServiceClass OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indicates which service class is default one for packets whose COS is undetermined."
    ::= { rlPolicyServiceClass 2 }

rlPolicyActiveServiceClassTable OBJECT-TYPE
    SYNTAX INTEGER {
                active(1),
        notActive(2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Specifies the Service Class table preform active action
        (usuarlly after set of entries at the service class tentative table).
         Specifies the current status of a table, there could be two options,
         tentative/active table. only the tentative table is the read-write
         and the active table is read-only. at set to activeAction the
         tentative table will be copied to the active table."
    ::= { rlPolicyServiceClass 3 }

--
--  Service Class Table
--
rlPolicyServiceClassTentativeTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlPolicyServiceClassTentativeEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This table defines the service classes for the system ie. the queue
         discipline and weight characteristics that are implemented on each
         port unless the user configures a port specific value in ....
         The total number of service classes defined can not exceed
         rlPolicyNumberOfTransmitQueuesPerPort."
    ::= { rlPolicyServiceClass 4 }

rlPolicyServiceClassTentativeEntry OBJECT-TYPE
    SYNTAX  RlPolicyServiceClassTentativeEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
         "Each multifield classification statement consists of the following
          parameters"
    INDEX  { rlPolicyServiceClassTentativeIndex }
    ::= { rlPolicyServiceClassTentativeTable 1 }

RlPolicyServiceClassTentativeEntry ::=  SEQUENCE  {
    rlPolicyServiceClassTentativeIndex          INTEGER,
    rlPolicyServiceClassTentativeName           DisplayString,
    rlPolicyServiceClassTentativePhbType        INTEGER,
    rlPolicyServiceClassTentativeMinRate        INTEGER,
    rlPolicyServiceClassTentativeMaxRate        INTEGER,
    rlPolicyServiceClassTentativePriority       INTEGER,
    rlPolicyServiceClassTentative8021DPri       INTEGER,
    rlPolicyServiceClassTentativeStatus         RowStatus,
    rlPolicyServiceClassTentativeTdThersholdDp0 INTEGER,
    rlPolicyServiceClassTentativeTdThersholdDp1 INTEGER,
    rlPolicyServiceClassTentativeTdThersholdDp2 INTEGER,
    rlPolicyServiceClassTentativeRedMinDp0      INTEGER,
    rlPolicyServiceClassTentativeRedMaxDp0      INTEGER,
    rlPolicyServiceClassTentativeRedProbDp0     INTEGER,
    rlPolicyServiceClassTentativeRedMinDp1      INTEGER,
    rlPolicyServiceClassTentativeRedMaxDp1      INTEGER,
    rlPolicyServiceClassTentativeRedProbDp1     INTEGER,
    rlPolicyServiceClassTentativeRedMinDp2      INTEGER,
    rlPolicyServiceClassTentativeRedMaxDp2      INTEGER,
    rlPolicyServiceClassTentativeRedProbDp2     INTEGER,
    rlPolicyServiceClassTentativeRedQweight     INTEGER,
    rlPolicyServiceClassTentativeShaperStatus   TruthValue,
    rlPolicyServiceClassTentativeCirQueueShaper INTEGER,
    rlPolicyServiceClassTentativeCbsQueueShaper INTEGER

}

rlPolicyServiceClassTentativeIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This enumerates the ServiceClass Tentative entry."
    ::= { rlPolicyServiceClassTentativeEntry 1 }

rlPolicyServiceClassTentativeName OBJECT-TYPE
    SYNTAX  DisplayString(SIZE(0..20))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The name given by the system administrator to the class."
    ::= { rlPolicyServiceClassTentativeEntry 2 }

rlPolicyServiceClassTentativePhbType OBJECT-TYPE
    SYNTAX  INTEGER {
        expeditedForwarding(1),
        assuredForwarding(2),
        bestEffort(3)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates the type of Diffserv per-hop behaviour that this service
         class is intended to support. This object can be set by the user
         only in DiffServ mode (i.e. rlDiffservModeEnabled = enabled)."
    DEFVAL { bestEffort }
    ::= { rlPolicyServiceClassTentativeEntry 3 }

rlPolicyServiceClassTentativeMinRate OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies either the minimum throughput of the queue as a percentage
         of the throughput of  each output port on which the service class is
         implemented.  If zero, there is no minimum rate. This field can not
         be set by the user if rlDiffservModeEnabled = disabled and
         rlPolicyServiceClassPriority > 0 or rlDiffservModeEnabled = enabled
         and rlPolicyServiceClassPhbType = expeditedForwarding."
    ::= { rlPolicyServiceClassTentativeEntry 4 }

rlPolicyServiceClassTentativeMaxRate OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specifies either the upper limit on the throughput of the queue as a
         percentage of the throughput of  each output port on which the service
         class is implemented.  If zero, there is no maximum rate.
         This field can not be set by the user
         if rlDiffservModeEnabled = disabled and
         rlPolicyServiceClassPriority = 0 or
         rlDiffservModeEnabled = enabled and
         rlPolicyServiceClassPhbType != expeditedForwarding or
         rlBoundedPriorityQueueSupport = notSupported."
    ::= { rlPolicyServiceClassTentativeEntry 5 }

rlPolicyServiceClassTentativePriority OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If non-zero, this service class will operate as a priority service
         class with the specified priority value.  This object can not be set
         in Diffserv mode (i.e. rlDiffservModeEnabled = enabled), in which case
         rlServiceClassPhbType should be used instead. It can't be set when
         rlBoundedPriorityQueueSupport = notSupported as well."
    ::= { rlPolicyServiceClassTentativeEntry 6 }

rlPolicyServiceClassTentative8021DPri OBJECT-TYPE
    SYNTAX  INTEGER (0 .. 7)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "802.1D Priority Tag that will be written to routed packets and
         untagged bridged packets transmitted with this service class."
    ::= { rlPolicyServiceClassTentativeEntry 7 }

rlPolicyServiceClassTentativeStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Status of this entry."
    ::= { rlPolicyServiceClassTentativeEntry 8 }

rlPolicyServiceClassTentativeTdThersholdDp0 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 0.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassTentativeEntry 9 }

rlPolicyServiceClassTentativeTdThersholdDp1 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 1.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassTentativeEntry 10 }

rlPolicyServiceClassTentativeTdThersholdDp2 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 2.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassTentativeEntry 11 }

rlPolicyServiceClassTentativeRedMinDp0 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 0.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassTentativeEntry 12 }

rlPolicyServiceClassTentativeRedMaxDp0 OBJECT-TYPE
    SYNTAX INTEGER  (0..100)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 0.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassTentativeEntry 13 }

rlPolicyServiceClassTentativeRedProbDp0 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 0."
    ::= { rlPolicyServiceClassTentativeEntry 14 }

rlPolicyServiceClassTentativeRedMinDp1 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 1.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassTentativeEntry 15 }

rlPolicyServiceClassTentativeRedMaxDp1 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 1.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassTentativeEntry 16 }

rlPolicyServiceClassTentativeRedProbDp1 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 1."
    ::= { rlPolicyServiceClassTentativeEntry 17 }

rlPolicyServiceClassTentativeRedMinDp2 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 2.
         UNITS percent 0-100"
    ::= { rlPolicyServiceClassTentativeEntry 18 }

rlPolicyServiceClassTentativeRedMaxDp2 OBJECT-TYPE
    SYNTAX INTEGER  (0..100)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 2.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassTentativeEntry 19 }

rlPolicyServiceClassTentativeRedProbDp2 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 2."
    ::= { rlPolicyServiceClassTentativeEntry 20 }

rlPolicyServiceClassTentativeRedQweight OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "additional parameter for the WRED algorithem supporting
        the Queue weight exponentail factor"
    ::= { rlPolicyServiceClassTentativeEntry 21 }

rlPolicyServiceClassTentativeShaperStatus OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "If there is shaper on the Queue"
    ::= { rlPolicyServiceClassTentativeEntry 22 }

rlPolicyServiceClassTentativeCirQueueShaper OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CIR for the Queue shaper.
         N/A when the shper is disabled.
         UNITS bps bits per second"
    ::= { rlPolicyServiceClassTentativeEntry 23 }

rlPolicyServiceClassTentativeCbsQueueShaper OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CBS for the Queue shaper.
         N/A when the shper is disabled.
         UNITS bytes"
    ::= { rlPolicyServiceClassTentativeEntry 24 }





rlPolicyServiceClassActiveTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlPolicyServiceClassActiveEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This table defines the service classes for the system ie. the queue
         discipline and weight characteristics that are implemented on each
         port unless the user configures a port specific value in ....
         The total number of service classes defined can not exceed
         rlPolicyNumberOfTransmitQueuesPerPort."
    ::= { rlPolicyServiceClass 5 }

rlPolicyServiceClassActiveEntry OBJECT-TYPE
    SYNTAX  RlPolicyServiceClassActiveEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
         "Each multifield classification statement consists of the following
          parameters"
    INDEX  { rlPolicyServiceClassActiveIndex }
    ::= { rlPolicyServiceClassActiveTable 1 }

RlPolicyServiceClassActiveEntry ::=  SEQUENCE  {
    rlPolicyServiceClassActiveIndex          INTEGER,
    rlPolicyServiceClassActiveName           DisplayString,
    rlPolicyServiceClassActivePhbType        INTEGER,
    rlPolicyServiceClassActiveMinRate        INTEGER,
    rlPolicyServiceClassActiveMaxRate        INTEGER,
    rlPolicyServiceClassActivePriority       INTEGER,
    rlPolicyServiceClassActive8021DPri       INTEGER,
    rlPolicyServiceClassActiveTdThersholdDp0 INTEGER,
    rlPolicyServiceClassActiveTdThersholdDp1 INTEGER,
    rlPolicyServiceClassActiveTdThersholdDp2 INTEGER,
    rlPolicyServiceClassActiveRedMinDp0      INTEGER,
    rlPolicyServiceClassActiveRedMaxDp0      INTEGER,
    rlPolicyServiceClassActiveRedProbDp0     INTEGER,
    rlPolicyServiceClassActiveRedMinDp1      INTEGER,
    rlPolicyServiceClassActiveRedMaxDp1      INTEGER,
    rlPolicyServiceClassActiveRedProbDp1     INTEGER,
    rlPolicyServiceClassActiveRedMinDp2      INTEGER,
    rlPolicyServiceClassActiveRedMaxDp2      INTEGER,
    rlPolicyServiceClassActiveRedProbDp2     INTEGER,
    rlPolicyServiceClassActiveRedQweight     INTEGER,
    rlPolicyServiceClassActiveShaperStatus   TruthValue,
    rlPolicyServiceClassActiveCirQueueShaper INTEGER,
    rlPolicyServiceClassActiveCbsQueueShaper INTEGER
   }

rlPolicyServiceClassActiveIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This enumerates the ServiceClass Active entry."
    ::= { rlPolicyServiceClassActiveEntry 1 }

rlPolicyServiceClassActiveName OBJECT-TYPE
    SYNTAX  DisplayString(SIZE(0..20))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The name given by the system administrator to the class."
    ::= { rlPolicyServiceClassActiveEntry 2 }

rlPolicyServiceClassActivePhbType OBJECT-TYPE
    SYNTAX  INTEGER {
        expeditedForwarding(1),
        assuredForwarding(2),
        bestEffort(3)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates the type of Diffserv per-hop behaviour that this service
         class is intended to support. This object can be set by the user
         only in DiffServ mode (i.e. rlDiffservModeEnabled = enabled)."
    DEFVAL { bestEffort }
    ::= { rlPolicyServiceClassActiveEntry 3 }

rlPolicyServiceClassActiveMinRate OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies either the minimum throughput of the queue as a percentage
         of the throughput of  each output port on which the service class is
         implemented.  If zero, there is no minimum rate. This field can not
         be set by the user if rlDiffservModeEnabled = disabled and
         rlPolicyServiceClassPriority > 0 or rlDiffservModeEnabled = enabled
         and rlPolicyServiceClassPhbType = expeditedForwarding."
    ::= { rlPolicyServiceClassActiveEntry 4 }

rlPolicyServiceClassActiveMaxRate OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specifies either the upper limit on the throughput of the queue as a
         percentage of the throughput of  each output port on which the service
         class is implemented.  If zero, there is no maximum rate.
         This field can not be set by the user
         if rlDiffservModeEnabled = disabled and
         rlPolicyServiceClassPriority = 0 or
         rlDiffservModeEnabled = enabled and
         rlPolicyServiceClassPhbType != expeditedForwarding or
         rlBoundedPriorityQueueSupport = notSupported."
    ::= { rlPolicyServiceClassActiveEntry 5 }

rlPolicyServiceClassActivePriority OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "If non-zero, this service class will operate as a priority service
         class with the specified priority value.  This object can not be set
         in Diffserv mode (i.e. rlDiffservModeEnabled = enabled), in which case
         rlServiceClassPhbType should be used instead. It can't be set when
         rlBoundedPriorityQueueSupport = notSupported as well."
    ::= { rlPolicyServiceClassActiveEntry 6 }

rlPolicyServiceClassActive8021DPri OBJECT-TYPE
    SYNTAX  INTEGER (0 .. 7)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "802.1D Priority Tag that will be written to routed packets and
         untagged bridged packets transmitted with this service class."
    ::= { rlPolicyServiceClassActiveEntry 7 }

rlPolicyServiceClassActiveTdThersholdDp0 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 0.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassActiveEntry 8 }

rlPolicyServiceClassActiveTdThersholdDp1 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 1.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassActiveEntry 9 }

rlPolicyServiceClassActiveTdThersholdDp2 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 2.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassActiveEntry 10 }

rlPolicyServiceClassActiveRedMinDp0 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 0.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassActiveEntry 11 }

rlPolicyServiceClassActiveRedMaxDp0 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 0.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassActiveEntry 12 }

rlPolicyServiceClassActiveRedProbDp0 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 0."
    ::= { rlPolicyServiceClassActiveEntry 13 }

rlPolicyServiceClassActiveRedMinDp1 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 1.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassActiveEntry 14 }

rlPolicyServiceClassActiveRedMaxDp1 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 1.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassActiveEntry 15 }

rlPolicyServiceClassActiveRedProbDp1 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 1."
    ::= { rlPolicyServiceClassActiveEntry 16 }

rlPolicyServiceClassActiveRedMinDp2 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 2.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassActiveEntry 17 }

rlPolicyServiceClassActiveRedMaxDp2 OBJECT-TYPE
    SYNTAX INTEGER (0..100)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 2.
        UNITS percent 0-100"
    ::= { rlPolicyServiceClassActiveEntry 18 }

rlPolicyServiceClassActiveRedProbDp2 OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 2."
    ::= { rlPolicyServiceClassActiveEntry 19 }


rlPolicyServiceClassActiveRedQweight OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "additional parameter for the WRED algorithem supporting
        the Queue weight exponentail factor"
    ::= { rlPolicyServiceClassActiveEntry 20 }

rlPolicyServiceClassActiveShaperStatus OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "If there is shaper on the Queue"
    ::= { rlPolicyServiceClassActiveEntry 21 }

rlPolicyServiceClassActiveCirQueueShaper OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The CIR for the queue shaper.
         N/A when the shper is disabled
         UNITS bps bits per second"
    ::= { rlPolicyServiceClassActiveEntry 22 }

rlPolicyServiceClassActiveCbsQueueShaper OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The CBS for the queue shaper.
         N/A when the shper is disabled.
         UNITS bytes"
    ::= { rlPolicyServiceClassActiveEntry 23 }




--
-- Port configuration table.
--
rlPolicyPortConfigurationTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlPolicyPortCfgEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This table enables the network administrator to fine-tune
         the bandwidth given to each service class on each port.
         The values in this table will thus override those of the
         rlServiceClassTable (THIS TABLE IS MANAGE FROM 3SW). "
    ::= { rlPolicyServiceClass 6 }

rlPolicyPortCfgEntry OBJECT-TYPE
    SYNTAX  RlPolicyPortCfgEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Configuration parameters for each port/service class."
    INDEX  { rlPolicyPortCfgIfIndex  }
    ::= { rlPolicyPortConfigurationTable 1 }

RlPolicyPortCfgEntry ::= SEQUENCE {
    rlPolicyPortCfgIfIndex                 InterfaceIndex,
    rlPolicyPortCfgMinimalBandwidth        OBJECT IDENTIFIER,
    rlPolicyPortCfgMaximalBandwidth        OBJECT IDENTIFIER,
    rlPolicyPortCfgStatus                  RowStatus,
    rlpolicyDropProfilePointer             INTEGER,
    rlPolicyPortCfgQueueShaperStatus       OBJECT IDENTIFIER,
    rlPolicyPortCfgCirQueueShaper          OBJECT IDENTIFIER,
    rlPolicyPortCfgCbsQueueShaper          OBJECT IDENTIFIER,
    rlPolicyPortCfgPortShaperStatus        TruthValue,
    rlPolicyPortCfgCirPortShaper           INTEGER,
    rlPolicyPortCfgCbsPortShaper           INTEGER,
    rlPolicyPortCfgPortRateLimitStatus     TruthValue,
    rlPolicyPortCfgCirPortRateLimit        INTEGER,
    rlPolicyPortCfgCbsPortRateLimit        INTEGER
   }

rlPolicyPortCfgIfIndex OBJECT-TYPE
    SYNTAX  InterfaceIndex
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Interface index."
    ::= { rlPolicyPortCfgEntry 1 }

rlPolicyPortCfgMinimalBandwidth  OBJECT-TYPE
    SYNTAX   OBJECT IDENTIFIER
    MAX-ACCESS   read-write
    STATUS   current
    DESCRIPTION
        "The list of objects contain parameters at Precents type for the minimal bandwidth
         to this port/service class at WWR . The OID length is based on the number of the
         service class number,  every OID define parameter of service class."
    ::= { rlPolicyPortCfgEntry 2 }

rlPolicyPortCfgMaximalBandwidth OBJECT-TYPE
    SYNTAX   OBJECT IDENTIFIER
    MAX-ACCESS   read-write
    STATUS   current
    DESCRIPTION
         "The list of objects contain parameters at Precents type for the maximal bandwidth
         to this port/service class at SP . The OID length is based on the number of the
         service class number,  every OID define parameter of service class."
    ::= { rlPolicyPortCfgEntry 3 }

rlPolicyPortCfgStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Status of this entry."
    ::= { rlPolicyPortCfgEntry 4 }


rlpolicyDropProfilePointer OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "pointing to drop algorithem profile.
        the profile describs the drop algorithem
        (tail, red)and params"
    ::= { rlPolicyPortCfgEntry 5 }



rlPolicyPortCfgQueueShaperStatus OBJECT-TYPE
    SYNTAX OBJECT IDENTIFIER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "If there is shaper on the Queue"
    ::= { rlPolicyPortCfgEntry 6 }

rlPolicyPortCfgCirQueueShaper OBJECT-TYPE
    SYNTAX OBJECT IDENTIFIER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CIR for the Queue shaper.
         N/A when the shper is disabled
         UNITS bps bits per second"
    ::= { rlPolicyPortCfgEntry 7 }

rlPolicyPortCfgCbsQueueShaper OBJECT-TYPE
    SYNTAX OBJECT IDENTIFIER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CBS for the Queue shaper.
         N/A when the shper is disabled.
         UNITS bytes"
    ::= { rlPolicyPortCfgEntry 8 }

rlPolicyPortCfgPortShaperStatus OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "If there is shaper on the port"
    ::= { rlPolicyPortCfgEntry 9 }

rlPolicyPortCfgCirPortShaper OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CIR for the port shaper.
         N/A when the shper is disabled
         UNITS bps bits per second"
    ::= { rlPolicyPortCfgEntry 10 }

rlPolicyPortCfgCbsPortShaper OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CBS for the port shaper.
         N/A when the shper is disabled.
         UNITS bytes"
    ::= { rlPolicyPortCfgEntry 11 }

rlPolicyPortCfgPortRateLimitStatus OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "If there is Rate Limit on the port"
    DEFVAL { false }
    ::= { rlPolicyPortCfgEntry 12 }

rlPolicyPortCfgCirPortRateLimit OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CIR for the port Rate limit.
         N/A when the Rate limit is disabled
         UNITS bps bits per second"
    DEFVAL { 0 }
    ::= { rlPolicyPortCfgEntry 13 }

rlPolicyPortCfgCbsPortRateLimit OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CBS for the port Rate Limit.
         N/A when the Rate Limit is disabled.
         UNITS bytes"
    DEFVAL { 0 }
    ::= { rlPolicyPortCfgEntry 14 }


--
-- drop profile table.
--


rlPolicyDropProfileTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlPolicyDropProfileEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        " this table defines drop profile
          which describ the queue's drop
          algorithems"



    ::= { rlPolicyServiceClass 7 }

rlPolicyDropProfileEntry OBJECT-TYPE
    SYNTAX  RlPolicyDropProfileEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Configuration parameters for each port/service class."
    INDEX  { rlPolicyDropProfileIndex,rlPolicyDropProfileQueueNumber}
    ::= { rlPolicyDropProfileTable 1 }

RlPolicyDropProfileEntry ::= SEQUENCE {
    rlPolicyDropProfileIndex                   INTEGER,
    rlPolicyDropProfileQueueNumber             INTEGER,
    rlPolicyDropProfileTdThersholdDp0          INTEGER,
    rlPolicyDropProfileTdThersholdDp1          INTEGER,
    rlPolicyDropProfileTdThersholdDp2          INTEGER,
    rlPolicyDropProfileRedMinDp0               INTEGER,
    rlPolicyDropProfileRedMaxDp0               INTEGER,
    rlPolicyDropProfileRedProbDp0              INTEGER,
    rlPolicyDropProfileRedMinDp1               INTEGER,
    rlPolicyDropProfileRedMaxDp1               INTEGER,
    rlPolicyDropProfileRedProbDp1              INTEGER,
    rlPolicyDropProfileRedMinDp2               INTEGER,
    rlPolicyDropProfileRedMaxDp2               INTEGER,
    rlPolicyDropProfileRedProbDp2              INTEGER,
    rlPolicyDropProfileRedQweight              INTEGER,
    rlPolicyDropProfileStatus                  RowStatus
    }

rlPolicyDropProfileIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Interface index."
    ::= { rlPolicyDropProfileEntry 1 }

rlPolicyDropProfileQueueNumber OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Interface Queue number."
    ::= { rlPolicyDropProfileEntry 2 }




rlPolicyDropProfileTdThersholdDp0 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 0.
        UNITS  percent 0-100"
    ::= { rlPolicyDropProfileEntry 3 }

rlPolicyDropProfileTdThersholdDp1 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 1.
        UNITS percent 0-100"
    ::= { rlPolicyDropProfileEntry 4 }

rlPolicyDropProfileTdThersholdDp2 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Tail Drop Threshold for Drop Precedence 2.
        UNITS percent 0-100"
    ::= { rlPolicyDropProfileEntry 5 }

rlPolicyDropProfileRedMinDp0 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 0.
        UNITS percent 0-100"
    ::= { rlPolicyDropProfileEntry 6 }

rlPolicyDropProfileRedMaxDp0 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 0.
        UNITS percent 0-100 0-100"
    ::= { rlPolicyDropProfileEntry 7 }

rlPolicyDropProfileRedProbDp0 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 0."
    ::= { rlPolicyDropProfileEntry 8 }

rlPolicyDropProfileRedMinDp1 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 1.
        UNITS percent 0-100"
    ::= { rlPolicyDropProfileEntry 9 }

rlPolicyDropProfileRedMaxDp1 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 1.
        UNITS percent 0-100"
    ::= { rlPolicyDropProfileEntry 10 }

rlPolicyDropProfileRedProbDp1 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 1."
    ::= { rlPolicyDropProfileEntry 11 }

rlPolicyDropProfileRedMinDp2 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Min Threshold for Drop Precedence 2.
        UNITS percent 0-100"
    ::= { rlPolicyDropProfileEntry 12 }

rlPolicyDropProfileRedMaxDp2 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED Max Threshold for Drop Precedence 2.
        UNITS percent 0-100"
    ::= { rlPolicyDropProfileEntry 13 }

rlPolicyDropProfileRedProbDp2 OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "WRED probability for Drop Precedence 2."
    ::= { rlPolicyDropProfileEntry 14 }

rlPolicyDropProfileRedQweight OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "additional parameter for the WRED algorithem supporting
        the Queue weight exponentail factor"
    ::= { rlPolicyDropProfileEntry 15 }

rlPolicyDropProfileStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Status of this entry."
    ::= { rlPolicyDropProfileEntry 16 }

--
-- Vlan Configuration table.
--

rlPolicyVlanConfigurationTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlPolicyVlanCfgEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "This table enables the network administrator to fine-tune
         the rate limit given to each vlan.
         The values in this table will thus override those of the
         rlQosIfPolicyTable (THIS TABLE IS MANAGED FROM 3SW). "
    ::= { rlPolicyServiceClass 8 }

rlPolicyVlanCfgEntry OBJECT-TYPE
    SYNTAX  RlPolicyVlanCfgEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Configuration parameters for each vlan."
    INDEX  { rlPolicyVlanCfgVlanId  }
    ::= { rlPolicyVlanConfigurationTable 1 }

RlPolicyVlanCfgEntry ::= SEQUENCE {
    rlPolicyVlanCfgVlanId                      VlanId,
    rlPolicyVlanCfgPortRateLimitStatus         TruthValue,
    rlPolicyVlanCfgCirPortRateLimit            INTEGER,
    rlPolicyVlanCfgCbsPortRateLimit            INTEGER,
    rlPolicyVlanCfgStatus                      RowStatus
   }

rlPolicyVlanCfgVlanId OBJECT-TYPE
    SYNTAX  VlanId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Interface index."
    ::= { rlPolicyVlanCfgEntry 1 }


rlPolicyVlanCfgPortRateLimitStatus OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "If there is Rate Limit on the vlan"
    DEFVAL { false }
    ::= { rlPolicyVlanCfgEntry 2 }

rlPolicyVlanCfgCirPortRateLimit OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CIR for the port Rate limit.
         N/A when the Rate limit is disabled
         UNITS bps bits per second"
    ::= { rlPolicyVlanCfgEntry 3 }

rlPolicyVlanCfgCbsPortRateLimit OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The CBS for the port Rate Limit.
         N/A when the Rate Limit is disabled.
         UNITS bytes"
    ::= { rlPolicyVlanCfgEntry 4 }


rlPolicyVlanCfgStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Status of this entry."
    ::= { rlPolicyVlanCfgEntry 5 }

------------
-- DiffServ
---
rlPolicyDiffServ OBJECT IDENTIFIER ::= { rlPolicy 7 }

rlPolicyDiffServPlatDependParams OBJECT IDENTIFIER ::= { rlPolicyDiffServ 1 }

rlDiffservModeSupported OBJECT-TYPE
    SYNTAX INTEGER {
        supported(1),
        notSupported(2)
    }
    MAX-ACCESS read-only
    STATUS obsolete
    DESCRIPTION
        "Indicates whether Diffserv mode is supported on the platform."
    ::= { rlPolicyDiffServPlatDependParams 1 }

rlDiffservModeEnabled OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indicates whether Diffserv mode is currently enabled."
    ::= { rlPolicyDiffServ 2 }

--
-- Diffserv Boundary / Interior port table for DiffServ mode
--
rlDiffservBoundaryTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlDiffservBoundaryEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Indicates whether a port is considered a boundary or an interior
         node of  the Diffserv domain"
    ::= { rlPolicyDiffServ 3 }

rlDiffservBoundaryEntry OBJECT-TYPE
    SYNTAX  RlDiffservBoundaryEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Each boundary/interior ports table entry consists of the following
         parameters"
    INDEX  { rlDiffservBoundaryIfIndex }
    ::= { rlDiffservBoundaryTable 1 }

RlDiffservBoundaryEntry ::=   SEQUENCE  {
    rlDiffservBoundaryIfIndex    INTEGER,
    rlDiffservBoundaryPortType   INTEGER,
    rlDiffservBoundaryStatus     RowStatus
}

rlDiffservBoundaryIfIndex OBJECT-TYPE
    SYNTAX   INTEGER (1..2147483647)
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
         "The Interface index whose type is being defined"
    ::= { rlDiffservBoundaryEntry 1 }

rlDiffservBoundaryPortType OBJECT-TYPE
    SYNTAX  INTEGER {
        boundary(1),
        interior(2)
    }
    MAX-ACCESS   read-write
    STATUS   current
    DESCRIPTION
         "The boundary status of the port."
    DEFVAL { boundary }
    ::= { rlDiffservBoundaryEntry 2 }

rlDiffservBoundaryStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Status of this entry."
    ::= { rlDiffservBoundaryEntry 3 }

--
-- Global Params
--
rlPolicyGlobalParams OBJECT IDENTIFIER  ::= { rlPolicy 9 }

rlPolicyGlobalOperationEnabled OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indicates whether Policy is currently enabled."
    DEFVAL{ disabled }
    ::= { rlPolicyGlobalParams 1 }


rlPolicyGlobalDefaultForwarding OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates whether or not the unmach traffic
        is forwarded or blocked."
    ::= { rlPolicyGlobalParams 2 }

rlPolicyGlobalAdminTrapfrequency OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "define the the min number of seconds between successive traps.
         0 means no traps will be sent, uints in Sec"
    DEFVAL { 0 }
    ::= { rlPolicyGlobalParams 3 }

rlPolicyGlobalOperTrapElapsedTime OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "show the time out elaps from the last trap sent
        uints in Sec."
    ::= { rlPolicyGlobalParams 4 }


rlPolicyGlobalQosMode OBJECT-TYPE
    SYNTAX  RlPolicyQosMode
    MAX-ACCESS  read-write
    STATUS  deprecated
    DESCRIPTION
        "V750 DEPRECATED - replaced with rlPolicyGlobalQosMode field in rlPolicyQosModeGlobalCfg table.
        user can set the system to operate either in the Basic mode or in the Advanced mode"
    ::= { rlPolicyGlobalParams 5 }



rlPolicyGlobalTrustMode OBJECT-TYPE
    SYNTAX RlPolicyTrustTypes
    MAX-ACCESS read-write
    STATUS deprecated
    DESCRIPTION
        "V750 DEPRECATED - replaced with rlPolicyGlobalTrustMode field in rlPolicyQosModeGlobalCfg table.
        Global Trust state. the value refered to Basic mode and specify
        the trust mode the device is support. all phisical ports are trusted  "
    ::= { rlPolicyGlobalParams 6 }


--
-- Global Params for Qos mib
--


rlPolicyGlobalDeviceQosOperationTypes OBJECT-TYPE
    SYNTAX INTEGER {
        disable(1),
        basic(2),
        advanced(3),
        all(4),
        notSupported(5)
}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates if the system support basic
         or advanced mode  or Both basic and Advanced"
    ::= { rlPolicyGlobalParams 7 }


rlPolicyGlobalDscpMutationSupported OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "mutation over the ingress packet dscp field
         supported for the device."
    ::= { rlPolicyGlobalParams 8 }

rlPolicyGlobalClassifyIpPrecedenceSupported OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS obsolete
    DESCRIPTION
        "Indicates if the system support
         classification according ip precedence
         most significant 3 bits in the TOS byte"
    ::= { rlPolicyGlobalParams 9 }



rlPolicyGlobalDeviceShapingTypeSupported OBJECT-TYPE
    SYNTAX INTEGER {
        portShaper(1),
        queueShaper(2),
        portAndQueueShaper(3),
        notSupported(4)}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the shaper shaper type supported for the device"
    ::= { rlPolicyGlobalParams 10 }


rlPolicyGlobalDscpRemarkingSupported OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates if dscp remarking
         supported for the device"
    ::= { rlPolicyGlobalParams 11 }


rlPolicyGlobalqueueSchedulerPerDeviceOrPort OBJECT-TYPE
    SYNTAX INTEGER {
        device(1),
        port(2)}
    MAX-ACCESS read-only
    STATUS obsolete
    DESCRIPTION
        "indicates if the system support scheduling
         configuration per port or per device.
         device (1 ) or port (2)"
    ::= { rlPolicyGlobalParams 12 }


---
--- policy mapping
---
rlPolicyMapping OBJECT IDENTIFIER ::= { rlPolicy 10 }



---  Policy DSCP to ServiceClass mapping

rlPolicyDscpServiceClassTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyDscpServiceClassEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The DSCP
         to ServiceClass map table"
    ::= { rlPolicyMapping 1 }

rlPolicyDscpServiceClassEntry OBJECT-TYPE
    SYNTAX RlPolicyDscpServiceClassEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes The ServiceClass assigned to a Dscp value.
         The index is DSCP represent by rlPolicyDscpIndex"
    INDEX { rlPolicyDscpIndex }
    ::= { rlPolicyDscpServiceClassTable 1 }

RlPolicyDscpServiceClassEntry::= SEQUENCE {
        rlPolicyDscpIndex                       INTEGER,
        rlPolicyServiceClassValue               INTEGER,
        rlPolicyDscpServiceClassStatus          RowStatus
    }


rlPolicyDscpIndex OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "DSCP value."
    ::= { rlPolicyDscpServiceClassEntry 1 }

rlPolicyServiceClassValue OBJECT-TYPE
    SYNTAX INTEGER(1..8)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "ServiceClass value."
    ::= { rlPolicyDscpServiceClassEntry 2 }

    rlPolicyDscpServiceClassStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlPolicyDscpServiceClassEntry 3 }

-- Policy TCP-UDP port to Service Class map

rlPolicyTcpUdpPortServiceClassTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyTcpUdpPortServiceClassEntry
    MAX-ACCESS not-accessible
    STATUS obsolete
    DESCRIPTION
        "This table specifies TCP/UDP
         Port to ServiceClass map table"
    ::= { rlPolicyMapping 2 }

rlPolicyTcpUdpPortServiceClassEntry OBJECT-TYPE
    SYNTAX RlPolicyTcpUdpPortServiceClassEntry
    MAX-ACCESS not-accessible
    STATUS obsolete
    DESCRIPTION
        "Each entry in this table describes The
         ServiceClass Value.
         The index is TCP/UDP port represent by rlPolicyTcpUdpPort"
    INDEX { rlPolicyProtocolType , rlPolicyTcpUdpPort  }
    ::= { rlPolicyTcpUdpPortServiceClassTable 1 }

RlPolicyTcpUdpPortServiceClassEntry::= SEQUENCE {
        rlPolicyProtocolType                             L4ProtType,
        rlPolicyTcpUdpPort                               INTEGER,
        rlPolicyMappedServiceClass                             INTEGER,
        rlPolicyTcpUdpPortServiceClassStatus                     RowStatus
    }

rlPolicyProtocolType OBJECT-TYPE
    SYNTAX L4ProtType
    MAX-ACCESS read-only
    STATUS obsolete
    DESCRIPTION
        "TCP/UDP port type. "
    ::= { rlPolicyTcpUdpPortServiceClassEntry 1 }

rlPolicyTcpUdpPort OBJECT-TYPE
    SYNTAX INTEGER(0..65535)
    MAX-ACCESS read-only
    STATUS obsolete
    DESCRIPTION
        "TCP/UDP port number. "
    ::= { rlPolicyTcpUdpPortServiceClassEntry 2 }



rlPolicyMappedServiceClass OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS obsolete
    DESCRIPTION
        "ServiceClass value."
    ::= { rlPolicyTcpUdpPortServiceClassEntry 3 }

rlPolicyTcpUdpPortServiceClassStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlPolicyTcpUdpPortServiceClassEntry 4 }


-- Policy ServiceClass Remark mapping



rlPolicyDscpRemarkTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyDscpRemarkEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The DSCP
         Remark table"
    ::= { rlPolicyMapping 3 }

rlPolicyDscpRemarkEntry OBJECT-TYPE
    SYNTAX RlPolicyDscpRemarkEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the new
         DSCP for the packet.
         The index is Old DSCP represent by rlPolicyOldDscp"
    INDEX { rlPolicyRmOldDscp }
    ::= { rlPolicyDscpRemarkTable 1 }

RlPolicyDscpRemarkEntry::= SEQUENCE {
        rlPolicyRmOldDscp                INTEGER,
        rlPolicyRmNewDscp                INTEGER,
        rlPolicyDscpRemarkStatus         RowStatus,
        rlPolicyRmNewExceedDscp          INTEGER
    }

rlPolicyRmOldDscp OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Old DSCP."
    ::= { rlPolicyDscpRemarkEntry 1 }

rlPolicyRmNewDscp OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "New DSCP for the violation action."
    ::= { rlPolicyDscpRemarkEntry 2 }


rlPolicyDscpRemarkStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlPolicyDscpRemarkEntry 3 }
    
    
rlPolicyRmNewExceedDscp OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "New DSCP for the exceed action."
    ::= { rlPolicyDscpRemarkEntry 4 }    


-- Policy DSCP Mutation Table


rlPolicyDscpMutationTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyDscpMutationEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The DSCP
         Mutation table"
    ::= { rlPolicyMapping 4 }

rlPolicyDscpMutationEntry OBJECT-TYPE
    SYNTAX RlPolicyDscpMutationEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the new
         DSCP for the packet.
         The index is Old DSCP represent by rlPolicyOldDscp"
    INDEX { rlPolicyOldDscp }
    ::= { rlPolicyDscpMutationTable 1 }

RlPolicyDscpMutationEntry::= SEQUENCE {
        rlPolicyOldDscp                INTEGER,
        rlPolicyNewDscp                INTEGER,
        rlPolicyDscpMutationStatus     RowStatus
    }

rlPolicyOldDscp OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Old DSCP."
    ::= { rlPolicyDscpMutationEntry 1 }

rlPolicyNewDscp OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "New DSCP."
    ::= { rlPolicyDscpMutationEntry 2 }


rlPolicyDscpMutationStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlPolicyDscpMutationEntry 3 }



-- Policy Port set per trust mode table


rlPolicyTrustModeTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyTrustModeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies the port state for the trusted basic mode"
    ::= { rlPolicyMapping 5 }

rlPolicyTrustModeEntry OBJECT-TYPE
    SYNTAX RlPolicyTrustModeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "describes the ports status  that belongs to the global trusted state "
    INDEX { rlPolicyTrustModePortNumber }
    ::= { rlPolicyTrustModeTable 1 }

RlPolicyTrustModeEntry::= SEQUENCE {
        rlPolicyTrustModePortNumber    INTEGER,
        rlPolicyTrustModePortState     INTEGER
    }

rlPolicyTrustModePortNumber OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "phisical port number ."
    ::= { rlPolicyTrustModeEntry 1 }

rlPolicyTrustModePortState OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "the port state for the trusted mode.
        the port can be enabled or disabled for the basic trust mode "
    ::= { rlPolicyTrustModeEntry 2 }

---  Policy DSCP to VPT mapping

rlPolicyDscpVptTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyDscpVptEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The DSCP to VPT map table"
    ::= { rlPolicyMapping 6 }

rlPolicyDscpVptEntry OBJECT-TYPE
    SYNTAX RlPolicyDscpVptEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes The VPT assigned to a Dscp value.
         The index is DSCP represent by rlPolicyDscpValue."
    INDEX { rlPolicyDscpValue }
    ::= { rlPolicyDscpVptTable 1 }

RlPolicyDscpVptEntry::= SEQUENCE {
        rlPolicyDscpValue                       INTEGER,
        rlPolicyVptValue                        INTEGER,
        rlPolicyDscpVptStatus                   RowStatus
    }


rlPolicyDscpValue OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "DSCP value."
    ::= { rlPolicyDscpVptEntry 1 }

rlPolicyVptValue OBJECT-TYPE
    SYNTAX INTEGER(0..7)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "VPT value."
    ::= { rlPolicyDscpVptEntry 2 }

rlPolicyDscpVptStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlPolicyDscpVptEntry 3 }


-- Policy DSCP to DP Table


rlPolicyDscpToDpTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyDscpToDpEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The DSCP
         To Dp table"
    ::= { rlPolicyMapping 7 }

rlPolicyDscpToDpEntry OBJECT-TYPE
    SYNTAX RlPolicyDscpToDpEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes the new
         DP for the packet.
         The index is DSCP represent by rlPolicyDscp"
    INDEX { rlPolicyDscp }
    ::= { rlPolicyDscpToDpTable 1 }

RlPolicyDscpToDpEntry::= SEQUENCE {
        rlPolicyDscp               INTEGER,
        rlPolicyDp                 INTEGER,
        rlPolicyDscpToDpStatus     RowStatus
    }

rlPolicyDscp OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Packet DSCP."
    ::= { rlPolicyDscpToDpEntry 1 }

rlPolicyDp OBJECT-TYPE
    SYNTAX INTEGER(0..2)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "New DP."
    ::= { rlPolicyDscpToDpEntry 2 }


rlPolicyDscpToDpStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlPolicyDscpToDpEntry 3 }



-- Policy Default Forwarding  Table


rlPolicyDefaultForwardingTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyDefaultForwardingEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies The default forwarding
         values : permit or deny for list of specific ports , vlans"
    ::= { rlPolicy 11 }

rlPolicyDefaultForwardingEntry OBJECT-TYPE
    SYNTAX RlPolicyDefaultForwardingEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Since the table is search to find match according to first match
         Entries with specific protocol should be set before entries for entire layer."
    INDEX { rlPolicyDefaultForwardingIndex }
    ::= { rlPolicyDefaultForwardingTable 1 }

RlPolicyDefaultForwardingEntry::= SEQUENCE {
        rlPolicyDefaultForwardingIndex              INTEGER,
        rlPolicyDefaultForwardingPortList           PortList,
        rlPolicyDefaultForwardingVlanId1To1024      VlanList1,
        rlPolicyDefaultForwardingVlanId1025To2048   VlanList2,
        rlPolicyDefaultForwardingVlanId2049To3072   VlanList3,
        rlPolicyDefaultForwardingVlanId3073To4096   VlanList4,
        rlPolicyDefaultForwardingLayer              INTEGER,
        rlPolicyDefaultForwardingAction             INTEGER,
        rlPolicyDefaultForwardingStatus             RowStatus,
        rlPolicyDefaultForwardingProtocol           INTEGER
    }

rlPolicyDefaultForwardingIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Default Forwarding Index."
    ::= { rlPolicyDefaultForwardingEntry 1 }

rlPolicyDefaultForwardingPortList OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Default Forwarding Port List."
    ::= { rlPolicyDefaultForwardingEntry 2 }


rlPolicyDefaultForwardingVlanId1To1024 OBJECT-TYPE
    SYNTAX  VlanList1
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "Default Forwarding VlanId List 1."
    ::= { rlPolicyDefaultForwardingEntry 3 }

rlPolicyDefaultForwardingVlanId1025To2048 OBJECT-TYPE
    SYNTAX  VlanList2
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "Default Forwarding VlanId List 2."
    ::= { rlPolicyDefaultForwardingEntry 4 }

rlPolicyDefaultForwardingVlanId2049To3072 OBJECT-TYPE
    SYNTAX  VlanList3
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "Default Forwarding VlanId List 3."
    ::= { rlPolicyDefaultForwardingEntry 5 }

rlPolicyDefaultForwardingVlanId3073To4096 OBJECT-TYPE
    SYNTAX  VlanList4
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "Default Forwarding VlanId List 4."
    ::= { rlPolicyDefaultForwardingEntry 6 }

rlPolicyDefaultForwardingLayer OBJECT-TYPE
    SYNTAX INTEGER {
        l2(1),
        l3(2),
        l3-ipv6(3)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "Default Forwarding Action specify layer l2 l3 l3-ipv6"
    ::= { rlPolicyDefaultForwardingEntry 7 }

rlPolicyDefaultForwardingAction OBJECT-TYPE
    SYNTAX  INTEGER{
        permit(1),
        deny(2)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "Default Forwarding Action specify permit or deny "
    ::= { rlPolicyDefaultForwardingEntry 8 }

rlPolicyDefaultForwardingStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlPolicyDefaultForwardingEntry 9 }

rlPolicyDefaultForwardingProtocol OBJECT-TYPE
    SYNTAX  INTEGER {
        bpdu(1),
        icmpv6(2),
        none(255)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The protocol type to be applied with the default action."
   DEFVAL{255}
    ::= { rlPolicyDefaultForwardingEntry 10 }

rlPolicyStatistics
        OBJECT IDENTIFIER ::= { rlPolicy 12 }

rlPolicyPortPolicyStatisticsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyPortPolicyStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies statistics counter for policies with specific actions"
    ::= { rlPolicyStatistics 1}

rlPolicyPortPolicyStatisticsEntry OBJECT-TYPE
    SYNTAX RlPolicyPortPolicyStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes counter per port.
        The index is port represent by rlIfIndex.
        In each entry represents counter, it's type , it's size and whether it's enabled. "
    INDEX { rlPolicyPortPolicyStatisticsIfIndex,rlPolicyPortPolicyStatisticsCntrType }
    ::= { rlPolicyPortPolicyStatisticsTable 1 }

RlPolicyPortPolicyStatisticsEntry::= SEQUENCE {
        rlPolicyPortPolicyStatisticsIfIndex               INTEGER,
        rlPolicyPortPolicyStatisticsCntrType              StatisticsCntrType,
        rlPolicyPolicyStatisticsCntrSize                  StatisticsCntrNumOfBitsType,
        rlPolicyPolicyStatisticsEnableCounting            TruthValue,
        rlPolicyPolicyStatisticsCounterValue              Counter64

    }

rlPolicyPortPolicyStatisticsIfIndex     OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Interface index."
    ::= { rlPolicyPortPolicyStatisticsEntry 1 }

rlPolicyPortPolicyStatisticsCntrType     OBJECT-TYPE
    SYNTAX StatisticsCntrType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter type."
    ::= { rlPolicyPortPolicyStatisticsEntry 2 }

rlPolicyPolicyStatisticsCntrSize     OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits."
    ::= { rlPolicyPortPolicyStatisticsEntry 3 }

rlPolicyPolicyStatisticsEnableCounting OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication whether the counter is enabled."
    DEFVAL { false }
    ::= { rlPolicyPortPolicyStatisticsEntry 4 }

rlPolicyPolicyStatisticsCounterValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        " Counter value. "
    ::= { rlPolicyPortPolicyStatisticsEntry 5 }


rlPolicyOutQueueStatisticsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyOutQueueStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes counter per any permutation of
        Port/VLAN/Queue/Drop Precedence . Each of the above can a group off 'All'.
        The index is port represent by  rlPolicyOutQueueStatisticsCountrID.
        In each entry there are fields representing
        whether the counter is enabled and counters value. "
    ::= { rlPolicyStatistics 2 }

rlPolicyOutQueueStatisticsEntry OBJECT-TYPE
    SYNTAX RlPolicyOutQueueStatisticsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry includes port, vlan, queue, drop precedence and counter value."
    INDEX { rlPolicyOutQueueStatisticsCountrID }
    ::= { rlPolicyOutQueueStatisticsTable 1 }

RlPolicyOutQueueStatisticsEntry::= SEQUENCE {
       rlPolicyOutQueueStatisticsCountrID                   INTEGER,
       rlPolicyOutQueueStatisticsIfIndexList                PortList,
       rlPolicyOutQueueStatisticsPortAll                    TruthValue,
       rlPolicyOutQueueStatisticsVlan                       INTEGER,
       rlPolicyOutQueueStatisticsVlanAll                    TruthValue,
       rlPolicyOutQueueStatisticsQueue                      INTEGER,
       rlPolicyOutQueueStatisticsQueueAll                   TruthValue,
       rlPolicyOutQueueStatisticsDP                         StatisticsDPType,
       rlPolicyOutQueueStatisticsDPAll                      TruthValue,
       rlPolicyOutQueueStatisticsCounterTailDropValue       Counter64,
       rlPolicyOutQueueStatisticsCounterAllValue            Counter64,
       rlPolicyOutQueueStatisticsCntrNumOfBits              StatisticsCntrNumOfBitsType,
       rlPolicyOutQueueStatisticsStatus                     RowStatus
    }

rlPolicyOutQueueStatisticsCountrID OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter id, the key of the table."
    ::= { rlPolicyOutQueueStatisticsEntry 1 }

rlPolicyOutQueueStatisticsIfIndexList OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Port for which the flow is counted."
    ::= { rlPolicyOutQueueStatisticsEntry 2 }

rlPolicyOutQueueStatisticsPortAll  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication for whether the port is configured as range of all the ports"
    DEFVAL { false }
    ::= { rlPolicyOutQueueStatisticsEntry 3}

rlPolicyOutQueueStatisticsVlan OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "VLAN for which the flow is counted."
    ::= { rlPolicyOutQueueStatisticsEntry 4 }

rlPolicyOutQueueStatisticsVlanAll  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication for whether the Vlan is configured as range of all the Vlans"
    DEFVAL { false }
    ::= { rlPolicyOutQueueStatisticsEntry 5}

rlPolicyOutQueueStatisticsQueue OBJECT-TYPE
    SYNTAX INTEGER(1..8)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Queue for which the flow is counted."
    ::= { rlPolicyOutQueueStatisticsEntry 6 }

rlPolicyOutQueueStatisticsQueueAll  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication for whether the Queue is configured as range of all the Queues"
    DEFVAL { false }
    ::= { rlPolicyOutQueueStatisticsEntry 7}

rlPolicyOutQueueStatisticsDP OBJECT-TYPE
    SYNTAX StatisticsDPType
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Drop Precedence for which the flow is counted."
    ::= { rlPolicyOutQueueStatisticsEntry 8 }

rlPolicyOutQueueStatisticsDPAll  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Indication for whether the DP is configured as range of all the DPs"
    DEFVAL { false }
    ::= { rlPolicyOutQueueStatisticsEntry 9}

rlPolicyOutQueueStatisticsCounterTailDropValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The counter for tail dropped value."
    ::= { rlPolicyOutQueueStatisticsEntry 10 }

rlPolicyOutQueueStatisticsCounterAllValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The counter for all traffic value."
    ::= { rlPolicyOutQueueStatisticsEntry 11 }

rlPolicyOutQueueStatisticsCntrNumOfBits       OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits for the counter."
    ::= { rlPolicyOutQueueStatisticsEntry 12 }

rlPolicyOutQueueStatisticsStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of a table entry.
         It is used to delete an entry from this table."
    ::= { rlPolicyOutQueueStatisticsEntry 13 }

-- Global Counter for statistics

rlPolicyGlobalStatisticsCntrsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyGlobalStatisticsCntrsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies statistics global counters  for specific rules for
         all ports that they are connected to "
    ::= { rlPolicyStatistics 3 }

rlPolicyGlobalStatisticsCntrsEntry OBJECT-TYPE
    SYNTAX RlPolicyGlobalStatisticsCntrsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry represents global counter."
    INDEX {rlPolicyGlobalStatisticsCntrsType}
    ::= { rlPolicyGlobalStatisticsCntrsTable 1 }

RlPolicyGlobalStatisticsCntrsEntry::= SEQUENCE {
       rlPolicyGlobalStatisticsCntrsType            StatisticsCntrType,
       rlPolicyGlobalStatisticsCntrsNumOfBits       StatisticsCntrNumOfBitsType,
       rlPolicyGlobalStatisticsCntrsCounterValue    Counter64,
       rlPolicyGlobalStatisticsStatus               RowStatus
}

rlPolicyGlobalStatisticsCntrsType          OBJECT-TYPE
    SYNTAX StatisticsCntrType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter type."
    ::= { rlPolicyGlobalStatisticsCntrsEntry 1 }

rlPolicyGlobalStatisticsCntrsNumOfBits          OBJECT-TYPE
    SYNTAX StatisticsCntrNumOfBitsType
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter size in bits."
    ::= { rlPolicyGlobalStatisticsCntrsEntry 2 }

rlPolicyGlobalStatisticsCntrsCounterValue OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Counter value."
    ::= { rlPolicyGlobalStatisticsCntrsEntry 3 }

rlPolicyGlobalStatisticsStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The status of a table entry.
         It is used to delete an entry from this table."
    ::= { rlPolicyGlobalStatisticsCntrsEntry 4 }

    -- clear scalar

rlPolicyClearCounters OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This scalar indicates to clear all the counters."
    ::= { rlPolicyStatistics 4 }

-- ********************
-- Classifier Utilization Table
-- ********************
    rlPolicyClassifierUtilization OBJECT IDENTIFIER
      ::= { rlPolicy 13 }


    rlPolicyClassifierUtilizationTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF RlPolicyClassifierUtilizationEntry
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "A table containing Classifier utilization information.
           Each row represents objects for a particular Unit
           present in this system."
      ::= { rlPolicyClassifierUtilization 1 }

    rlPolicyClassifierUtilizationEntry OBJECT-TYPE
      SYNTAX         RlPolicyClassifierUtilizationEntry
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "A Single entry containing Classifier utilization information."
      INDEX          { rlPolicyClassifierUtilizationUnitId }
      ::= { rlPolicyClassifierUtilizationTable 1 }

    RlPolicyClassifierUtilizationEntry ::= SEQUENCE {
      rlPolicyClassifierUtilizationUnitId            Unsigned32,
      rlPolicyClassifierUtilizationPercent           Unsigned32,
      rlPolicyClassifierUtilizationRulesNumber       Unsigned32
    }

     rlPolicyClassifierUtilizationUnitId OBJECT-TYPE
      SYNTAX         Unsigned32  (1..4294967295)
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "The Unit ID of this Classifier. must be unique per entry.
            This is an index into the table."
      ::= { rlPolicyClassifierUtilizationEntry 1 }


    rlPolicyClassifierUtilizationPercent OBJECT-TYPE
      SYNTAX         Unsigned32  (0..100)
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "The classifier utilization percentage. "
      DEFVAL { 0 }
      ::= { rlPolicyClassifierUtilizationEntry 2 }

    rlPolicyClassifierUtilizationRulesNumber OBJECT-TYPE
      SYNTAX         Unsigned32  (0..4294967295)
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "The classifier utilization number of used rules, in short rules resolution."
      DEFVAL { 0 }
      ::= { rlPolicyClassifierUtilizationEntry 3 }

    -- reserved tcs scalar

    rlPolicyIsTCAvailable OBJECT-TYPE
        SYNTAX     Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
            "This scalar indicates the number of currently reserved amount
             of traffic conditioners."
        ::= { rlPolicy 14 }

rlPolicyCPUSafeGuardEnable OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This scalar enables/disables CPU Safeguard."
    ::= { rlPolicy 15 }

rlPolicyQosModeGlobalCfgTable  OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPolicyQosModeGlobalCfgEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table responsible to set the global qos mode configuration:
        qos mode, qos trust mode, and if port are trusted by default in qos advanced
        mode."
    ::= { rlPolicy 16 }

rlPolicyQosModeGlobalCfgEntry OBJECT-TYPE
    SYNTAX RlPolicyQosModeGlobalCfgEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table responsible to set the global qos mode configuration:
        qos mode, qos trust mode, and if port are trusted by default in qos advanced
        mode.
        Current implemnetaion assumes only one entry exist."
    INDEX { rlPolicyGlobalIndex}
    ::= { rlPolicyQosModeGlobalCfgTable 1 }

RlPolicyQosModeGlobalCfgEntry ::= SEQUENCE {
    rlPolicyGlobalIndex                  INTEGER,
    rlPolicyGlobalQoSMode                RlPolicyQosMode,
    rlPolicyBasicGlobalTrustMode         RlPolicyTrustTypes,
    rlPolicyAdvcGlobalTrustMode          RlPolicyTrustTypes,
    rlPolicyPortTrustAdvancedMode        TruthValue,
    rlPolicyDscpMutationEnable           TruthValue,
    rlPolicyModeGlobalCfgStatus          RowStatus
    }

rlPolicyGlobalIndex OBJECT-TYPE
    SYNTAX     INTEGER
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entry index - currenly only one entry can exist, indexes hard coded with value '1'."
    ::= { rlPolicyQosModeGlobalCfgEntry 1 }

rlPolicyGlobalQoSMode OBJECT-TYPE
    SYNTAX     RlPolicyQosMode
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This field replaces deprecated scalar rlPolicyCliQosMode.
        Defines the global qos operation mode: disable, basic or advnaced. "
    ::= { rlPolicyQosModeGlobalCfgEntry 2 }

rlPolicyBasicGlobalTrustMode OBJECT-TYPE
    SYNTAX     RlPolicyTrustTypes
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This field replaces deprecated scalar rlPolicyCliBasicModeCfg.
        Defines the global qos trust operation mode when qos mode is basic. "
    ::= { rlPolicyQosModeGlobalCfgEntry 3 }

rlPolicyAdvcGlobalTrustMode OBJECT-TYPE
    SYNTAX     RlPolicyTrustTypes
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This field replaces deprecated scalar rlPolicyCliBasicModeCfg.
        Defines the global qos trust operation mode when qos mode is advanced. "
    ::= { rlPolicyQosModeGlobalCfgEntry 4 }

rlPolicyPortTrustAdvancedMode OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This field specified whether ports are set to trused or not-trusted by
        default when switching to qos advanced mode."
    DEFVAL{ false }
    ::= { rlPolicyQosModeGlobalCfgEntry 5 }

rlPolicyDscpMutationEnable  OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
         "This field indicates if dscp to dscp mutation mode is enable.
        It can be set to true in the following terms:
        1.rlQosGlobalTrustMode is in {dscp, vpt-dscp} ( rlQosGlobalQoSMode must be basic or advanced)
        2.if rlQosGlobalQoSMode is advanced then rlQoSPortTrustAdvancedMode must be set to true."
    DEFVAL{ false }
    ::= { rlPolicyQosModeGlobalCfgEntry 6}

rlPolicyModeGlobalCfgStatus OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "This status of entry action.
        In current implementation only one entry exist, therefor only status = active is
        acceptable."
    ::= { rlPolicyQosModeGlobalCfgEntry 7 }


END


