RADLAN-PORT-STATISTICS-MIB DEFINITIONS ::= BEGIN

-- -------------------------------------------------------------
-- PORT-STATISTICS MIB
-- Title:      Marvell Port-Statistics Private MIB
--             This Private MIB manages Port-Statistics display messages
-- Version:    8.00
-- Date:       06 April 2015
--
-- -------------------------------------------------------------

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Unsigned32,
    Counter64, Integer32                            FROM SNMPv2-SMI
    DisplayString, TEXTUAL-CONVENTION, TruthValue, 
    RowStatus                                       FROM SNMPv2-TC
    PortList                                        FROM Q-BRIDGE-MIB
    InterfaceIndex, ifIndex                         FROM IF-MIB
    rnd                                             FROM RADLAN-MIB;
    
----------------------------------------------------
--              MIBS definitions                  --
----------------------------------------------------

rlPortStat MODULE-IDENTITY
    LAST-UPDATED "201504060000Z"
    ORGANIZATION "Marvell Computer Communications Ltd."
    CONTACT-INFO
           "marvell.com"
    DESCRIPTION
           "This private MIB module for Port-Statistics"
    REVISION "201504060000Z"
    DESCRIPTION
           "Initial revision."
     ::= { rnd 223 }
     
     
PortStatisticsSubType ::= TEXTUAL-CONVENTION
     STATUS  current
     DESCRIPTION
         "Specifies port-statistic sub-type"
     SYNTAX INTEGER {
        second(1),
        minute(2),
        hour(3),
        day(4),
        week(5)
    }

PortStatisticsSampleClockSource ::= TEXTUAL-CONVENTION
     STATUS  current
     DESCRIPTION
         "Specifies port-statistic sample clock-source"
     SYNTAX INTEGER {
        internal(1),
        sntp(2),
        userDefined(3)
    }
    
PortStatisticsCounterName ::= TEXTUAL-CONVENTION
     STATUS  current
     DESCRIPTION
         "Specifies port-statistic counter-name"
     SYNTAX INTEGER {
        anyCounter(0),

        unicastFrameSent(1),
        broadcastFrameSent(2),
        multicastFrameSent(3),
        goodOctetsSent(4),
        txUtilization(5),
        goodUnicastFrameReceived(6),
        broadcastFrameReceived(7),
        multicastFrameReceived(8),
        rxErrorFrameReceived(9),
        totalOctetsReceived(10),
        rxUtilization(11),
        txRxUtilization(12),
        frames64B(13),
        frames65To127B(14),
        frames128To255B(15),
        frames256To511B(16),
        frames512To1023B(17),
        frames1024To1518B(18),

        dot3StatsFCSErrors(19),
        dot3StatsSingleCollisionFrames(20),
        dot3StatsLateCollisions(21),
        dot3StatsExcessiveCollisions(22),
        dot3StatsFrameTooLongs(23),
        dot3StatsInternalMacReceiveErrors(24),
        dot3InPauseFrames(25),
        dot3OutPauseFrames(26),
        etherStatsDropEvents(27),
        etherStatsCRCAlignErrors(28),
        etherStatsUndersizePkts(29),
        etherStatsOversizePkts(30),
        etherStatsFragments(31),
        etherStatsJabbers(32),
        etherStatsCollisions(33),

        goodOctetsReceived(34),
        badOctetsReceived(35),
        goodFrameSent(36),
        goodFrameReceived(37),

        snaPortUtilizationRxColor(38),
        snaPortUtilizationTxColor(39),

        poePowerConsumption(40),
        poePowerSavings(41),
        
        poeOverload(42),
        poeShort(43),
        poeDenied(44),     
        poeAbsent(45),     
        poeInvalidSignature(46),

        -- must be last
        lastCounterSpecifier(47)
    }
    
-----------------------------------
-- rlPortStatEnabledPorts (scalar)
-----------------------------------
rlPortStatEnabledPorts OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Port-set to determine from which port to collect port-statistics"
    ::= { rlPortStat 1 }
    
-----------------------------------
-- rlPortStatClearPorts (scalar)
-----------------------------------
-- this is an action MIB for clearing 
-- port-statistics history per-port
-----------------------------------
rlPortStatClearPorts OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Action MIB for clearing port-statistics history on a
         list of selected ports"
    ::= { rlPortStat 2 }

-----------------------------------
-- rlPortStatSampleTable
-----------------------------------
rlPortStatSampleTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPortStatSampleEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The table holds port-statistics for Ethernet ports
         This is a read-only MIB for presentation purposes."
    ::= {rlPortStat 3 }

rlPortStatSampleEntry  OBJECT-TYPE
    SYNTAX      RlPortStatSampleEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry in the rlPortStatSampleTable."
    INDEX    { rlPortStatSampleIfIndex,
               rlPortStatSampleStatSubType,
               rlPortStatSampleCounterName,
               rlPortStatSampleStatID }
    ::= { rlPortStatSampleTable 1 }
    
RlPortStatSampleEntry ::= SEQUENCE {
    -- keys
    rlPortStatSampleIfIndex                     InterfaceIndex,
    rlPortStatSampleStatSubType                 PortStatisticsSubType,
    rlPortStatSampleCounterName                 PortStatisticsCounterName,
    rlPortStatSampleStatID                      Unsigned32,
    -- fields
    rlPortStatSampleCollectionInterval          Unsigned32,
    rlPortStatSampleSystemCollectionTime        Unsigned32,
    rlPortStatSampleCollectionTime              Unsigned32,
    rlPortStatSampleCollectionTimeStr           DisplayString (SIZE(0..15)),
    rlPortStatSampleCounterValue                Counter64,
    rlPortStatSamplePartialFlag                 TruthValue,
    rlPortStatSampleClockSource                 PortStatisticsSampleClockSource
}

-----------------------------------
-- rlPortStatSampleTable Keys
------------------------------------

rlPortStatSampleIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Interface Index.
         This variable is a key in port-statistics table."
    ::= { rlPortStatSampleEntry 1 }
    
rlPortStatSampleStatSubType OBJECT-TYPE
    SYNTAX      PortStatisticsSubType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Port-statistic sub-type.
         This variable is a key in port-statistics table."
    ::= { rlPortStatSampleEntry 2 }
    
rlPortStatSampleCounterName OBJECT-TYPE
    SYNTAX      PortStatisticsCounterName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Port-statistic counter-name.
         This variable is a key in port-statistics table."
    ::= { rlPortStatSampleEntry 3 }
    
rlPortStatSampleStatID OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Statistics ID.
         This variable is a key in port-statistics table."
    ::= { rlPortStatSampleEntry 4 }

-----------------------------------
-- rlPortStatSampleTable Fields
------------------------------------

rlPortStatSampleCollectionInterval OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Port-statistic collection time interval (in seconds)."
    ::= { rlPortStatSampleEntry 5 }

rlPortStatSampleSystemCollectionTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system up-time when the samples were taken, 
         formatted in posix-time format"
    ::= { rlPortStatSampleEntry 6 }
    
rlPortStatSampleCollectionTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The absolute time when the samples were taken, 
         formatted in posix-time format"
    ::= { rlPortStatSampleEntry 7 }
    
rlPortStatSampleCollectionTimeStr OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..15))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The absolute time when the samples were taken, 
         in string format - 'hhmmssddMMYYYYw'
         where 'w' stands for weekDay (1-7)"
    ::= { rlPortStatSampleEntry 8 }

rlPortStatSampleCounterValue OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Port-Statistics counter value"
    ::= { rlPortStatSampleEntry 9 }
    
rlPortStatSamplePartialFlag OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether the collected statistics for
         the current entry are partial."
    ::= { rlPortStatSampleEntry 10 }

rlPortStatSampleClockSource OBJECT-TYPE
    SYNTAX      PortStatisticsSampleClockSource
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the clock-source used for marking the 
         collection-time of the collected sample"
    ::= { rlPortStatSampleEntry 11 }



-----------------------------------
-- rlPortStatLastSampleTable
-----------------------------------
rlPortStatLastSampleTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPortStatLastSampleEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The table holds the last sample from port-statistics. 
         This is a read-only MIB for presentation purposes."
    ::= { rlPortStat 4 }

rlPortStatLastSampleEntry  OBJECT-TYPE
    SYNTAX      RlPortStatLastSampleEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry in the rlPortStatLastSampleTable."
    INDEX    { rlPortStatLastSampleIfIndex,
               rlPortStatLastSampleStatSubType,
               rlPortStatLastSampleCounterName }
    ::= { rlPortStatLastSampleTable 1 }
    
RlPortStatLastSampleEntry ::= SEQUENCE {
    -- keys
    rlPortStatLastSampleIfIndex                     InterfaceIndex,
    rlPortStatLastSampleStatSubType                 PortStatisticsSubType,
    rlPortStatLastSampleCounterName                 PortStatisticsCounterName,
    -- fields
    rlPortStatLastSampleStatID                      Unsigned32,
    rlPortStatLastSampleCollectionInterval          Unsigned32,
    rlPortStatLastSampleSystemCollectionTime        Unsigned32,
    rlPortStatLastSampleCollectionTime              Unsigned32,
    rlPortStatLastSampleCollectionTimeStr           DisplayString (SIZE(0..15)),
    rlPortStatLastSampleCounterValue                Counter64,
    rlPortStatLastSamplePartialFlag                 TruthValue,
    rlPortStatLastSampleClockSource                 PortStatisticsSampleClockSource
}

-----------------------------------
-- rlPortStatLastSampleTable Keys
------------------------------------

rlPortStatLastSampleIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Interface Index.
         This variable is a key in port-statistics table."
    ::= { rlPortStatLastSampleEntry 1 }
    
rlPortStatLastSampleStatSubType OBJECT-TYPE
    SYNTAX      PortStatisticsSubType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Port-statistic sub-type.
         This variable is a key in port-statistics table."
    ::= { rlPortStatLastSampleEntry 2 }
    
rlPortStatLastSampleCounterName OBJECT-TYPE
    SYNTAX      PortStatisticsCounterName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Port-statistic counter-name.
         This variable is a key in port-statistics table."
    ::= { rlPortStatLastSampleEntry 3 }
    
-----------------------------------
-- rlPortStatLastSampleTable Fields
------------------------------------

rlPortStatLastSampleStatID OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Statistics ID.
         This variable is a key in port-statistics table."
    ::= { rlPortStatLastSampleEntry 4 }

rlPortStatLastSampleCollectionInterval OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Port-statistic collection time interval (in seconds)."
    ::= { rlPortStatLastSampleEntry 5 }

rlPortStatLastSampleSystemCollectionTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system up-time when the samples were taken, 
         formatted in posix-time format"
    ::= { rlPortStatLastSampleEntry 6 }
    
rlPortStatLastSampleCollectionTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The absolute time when the samples were taken, 
         formatted in posix-time format"
    ::= { rlPortStatLastSampleEntry 7 }
    
rlPortStatLastSampleCollectionTimeStr OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..15))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The absolute time when the samples were taken, 
         in string format - 'hhmmssddMMYYYYw'
         where 'w' stands for weekDay (1-7)"
    ::= { rlPortStatLastSampleEntry 8 }

rlPortStatLastSampleCounterValue OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Port-Statistics counter value"
    ::= { rlPortStatLastSampleEntry 9 }
    
rlPortStatLastSamplePartialFlag OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether the collected statistics for
         the current entry are partial."
    ::= { rlPortStatLastSampleEntry 10 }

rlPortStatLastSampleClockSource OBJECT-TYPE
    SYNTAX      PortStatisticsSampleClockSource
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the clock-source used for marking the 
         collection-time of the collected sample"
    ::= { rlPortStatLastSampleEntry 11 }


-----------------------------------
-- rlPortStatLastEventTable
-----------------------------------
rlPortStatLastEventTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlPortStatLastEventEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "This table holds records of the last time an ether-like counter
         changed its value and time when the change had occoured.
         This is a read-only MIB for presentation purposes."
    ::= {rlPortStat 5 }

rlPortStatLastEventEntry OBJECT-TYPE
    SYNTAX      RlPortStatLastEventEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry in the rlPortStatLastEventTable."
    INDEX    { rlPortStatLastEventIfIndex,
               rlPortStatLastEventCounterName }
    ::= { rlPortStatLastEventTable 1 }

RlPortStatLastEventEntry ::= SEQUENCE {
    -- keys
    rlPortStatLastEventIfIndex          InterfaceIndex,
    rlPortStatLastEventCounterName      PortStatisticsCounterName,
    -- fields
    rlPortStatLastEventSystemTime       Unsigned32,
    rlPortStatLastEventPosixTime        Unsigned32,
    rlPortStatLastEventTimeStr          DisplayString (SIZE(0..15)),
    rlPortStatLastEventCounter          PortStatisticsCounterName,
    rlPortStatLastEventCounterValue     Counter64
}


-----------------------------------
-- rlPortStatLastEventTable Keys
------------------------------------
rlPortStatLastEventIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Interface Index.
         This variable is a key in last-event table."
    ::= { rlPortStatLastEventEntry 1 }

rlPortStatLastEventCounterName OBJECT-TYPE
    SYNTAX      PortStatisticsCounterName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Port-statistic counter-name.
         use 'anyCounter' (0) enum value to extract the 
         last event that occoured in a given port / ifIndex.
         This variable is a key in last-event table."
    ::= { rlPortStatLastEventEntry 2 }

-----------------------------------
-- rlPortStatLastEventTable Fields
------------------------------------

rlPortStatLastEventSystemTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system up-time of the event, 
         formatted in posix-time format"
    ::= { rlPortStatLastEventEntry 3 } 


rlPortStatLastEventPosixTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The absolute time of the event, 
         formatted in posix-time format"
    ::= { rlPortStatLastEventEntry 4 }
      
rlPortStatLastEventTimeStr OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..15))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The absolute time of the event, 
         in string format - 'hhmmssddMMYYYYw'
         where 'w' stands for weekDay (1-7)"
    ::= { rlPortStatLastEventEntry 5 }
        
rlPortStatLastEventCounter OBJECT-TYPE
    SYNTAX      PortStatisticsCounterName
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Port-statistic counter-name"
    ::= { rlPortStatLastEventEntry 6 }
            
rlPortStatLastEventCounterValue OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Port-Statistics counter value"
    ::= { rlPortStatLastEventEntry 7 }

-----------------------------------
-- rlPortStatClearPOEConsumptionPorts (scalar)
-----------------------------------
-- this is an action MIB for clearing 
-- POE port-statistics history per-port
-----------------------------------
rlPortStatClearPOEConsumptionPorts OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Action MIB for clearing port-statistics POE consumption history on a
         list of selected ports"
    ::= { rlPortStat 6 }

-----------------------------------
-- rlPortStatPOECumulativeEnergySaved (scalar)
-----------------------------------
rlPortStatPOECumulativeEnergySaved OBJECT-TYPE
    SYNTAX           Counter64
    UNITS            "Watt*Hour"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "POE cumulative energy savings per system due to time-range feature in Watt*Hour units"
    ::= { rlPortStat 7 }

-----------------------------------
-- rlPortStatGreenEthCumulativeEnergySaved (scalar)
-----------------------------------
rlPortStatGreenEthCumulativeEnergySaved OBJECT-TYPE
    SYNTAX           Counter64
    UNITS            "Watt*Hour"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Green Ethernet cumulative energy savings per system in Watt*Hour units"
    ::= { rlPortStat 8 }

-----------------------------------
-- rlPortStatGreenEthEstimatedAnnualEnergySaved (scalar)
-----------------------------------
rlPortStatGreenEthEstimatedAnnualEnergySaved OBJECT-TYPE
    SYNTAX           Counter64
    UNITS            "Watt*Hour"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Green Ethernet estimated anual energy savings per system in Watt*Hour units
		 Annual estimate is based on the saving during the previous week multiplied by 52"
    ::= { rlPortStat 9 }

-----------------------------------
-- rlPortStatClearPortEventsCategory (scalar)
-----------------------------------
rlPortStatClearPortEventsCategory  OBJECT-TYPE
	SYNTAX INTEGER {
		macCounters(1),
		poeCounters(2)
	}
	MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Scalar for determining the type of counters to be cleared 
		 when invoking rlPortStatClearPortEvents action MIB"
    ::= { rlPortStat 10 }

-----------------------------------
-- rlPortStatClearPortEvents (scalar)
-----------------------------------
rlPortStatClearPortEvents OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Action MIB for clearing port-statistics event history on a
         list of selected ports"
    ::= { rlPortStat 11 }

-----------------------------------
-- rlPortStatPOEEstimatedAnnualEnergySaved (scalar)
-----------------------------------
rlPortStatPOEEstimatedAnnualEnergySaved OBJECT-TYPE
    SYNTAX           Counter64
    UNITS            "Watt*Hour"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "PoE estimated anual energy savings per system in Watt*Hour units
		 Annual estimate is based on the saving during the previous week multiplied by 52"
    ::= { rlPortStat 12 }

-----------------------------------
-- rlPortStatPOEEstimatedAnnualEnergySavedAvailable (scalar)
-----------------------------------
rlPortStatPOEEstimatedAnnualEnergySavedAvailable OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Determines wether PoE estimated anual energy savings is available.
		 Annual estimate is available when device contains energy-savings statistics from
		 previous week."
    ::= { rlPortStat 13 }

-----------------------------------
-- rlPortStatGreenEthEstimatedAnnualEnergySavedAvailable (scalar)
-----------------------------------
rlPortStatGreenEthEstimatedAnnualEnergySavedAvailable OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Determines wether Green Ethernet estimated anual energy savings is available.
		 Annual estimate is available when device contains energy-savings statistics from
		 previous week."
    ::= { rlPortStat 14 }

-----------------------------------
-- rlPortStatPOECurrentEnergySaved (scalar)
-----------------------------------
rlPortStatPOECurrentEnergySaved OBJECT-TYPE
    SYNTAX           Counter64
    UNITS            "Watt*Hour"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "POE current energy savings per system due to time-range feature in Watt*Hour units"
    ::= { rlPortStat 15 }

-----------------------------------
-- rlPortStatClearGreenEthCumulativeEnergySaved (scalar)
-----------------------------------
-- this is an action MIB for clearing 
-- Green-Ethernet cumulative energy saved
-----------------------------------
rlPortStatClearGreenEthCumulativeEnergySaved OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Action MIB for setting Green-Ethernet-Cumulative-Energy-Saved value to zero."
    ::= { rlPortStat 16 }

-----------------------------------
-- rlPortStatEnabled (scalar)
-----------------------------------
rlPortStatEnabled OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Determine whether port-statistics is globally enabled or disabled"
    ::= { rlPortStat 17 }

END
    