ELTEX-VPC-MIB DEFINITIONS ::= BEGIN

-- Title:   ELTEX VPC MIB
-- Version: 1.0
-- Date:    17 September 2018

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Unsigned32, IpAddress
         FROM SNMPv2-SMI

    TruthValue, RowStatus, MacAddress, DisplayString
         FROM SNMPv2-TC

    InterfaceIndexOrZero
         FROM IF-MIB

    eltexLtd
         FROM ELTEX-SMI-ACTUAL

    VlanList1, VlanList2, VlanList3, VlanList4
         FROM RADLAN-BRIDGEMIBOBJECTS-MIB;

eltexVpcMIB MODULE-IDENTITY
    LAST-UPDATED "201810310000Z"
    ORGANIZATION "Eltex Enterprise, Ltd."
        CONTACT-INFO
          "www.eltex-co.ru"
    DESCRIPTION
        "The ELTEX-VPC-MIB is used for management of the VPC(MLAG) configuration"
    REVISION     "201809170000Z"
    DESCRIPTION  "Initial revision of ELTEX-VPC-MIB."
    ::= { eltexLtd 125 }
    
--**************************************************************************************
-- Textual Conventions.




eltexVpcMIBObjects                  OBJECT IDENTIFIER ::= { eltexVpcMIB 1 }

--**************************************************************************************
-- eltexVpcConfigGroup
--
--**************************************************************************************

  eltexVpcConfigGroup            OBJECT IDENTIFIER ::= { eltexVpcMIBObjects 1 }

     eltexVpcMode OBJECT-TYPE
         SYNTAX      INTEGER {
                     enabled(1),
                     disabled(2)
                  }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To enable VPC globally. The VPC role election happens if both
                      the VPC feature is enabled and if the keepalive state machine is
                      enabled.
                      The following options are supported:

                      Note: VPC is supported only on standalone device. VPC is not supported on
                      stacked devices. VPC behavior is undefined if the device is stacked with
                      one another.
                     "
          ::= { eltexVpcConfigGroup 1 }

     eltexVpcDomainConfigTable        OBJECT-TYPE
         SYNTAX        SEQUENCE OF EltexVpcDomainConfigEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain config table."
          ::= { eltexVpcConfigGroup 2 }

     eltexVpcDomainConfigEntry       OBJECT-TYPE
         SYNTAX        EltexVpcDomainConfigEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain config entry."
         INDEX         { eltexVpcDomainIndex }
          ::= { eltexVpcDomainConfigTable 1 }

     EltexVpcDomainConfigEntry ::= SEQUENCE {
         eltexVpcDomainIndex
             Unsigned32,
         eltexVpcDomainPeerLink
             InterfaceIndexOrZero,
         eltexVpcDomainKeepalivePriority
             Unsigned32,
         eltexVpcDomainKeepaliveTimeout
             Unsigned32,
         eltexVpcDomainKeepaliveMode
             INTEGER,
         eltexVpcDomainSystemMac
             MacAddress,
         eltexVpcDomainSystemPriority
             Unsigned32,
         eltexVpcDomainPeerDetectionMode
             INTEGER,
         eltexVpcDomainPeerDetectionInterval
             Unsigned32,
         eltexVpcDomainPeerDetectionTimeout
             Unsigned32,
         eltexVpcDomainPeerIpAddr
             IpAddress,
         eltexVpcDomainSourceIpAddr
             IpAddress,
         eltexVpcDomainDcpdpUdpPort
             Unsigned32,
         eltexVpcDomainStatus
             RowStatus,
         eltexVpcDomainInitialWaitTimeout
             Unsigned32,
         eltexVpcDomainMrid
             Unsigned32,
         eltexVpcPeerGatewayIncludeVlanList1to1024
             VlanList1,
         eltexVpcPeerGatewayIncludeVlanList1025to2048
             VlanList2,
         eltexVpcPeerGatewayIncludeVlanList2049to3072
             VlanList3,
         eltexVpcPeerGatewayIncludeVlanList3073to4094
             VlanList4,
         eltexVpcPeerGatewayIncludeVlanAll
             TruthValue
         }

    eltexVpcDomainIndex   OBJECT-TYPE
         SYNTAX      Unsigned32(1..255)
         MAX-ACCESS  read-write 
         STATUS      current
         DESCRIPTION
                     "VPC Domain ID."
          ::= { eltexVpcDomainConfigEntry 1 }

     eltexVpcDomainPeerLink OBJECT-TYPE
         SYNTAX      InterfaceIndexOrZero
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configures a port channel as the VPC peer link.
                      The configurable range is a valid port channel interface index."
          ::= { eltexVpcDomainConfigEntry 2 }
          
    eltexVpcDomainKeepalivePriority OBJECT-TYPE
         SYNTAX      Unsigned32(1..255)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure the priority of the VPC switch. This value is used
                      for the VPC role election.
                      Note: The VPC switch with lower priority becomes the Primary. If
                            both the VPC peer switches have the same role priority, the
                            device with lower system MAC address becomes the Primary.
                            "
          DEFVAL {100}
          ::= { eltexVpcDomainConfigEntry 3 }

    eltexVpcDomainKeepaliveTimeout OBJECT-TYPE
         SYNTAX      Unsigned32(2..15)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure the peer keepalive timeout value (in seconds). If
                      an VPC switch does not receive keepalive messages from the peer
                      for this timeout value, it takes the decision to transition its
                      role (if required).
                      Note: The keepalive state machine is not restarted if keepalive
                      priority is modified post election."
          DEFVAL {5}
          ::= { eltexVpcDomainConfigEntry 4 }

      eltexVpcDomainKeepaliveMode OBJECT-TYPE
         SYNTAX      INTEGER {
                     enabled(1),
                     disabled(2)
                  }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To start/stop the keepalive state machine on the VPC device, if
                     VPC is globally enabled."
          DEFVAL {disabled}
          ::= { eltexVpcDomainConfigEntry 5 }

     eltexVpcDomainSystemMac OBJECT-TYPE
         SYNTAX      MacAddress
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure the MAC address for the VPC domain. This mac-address 
                     is used in the LACP PDUs and STP BPDUs 
                     that are sent out on VPC member ports. For the VPC domain to use 
                     the manually configured VPC MAC address, it should be manually 
                     configured on both the VPC peers and should be the same. If VPC 
                     is configured on only one of the VPC peers or is configured 
                     different on VPC peers, auto-generated MAC address is used. 
                     The specified MAC address should be a unicast MAC address in 
                     <aa:bb:cc:dd:ee:ff> format and should not be equal to the 
                     MAC address of either primary VPC or secondary VPC device.  
                     The manually configured VPC MAC address is used instead of 
                     auto-generated VPC MAC address only if the VPC feature is 
                     re-enabled after configuring the VPC MAC address."

          ::= { eltexVpcDomainConfigEntry 6 }

     eltexVpcDomainSystemPriority OBJECT-TYPE
         SYNTAX      Unsigned32(1..65535)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure the system priority for the VPC domain. This is used 
                      in the STP BPDU sent out on VPC member ports. System-priority 
                      should be configured same on both the VPC peers. If the configured 
                      VPC system priority is different on VPC peers, then VPC will not 
                      come up."
          DEFVAL {32768}
          ::= { eltexVpcDomainConfigEntry 7 }

 eltexVpcDomainPeerDetectionMode OBJECT-TYPE
         SYNTAX      INTEGER {
                     enabled(1),
                     disabled(2)
                  }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To start/stop the dual control peer detection protocol on the
                      VPC switch.
                      The following options are supported:

                      Note: The peer VPC switch's IP address has to be configured for
                            the peer detection protocol to start on an VPC switch."
         DEFVAL {disabled}
          ::= { eltexVpcDomainConfigEntry 8 }
          
     eltexVpcDomainPeerDetectionInterval OBJECT-TYPE
         SYNTAX      Unsigned32(200..4000)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure the peer detection protocol transmission interval.
                     Configurable range is 200 to 4000 mseconds."
         DEFVAL {700}
          ::= { eltexVpcDomainConfigEntry 9 }

     eltexVpcDomainPeerDetectionTimeout OBJECT-TYPE
         SYNTAX      Unsigned32(700..14000)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure the peer detection protocol reception timeout.
                     Configurable range is 700 to 14000 mseconds."
         DEFVAL {5000}
          ::= { eltexVpcDomainConfigEntry 10 }

     eltexVpcDomainPeerIpAddr OBJECT-TYPE
         SYNTAX      IpAddress
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure IP address of the peer VPC switch. This
                      configuration is used by the dual control plane detection
                      protocol on the VPC switches.

                      NOTE: In order to set value for the object, need to set values for 
                      IP address of the peer VPC switch and destination IP of the peer 
                      detection protocol message simultaneously."
          DEFVAL {'00000000'H}
          ::= { eltexVpcDomainConfigEntry 11 }

     eltexVpcDomainSourceIpAddr OBJECT-TYPE
         SYNTAX      IpAddress
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure Self IP address of the VPC switch that is used as
                      the source IP by the dual control plane detection protocol 
                      on the VPC switches.

                      NOTE: In order to set value for the object, need to set values for 
                      IP address of the peer VPC switch and destination IP of the peer 
                      detection protocol message simultaneously."
          DEFVAL {'00000000'H}
          ::= { eltexVpcDomainConfigEntry 12 }

     eltexVpcDomainDcpdpUdpPort OBJECT-TYPE
         SYNTAX      Unsigned32(1..65535)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure the UDP port on which the VPC switch listens to
                      the peer detection protocol messages."
         DEFVAL {50000}
          ::= { eltexVpcDomainConfigEntry 13 }

     eltexVpcDomainStatus OBJECT-TYPE
         SYNTAX      RowStatus
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                       "Status of VPC Domain."
          ::= { eltexVpcDomainConfigEntry 14 }

     eltexVpcDomainInitialWaitTimeout OBJECT-TYPE
         SYNTAX      Unsigned32(60..1800)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "To configure the initial-wait timeout value (in seconds).
                      If after system start a VPC switch does not receive
                      keepalive or peer detection messages from the peer,
                      it will remain in the standby state until the initial-wait timer expires."
          DEFVAL {60}
          ::= { eltexVpcDomainConfigEntry 15 }

     eltexVpcDomainMrid OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "MRID that is used for peer detection."
         DEFVAL {1}
          ::= { eltexVpcDomainConfigEntry 16 }

     eltexVpcPeerGatewayIncludeVlanList1to1024 OBJECT-TYPE
         SYNTAX      VlanList1
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Peer gateway include from 1 to 1024.
                      Default value is {0}"
         DEFVAL {'00'H}
          ::= { eltexVpcDomainConfigEntry 17 }

     eltexVpcPeerGatewayIncludeVlanList1025to2048 OBJECT-TYPE
         SYNTAX      VlanList2
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Peer gateway include from 1025 to 2048.
                      Default value is {0}"
         DEFVAL {'00'H}
          ::= { eltexVpcDomainConfigEntry 18 }

     eltexVpcPeerGatewayIncludeVlanList2049to3072 OBJECT-TYPE
         SYNTAX      VlanList3
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Peer gateway include from 2049 to 3072.
                      Default value is {0}"
         DEFVAL {'00'H}
          ::= { eltexVpcDomainConfigEntry 19 }

     eltexVpcPeerGatewayIncludeVlanList3073to4094 OBJECT-TYPE
         SYNTAX      VlanList4
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Peer gateway include from 3073 to 4094.
                      Default value is {0}"
         DEFVAL {'00'H}
          ::= { eltexVpcDomainConfigEntry 20 }

     eltexVpcPeerGatewayIncludeVlanAll OBJECT-TYPE
         SYNTAX      TruthValue
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "This field indicates whether the bridge should automatically
                      include all available static VLANs in the peer gateway."
         DEFVAL {false}
          ::= { eltexVpcDomainConfigEntry 21 }


--**************************************************************************************
-- eltexVpcGroupStatus
--
--**************************************************************************************

     eltexVpcGroupConfigTable        OBJECT-TYPE
         SYNTAX      SEQUENCE OF EltexVpcGroupConfigEntry 
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "VPC group config table."
          ::= { eltexVpcConfigGroup 3 }

     eltexVpcGroupConfigEntry       OBJECT-TYPE
         SYNTAX         EltexVpcGroupConfigEntry
         MAX-ACCESS     not-accessible
         STATUS         current
         DESCRIPTION    
                      "VPC status entry."
          INDEX    {eltexVpcGroupIndex}
          ::= {  eltexVpcGroupConfigTable 1 }

     EltexVpcGroupConfigEntry  ::= SEQUENCE {
          eltexVpcGroupIndex
              Unsigned32,
          eltexVpcGroupDomainIndex
              Unsigned32,
          eltexVpcGroupPortChannelIfIndex
              InterfaceIndexOrZero,
          eltexVpcGroupOperationalStatus
              INTEGER,
          eltexVpcGroupInterfaceState
              INTEGER,
          eltexVpcGroupStatus
             RowStatus
          }

     eltexVpcGroupIndex      OBJECT-TYPE
          SYNTAX        Unsigned32 (1..63)
          MAX-ACCESS    read-write
          STATUS        current
          DESCRIPTION   
                        "VPC group Index."
             ::= {eltexVpcGroupConfigEntry 1}

    eltexVpcGroupDomainIndex   OBJECT-TYPE
         SYNTAX      Unsigned32(0..255)
         MAX-ACCESS  read-write 
         STATUS      current
         DESCRIPTION
                     "VPC Domain Index uncluded Vpc Group"
         DEFVAL {0}
          ::= { eltexVpcGroupConfigEntry 2 }
          
     eltexVpcGroupPortChannelIfIndex      OBJECT-TYPE
          SYNTAX        InterfaceIndexOrZero
          MAX-ACCESS    read-write
          STATUS        current
          DESCRIPTION
                      "To configures a port channel as the VPC group member port.
                      The configurable range is a valid port channel interface index."
          DEFVAL{0}
             ::= {eltexVpcGroupConfigEntry 3}

     eltexVpcGroupOperationalStatus    OBJECT-TYPE
          SYNTAX        INTEGER {
                          enabled (1),
                          disabled (2)
                        }
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "VPC operational status."
             ::= {eltexVpcGroupConfigEntry 4}

     eltexVpcGroupInterfaceState   OBJECT-TYPE
          SYNTAX        INTEGER {
                          disabled (1),
                          wait     (2),
                          error    (3),
                          active   (4),
                          inactive (5)
                        }
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "The following states of a VPC port-channel interface mean:
                         DISABLE:  The state of a port-channel before VPC functionality is enabled on it.
                         WAIT:     The VPC port-channel 'waits' for the VPC functionality 
                                   to be enabled on a port-channel of the peer switch.
                         ERROR:    After VPC is enabled on a port-channel of both peer switches, 
                                   the DOT3AD component checks to see if all entry criteria are met 
                                   for the port-channel to be operational. 
                         ACTIVE:   If the entry criteria are satisfied, then the VPC interface is set 
                                   to ACTIVE and is operationally enabled. 
                                   Traffic is now allowed to flow through the VPC member ports.
                         INACTIVE: If links connected to the VPC member ports are down, 
                                   then the VPC interface is set to INACTIVE on the switch. 
                                   The VPC will remain ACTIVE on the peer switch."
             ::= {eltexVpcGroupConfigEntry 5}          

    eltexVpcGroupStatus OBJECT-TYPE
         SYNTAX      RowStatus
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                       "Status of VPC Group."
          ::= { eltexVpcGroupConfigEntry 6}

--**************************************************************************************
-- eltexVpcStatusGroup
--
--**************************************************************************************

  eltexVpcStatusGroup                      OBJECT IDENTIFIER ::= { eltexVpcMIBObjects 2 }

--**************************************************************************************
-- eltexVpcDomainStatusTable
--
--**************************************************************************************
     eltexVpcDomainStatusTable        OBJECT-TYPE
         SYNTAX        SEQUENCE OF EltexVpcDomainStatusEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain stats table."
          ::= { eltexVpcStatusGroup 1 }

     eltexVpcDomainStatusEntry       OBJECT-TYPE
         SYNTAX        EltexVpcDomainStatusEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain stats entry."
         INDEX         { eltexVpcDomainIndex }
          ::= { eltexVpcDomainStatusTable 1 }

     EltexVpcDomainStatusEntry ::= SEQUENCE {
         eltexVpcDomainTotalVpcConfigured
             Unsigned32,
         eltexVpcDomainTotalVpcOperational
             Unsigned32,
         eltexVpcDomainSelfRole
             INTEGER,
         eltexVpcDomainOperationMode
             INTEGER,
         eltexVpcDomainState
             INTEGER,
         eltexVpcDomainOperationalSystemPriority
             Unsigned32,
         eltexVpcDomainOperationalMac
             MacAddress,
         eltexVpcDomainLocalSystemMac
             MacAddress,
         eltexVpcDomainPeerRole
             INTEGER,
         eltexVpcDomainPeerRolePriority
             Unsigned32,
         eltexVpcDomainPeerConfSystemPriority
             Unsigned32,
         eltexVpcDomainPeerOperSystemPriority
             Unsigned32,
         eltexVpcDomainPeerConfMac
             MacAddress,
         eltexVpcDomainPeerOperMac
             MacAddress,
         eltexVpcDomainPeerLocalSystemMac
             MacAddress,
         eltexVpcDomainPeerKeepaliveDetected
             TruthValue,
         eltexVpcDomainPeerDetectionStatus
             TruthValue,
         eltexVpcDomainPeerDetectionDetected
             TruthValue
         }
          
     eltexVpcDomainTotalVpcConfigured   OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of VPC's configured."
          ::= { eltexVpcDomainStatusEntry 1 }
          
     eltexVpcDomainTotalVpcOperational    OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of VPC's operational."
          ::= { eltexVpcDomainStatusEntry 2 }
          
     eltexVpcDomainSelfRole              OBJECT-TYPE
         SYNTAX      INTEGER {
                       none (1),
                       primary (2),
                       secondary (3)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "VPC role."
          ::= { eltexVpcDomainStatusEntry 3 }

     eltexVpcDomainOperationMode    OBJECT-TYPE
          SYNTAX        INTEGER {
                          enabled  (1),
                          disabled (2)
                        }
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "VPC operational mode."
           ::= { eltexVpcDomainStatusEntry 4 }

     eltexVpcDomainState            OBJECT-TYPE
          SYNTAX        INTEGER {
                          disabled  (1),
                          listen    (2),
                          ready     (3),
                          primary   (4),
                          secondary (5)
                        }
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "The following states of a VPC mean:
                        DISABLE:   In this state, the VPC interfaces, if any are shut down.
                        LISTEN:    The keepalive does not advertise any packets.
                        READY:     The keepalive component starts sending keepalive messages periodically with the state as READY.
                        PRIMARY:   Traffic over VPC interfaces is allowed to be forwarded. 
                                   The keepalive protocol continues to advertise keepalive messages with the state as PRIMARY.
                        SECONDARY: Traffic over VPC interfaces is allowed to be forwarded. 
                                   The keepalive protocol continues to advertise keepalive messages with the state as SECONDARY."
           ::= { eltexVpcDomainStatusEntry 5 }

     eltexVpcDomainOperationalSystemPriority OBJECT-TYPE
         SYNTAX      Unsigned32(1..65535)
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "To operational the system priority for the VPC domain. This is used 
                      in the LACP PDUs sent out on VPC member ports."
            ::= { eltexVpcDomainStatusEntry 6 }

     eltexVpcDomainOperationalMac   OBJECT-TYPE
         SYNTAX      MacAddress
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Operational MAC address for the VPC domain. This mac-address 
                     is used in the LACP PDUs and STP BPDUs that are sent out on 
                     VPC member ports."
            ::= { eltexVpcDomainStatusEntry 7 }

     eltexVpcDomainLocalSystemMac   OBJECT-TYPE
         SYNTAX      MacAddress
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Local system MAC."
            ::= { eltexVpcDomainStatusEntry 8 }

     eltexVpcDomainPeerRole         OBJECT-TYPE
          SYNTAX        INTEGER {
                          none      (1),
                          primary   (2),
                          secondary (3)
                        }
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
                        "Vpc peer role."
            ::= { eltexVpcDomainStatusEntry 9 }

     eltexVpcDomainPeerRolePriority     OBJECT-TYPE
          SYNTAX        Unsigned32
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "VPC peer role priority."
            ::= { eltexVpcDomainStatusEntry 10 }

     eltexVpcDomainPeerConfSystemPriority     OBJECT-TYPE
          SYNTAX        Unsigned32
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "VPC peer configured system priority."
            ::= { eltexVpcDomainStatusEntry 11 }

     eltexVpcDomainPeerOperSystemPriority     OBJECT-TYPE
          SYNTAX        Unsigned32
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "VPC peer operational system priority."
            ::= { eltexVpcDomainStatusEntry 12 }
           
     eltexVpcDomainPeerConfMac    OBJECT-TYPE
          SYNTAX        MacAddress
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "VPC peer configured MAC address."
            ::= { eltexVpcDomainStatusEntry 13 }
           
     eltexVpcDomainPeerOperMac    OBJECT-TYPE
          SYNTAX        MacAddress
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "VPC peer operational MAC address."
            ::= { eltexVpcDomainStatusEntry 14 }

     eltexVpcDomainPeerLocalSystemMac   OBJECT-TYPE
         SYNTAX      MacAddress
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer local system MAC."
            ::= { eltexVpcDomainStatusEntry 15 }

     eltexVpcDomainPeerKeepaliveDetected   OBJECT-TYPE
         SYNTAX        TruthValue
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
                       "Indicates if the VPC peer is detected over peer-link with keepalive protocol."
            ::= { eltexVpcDomainStatusEntry 16 }

     eltexVpcDomainPeerDetectionStatus    OBJECT-TYPE
          SYNTAX        TruthValue
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "VPC peer detection status."
           ::= { eltexVpcDomainStatusEntry 17 }

     eltexVpcDomainPeerDetectionDetected   OBJECT-TYPE
          SYNTAX        TruthValue
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "Indicates if the VPC peer is detected over peer detection protocol (l3 network)."
           ::= { eltexVpcDomainStatusEntry 18 }

--**************************************************************************************
-- eltexVpcDomainPeerKeepAliveStatsTable
--
--**************************************************************************************
     eltexVpcDomainPeerKeepAliveStatsTable        OBJECT-TYPE
         SYNTAX        SEQUENCE OF EltexVpcDomainPeerKeepAliveStatsEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain KeepAlive stats table."
          ::= { eltexVpcStatusGroup 2 }

     eltexVpcDomainPeerKeepAliveStatsEntry       OBJECT-TYPE
         SYNTAX        EltexVpcDomainPeerKeepAliveStatsEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain KeepAliveStats entry."
         INDEX         { eltexVpcDomainIndex }
          ::= { eltexVpcDomainPeerKeepAliveStatsTable 1 }

     EltexVpcDomainPeerKeepAliveStatsEntry ::= SEQUENCE {
         eltexVpcDomainKeepaliveOperationalMode
             INTEGER,    
         eltexVpcDomainPeerKeepAliveTotalTx
             Unsigned32,
         eltexVpcDomainPeerKeepAliveSuccessTx
             Unsigned32,
         eltexVpcDomainPeerKeepAliveTxErrors
             Unsigned32,
         eltexVpcDomainPeerKeepAliveTotalRx
             Unsigned32,
         eltexVpcDomainPeerKeepAliveSuccessRx
             Unsigned32,
         eltexVpcDomainPeerKeepAliveRxErrors
             Unsigned32,
         eltexVpcDomainPeerKeepAliveTimeoutCount
             Unsigned32
         }

     eltexVpcDomainKeepaliveOperationalMode    OBJECT-TYPE
          SYNTAX        INTEGER {
                          enabled  (1),
                          disabled (2)
                        }
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION
                        "VPC keepalive operational mode."
           ::= { eltexVpcDomainPeerKeepAliveStatsEntry 1 }
             
    eltexVpcDomainPeerKeepAliveTotalTx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Total Packets transmitted"
          ::= { eltexVpcDomainPeerKeepAliveStatsEntry 2 }

    eltexVpcDomainPeerKeepAliveSuccessTx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Successfully Transmitted Packets."
          ::= { eltexVpcDomainPeerKeepAliveStatsEntry 3 }

    eltexVpcDomainPeerKeepAliveTxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Transmit Failed Packets."

          ::= { eltexVpcDomainPeerKeepAliveStatsEntry 4 }

     eltexVpcDomainPeerKeepAliveTotalRx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Total Packets Received."
          ::= { eltexVpcDomainPeerKeepAliveStatsEntry 5 }

     eltexVpcDomainPeerKeepAliveSuccessRx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Successfully Received Packets."
          ::= { eltexVpcDomainPeerKeepAliveStatsEntry 6 }

      eltexVpcDomainPeerKeepAliveRxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of packets received with errors."
          ::= { eltexVpcDomainPeerKeepAliveStatsEntry 7 }

      eltexVpcDomainPeerKeepAliveTimeoutCount OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Timeout counter."
          ::= { eltexVpcDomainPeerKeepAliveStatsEntry 8 }


--**************************************************************************************
-- eltexVpcPeerLinkStatsTable
--
--**************************************************************************************
     eltexVpcDomainPeerLinkStatsTable        OBJECT-TYPE
         SYNTAX        SEQUENCE OF EltexVpcDomainPeerLinkStatsEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain PeerLink stats table."
          ::= { eltexVpcStatusGroup 3 }

     eltexVpcDomainLinkStatsEntry       OBJECT-TYPE
         SYNTAX        EltexVpcDomainPeerLinkStatsEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain KeepAliveStats entry."
         INDEX         { eltexVpcDomainIndex }
          ::= { eltexVpcDomainPeerLinkStatsTable 1 }

     EltexVpcDomainPeerLinkStatsEntry ::= SEQUENCE {
         eltexVpcDomainPeerLinkStatus
             TruthValue,
         eltexVpcDomainPeerLinkControlMsgTx
             Unsigned32,
         eltexVpcDomainPeerLinkTxErrors
             Unsigned32,
         eltexVpcDomainPeerLinkTxTimeout
             Unsigned32,
         eltexVpcDomainPeerLinkControlMsgAckTx
             Unsigned32,
         eltexVpcDomainPeerLinkControlMsgAckErrors
             Unsigned32,
         eltexVpcDomainPeerLinkControlMsgRx
             Unsigned32,
         eltexVpcDomainPeerLinkDataMsgTx
             Unsigned32,
         eltexVpcDomainPeerLinkDataMsgTxErrors
             Unsigned32,
         eltexVpcDomainPeerLinkDataMsgTxTimeout
             Unsigned32,
         eltexVpcDomainPeerLinkDataMsgRx
             Unsigned32,
         eltexVpcDomainPeerLinkBPDUTx
             Unsigned32,
         eltexVpcDomainPeerLinkBPDUTxErrors
             Unsigned32,
         eltexVpcDomainPeerLinkBPDURx
             Unsigned32,
         eltexVpcDomainPeerLinkBPDURxErrors
             Unsigned32,
         eltexVpcDomainPeerLinkLACPDUTx
             Unsigned32,
         eltexVpcDomainPeerLinkLACPDUTxErrors
             Unsigned32,
         eltexVpcDomainPeerLinkLACPDURx
             Unsigned32,
         eltexVpcDomainPeerLinkLACPDURxErrors
             Unsigned32,
         eltexVpcDomainPeerLinkBulkTx
             Unsigned32,
         eltexVpcDomainPeerLinkBulkTxTimeout
             Unsigned32,
         eltexVpcDomainPeerLinkBulkTxErrors
             Unsigned32,
         eltexVpcDomainPeerLinkBulkRx
             Unsigned32,
         eltexVpcDomainPeerLinkBulkRxErrors
             Unsigned32
         }

     eltexVpcDomainPeerLinkStatus    OBJECT-TYPE
         SYNTAX      TruthValue
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link operational status."
          ::= { eltexVpcDomainLinkStatsEntry 2 }
          
     eltexVpcDomainPeerLinkControlMsgTx    OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link control messages transmitted."
          ::= { eltexVpcDomainLinkStatsEntry 3 }
          
     eltexVpcDomainPeerLinkTxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link control messages Tx errors."
          ::= { eltexVpcDomainLinkStatsEntry 4 }
          
     eltexVpcDomainPeerLinkTxTimeout OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link control messages Tx timeout."
          ::= { eltexVpcDomainLinkStatsEntry 5 }
          
     eltexVpcDomainPeerLinkControlMsgAckTx    OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link control messages ACK transmitted."
          ::= { eltexVpcDomainLinkStatsEntry 6 }
          
     eltexVpcDomainPeerLinkControlMsgAckErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link control messages ACK Tx errors."
          ::= { eltexVpcDomainLinkStatsEntry 7 }
          
     eltexVpcDomainPeerLinkControlMsgRx  OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link control messages received."
          ::= { eltexVpcDomainLinkStatsEntry 8 }
          
     eltexVpcDomainPeerLinkDataMsgTx    OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link data messages transmitted."
          ::= { eltexVpcDomainLinkStatsEntry 9 }
          
     eltexVpcDomainPeerLinkDataMsgTxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link data messages Tx errors."
          ::= { eltexVpcDomainLinkStatsEntry 10 }
          
     eltexVpcDomainPeerLinkDataMsgTxTimeout OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link data messages Tx timeout."
          ::= { eltexVpcDomainLinkStatsEntry 11 }

     eltexVpcDomainPeerLinkDataMsgRx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link data messages received."
          ::= { eltexVpcDomainLinkStatsEntry 12 }
          
     eltexVpcDomainPeerLinkBPDUTx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link BPDU's transmitted to peer."
          ::= { eltexVpcDomainLinkStatsEntry 13 }
          
     eltexVpcDomainPeerLinkBPDUTxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link BPDU's Tx errors."
          ::= { eltexVpcDomainLinkStatsEntry 14 }
          
     eltexVpcDomainPeerLinkBPDURx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link BPDU's received from peer."
          ::= { eltexVpcDomainLinkStatsEntry 15 }
          
     eltexVpcDomainPeerLinkBPDURxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link BPDU's Rx errors."
          ::= { eltexVpcDomainLinkStatsEntry 16 }
          
     eltexVpcDomainPeerLinkLACPDUTx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link LACPDU's tranmsitted to peer."
          ::= { eltexVpcDomainLinkStatsEntry 17 }
          
     eltexVpcDomainPeerLinkLACPDUTxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link LACPDU's Tx errors."
          ::= { eltexVpcDomainLinkStatsEntry 18 }
          
     eltexVpcDomainPeerLinkLACPDURx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link MAC-address data base received from peer."
          ::= { eltexVpcDomainLinkStatsEntry 19 }
          
     eltexVpcDomainPeerLinkLACPDURxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link LACPDU's Rx errors."
          ::= { eltexVpcDomainLinkStatsEntry 20 }
          
     eltexVpcDomainPeerLinkBulkTx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link MAC-address data base tranmsitted to peer."
          ::= { eltexVpcDomainLinkStatsEntry 21 }
          
     eltexVpcDomainPeerLinkBulkTxTimeout OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link MAC-address data base Tx timeout."
          ::= { eltexVpcDomainLinkStatsEntry 22 }
          
     eltexVpcDomainPeerLinkBulkTxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link MAC-address data base Tx errors."
          ::= { eltexVpcDomainLinkStatsEntry 23 }
          
     eltexVpcDomainPeerLinkBulkRx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link MAC-address data base received from peer."
          ::= { eltexVpcDomainLinkStatsEntry 24 }
          
     eltexVpcDomainPeerLinkBulkRxErrors OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer link MAC-address data base Rx errors."
          ::= { eltexVpcDomainLinkStatsEntry 25 }

--**************************************************************************************
-- eltexVpcPeerDetectionStatsTable
--
--**************************************************************************************
     eltexVpcDomainPeerDetectionStatsTable        OBJECT-TYPE
         SYNTAX        SEQUENCE OF EltexVpcDomainDetectionStatsEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain peer detection protocol statistics table."
          ::= { eltexVpcStatusGroup 4 }

     eltexVpcDomainPeerDetectionStatsEntry       OBJECT-TYPE
         SYNTAX        EltexVpcDomainDetectionStatsEntry
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
                       "VPC domain peer detection protocol entry."
         INDEX         { eltexVpcDomainIndex }
          ::= { eltexVpcDomainPeerDetectionStatsTable 1 }

     EltexVpcDomainDetectionStatsEntry ::= SEQUENCE {
         eltexVpcDomainPeerDetectionEnabled
             Unsigned32,
         eltexVpcDomainPeerDetectionEnableFailure
             Unsigned32,
         eltexVpcDomainPeerDetectionDisabled
             Unsigned32,
         eltexVpcDomainPeerDetectionPeerTimeout
             Unsigned32,
         eltexVpcDomainPeerDetectionPeerAdminDisable
             Unsigned32,
         eltexVpcDomainPeerDetectionTx
             Unsigned32,
         eltexVpcDomainPeerDetectionTxError
             Unsigned32,
         eltexVpcDomainPeerDetectionTxFdMsg
             Unsigned32,
         eltexVpcDomainPeerDetectionTxFdAckMsg
             Unsigned32,
         eltexVpcDomainPeerDetectionRx
             Unsigned32,
         eltexVpcDomainPeerDetectionRxError
             Unsigned32,
         eltexVpcDomainPeerDetectionRxFdMsg
             Unsigned32,
         eltexVpcDomainPeerDetectionRxFdAckMsg
             Unsigned32
         }

     eltexVpcDomainPeerDetectionEnabled    OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of peer detection protocol enabled."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 2 }
          
     eltexVpcDomainPeerDetectionEnableFailure    OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of peer detection protocol enabled errors."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 3 }
          
     eltexVpcDomainPeerDetectionDisabled OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of peer detection protocol disabled."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 4 }
          
     eltexVpcDomainPeerDetectionPeerTimeout OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of peer timeout detected."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 5 }
          
     eltexVpcDomainPeerDetectionPeerAdminDisable    OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of peer detection protocol admin disabled."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 6 }
          
     eltexVpcDomainPeerDetectionTx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer detection messages transmitted."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 7 }
          
     eltexVpcDomainPeerDetectionTxError  OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer detection messages transmitted errors."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 8 }
          
     eltexVpcDomainPeerDetectionTxFdMsg    OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer detection fast detect messages transmitted."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 9 }
          
     eltexVpcDomainPeerDetectionTxFdAckMsg OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer detection fast detect ack messages transmitted."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 10 }
          
     eltexVpcDomainPeerDetectionRx OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer detection messages received."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 11 }

     eltexVpcDomainPeerDetectionRxError OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer detection messages received errors."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 12 }
          
     eltexVpcDomainPeerDetectionRxFdMsg OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer detection fast detect messages received."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 13 }
          
     eltexVpcDomainPeerDetectionRxFdAckMsg OBJECT-TYPE
         SYNTAX      Unsigned32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Peer detection fast detect ack messages received."
          ::= { eltexVpcDomainPeerDetectionStatsEntry 14 }

--**************************************************************************************
-- eltexVpcSelfMemberStatus
--
--**************************************************************************************
    eltexVpcMemberStatusTable      OBJECT-TYPE
          SYNTAX        SEQUENCE OF EltexVpcMemberStatusEntry 
          MAX-ACCESS    not-accessible
          STATUS        current
          DESCRIPTION
                        "VPC member ports status table."
             ::= { eltexVpcStatusGroup 5 }

    eltexVpcMemberStatusEntry      OBJECT-TYPE
          SYNTAX        EltexVpcMemberStatusEntry
          MAX-ACCESS    not-accessible
          STATUS        current
          DESCRIPTION    
                        "VPC member port status entry."
          INDEX         { eltexVpcMemberStatusVpcGroupIndex, 
                          eltexVpcMemberStatusIfIndex }
             ::= { eltexVpcMemberStatusTable 1 }

    EltexVpcMemberStatusEntry ::= SEQUENCE {
          eltexVpcMemberStatusVpcGroupIndex
               Unsigned32,
          eltexVpcMemberStatusIfIndex
               InterfaceIndexOrZero,
          eltexVpcSelfMemberStatusIntfState
               INTEGER,
          eltexVpcPeerMemberStatusIntfState
               INTEGER,
          eltexVpcSelfMemberStatusLacpState
               INTEGER,
          eltexVpcPeerMemberStatusLacpState
               INTEGER,
          eltexVpcMemberStatusIfIndexName
               DisplayString
          }

    eltexVpcMemberStatusVpcGroupIndex      OBJECT-TYPE
          SYNTAX        Unsigned32 (1..63)
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION   
                        "VPC Group Index."
             ::= { eltexVpcMemberStatusEntry 1 }

    eltexVpcMemberStatusIfIndex     OBJECT-TYPE
          SYNTAX        InterfaceIndexOrZero
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION   
                        "Interface Index."
             ::= { eltexVpcMemberStatusEntry 2 }

    eltexVpcSelfMemberStatusIntfState  OBJECT-TYPE
          SYNTAX        INTEGER {
                          up   (1),
                          down (2),
                          notpresent (3) 
                        }
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION   
                        "VPC self member interface status."
             ::= { eltexVpcMemberStatusEntry 3 }
             
       eltexVpcPeerMemberStatusIntfState  OBJECT-TYPE
          SYNTAX        INTEGER {
                          up   (1),
                          down (2),
                          notpresent (3) 
                        }
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION   
                        "VPC peer member interface status."
             ::= { eltexVpcMemberStatusEntry 4 }

          eltexVpcSelfMemberStatusLacpState  OBJECT-TYPE
          SYNTAX        INTEGER {
                          active   (1),
                          inactive (2),
                          notpresent (3) 
                        }
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION   
                        "VPC self member LACP interface status."
             ::= { eltexVpcMemberStatusEntry 5 }
             
          eltexVpcPeerMemberStatusLacpState  OBJECT-TYPE
          SYNTAX        INTEGER {
                          active   (1),
                          inactive (2),
                          notpresent (3) 
                        }
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION   
                        "VPC peer member LACP interface status."
             ::= { eltexVpcMemberStatusEntry 6 }

          eltexVpcMemberStatusIfIndexName OBJECT-TYPE
          SYNTAX        DisplayString
          MAX-ACCESS    read-only
          STATUS        current
          DESCRIPTION 
                        "The original name of interface from peer."
             ::= { eltexVpcMemberStatusEntry 7 }

--**************************************************************************************
-- eltexVpcStatusGroup
--
--**************************************************************************************

eltexVpcMIBNotification                  OBJECT IDENTIFIER ::= { eltexVpcMIB 2 }
     
     
END
