
RADLAN-openflow-MIB DEFINITIONS ::= BEGIN

-- Title:      RADLAN open flow Configuration
-- Version:    7.50.00.00
-- Date:       24-November-2010
-- E-mail:     yahal@marvell.com
--

IMPORTS
    TruthValue, TEXTUAL-CONVENTION, TimeStamp,
    DisplayString, DateAndTime, RowStatus                FROM SNMPv2-TC
    TimeTicks, IpAddress, NOTIFICATION-TYPE,
    MODULE-IDENTITY, OBJECT-TYPE, Unsigned32             FROM SNMPv2-SMI
    rnd                                                  FROM RADLAN-MIB;


rlOpenFlow  OBJECT IDENTIFIER ::= { rnd 319 }


-------------------------------------------------------------------------------
rlOpenFlowSupported OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Open Flow support in the switch."
    ::= { rlOpenFlow 1 }

-------------------------------------------------------------------------------
rlOpenFlowTcpPort OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Open Flow TCP port."
    DEFVAL { 6633 }
    ::= { rlOpenFlow 2 }

-------------------------------------------------------------------------------
rlOpenFlowServerIpAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Open Flow server IP address."
    DEFVAL {'00000000'H}
    ::= { rlOpenFlow 3 }


-------------------------------------------------------------------------------
rlOpenFlowProtocolType OBJECT-TYPE
    SYNTAX          INTEGER {
        tcp(0),
        tls(1)
                            }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION     "OpenFlow protocol. tls or tcp.
                     The default value is tcp."
    DEFVAL{ tcp }
    ::= { rlOpenFlow 4 }


-------------------------------------------------------------------------------
rlOpenFlowDefaultForwardAction OBJECT-TYPE
    SYNTAX          INTEGER {
        forward(0),
        drop(1),
        toController(2)
                            }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION     "OpenFlow Forward Action to controller.
                     forward, drop or toController.
                     The default value is forward."
    DEFVAL{ forward }
    ::= { rlOpenFlow 5 }

-------------------------------------------------------------------------------
rlOpenFlowEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "OpenFlow global enable mode."
    ::= { rlOpenFlow 6 }

-------------------------------------------------------------------------------
rlOpenFlowEnableAfterReset OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "OpenFlow global enable mode after reset."
    DEFVAL { false }
    ::= { rlOpenFlow 7 }


END

