rndEthernet  OBJECT IDENTIFIER ::= { rnd 37 }
rndEthIfTable    OBJECT-TYPE
    SYNTAX  SEQUENCE  OF RndEthIfEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
      "Ethernet media specific information and configuration of the device 
       interfaces."
    ::=  { rndEthernet 1 }
    
rndEthIfEntry OBJECT-TYPE
    SYNTAX  RndEthIfEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
      "Defines the contents of each line in the rndEthIfTable table."
    INDEX   { rndEthIfIndex }
    ::=  { rndEthIfTable 1 }

RndEthIfEntry ::= SEQUENCE {
    rndEthIfIndex         INTEGER,
    rndEthDuplexMode      INTEGER,
    rndEthIfSpeed         INTEGER,
    rndEthTransceiverType INTEGER
    }

rndEthIfIndex OBJECT-TYPE
    SYNTAX   INTEGER
    ACCESS   read-only
    STATUS   mandatory
    DESCRIPTION
     "Index to the rndEthIfTable. The interface defined by a
     particular value of this index is the same interface as
     identified by the same value of ifIndex (MIBII)."
         ::= {  rndEthIfEntry 1  }

    rndEthDuplexMode  OBJECT-TYPE
      SYNTAX  INTEGER {
         half(1),
         full(2)
        }
      ACCESS   read-write
      STATUS   mandatory
      DESCRIPTION
        " This variable indicates whether this interface operates in half
          duplex or full duplex mode."
         ::= {  rndEthIfEntry 2  }

    rndEthIfSpeed  OBJECT-TYPE
      SYNTAX  INTEGER {
         speed10BT(1),
         speed100BT(2)
        }
      ACCESS   read-write
      STATUS   mandatory
      DESCRIPTION
        " This variable indicates whether this interface operates at 10BT 
          or 100BT speed."
         ::= {  rndEthIfEntry 3  }

    rndEthTransceiverType  OBJECT-TYPE
      SYNTAX  INTEGER {
         regular(1),
         fiberOptics(2)
        }
      ACCESS   read-only
      STATUS   mandatory
      DESCRIPTION
        " This variable indicates the transceiver type of this interface."
         ::= {  rndEthIfEntry 4  }
