RADLAN-BRIDGE-SECURITY DEFINITIONS ::= BEGIN

-- Version:    7.43
-- Date:       02-Apr-2006

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    Unsigned32, IpAddress, Counter32                FROM SNMPv2-SMI
    InterfaceIndex, ifIndex                         FROM IF-MIB
    RowStatus, TEXTUAL-CONVENTION, MacAddress,
    DisplayString, TruthValue                       FROM SNMPv2-TC
    InetAddress, InetAddressType,
    InetAddressPrefixLength,
    InetVersion, InetZoneIndex                      FROM INET-ADDRESS-MIB
    VlanId                                          FROM Q-BRIDGE-MIB
    rnd                                             FROM RADLAN-MIB;

rlVoipSnoop MODULE-IDENTITY
        LAST-UPDATED "200604020000Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO 
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
		DESCRIPTION
                "The private MIB module definition for VOIP Snoop."
        ::= { rnd  213}


rlVoipMngSnoopEnableScalar OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "VOIP Global Enable/Disable."
    ::= { rlVoipSnoop 1 }




RlVoipQosType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "Type of QoS: VPT or DSCP."
    SYNTAX  INTEGER {
        queue(1),
        vpt(2),
        dscp(3)
}


rlVoipMngSnoopQosTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlVoipMngSnoopQosEntry
    MAX-ACCESS   not-accessible
    STATUS   current
    DESCRIPTION
       "The (conceptual) table for configuration of VOIP QOS."
    ::= {  rlVoipSnoop 2 }

rlVoipMngSnoopQosEntry OBJECT-TYPE
    SYNTAX      RlVoipMngSnoopQosEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the rlVoipMngSnoopQosTable."
    INDEX  { rlVoipMngSnoopQosType }
    ::= { rlVoipMngSnoopQosTable 1 }

RlVoipMngSnoopQosEntry::= SEQUENCE {
   rlVoipMngSnoopQosType                                  RlVoipQosType,
   rlVoipMngSnoopQosValue                                 INTEGER
}


rlVoipMngSnoopQosType OBJECT-TYPE
    SYNTAX      RlVoipQosType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Current type of QoS of VOIP packets"
    ::= { rlVoipMngSnoopQosEntry 1 }

rlVoipMngSnoopQosValue OBJECT-TYPE
    SYNTAX      INTEGER (0..63)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value depends on rlVoipMngSnoopQosType, that will be assigned to each VOIP packet.
        The range of VPT value is 0..7. The range of DSCP value is 0..63.
        The range of queue value is 0..7."
    ::= { rlVoipMngSnoopQosEntry 2 }



--
--  VOIP Ports table
--


RlVoipMngSnoopIfIndexStatus ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "VOIP status of the port: enable or disable."
    SYNTAX  INTEGER {
        disable(0),
        enable(1)
}


rlVoipMngSnoopIfIndexTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlVoipMngSnoopIfIndexEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "VOIP ports entry. The entry created when VOIP snooping
        enabled on port."
  ::= { rlVoipSnoop 3 }

rlVoipMngSnoopIfIndexEntry OBJECT-TYPE
   SYNTAX      RlVoipMngSnoopIfIndexEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION        "The row definition for this table."
   INDEX {rlVoipMngSnoopIfIndex}
::= { rlVoipMngSnoopIfIndexTable 1 }

RlVoipMngSnoopIfIndexEntry ::= SEQUENCE {
   rlVoipMngSnoopIfIndex             INTEGER,
   rlVoipMngSnoopIfIndexStatus       RlVoipMngSnoopIfIndexStatus
}

rlVoipMngSnoopIfIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Interface Index."
    ::= { rlVoipMngSnoopIfIndexEntry 1 }

rlVoipMngSnoopIfIndexStatus OBJECT-TYPE
   SYNTAX       RlVoipMngSnoopIfIndexStatus
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
       "Enable or Disable VOIP status on the ifIndex."
  ::= { rlVoipMngSnoopIfIndexEntry  2 }




--
--  VOIP sessions table
--


RlVoipProtocolType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "Type of protocol."
    SYNTAX  INTEGER {
        sip(1),
        h323(2),
        sccp(3)
}

RlVoipTcpUdpType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "Type of IP protocol."
    SYNTAX  INTEGER {
        udp(1),
        tcp(2)
}


rlVoipMngSnoopSessionTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlVoipMngSnoopSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "VOIP session entry. The entry created when VOIP snooping
        creates the RTP session."
  ::= { rlVoipSnoop 4 }

rlVoipMngSnoopSessionEntry OBJECT-TYPE
   SYNTAX      RlVoipMngSnoopSessionEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION        "The row definition for this table."
   INDEX {rlVoipMngSnoopSessionDstIpAddrType,rlVoipMngSnoopSessionDstIpAddr,
          rlVoipMngSnoopSessionSrcIpAddrType,rlVoipMngSnoopSessionSrcIpAddr,
          rlVoipMngSnoopSessionDstUdpRtp,rlVoipMngSnoopSessionDstUdpRtcp,
          rlVoipMngSnoopSessionSrcUdpRtp,rlVoipMngSnoopSessionSrcUdpRtcp}
::= { rlVoipMngSnoopSessionTable 1 }

RlVoipMngSnoopSessionEntry ::= SEQUENCE {
   rlVoipMngSnoopSessionDstIpAddrType          InetAddressType,
   rlVoipMngSnoopSessionDstIpAddr              InetAddress,
   rlVoipMngSnoopSessionSrcIpAddrType          InetAddressType,
   rlVoipMngSnoopSessionSrcIpAddr              InetAddress,
   rlVoipMngSnoopSessionDstUdpRtp              INTEGER,
   rlVoipMngSnoopSessionDstUdpRtcp             INTEGER,
   rlVoipMngSnoopSessionSrcUdpRtp              INTEGER,
   rlVoipMngSnoopSessionSrcUdpRtcp             INTEGER,
   rlVoipMngSnoopSessionProtocolType           RlVoipProtocolType,
   rlVoipMngSnoopSessionSessionId              INTEGER,
   rlVoipMngSnoopSessionTcpUdpType             RlVoipTcpUdpType
}

rlVoipMngSnoopSessionDstIpAddrType OBJECT-TYPE
    SYNTAX     InetAddressType
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The address type of rlVoipMngSnoopSessionDstIpAddr."
    ::= { rlVoipMngSnoopSessionEntry 1 }


rlVoipMngSnoopSessionDstIpAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Destination IP address."
    ::= { rlVoipMngSnoopSessionEntry 2 }


rlVoipMngSnoopSessionSrcIpAddrType OBJECT-TYPE
    SYNTAX     InetAddressType
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The address type of rlVoipMngSnoopSessionSrcIpAddr."
    ::= { rlVoipMngSnoopSessionEntry 3 }

rlVoipMngSnoopSessionSrcIpAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Source IP address."
    ::= { rlVoipMngSnoopSessionEntry 4 }


rlVoipMngSnoopSessionDstUdpRtp OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Destination Udp RTP port."
    ::= { rlVoipMngSnoopSessionEntry 5 }

rlVoipMngSnoopSessionDstUdpRtcp OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Destination Udp RTCP port."
    ::= { rlVoipMngSnoopSessionEntry 6 }

rlVoipMngSnoopSessionSrcUdpRtp OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Source Udp RTP port."
    ::= { rlVoipMngSnoopSessionEntry 7 }

rlVoipMngSnoopSessionSrcUdpRtcp OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Source Udp RTCP port."
    ::= { rlVoipMngSnoopSessionEntry 8 }

rlVoipMngSnoopSessionProtocolType OBJECT-TYPE
    SYNTAX      RlVoipProtocolType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Type of signalling protocol."
    ::= { rlVoipMngSnoopSessionEntry 9 }

rlVoipMngSnoopSessionSessionId OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Destination Udp RTCP port."
    ::= { rlVoipMngSnoopSessionEntry 10 }


rlVoipMngSnoopSessionTcpUdpType OBJECT-TYPE
    SYNTAX      RlVoipTcpUdpType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IP TCP or UDP protocol."
    ::= { rlVoipMngSnoopSessionEntry 11 }


















END

