RADLAN-STORMCTRL-MIB DEFINITIONS ::= BEGIN

-- Title:                RADLAN ROS
--                       Private STORM CTRL MIB
-- Version:              7.46
-- Date:                 15-Jan-2007

IMPORTS
    rnd                                                     FROM RADLAN-MIB
    OBJECT-TYPE, MODULE-IDENTITY, Unsigned32, Counter64     FROM SNMPv2-SMI
    TruthValue, DisplayString, TEXTUAL-CONVENTION           FROM SNMPv2-TC
    InterfaceIndex                                          FROM IF-MIB
    dot1dBasePort                                           FROM BRIDGE-MIB;


    RlStormCtrlRateUnit ::= INTEGER {
        packetsPerSecond(1),
        bytesPerSecond(2),
        framesPerBuffer(3),
        precentages(4),
        kiloBytesPerSecond(5),
        kiloBitsPerSecond(6)
    }

RlStormCtrlRateLimTrafficType ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION
        "traffic type for storm-control and rate-limit."
    SYNTAX     INTEGER {
        broadcast(1),
        multicastRegistred(2),
        multicastUnregistred(3),
        multicastAll(4),
        unknownUnicast(5),
        all(6)
    }

RlStormCtrlTrafficTypeBits ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Storm control traffic type bits."
    SYNTAX BITS {
        broadcast(0),
        multicastAll(1),
        unknownUnicast(2)
    }

RlStormCtrlOwner ::= INTEGER {
        none(0),
        user(1),
        global(2)
    }

    RlStormCtrlRateUnitType ::= INTEGER {
        kiloBitsPerSecond(1),
        precentages(2)
    }

    RlStormCtrlActionType ::= INTEGER {
        none(1),
        trap(2),
        shutdown(3),
        trapAndShutdown(4)
    }

rlStormCtrl MODULE-IDENTITY
                LAST-UPDATED "200701020000Z"
                ORGANIZATION "Marvell Semiconductor, Inc."
                CONTACT-INFO
					"5488 Marvell Lane
					Santa Clara, CA 95054
					USA

					Website:  www.marvell.com"
                DESCRIPTION
                      "This private MIB module defines storm control private MIBs."
                REVISION "200701020000Z"
                DESCRIPTION
                      "Initial revision."
        ::= { rnd 77 }

rlStormCtrlSupport OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "Identify if the strom control protection is supported"
    ::= { rlStormCtrl 1 }

rlStormCtrlMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "MIB's version, the current version is 3."
    ::= { rlStormCtrl 2 }

rlStormCtrlRateUnitTypeSupport OBJECT-TYPE
--    SYNTAX      BITS {
--            packetsPerSecond(0),
--            bytesPerSecond(1),
--            framesPerBuffer(2),
--            percentages(3),
--            kiloBytesPerSecond(4),
--            kiloBitsPerSecond(5)
--    }
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  obsolete
    DESCRIPTION
        "the supported rate unit type for the storm rate control"
    ::= { rlStormCtrl 3 }

rlStormCtrlTypeSupport  OBJECT-TYPE
--    SYNTAX      BITS {
--            unknownUnicast(0),
--            unknownMulticast(1),
--            broadcast(2),
--            multicast(3),
--    }
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  obsolete
    DESCRIPTION
        "the supported frame type for the storm control protection"
    ::= { rlStormCtrl 4 }

rlStormCtrlRateSupportPerType OBJECT-TYPE
--    SYNTAX      BITS {
--            unknownUnicast(0),
--            unknownMulticast(1),
--            broadcast(2),
--            multicast(3),
--    }
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  obsolete
    DESCRIPTION
        "identify if rate control is supported for each frame type"
    ::= { rlStormCtrl 5 }

rlStormCtrlEnbaleDependencyBetweenTypes OBJECT-TYPE
--    SYNTAX      BITS {
--            unknownUnicast(0),
--            unknownMulticast(1),
--            broadcast(2),
--            multicast(3),
--    }
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  obsolete
    DESCRIPTION
        "indicate enable limitation of dependency between frame types,
         such as enabling of multicast should be with the enabling of
         broadcast type (bcm 5632)"
    ::= { rlStormCtrl 6 }

rlStormCtrlRateDependencyBetweenTypes OBJECT-TYPE
--    SYNTAX      BITS {
--            unknownUnicast(0),
--            unknownMulticast(1),
--            broadcast(2),
--            multicast(3),
--    }
    SYNTAX  OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS  obsolete
    DESCRIPTION
        "indicate limitation of dependency between frame types for
         rate assignment, for example: assigning of rate limit for unicast
         frame must assigning the same rate for multicast and bradcast
         frame (bcm 5615), in case the device support enbale per each frame
         type but with the same rate limitation."
    ::= { rlStormCtrl 7 }

--
-- rlStormCtrlTable
--
rlStormCtrlTable   OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlStormCtrlEntry
    MAX-ACCESS  not-accessible
    STATUS  obsolete
    DESCRIPTION
        "The table contains the storm control protection per port"
    ::= { rlStormCtrl 8 }

rlStormCtrlEntry   OBJECT-TYPE
    SYNTAX  RlStormCtrlEntry
    MAX-ACCESS  not-accessible
    STATUS  obsolete
    DESCRIPTION
        "storm control protection, defined per port,frame type and rate"
    INDEX { dot1dBasePort }
    ::= { rlStormCtrlTable 1 }

RlStormCtrlEntry ::= SEQUENCE {
    rlStormCtrlRateType                         RlStormCtrlRateUnit,
    rlStormCtrlUnknownUnicastEnable             TruthValue,
    rlStormCtrlUnknownUnicastRate               Unsigned32,
    rlStormCtrlUnknownMulticastEnable           TruthValue,
    rlStormCtrlUnknownMulticastRate             Unsigned32,
    rlStormCtrlBroadcastEnable                  TruthValue,
    rlStormCtrlBroadcastRate                    Unsigned32,
    rlStormCtrlMulticastEnable                  TruthValue,
    rlStormCtrlMulticastRate                    Unsigned32,
    rlStormCtrlSetDefaultRateType               TruthValue,
    rlStormCtrlSetDefaultUnknownUnicastEnable   TruthValue,
    rlStormCtrlSetDefaultUnknownUnicastRate     TruthValue,
    rlStormCtrlSetDefaultUnknownMulticastEnable TruthValue,
    rlStormCtrlSetDefaultUnknownMulticastRate   TruthValue,
    rlStormCtrlSetDefaultBroadcastEnable        TruthValue,
    rlStormCtrlSetDefaultBroadcastRate          TruthValue,
    rlStormCtrlSetDefaultMulticastEnable        TruthValue,
    rlStormCtrlSetDefaultMulticastRate          TruthValue,
    rlStormCtrlBroadcastOperRate                Unsigned32
}

rlStormCtrlRateType OBJECT-TYPE
    SYNTAX  RlStormCtrlRateUnit
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate the rate unit type"
    ::= { rlStormCtrlEntry 1 }

rlStormCtrlUnknownUnicastEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "enable or disable the storm control for unknown unicast frames"
    DEFVAL { false }
    ::= { rlStormCtrlEntry 2 }

rlStormCtrlUnknownUnicastRate OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "set the storm control rate limit for the unknown unicast frames,
        0 indicate blocking of frames from this type."
    DEFVAL { 0 }
    ::= { rlStormCtrlEntry 3 }

rlStormCtrlUnknownMulticastEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "enable or disable the storm control for unknown multicast frames"
    DEFVAL { false }
    ::= { rlStormCtrlEntry 4 }

rlStormCtrlUnknownMulticastRate OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "set the storm control rate limit for the unknown multicast frames,
        0 indicate blocking of frames from this type."
    DEFVAL { 0 }
    ::= { rlStormCtrlEntry 5 }

rlStormCtrlBroadcastEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "enable or disable the storm control for Broadcast frames"
    DEFVAL { false }
    ::= { rlStormCtrlEntry 6 }

rlStormCtrlBroadcastRate OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "set the storm control rate limit for the Broadcast frames,
        0 indicate blocking of frames from this type."
    DEFVAL { 0 }
    ::= { rlStormCtrlEntry 7 }

rlStormCtrlMulticastEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "enable or disable the storm control for multicast frames"
    DEFVAL { false }
    ::= { rlStormCtrlEntry 8 }

rlStormCtrlMulticastRate OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "set the storm control rate limit for the multicast frames,
        0 indicate blocking of frames from this type."
    DEFVAL { 0 }
    ::= { rlStormCtrlEntry 9 }

rlStormCtrlSetDefaultRateType OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate if return the rate unit type to its default."
    DEFVAL { false }
    ::= { rlStormCtrlEntry 10 }

rlStormCtrlSetDefaultUnknownUnicastEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate if return the storm control enable for unknown unicast frames
         to its default."
    DEFVAL { false }
    ::= { rlStormCtrlEntry 11 }

rlStormCtrlSetDefaultUnknownUnicastRate OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate if return the storm control rate limit for the unknown unicast frames
         to its default."
    DEFVAL { false }
    ::= { rlStormCtrlEntry 12 }

rlStormCtrlSetDefaultUnknownMulticastEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate if return the storm control enable for unknown multicast frames
         to its default."
    DEFVAL { false }
    ::= { rlStormCtrlEntry 13 }

rlStormCtrlSetDefaultUnknownMulticastRate OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate if return the storm control rate limit for the unknown multicast frames
         to its default."
    DEFVAL { false }
    ::= { rlStormCtrlEntry 14 }

rlStormCtrlSetDefaultBroadcastEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate if return the storm control enable for Broadcast frames
         to its default."
    DEFVAL { false }
    ::= { rlStormCtrlEntry 15 }

rlStormCtrlSetDefaultBroadcastRate OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate if return the storm control rate limit for the Broadcast frames
         to its default."
    DEFVAL { false }
    ::= { rlStormCtrlEntry 16 }

rlStormCtrlSetDefaultMulticastEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate if return the storm control for multicast frames
         to its default."
    DEFVAL { false }
    ::= { rlStormCtrlEntry 17 }

rlStormCtrlSetDefaultMulticastRate OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  obsolete
    DESCRIPTION
        "indicate if return the storm control rate limit for the multicast frames
         to its default."
    DEFVAL { false }
    ::= { rlStormCtrlEntry 18 }

rlStormCtrlBroadcastOperRate OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-only
    STATUS  obsolete
    DESCRIPTION
        "Operative storm control rate limit for the Broadcast frames.
         The value will be 0 if rlStormCtrlRateType is not from type precentages."
    ::= { rlStormCtrlEntry 19 }

--
-- rlStormCtrlGroupTable
--
rlStormCtrlGroupTable   OBJECT-TYPE
    SYNTAX   SEQUENCE OF RlStormCtrlGroupEntry
    MAX-ACCESS   not-accessible
    STATUS   obsolete
    DESCRIPTION
        "The table contains per port for each supported frame type
        to which group it belongs."
    ::= { rlStormCtrl 9 }

rlStormCtrlGroupEntry   OBJECT-TYPE
    SYNTAX   RlStormCtrlGroupEntry
    MAX-ACCESS   not-accessible
    STATUS   obsolete
    DESCRIPTION
        "group id for each supported frame type defined per port."
    INDEX { dot1dBasePort }
    ::= { rlStormCtrlGroupTable 1 }

RlStormCtrlGroupEntry ::= SEQUENCE {
    rlStormCtrlGroupUnknownUnicastId      INTEGER,
    rlStormCtrlGroupUnknownMulticastId    INTEGER,
    rlStormCtrlGroupBroadcastId           INTEGER,
    rlStormCtrlGroupMulticastId           INTEGER
}

rlStormCtrlGroupUnknownUnicastId OBJECT-TYPE
    SYNTAX   INTEGER
    MAX-ACCESS   read-only
    STATUS   obsolete
    DESCRIPTION
        "Indicates the id of the group for unknown unicast frame type that
        the port belongs to,
        0 indicates that unknown unicast frame type is not supported."
    ::= { rlStormCtrlGroupEntry 1 }

rlStormCtrlGroupUnknownMulticastId OBJECT-TYPE
    SYNTAX   INTEGER
    MAX-ACCESS   read-only
    STATUS   obsolete
    DESCRIPTION
        "Indicates the id of the group for unknown multicast frame type that
        the port belongs to,
        0 indicates that unknown multicast frame type is not supported."
    ::= { rlStormCtrlGroupEntry 2 }

rlStormCtrlGroupBroadcastId OBJECT-TYPE
    SYNTAX   INTEGER
    MAX-ACCESS   read-only
    STATUS   obsolete
    DESCRIPTION
        "Indicates the id of the group for broadcast frame type that
        the port belongs to,
        0 indicates that broadcast frame type is not supported."
    ::= { rlStormCtrlGroupEntry 3 }

rlStormCtrlGroupMulticastId  OBJECT-TYPE
    SYNTAX   INTEGER
    MAX-ACCESS   read-only
    STATUS   obsolete
    DESCRIPTION
        "Indicates the id of the group for multicast frame type that
        the port belongs to,
        0 indicates that multicast frame type is not supported."
    ::= { rlStormCtrlGroupEntry 4 }

rlStormCtrlRateLimSupport OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Identify if the strom-control and rate-limit is supported"
    ::= { rlStormCtrl 10 }

rlStormCtrlRateLimMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "MIB's version, the current version is 1."
    ::= { rlStormCtrl 11 }

--
-- rlStormCtrlRateLimCfgTable
--
rlStormCtrlRateLimCfgTable   OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlStormCtrlRateLimCfgEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table contains the storm-control and rate-limit configuration per port"
    ::= { rlStormCtrl 12 }

rlStormCtrlRateLimCfgEntry   OBJECT-TYPE
    SYNTAX  RlStormCtrlRateLimCfgEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "storm-control and rate-limit configuration, defined per port"
    INDEX { dot1dBasePort, rlStormCtrlRateLimCfgTraffic }
    ::= { rlStormCtrlRateLimCfgTable 1 }

RlStormCtrlRateLimCfgEntry ::= SEQUENCE {
    rlStormCtrlRateLimCfgTraffic           RlStormCtrlRateLimTrafficType,
    rlStormCtrlRateLimCfgRate              Unsigned32,
    rlStormCtrlRateLimCfgUnit              RlStormCtrlRateUnitType,
    rlStormCtrlRateLimCfgAction            RlStormCtrlActionType,
    rlStormCtrlRateLimCfgBurst             Unsigned32,
	rlStormCtrlRateLimBCOwner              RlStormCtrlOwner,
	rlStormCtrlRateLimMCOwner              RlStormCtrlOwner,
	rlStormCtrlRateLimUCOwner              RlStormCtrlOwner
}

rlStormCtrlRateLimCfgTraffic OBJECT-TYPE
    SYNTAX      RlStormCtrlRateLimTrafficType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "traffic type for storm-control and rate-limit."
    ::= { rlStormCtrlRateLimCfgEntry 1 }

rlStormCtrlRateLimCfgRate OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "block the flooding of packets when the value specified is reached."
    ::= { rlStormCtrlRateLimCfgEntry 2 }

rlStormCtrlRateLimCfgUnit OBJECT-TYPE
    SYNTAX  RlStormCtrlRateUnitType
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "suppression level in percentage (for storm-control only) or in kilobits per second."
    ::= { rlStormCtrlRateLimCfgEntry 3 }

rlStormCtrlRateLimCfgAction OBJECT-TYPE
    SYNTAX  RlStormCtrlActionType
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "send a trap when a storm occurs on a port or/and shut down a port when a storm occurs on the port."
    ::= { rlStormCtrlRateLimCfgEntry 4 }

rlStormCtrlRateLimCfgBurst OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "committed burst in bytes for rate-limit"
    ::= { rlStormCtrlRateLimCfgEntry 5 }

rlStormCtrlRateLimBCOwner OBJECT-TYPE
    SYNTAX  RlStormCtrlOwner
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "indicates who is the owner for broadcast type that is configured."	
	DEFVAL { none }
    ::= { rlStormCtrlRateLimCfgEntry 6 }

rlStormCtrlRateLimMCOwner OBJECT-TYPE
    SYNTAX  RlStormCtrlOwner
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "indicates who is the owner for multicast type that is configured."	
	DEFVAL { none }
    ::= { rlStormCtrlRateLimCfgEntry 7 }

rlStormCtrlRateLimUCOwner OBJECT-TYPE
    SYNTAX  RlStormCtrlOwner
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "indicates who is the owner for unicast type that is configured."
	DEFVAL { none }
    ::= { rlStormCtrlRateLimCfgEntry 8 }

--
-- rlStormCtrlRateLimOperTable
--
rlStormCtrlRateLimOperTable   OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlStormCtrlRateLimOperEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table contains the operative values for storm-control and rate-limit per port"
    ::= { rlStormCtrl 13 }

rlStormCtrlRateLimOperEntry   OBJECT-TYPE
    SYNTAX  RlStormCtrlRateLimOperEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "storm-control and rate-limit operative values per port"
    INDEX { dot1dBasePort, rlStormCtrlRateLimCfgTraffic }
    ::= { rlStormCtrlRateLimOperTable 1 }

RlStormCtrlRateLimOperEntry ::= SEQUENCE {
    rlStormCtrlRateLimOperPassCnt          Counter64,
    rlStormCtrlRateLimOperDropCnt          Counter64,
    rlStormCtrlRateLimOperLastDropTime     DisplayString
}

rlStormCtrlRateLimOperPassCnt OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "number of passed counter in bytes."
    ::= { rlStormCtrlRateLimOperEntry 1 }

rlStormCtrlRateLimOperDropCnt OBJECT-TYPE
    SYNTAX  Counter64
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "number of dropped counter in bytes."
    ::= { rlStormCtrlRateLimOperEntry 2 }

rlStormCtrlRateLimOperLastDropTime OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "last Drop time in format ddmmyyyyhhmmss."
    ::= { rlStormCtrlRateLimOperEntry 3 }

--
-- rlStormCtrlClearCountersTable
--
rlStormCtrlClearCountersTable   OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlStormCtrlClearCountersEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table clear storm-control counters"
    ::= { rlStormCtrl 14 }

rlStormCtrlClearCountersEntry   OBJECT-TYPE
    SYNTAX  RlStormCtrlClearCountersEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "clear storm-control counters"
    INDEX { rlStormCtrlClearCountersIndex }
    ::= { rlStormCtrlClearCountersTable 1 }

RlStormCtrlClearCountersEntry ::= SEQUENCE {
    rlStormCtrlClearCountersIndex          Unsigned32,
    rlStormCtrlClearCountersTraffic        RlStormCtrlRateLimTrafficType,
    rlStormCtrlClearCountersInterface      InterfaceIndex

}

rlStormCtrlClearCountersIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Index of the table that equals to 1 always."
    ::= { rlStormCtrlClearCountersEntry 1 }

rlStormCtrlClearCountersTraffic OBJECT-TYPE
    SYNTAX      RlStormCtrlRateLimTrafficType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Traffic type for storm-control counter."
    ::= { rlStormCtrlClearCountersEntry 2 }

rlStormCtrlClearCountersInterface OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The Port number or all ports."
    ::= { rlStormCtrlClearCountersEntry 3 }

rlStormCtrlGlobalTrafficTypes OBJECT-TYPE
    SYNTAX      RlStormCtrlTrafficTypeBits
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "global traffic types configured on the device."
    ::= { rlStormCtrl 15 }

END

