          RADLAN-CPU-COUNTERS-MIB DEFINITIONS ::= BEGIN

          IMPORTS
                rnd                                         FROM RADLAN-MIB
                Counter32, OBJECT-TYPE, MODULE-IDENTITY     FROM SNMPv2-SMI
                DisplayString,
                TruthValue                                  FROM SNMPv2-TC;


-- module

        rlCpuCounters MODULE-IDENTITY
            LAST-UPDATED "2007010600Z"
            ORGANIZATION "Marvell Semiconductor, Inc."
            CONTACT-INFO
				"5488 Marvell Lane
				Santa Clara, CA 95054
				USA

				Website:  www.marvell.com"
            DESCRIPTION
                "CPU Counter MIBs"
            REVISION "200705150000Z"
            DESCRIPTION
                    "Initial revision."

            ::={ rnd 124 }

-- table
          rlCpuCountersTable OBJECT-TYPE
              SYNTAX  SEQUENCE OF RlCpuCountersEntry
              MAX-ACCESS  not-accessible
              STATUS  current
              DESCRIPTION
                      "Table of rx&tx counter, the key is cpuCounters"
              ::= { rlCpuCounters 1 }
--entry:
          rlCpuCountersEntry OBJECT-TYPE
              SYNTAX  RlCpuCountersEntry
              MAX-ACCESS  not-accessible
              STATUS  current
              DESCRIPTION
                      "Table of rx&tx counters, the key is cpuCounters"
              INDEX   { rlCpuCountersTarget  }
              ::= { rlCpuCountersTable 1 }

--entry content
          RlCpuCountersEntry ::= SEQUENCE {
                  rlCpuCountersTarget INTEGER,
                  rlCpuCountersTxBC  Counter32,
                  rlCpuCountersTxMC  Counter32,
                  rlCpuCountersTxUC  Counter32,
                  rlCpuCountersTxOctets  Counter32,
                  rlCpuCountersRxBC  Counter32,
                  rlCpuCountersRxMC  Counter32,
                  rlCpuCountersRxUC  Counter32,
                  rlCpuCountersRxOctets  Counter32
              }
--field definition:

        rlCpuCountersTarget OBJECT-TYPE
              SYNTAX  INTEGER  {
                cpuCounters (0)
              }
              MAX-ACCESS  not-accessible
              STATUS  current
              DESCRIPTION
                      "Packet type can be Multicast (MC), Broadcast (BC) or Unicast(UC)"
              ::= { rlCpuCountersEntry 1 }

        rlCpuCountersTxBC  OBJECT-TYPE
              SYNTAX  Counter32
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "Number of received broadcast packets."
              ::= { rlCpuCountersEntry 2 }

        rlCpuCountersTxMC  OBJECT-TYPE
              SYNTAX  Counter32
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "Number of transmitted multicast packets."
              ::= { rlCpuCountersEntry 3 }

        rlCpuCountersTxUC  OBJECT-TYPE
              SYNTAX  Counter32
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "Number of transmitted unicast packets."
              ::= { rlCpuCountersEntry 4 }

        rlCpuCountersTxOctets  OBJECT-TYPE
              SYNTAX  Counter32
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "Number of transmitted octets."
              ::= { rlCpuCountersEntry 5 }

        rlCpuCountersRxBC  OBJECT-TYPE
              SYNTAX  Counter32
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "Number of received broadcast packets."
              ::= { rlCpuCountersEntry 6 }

          rlCpuCountersRxMC  OBJECT-TYPE
              SYNTAX  Counter32
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "Number of received mutlicast packets."
              ::= { rlCpuCountersEntry 7 }

        rlCpuCountersRxUC  OBJECT-TYPE
              SYNTAX  Counter32
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "Number of received unicast packets."
              ::= { rlCpuCountersEntry 8 }

        rlCpuCountersRxOctets  OBJECT-TYPE
              SYNTAX  Counter32
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "Number of received octets"
              ::= { rlCpuCountersEntry 9 }





-- rlCpuCountersReset:


        rlCpuCountersReset OBJECT-TYPE
            SYNTAX      TruthValue
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                "Setting true to this MIB object will reset the CPU counters."
            DEFVAL { false}
            ::= { rlCpuCounters 2 }

-- rlCpuCountersEnabled:

        rlCpuCountersEnabled OBJECT-TYPE
            SYNTAX      TruthValue
            MAX-ACCESS  read-write
            STATUS      current
            DESCRIPTION
                "True - feature is enabled, false - feature is disabled "
            DEFVAL { false}
            ::= { rlCpuCounters 3 }





          END

