RADLAN-rndMng DEFINITIONS ::= BEGIN

-- Title:      RADLAN Management Private Extension
-- Version:    7.45
-- Date:       19 Dec 2006
-- 28-Feb-2005  Added   rlCpuUtilEnable
-- 28-Feb-2005  Added   rlCpuUtilDuringLastSecond
-- 28-Feb-2005  Added   rlCpuUtilDuringLastMinute
-- 28-Feb-2005  Added   rlCpuUtilDuringLast5Minutes
-- 13-Jun-2006  Added   value {none} of rndAction
-- 20-Jun-2006  Added   rlRebootDelay
-- 19-Dec-2006  Added   resetToFactoryDefaults
-- 04-Apr-2012  Added   rlScheduledReload
-- 04-Dec-2012  Added   rlSysNameTable 
-- 10-Aug-2018  Added  rlDefaultSysName

IMPORTS
    rnd                                                     FROM RADLAN-MIB
    Unsigned32,
    MODULE-IDENTITY, OBJECT-TYPE, TimeTicks                 FROM SNMPv2-SMI
    RowStatus, TruthValue, DisplayString,
    TEXTUAL-CONVENTION                                      FROM SNMPv2-TC
    InetAddressType, InetAddress                            FROM INET-ADDRESS-MIB
    InterfaceIndex                                          FROM IF-MIB;


rndMng  MODULE-IDENTITY
        LAST-UPDATED "201212040000Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
             "The private MIB module definition for RND general management MIB."
        REVISION "201212040000Z"
        DESCRIPTION
             "Added rlSysNameTable object."
        REVISION "201204040000Z"
        DESCRIPTION
             "Added rlScheduledReload object."
        REVISION "200902240000Z"
        DESCRIPTION
             "Added rlRunningCDBequalToStartupCDB object."
        REVISION "200710240000Z"
        DESCRIPTION
             "Added rlGroupManagement branch."
        REVISION "200606200000Z"
        DESCRIPTION
             "Added rlRebootDelay object"
        REVISION "200406010000Z"
        DESCRIPTION
             "Initial version of this MIB."
        ::= { rnd 1 }


rndSysId OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Identification of an RND device. The device type for each
      integer clarifies the sysObjectID in MIB - II."
    ::= { rndMng 1  }

rndAction OBJECT-TYPE
    SYNTAX  INTEGER {
       reset(1),
       sendNetworkTab(2),
       deleteNetworkTab(3),
       sendRoutingTab(4),    -- Level II
       deleteRoutingTab(5),
       sendLanTab(6),
       deleteLanTab(7),
       deleteArpTab(8),
       sendArpTab(9),
       deleteRouteTab(10),   -- Level III
       sendRouteTab(11),
       backupSPFRoutingTab(12),
       backupIPRoutingTab(13),
       backupNetworkTab(14),
       backupLanTab(15),
       backupArpTab(16),
       backupIPXRipTab(17),
       backupIPXSAPTab(18),
       resetStartupCDB(19),
       eraseStartupCDB(20),
       deleteZeroHopRoutingAllocTab(21),
       slipDisconnect(22),
       deleteDynamicLanTab(23),
       eraseRunningCDB(24),
       copyStartupToRunning(25),
       none(26),
       resetToFactoryDefaults(27),
       
    -- Eltex additional values
       resetNoLogging(100),
       eraseCandidateCDB(101),
       commitCandidateCDB(102),
       confirmCandidateCDB(103)
     }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "This variable enables the operator to perform one of the
      specified actions on the tables maintained by the network device.
      Send actions require support of proprietery File exchange
      protocol."
   ::= { rndMng 2  }

rndFileName OBJECT-TYPE
    SYNTAX OCTET STRING -- SIZE 256
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "The name of the file used internally by RND for transferring
      tables maintained by network devices, using a prorietary File
      exchange protocol."
    ::=  { rndMng 3  }

rlSnmpVersionSupported OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(1))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the snmp versions that are supported by
        this device."
    ::= { rndMng 4 }

rlSnmpMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the snmp support version that is supported by
        this device."
    ::= { rndMng 5 }

rlCpuUtilEnable OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enables measurement of the device CPU utilization.
         In order to get real values for rlCpuUtilDuringLastSecond, rlCpuUtilDuringLastMinute
         and rlCpuUtilDuringLast5Minutes, the value of this object must be true."
    DEFVAL { true }
    ::= { rndMng 6 }

rlCpuUtilDuringLastSecond OBJECT-TYPE
    SYNTAX INTEGER (0..101)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Percentage of the device CPU utilization during last second.
         The value 101 is a dummy value, indicating that the CPU utilization was
         not measured (since measurement is disabled or was disabled during last second)."
    ::= { rndMng 7 }

rlCpuUtilDuringLastMinute OBJECT-TYPE
    SYNTAX INTEGER (0..101)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Percentage of the device CPU utilization during last minute.
         The value 101 is a dummy value, indicating that the CPU utilization was
         not measured (since measurement is disabled or was disabled during last minute)."
    ::= { rndMng 8 }

rlCpuUtilDuringLast5Minutes OBJECT-TYPE
    SYNTAX INTEGER (0..101)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Percentage of the device CPU utilization during the last 5 minutes.
         The value 101 is a dummy value, indicating that the CPU utilization was
         not measured (since measurement is disabled or was disabled during last 5 minutes)."
    ::= { rndMng 9 }

rlRebootDelay OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Setting the variable will cause the device to reboot rlRebootDelay timeticks
         from the moment this variable was set.
         If not set, the variable will return a value of 4294967295.
         If set to 4294967295, reboot action is cancelled.
         The maximum delay is set by the host parameter: reboot_delay_max"
    ::= { rndMng 10 }

rlGroupManagement OBJECT IDENTIFIER ::= { rndMng 11 }

rlGroupMngQuery OBJECT-TYPE
    SYNTAX INTEGER {query(1), idle(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Setting value query will cause the device to query for UPNP devices on the network.
         The device will always return value idle for GET."
    ::= { rlGroupManagement 1 }

rlGroupMngQueryPeriod OBJECT-TYPE
    SYNTAX      INTEGER
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Sets desired interval between queries for UPNP devices on the network.
         Setting 0 will result in no such query.
         Note that the actual query interval might be less than the set value
         if another application running in the device requested a shorter interval.
         Likewise setting 0 will not necessarily stop periodic queries if another
         application is still interested in periodic polling."
    DEFVAL { 0 }
    ::= { rlGroupManagement 2 }

rlGroupMngLastUpdate OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The last time rlGroupMng MIB was updated."
    ::= { rlGroupManagement 3 }


rlGroupMngDevicesTable OBJECT-TYPE
   SYNTAX SEQUENCE OF RlGroupMngDeviceEntry
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
    "The table showing the discovered  devices."
     ::= { rlGroupManagement 4 }

rlGroupMngDeviceEntry  OBJECT-TYPE

   SYNTAX RlGroupMngDeviceEntry
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
       " The row definition for this table."
   INDEX {  rlGroupMngDeviceIdType, rlGroupMngDeviceId,  rlGroupMngSubdevice }

::= { rlGroupMngDevicesTable 1 }


RlGroupMngDeviceEntry ::= SEQUENCE {
   rlGroupMngDeviceIdType                InetAddressType,
   rlGroupMngDeviceId                    InetAddress,
   rlGroupMngSubdevice                   INTEGER,
   rlGroupMngDeviceDescription           DisplayString,
   rlGroupMngGroupMngEnabled             TruthValue,
   rlGroupMngGroupLLDPDeviceId           DisplayString,
   rlGroupMngDeviceVendor                DisplayString,
   rlGroupMngDeviceAdvertisedCachingTime  INTEGER,
   rlGroupMngDeviceLocationURL           DisplayString,
   rlGroupMngDeviceLastSeen              TimeTicks
}

rlGroupMngDeviceIdType OBJECT-TYPE
   SYNTAX     InetAddressType
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
    "The IP address type of the discovered device  "
     ::=  { rlGroupMngDeviceEntry 1 }

rlGroupMngDeviceId OBJECT-TYPE
   SYNTAX     InetAddress
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
    "The IP address of the discovered device  "
     ::=  { rlGroupMngDeviceEntry 2 }

rlGroupMngSubdevice    OBJECT-TYPE
   SYNTAX     INTEGER
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
    "A subdevice within the rlGroupMngDeviceId. Only subdevices with greatest
     specifity will be kept (specific UUID device is more specific than  basic device which is in turn
     more specific than root device.  "
     ::=  { rlGroupMngDeviceEntry 3 }

rlGroupMngDeviceDescription OBJECT-TYPE
   SYNTAX     DisplayString
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
    "The discovery protocol description of the device."
     ::=  { rlGroupMngDeviceEntry 4 }


rlGroupMngGroupMngEnabled           OBJECT-TYPE
   SYNTAX     TruthValue
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
    "Indicates whether the device has Group Management enable."
     ::=  { rlGroupMngDeviceEntry 5 }

rlGroupMngGroupLLDPDeviceId        OBJECT-TYPE
   SYNTAX     DisplayString
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
    "The LLDP device id. If  it  is empty the device id is not known (either it is a non-MTS device or  a non-LLDP supporting MTS device."
     ::=  { rlGroupMngDeviceEntry 6 }

rlGroupMngDeviceVendor OBJECT-TYPE
   SYNTAX     DisplayString
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
    "The vendor of the device. If empty the vendor is not known."
     ::=  { rlGroupMngDeviceEntry 7 }

rlGroupMngDeviceAdvertisedCachingTime OBJECT-TYPE
   SYNTAX     INTEGER
   UNITS      "seconds"
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
        "The caching time advertised by the device. If no update for this
         device has been received during this caching time the system will assume
         that the device has left the network and will therefore remove its entry
         from the table."
     ::=  { rlGroupMngDeviceEntry 8 }

rlGroupMngDeviceLocationURL OBJECT-TYPE
   SYNTAX     DisplayString
   UNITS      "seconds"
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
        "The URL inidicating the location of the XML presenting the details of  the device."
     ::=  { rlGroupMngDeviceEntry 9 }

rlGroupMngDeviceLastSeen  OBJECT-TYPE
   SYNTAX     TimeTicks
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
      "The value of sysUpTime at the moment of last reception of an  update for
       this device. "
     ::=  { rlGroupMngDeviceEntry 10 }

rlPrivateMIBroot OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the object identifier of the private MIB root in this device."
    ::= { rndMng 12 }

rlRunningCDBequalToStartupCDB OBJECT-TYPE

   SYNTAX     TruthValue
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
      "Indicates whether there are changes in running CDB that were not saved in flash."
     ::=  { rndMng 13 }


rlClearMib OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Clear MIB value for scalars or tables:
     Delete all entries for tables with dynamic entries.
     Set table entries default values for table with static entries.
     Set scalar default value."
    ::=  { rndMng 14  }

-------------------------------------------------------------------------------
-- Scheduled Reload
-------------------------------------------------------------------------------
rlScheduledReload OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..10))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Used for requesting a delayed reload of the device in a
        specific desired time, should be configured in one of the following formats:
        'athhmmddMM' , 'inhhhmmm' or '', setting this value to an empty string
        will result in request for cancellation of a (previously) committed system reload.
        to complete the request, the 'rlScheduledReloadCommit' must also be set to either
        TRUE (apply) or FALSE (discard) for completion of the transaction.
        failing from doing so will result in an indefinite lock of the API"
    ::= { rndMng 15 }

rlScheduledReloadPendingDate OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..24))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Displays the most recently requested scheduled-reload due date
         in 'inhhhmmathhmmssddMMYYYYw' format. where 'w' stands for weekDay (1-7).
         if there is no pending/scheduled reload request, string will be empty"
    ::= { rndMng 16 }

rlScheduledReloadApprovedDate OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..24))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Displays the most recently approved/committed scheduled-reload date
         in 'inhhhmmathhmmssddMMYYYYw' format. where 'w' stands for weekDay (1-7).
         if there is no committed scheduled-reload , string will be empty"
    ::= { rndMng 17 }

rlScheduledReloadCommit OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "commits the pending scheduled-reload request, and completes the transaction.
        when this value is set to TRUE, the system is instructed to perform the
        requested reload operation at the requested date/time
        as was given in 'rlScheduledReload'.
        setting this value to FALSE will discard the request."
    ::= { rndMng 18 }

-------------------------------------------------------------------------------
-- System Name Configuration Table
-------------------------------------------------------------------------------
rlSysNameTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlSysNameEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Holds the current system name configuration."
    ::= { rndMng 19 }

rlSysNameEntry OBJECT-TYPE
    SYNTAX RlSysNameEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The row definition of this table."
    INDEX { rlSysNameSource,
            rlSysNameIfIndex }
    ::= { rlSysNameTable 1 }

RlSysNameEntry ::= SEQUENCE {
    rlSysNameSource    INTEGER,
    rlSysNameIfIndex   InterfaceIndex,
    rlSysNameName      DisplayString (SIZE (0..255)),
    rlSysNameRowStatus RowStatus
}

rlSysNameSource OBJECT-TYPE
    SYNTAX INTEGER {
        dhcpv6(1),
        dhcpv4(2),
        static(3)
    }
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
       "The system name source. 'static' if defined by user through CLI,
        'dhcpv6' or 'dhcpv4' if received by DHCP network protocol."
    DEFVAL  { static }
    ::=   { rlSysNameEntry 1 }

rlSysNameIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS  current
    DESCRIPTION
        "The IfIndex from which the system-name configuration was received,
         for static entries, value will always be 1."
    DEFVAL { 1 }
    ::=   { rlSysNameEntry 2 }

rlSysNameName OBJECT-TYPE
    SYNTAX DisplayString (SIZE (0..255))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "An administratively-assigned name for this managed node.
         By convention, this is the node's fully-qualified domain
         name.  If the name is unknown, the value is the zero-length
         string."
    ::=   { rlSysNameEntry 3 }

rlSysNameRowStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The row status variable, used according to
         row installation and removal conventions."
    ::= { rlSysNameEntry 4 }

-------------------------------------------------------------------------------

rlErrdisableLinkFlappingCause OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable/Disable Link flapping error disable in the switch."
    ::= { rndMng 20 }


-------------------------------------------------------------------------------

rlDefaultSysName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..160))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The default value for the administratively-assigned name for this managed node.
             If the name is unknown, the value is the zero-length string."
    ::= { rndMng 21 }
	
END

