RADLAN-vlanVoice-MIB DEFINITIONS ::= BEGIN

IMPORTS
    vlan                                        FROM RADLAN-vlan-MIB
    TruthValue, RowStatus,MacAddress,
    DisplayString                               FROM SNMPv2-TC
    ifIndex                                     FROM IF-MIB
    MODULE-IDENTITY, OBJECT-TYPE                FROM SNMPv2-SMI
    VlanIndex                                   FROM Q-BRIDGE-MIB
    VlanPriority                                FROM RADLAN-MIB;

vlanVoice MODULE-IDENTITY
              LAST-UPDATED "201001090000Z"
              ORGANIZATION "Marvell Semiconductor, Inc."
              CONTACT-INFO
					"5488 Marvell Lane
					Santa Clara, CA 95054
					USA

					Website:  www.marvell.com"
              DESCRIPTION
                      "The private MIB module definition for voice vlan support in Marvell devices."
              REVISION "201009260000Z"
              DESCRIPTION
                       "Editorial changes to support new MIB compilers."
              REVISION "201009260000Z"
              DESCRIPTION
                      "Initial version of this MIB."
          ::= { vlan 54 }

-- voice vlan

-- start from 6 since 1..5 are deprecated voice
vlanVoiceAdminState OBJECT-TYPE
   SYNTAX INTEGER {
        disabled(0),
        auto-enabled(1),
        auto-triggered(2),
        oui-enabled(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        " administrative voice vlan status "
    ::= { vlanVoice 6 }

vlanVoiceOperState OBJECT-TYPE
   SYNTAX INTEGER {
        disabled(0),
        auto-enabled(1),
        auto-triggered(2),
        oui-enabled(3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        " operational voice vlan status "
    ::= { vlanVoice 7 }

vlanVoiceAdminVid OBJECT-TYPE
    SYNTAX      INTEGER (1..4094)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "1-4094 actual vlan (must exist in dot1qvlan static table)"
    DEFVAL { 1 }
    ::= { vlanVoice 8 }

vlanVoiceOperVid OBJECT-TYPE
    SYNTAX      INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        " operational Voice Vlan ID"
    ::= { vlanVoice 9 }

-- Voice VLAN local configuration configuration Table
vlanVoiceUcDeviceTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF VlanVoiceUcDeviceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing static default and UC directly connected to device configuration."
    ::= { vlanVoice 10 }

vlanVoiceUcDeviceEntry OBJECT-TYPE
    SYNTAX      VlanVoiceUcDeviceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Static and dynamic per port information for a voice VLAN."
    INDEX { vlanVoiceUcDeviceType, vlanVoiceUcDeviceMacAddress, vlanVoiceUcDeviceInterface }
    ::= { vlanVoiceUcDeviceTable 1 }

VlanVoiceUcDeviceEntry ::= SEQUENCE {
    vlanVoiceUcDeviceType          INTEGER { default(0), static(1), uc(2) },
    vlanVoiceUcDeviceMacAddress    MacAddress,
    vlanVoiceUcDeviceInterface     INTEGER,
    vlanVoiceUcDeviceVid           INTEGER (1..4094),
    vlanVoiceUcDeviceVpt           INTEGER (0..7),
    vlanVoiceUcDeviceDscp          INTEGER (0..63),
    vlanVoiceUcDeviceIsBest        TruthValue
}

vlanVoiceUcDeviceType OBJECT-TYPE
    SYNTAX      INTEGER { default(0),
                          static(1),
                          uc(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "type of entry"
    ::= { vlanVoiceUcDeviceEntry 1 }


vlanVoiceUcDeviceMacAddress OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Mac address of UC"
    ::= { vlanVoiceUcDeviceEntry 2 }

vlanVoiceUcDeviceInterface OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Mac interface on which UC is connected"
    ::= { vlanVoiceUcDeviceEntry 3 }

vlanVoiceUcDeviceVid OBJECT-TYPE
    SYNTAX      INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Voice Vlan ID"
    ::= { vlanVoiceUcDeviceEntry 4 }

vlanVoiceUcDeviceVpt OBJECT-TYPE
    SYNTAX      INTEGER (0..7)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The entry VPT"
    ::= { vlanVoiceUcDeviceEntry 5 }

vlanVoiceUcDeviceDscp OBJECT-TYPE
    SYNTAX      INTEGER (0..63)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The entry DSCP value"
    ::= { vlanVoiceUcDeviceEntry 6 }

vlanVoiceUcDeviceIsBest OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether this entry is used as best local configuration"
    ::= { vlanVoiceUcDeviceEntry 7 }

-- voice vlan auto
vlanVoiceAuto  OBJECT IDENTIFIER ::= { vlanVoice 11 }

-- voice vlan auto admin

vlanVoiceAutoAdmin  OBJECT IDENTIFIER ::= { vlanVoiceAuto 1 }

vlanVoiceAutoAdminVpt OBJECT-TYPE
    SYNTAX      VlanPriority
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "user configured VPT for Voice Vlan operation"
    DEFVAL { 0 }
    ::= { vlanVoiceAutoAdmin 1 }

vlanVoiceAutoAdminDscp OBJECT-TYPE
    SYNTAX      INTEGER (0..63)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "user configured DSCP for Voice Vlan operation"
    DEFVAL { 0 }
    ::= { vlanVoiceAutoAdmin 2 }

-- voice vlan auto oper

vlanVoiceAutoOper  OBJECT IDENTIFIER ::= { vlanVoiceAuto 2 }

vlanVoiceAutoOperVpt OBJECT-TYPE
    SYNTAX      VlanPriority
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "operational VPT for Voice Vlan operation"
    ::= { vlanVoiceAutoOper 1 }

vlanVoiceAutoOperDscp OBJECT-TYPE
    SYNTAX      INTEGER (0..63)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "user configured DSCP for Voice Vlan operation"
    ::= { vlanVoiceAutoOper 2 }

vlanVoiceAutoOperSource OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Mac address of the switch by which we've selected the VVID"
    ::= {vlanVoiceAutoOper 3 }

vlanVoiceAutoOperPriority OBJECT-TYPE
    SYNTAX INTEGER {
        staticActive(0),    -- VVID selected according to user configuration of an active device
        staticInActive(1),  -- VVID selected according to user configuration of an inactive device
        ucActive(2),        -- VVID selected according to UC device + UC device is active
        ucInActive(3),      -- VVID selected according to UC device + UC device is inactive
        default(6),         -- VVID is at default (no UC device + no static configuration in lan)
        disabled(10)        -- Voice Vlan is disabled
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The reason for which Voice Vlan ID was selected."
    ::= { vlanVoiceAutoOper 4 }


vlanVoiceAutoRefresh  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "By setting the MIB to True, VSDP refresh will be executed."
    ::= { vlanVoiceAuto 3 }

vlanVoiceAutoAgreedVlanLastChange OBJECT-TYPE
   SYNTAX DisplayString (SIZE(12))
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
        "date format is DDMMYYHHMMSS"
    ::= { vlanVoiceAuto 4 }


-- voice vlan OUI

vlanVoiceOUIBased  OBJECT IDENTIFIER ::= { vlanVoice 12 }

vlanVoiceOUIBasedAdminPriority OBJECT-TYPE
    SYNTAX      VlanPriority
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An administratively assigned Priority, which will be used
        for all traffic on the voice vlan, this gives the packets
        the requested priority (CoS) within the bridge."
    DEFVAL { 6 }
     ::= { vlanVoiceOUIBased 1 }

vlanVoiceOUIBasedAdminRemark OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Remark VPT on tagged frames egress the voice vlan according.
         to priority true.false"
    DEFVAL { false }
    ::= { vlanVoiceOUIBased 2 }

vlanVoiceOUIBasedSetToDefault OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The vlanVoiceOUIBasedSetToDefault indicates that vlanVoiceOUIBasedTable
            should be set to it's default values if existed
            (OUI default prefixes).

            To do so the vlanVoiceOUIBasedTable should be previously deleted by usual
            entries destroying.

            This object behaviors as write-only than
            reading this object will always return 'false'."
    DEFVAL{ false }
    ::= { vlanVoiceOUIBased 3 }

-- Voice VLAN OUI Table
vlanVoiceOUIBasedTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF VlanVoiceOUIBasedEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing static global configuration information for Voice VLANs OUI MAC Prefixes.
        All entries are permanent and will be restored after the device is reset."
    ::= { vlanVoiceOUIBased 4 }

vlanVoiceOUIBasedEntry OBJECT-TYPE
    SYNTAX      VlanVoiceOUIBasedEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information for a voice VLANs OUI MAC Prefixes configured into the
        device by management."
    INDEX   { vlanVoiceOUIBasedPrefix }
    ::= { vlanVoiceOUIBasedTable  1 }

VlanVoiceOUIBasedEntry ::= SEQUENCE {
              vlanVoiceOUIBasedPrefix                      OCTET STRING,
              vlanVoiceOUIBasedDescription                 DisplayString,
              vlanVoiceOUIBasedEntryRowStatus              RowStatus,
              vlanVoiceOUIBasedDynamicType                 TruthValue
}

vlanVoiceOUIBasedPrefix   OBJECT-TYPE
    SYNTAX         OCTET STRING(SIZE(3))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The index value used to identify the OUI MAC Prefix component
             associated with this entry.

            The value of this object is used as an index to the
            vlanVoiceOUIBasedTable.

            Voice VLANs OUI Prefix is the first 3 most significant
            octets of the MAC address."
    ::= { vlanVoiceOUIBasedEntry 1 }

vlanVoiceOUIBasedDescription OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..160))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An optional text that describes the OUI."
    DEFVAL {""}
    ::=  { vlanVoiceOUIBasedEntry 2 }

vlanVoiceOUIBasedEntryRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the status of this entry."
    ::= { vlanVoiceOUIBasedEntry 3 }

vlanVoiceOUIBasedDynamicType OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates dynamic type of OUI record."
    ::= { vlanVoiceOUIBasedEntry 4 }

-- Voice VLAN per Port configuration Table
vlanVoiceOUIBasedPortTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF VlanVoiceOUIBasedPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing static and dynamic per port configuration information for Voice VLAN.
        All entries are permanent and will be restored after the device is reset."
    ::= { vlanVoiceOUIBased 5 }

vlanVoiceOUIBasedPortEntry OBJECT-TYPE
    SYNTAX      VlanVoiceOUIBasedPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Static and dynamic per port information for a voice VLAN."
    INDEX { ifIndex }
    ::= { vlanVoiceOUIBasedPortTable 1 }

VlanVoiceOUIBasedPortEntry ::= SEQUENCE {
              vlanVoiceOUIBasedPortEnable                           TruthValue,
              vlanVoiceOUIBasedPortVlanIndex                        VlanIndex,
              vlanVoiceOUIBasedPortSecure                           TruthValue,
              vlanVoiceOUIBasedPortCurrentMembership                INTEGER {active(1),notActive(2)},
              vlanVoiceOUIBasedPortQosMode                          INTEGER {src(1),all(2)}
}

vlanVoiceOUIBasedPortEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable this port to be a candidate to be added into the Voice VLAN."
    DEFVAL{ false }
    ::= { vlanVoiceOUIBasedPortEntry 1 }

vlanVoiceOUIBasedPortVlanIndex OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The Voice VLAN-ID the port is a candidate to be in."
    DEFVAL{ 4095 }
    ::= { vlanVoiceOUIBasedPortEntry 2 }

vlanVoiceOUIBasedPortSecure OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specify this port to be in Secure Mode when entering the Voice VLAN.
          In Secure mode only frames with MAC prefix matched to one of the OUI table prefixes
         are accepted, otherwise dropped."
    DEFVAL{ false }
    ::= { vlanVoiceOUIBasedPortEntry 3 }

vlanVoiceOUIBasedPortCurrentMembership OBJECT-TYPE
    SYNTAX  INTEGER {
            active(1),
            notActive(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Port's current status of membership in Voice VLAN.

         Port's possible values of membership in Voice VLAN:
          'Active(1)'    - Port is currently added to a Voice VLAN .
          'NotActive(2)' - Specifies either that port is a candidate to be
                           in Voice VLAN or disabled."
    ::= { vlanVoiceOUIBasedPortEntry 4 }

vlanVoiceOUIBasedPortQosMode OBJECT-TYPE
    SYNTAX  INTEGER {
            src(1),
            all(2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Port's current QOS mode in Voice VLAN.
         Possible values:
          'src(1)' - Only traffic with OUI prefix in the source MAC received QOS of the Voice Vlan.
          'all(2)' - All traffic through that port received QOS of the Voice Vlan."
    ::= { vlanVoiceOUIBasedPortEntry 5 }

vlanVoiceOUIBasedAgingTimeout OBJECT-TYPE
    SYNTAX      INTEGER (1..43200)
    UNITS       "minutes"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The vlanVoiceAgingTimeout indicates the time (in units of
            minutes) from when the last OUI MAC was ageout from the FDB the port
            will be removed from the Voice VLAN.

            The default value for vlanVoiceAgingTimeout object is 1440 minutes (24 hours).

            The value of this object must be restored from non-volatile
            storage after a re-initialization of the management system."
    DEFVAL      { 1440 }
    ::= { vlanVoiceOUIBased 6 }


END
