RADLAN-SENSORENTMIB DEFINITIONS ::= BEGIN

IMPORTS
        rlEnv
                FROM RADLAN-HWENVIROMENT
        MODULE-IDENTITY, OBJECT-TYPE,
        Integer32, Unsigned32, mib-2
                FROM SNMPv2-SMI
        entPhySensorEntry
                FROM ENTITY-SENSOR-MIB
        MODULE-COMPLIANCE, OBJECT-GROUP
                FROM SNMPv2-CONF
        TEXTUAL-CONVENTION, TimeStamp
                FROM SNMPv2-TC
        entPhysicalIndex, entityPhysicalGroup
                FROM ENTITY-MIB
        SnmpAdminString
                FROM SNMP-FRAMEWORK-MIB
        EntitySensorValue
                FROM ENTITY-SENSOR-MIB;

rlSensor MODULE-IDENTITY
        LAST-UPDATED "200309210000Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
                "The private MIB module definition for sensors in Radlan devices."
        REVISION "200309210000Z"
        DESCRIPTION
                "Add DDR sensor."
        REVISION "201906300000Z"
        DESCRIPTION
                "ADDED this MODULE-IDENTITY clause."
        ::= { rlEnv 4 }

rlEntPhySensorTable OBJECT-TYPE
        SYNTAX     SEQUENCE OF RlEntPhySensorEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
                "The addition to the table of sensors maintained by the environmental
                monitor."
        ::= { rlEnv 3 }

rlEntPhySensorEntry OBJECT-TYPE
        SYNTAX     RlEntPhySensorEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
                "An additon to the entry in the sensor table, representing the
                maximum/minimum values for the sensor associated."
        AUGMENTS     {entPhySensorEntry}
        ::= { rlEntPhySensorTable 1 }

RlEntPhySensorEntry ::=
        SEQUENCE {
                rlEnvPhySensorMinValue       EntitySensorValue,
                rlEnvPhySensorMaxValue       EntitySensorValue,
                rlEnvPhySensorTestValue      EntitySensorValue,
                rlEnvPhySensorLocation       SnmpAdminString
        }

rlEnvPhySensorMinValue OBJECT-TYPE
        SYNTAX     EntitySensorValue
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
                "Minimum value for the Sensor being instrumented."
        ::= { rlEntPhySensorEntry 1 }

rlEnvPhySensorMaxValue OBJECT-TYPE
        SYNTAX     EntitySensorValue
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
                "Maximum value for the Sensor being instrumented."
        ::= { rlEntPhySensorEntry 2 }

rlEnvPhySensorTestValue OBJECT-TYPE
        SYNTAX     EntitySensorValue
        MAX-ACCESS read-write
        STATUS     current
        DESCRIPTION
                "Test/reference value for the Sensor being instrumented."
        ::= { rlEntPhySensorEntry 3 }

rlEnvPhySensorLocation OBJECT-TYPE
        SYNTAX     SnmpAdminString
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
                "A textual description for the Location where the Sensor being instrumented."
        ::= { rlEntPhySensorEntry 4 }
END

