MARVELL-PBR-MIB DEFINITIONS ::= BEGIN

IMPORTS
    rnd                                                         FROM RADLAN-MIB
    InetAddressType,InetAddress,InetAddressIPv6                 FROM INET-ADDRESS-MIB -- RFC2851
    TEXTUAL-CONVENTION, DisplayString, RowStatus                FROM SNMPv2-TC
    InterfaceIndexOrZero, InterfaceIndex                        FROM IF-MIB              -- [RFC2863]
    OBJECT-TYPE, Unsigned32                                     FROM SNMPv2-SMI
    rlRouteMapPbrRouteMapName, rlRouteMapPbrRouteMapSectionId   FROM MARVELL-ROUTEMAP-MIB;


rlPolicyBasedRouting   MODULE-IDENTITY
        LAST-UPDATED "201506080000A"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
                "The private MIB module definition for Policy-Based Routing mechanism."
        REVISION "201506080000A"
        DESCRIPTION
                "Added this MODULE-IDENTITY clause."
        ::= { rnd 228 }

RlPBRInetType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "The inet type of a policy"
     SYNTAX INTEGER {
            ipv4(1),
            ipv6(2)
     }

RlPBRStatusType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "The types of status for policy-based routing entry"
     SYNTAX INTEGER {
            active(1),
            noIp(2),
            interfaceDown(3)
     }


-- ============================================================
--                     rlPBRTable
-- ============================================================

rlPBRTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlPBREntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION        "Table containing policy-based routing binding information."
   ::= { rlPolicyBasedRouting 1 }

rlPBREntry OBJECT-TYPE
    SYNTAX  RlPBREntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The row definition for this table."
    INDEX { rlPBRIfIndex,
            rlPBRInetType }
    ::= { rlPBRTable 1 }

RlPBREntry ::= SEQUENCE {
    rlPBRIfIndex            InterfaceIndex,
    rlPBRInetType           RlPBRInetType,
    rlPBRRouteMapName       DisplayString,
    rlPBRStatus             RlPBRStatusType,
    rlPBRRowStatus          RowStatus
}

rlPBRIfIndex OBJECT-TYPE
   SYNTAX       InterfaceIndex
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION  "IfIndex on which policy based routing is applied."
   ::= { rlPBREntry 1 }

rlPBRInetType OBJECT-TYPE
   SYNTAX       RlPBRInetType
   MAX-ACCESS   not-accessible
   STATUS       current
   DESCRIPTION  "Inet type of this entry."
   ::= { rlPBREntry 2 }

rlPBRRouteMapName OBJECT-TYPE
   SYNTAX       DisplayString (SIZE(1..64))
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION  "Route map name to apply."
   ::= { rlPBREntry 3 }

rlPBRStatus OBJECT-TYPE
   SYNTAX       RlPBRStatusType
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION  "The route status for this entry."
   ::= { rlPBREntry 4 }

rlPBRRowStatus OBJECT-TYPE
   SYNTAX       RowStatus
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION  "The row status of this entry."
   ::= { rlPBREntry 5 }


-- ============================================================
--                     rlPBRInfoTable
-- ============================================================

RlPBRNexthopStatusType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "The types of status of nexthop for policy-based routing entry"
     SYNTAX INTEGER {
            active(1),
            notReachable(2),
            notDirect(3)
     }

rlPBRInfoTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlPBRInfoEntry
   MAX-ACCESS  not-accessible
   STATUS current
   DESCRIPTION        "Table containing policy-based routing information."
   ::= { rlPolicyBasedRouting 2 }

rlPBRInfoEntry OBJECT-TYPE
    SYNTAX  RlPBRInfoEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The row definition for this table."
    INDEX { rlPBRInetType,
            rlPBRIfIndex,
            rlRouteMapPbrRouteMapName,
            rlRouteMapPbrRouteMapSectionId }
    ::= { rlPBRInfoTable 1 }

RlPBRInfoEntry ::= SEQUENCE {
    rlPBRInfoAccessListName         DisplayString,
    rlPBRInfoNexthopInetAddressType InetAddressType,
    rlPBRInfoNexthopInetAddress     InetAddress,
    rlPBRInfoNexthopIfIndex         InterfaceIndexOrZero,
    rlPBRInfoNexthopStatus          RlPBRNexthopStatusType
}

rlPBRInfoAccessListName OBJECT-TYPE
   SYNTAX       DisplayString(SIZE(1..32))
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION  "Access-list name of policy-based routing."
   ::= { rlPBRInfoEntry 1 }

rlPBRInfoNexthopInetAddressType OBJECT-TYPE
   SYNTAX       InetAddressType
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION  "Inet type of rlPBRInfoNexthopInetAddress"
   ::= { rlPBRInfoEntry 2 }

rlPBRInfoNexthopInetAddress OBJECT-TYPE
   SYNTAX       InetAddress
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION  "Inet address of nexthop, if used for action."
   ::= { rlPBRInfoEntry 3 }

rlPBRInfoNexthopIfIndex OBJECT-TYPE
   SYNTAX       InterfaceIndexOrZero
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION  "Inet address of nexthop, if used for action."
   ::= { rlPBRInfoEntry 4 }

rlPBRInfoNexthopStatus OBJECT-TYPE
   SYNTAX       RlPBRNexthopStatusType
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION  "Status of nexthop."
   ::= { rlPBRInfoEntry 5 }

END
