RADLAN-SYSLOG-MIB DEFINITIONS ::= BEGIN

-- Title:      RADLAN SYSLOG Private MIB
-- Version:    7.35
-- Date:       15 Jan 2005
--
-- 15-Jun-2003  Added rlSyslogFileMessagesLogged and rlSyslogCacheTotalMessages

IMPORTS
    rnd                                     FROM RADLAN-MIB
    OBJECT-TYPE, IpAddress, Unsigned32,Counter32,
    MODULE-IDENTITY                         FROM SNMPv2-SMI
    DisplayString, TEXTUAL-CONVENTION,
    TruthValue, RowStatus                   FROM SNMPv2-TC
	InetAddressType, InetAddress
                                            FROM INET-ADDRESS-MIB;

 rlSyslog MODULE-IDENTITY
          LAST-UPDATED "200602120000Z"
          ORGANIZATION "Marvell Semiconductor, Inc."
          CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
          DESCRIPTION
                  "The private MIB module definition for SYSLOG services in Radlan devices."
          REVISION "200602120000Z"
          DESCRIPTION
                  "Editorial changes to support new MIB compilers."
          REVISION "200309220000Z"
          DESCRIPTION
                  "Initial version of this MIB."
          ::= { rnd 82 }

RlSyslogSeverity ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "This textual convention maps out to the minimal severity levels
         of syslog messages, or indicate non Active. The syslog protocol
         uses the values 0 (emergency), to 7 (debug) last value notActive
         added to indicate inactivity."
    SYNTAX  INTEGER {
        emergency(0),
        alert(1),
        critical(2),
        error(3),
        warning(4),
        notice(5),
        info(6),
        debug(7),
        notActive(8)
    }

rlSyslogPrivate  OBJECT IDENTIFIER ::= { rlSyslog 2 }

rlSyslogGlobalEnable OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Global enable for syslog flash, syslog cache and syslog UDP.
         When set to false, only console logging is performed."
    DEFVAL  { true }
    ::= { rlSyslogPrivate 1 }

rlSyslogMinLogToConsoleSeverity OBJECT-TYPE
    SYNTAX  RlSyslogSeverity
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The minimal severity to log to console. Lower severity
         will not be written to console. Value notActive indicate this
         activity is disabled."
    DEFVAL  { info }
    ::= { rlSyslogPrivate 2 }

rlSyslogMinLogToFileSeverity OBJECT-TYPE
    SYNTAX  RlSyslogSeverity
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The minimal severity to log to LogFile. Lower severity
         will not be written to the LogFile. Value notActive indicates
         this activity is disabled."
    DEFVAL  { error }
    ::= { rlSyslogPrivate 3 }

rlSyslogMinLogToCacheSeverity OBJECT-TYPE
    SYNTAX  RlSyslogSeverity
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The minimal severity to log to memory cache. Lower severity
         will not be read from cache. Value notActive indicate this activity
         is disabled. Note that all events are logged to cache unless its
         severity is notActive."
    DEFVAL  { info }
    ::= { rlSyslogPrivate 4 }

rlSyslogClearLogfile OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting to a value other than 0 results in deleting the log file."
    ::= { rlSyslogPrivate 5 }

rlSyslogClearCache OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting to a value other than 0 results in clearing the memory cache."
    ::= { rlSyslogPrivate 6 }

rlSyslogMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS      read-only
    STATUS      current
    DESCRIPTION
        "The Syslog MIB's version. It's 1."
    ::= { rlSyslogPrivate 7 }

--
-- rlSyslogLog Table
--
rlSyslogLogTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSyslogLogEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table containing events sent to the system log file."
    ::= { rlSyslogPrivate 8 }

rlSyslogLogEntry OBJECT-TYPE
    SYNTAX  RlSyslogLogEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION  "A log entry "
    INDEX  { rlSyslogLogCounter   }
    ::= { rlSyslogLogTable 1 }

RlSyslogLogEntry ::=
    SEQUENCE {
        rlSyslogLogCounter          Unsigned32,
        rlSyslogLogDateTime         DisplayString,
        rlSyslogLogAppMnemonic      DisplayString,
        rlSyslogLogSeverity         RlSyslogSeverity,
        rlSyslogLogMessageMnemonic  DisplayString,
        rlSyslogLogText1            DisplayString,
        rlSyslogLogText2            DisplayString,
        rlSyslogLogText3            DisplayString,
        rlSyslogLogText4            DisplayString
    }
rlSyslogLogCounter   OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A counter that identifies this entry - used to differentiate logged
         entries. And the order given is the order of logging. A entries may
         not form sequence of this value. (Time is not a differentiating
         element as logged entries may come in a sequence."
    ::= { rlSyslogLogEntry 1 }

rlSyslogLogDateTime   OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time in string (formated DD-MMM-YYYY HH:MM:SS e.g
         14-Apr-2002 10:33:31), when the error was logged.."
    ::= { rlSyslogLogEntry 2 }

rlSyslogLogAppMnemonic OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..8))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Application that created this error."
    ::= { rlSyslogLogEntry 3 }

rlSyslogLogSeverity OBJECT-TYPE
    SYNTAX  RlSyslogSeverity
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Severity of the reported error."
    ::= { rlSyslogLogEntry 4 }

rlSyslogLogMessageMnemonic OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Short identifier of this message that created this error."
    ::= { rlSyslogLogEntry 5 }

rlSyslogLogText1 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 1."
    ::= { rlSyslogLogEntry 6 }

rlSyslogLogText2 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 2."
    ::= { rlSyslogLogEntry 7 }

rlSyslogLogText3 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 3."
    ::= { rlSyslogLogEntry 8 }

rlSyslogLogText4 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 4."
    ::= { rlSyslogLogEntry 9 }

--
-- rlSyslogLogCache Table
--
rlSyslogLogCacheTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSyslogLogCacheEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table containing errors registered to system cache."
    ::= { rlSyslogPrivate 9 }

rlSyslogLogCacheEntry OBJECT-TYPE
    SYNTAX  RlSyslogLogCacheEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION "A log history entry"
    INDEX  { rlSyslogLogCacheCounter   }
    ::= { rlSyslogLogCacheTable 1 }

RlSyslogLogCacheEntry ::=
    SEQUENCE {
        rlSyslogLogCacheCounter             Unsigned32,
        rlSyslogLogCacheDateTime            DisplayString,
        rlSyslogLogCacheAppMnemonic         DisplayString,
        rlSyslogLogCacheSeverity            RlSyslogSeverity,
        rlSyslogLogCacheMessageMnemonic     DisplayString,
        rlSyslogLogCacheText1               DisplayString,
        rlSyslogLogCacheText2               DisplayString,
        rlSyslogLogCacheText3               DisplayString,
        rlSyslogLogCacheText4               DisplayString
    }
rlSyslogLogCacheCounter   OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A counter that identifies this entry - used to differentiate logged
         entries. And the order given is the order of logging. A entries may
         not form sequence of this value. (Time is not a differentiating
         element as logged entries may come in a sequence."
    ::= { rlSyslogLogCacheEntry 1 }

rlSyslogLogCacheDateTime   OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time in string (formated DD-MMM-YYYY HH:MM:SS e.g
         14-Apr-2002 10:33:31), when the eroor was logged.."
    ::= { rlSyslogLogCacheEntry 2 }

rlSyslogLogCacheAppMnemonic OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..8))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Application that created this error."
    ::= { rlSyslogLogCacheEntry 3 }

rlSyslogLogCacheSeverity OBJECT-TYPE
    SYNTAX  RlSyslogSeverity
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Severity of the reported error."
    ::= { rlSyslogLogCacheEntry 4 }

rlSyslogLogCacheMessageMnemonic OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Short identifier of this message that created this error."
    ::= { rlSyslogLogCacheEntry 5 }

rlSyslogLogCacheText1 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 1."
    ::= { rlSyslogLogCacheEntry 6 }

rlSyslogLogCacheText2 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 2."
    ::= { rlSyslogLogCacheEntry 7 }

rlSyslogLogCacheText3 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 3."
    ::= { rlSyslogLogCacheEntry 8 }

rlSyslogLogCacheText4 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 4."
    ::= { rlSyslogLogCacheEntry 9 }

rlSyslogConsoleMessagesIgnored OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This is a count of messages not sent to the console
         because the severity level of the message was above
         rlSyslogMinLogToConsoleSeverity, the higher the level,
         the lower the severity."
    ::= { rlSyslogPrivate 10 }

rlSyslogFileMessagesIgnored OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This is a count of messages not sent to the file
         because the severity level of the message was above
         rlSyslogMinLogToFileSeverity, the higher the level,
         the lower the severity."
::= { rlSyslogPrivate 11 }

rlSyslogFileMessagesLogged OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This is a count of all the messages currently held in the
        Log file."
::= { rlSyslogPrivate 12 }

rlSyslogCacheTotalMessages OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This is a count of all the messages currently held in the
        cache."
::= { rlSyslogPrivate 13 }


rlSyslogAggregationEnable  OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "enable/disable Syslog aggregation"
    ::= { rlSyslogPrivate 14 }

rlSyslogAggregationAgingTime OBJECT-TYPE
    SYNTAX  Unsigned32  (15..3600)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "aging time for Syslog aggregated messages"
    DEFVAL {300}
    ::= { rlSyslogPrivate 15 }

rlSyslogMinLogToWebSeverity OBJECT-TYPE
    SYNTAX  RlSyslogSeverity
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The minimal severity to log to WEB client. Lower severity
         will not be displayed in WEB client.
         Value notActive indicate this activity
         is disabled."
    DEFVAL  { info }
    ::= { rlSyslogPrivate 16 }

rlSyslogAlarmFlag OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The MIB is initiated by false and it is set to true every time
        when a syslog message with severity >= min_severity_to_alarm_threshold (host parameter)
        is generated."
    DEFVAL  { false }
    ::= { rlSyslogPrivate 17 }

rlSyslogOriginId OBJECT-TYPE
    SYNTAX INTEGER {
        default(1),
        hostname (2),
        ip (3),
        ipv6 (4),
        string (5)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Defines the origin field of the SYSLOG message packets sent to the SYSLOG server"
    DEFVAL { default }
    ::= { rlSyslogPrivate 18 }

rlSyslogOriginIdString OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..160))
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Defines the string origin of the SYSLOG message packets sent to the SYSLOG server"
    ::= { rlSyslogPrivate 19 }

rlSyslogHeaderSendingEnabled OBJECT-TYPE
    SYNTAX  TruthValue
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enabled sending/not sending of syslog header in syslog messages to syslog collectors."
    DEFVAL  { true }
    ::= { rlSyslogPrivate 20 }

rlSyslogPhaseOneTests OBJECT IDENTIFIER ::= { rlSyslog 3}

rlSyslogPhaseOneTestGenerator OBJECT-TYPE
    SYNTAX  INTEGER {
        successfulRegistration(11),
        regTheSameComponentTwice (12),
        regWithInvalidComponentID(13),
        regWithInvalidApplicationID(14),
        regWithInvalidMessageString(15),
        regWithInvalidMessageList(16),
        regWithInvalidApplicationList(17),
        successfulLoggingWithNoParams(21),
        logWithUnregisteredComponentID(22),
        logWithInvalidComponentID(23),
        logWithBadApplicationID(24),
        logWithBadMessageID(25),
        paramFormatting(31),
        insufficientParams(32),
        incorrectParams(33),
        tooManyParams(34),
        oversizedParams(35),
        trapParams(36),
        successfulFatalError(41),
        fatalErrorThroughNonFatalInterface(42),
        nonFatalErrorThroughFatalInterface(43),
        nestedFatalErrors(47),
        snmpAccessToLongMessage(62)

    }
-- todo: once we have all of the tests, change them into an enum.
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
      "Writing a value to this leaf results in a test being run on the host."
    ::=  { rlSyslogPhaseOneTests 1 }

--------------------------------------------------------------
 -- rlSyslogCountersPerSeverityEntry
 --------------------------------------------------------------
rlSyslogCountersPerSeverityTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSyslogCountersPerSeverityEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table displays counters per syslog severity"
    ::= { rlSyslogPrivate 21 }

rlSyslogCountersPerSeverityEntry OBJECT-TYPE
    SYNTAX  RlSyslogCountersPerSeverityEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "Static row for this table."
    INDEX { rlSyslogCountersPerSeverityIndex }
    ::= { rlSyslogCountersPerSeverityTable 1 }

RlSyslogCountersPerSeverityEntry ::= SEQUENCE {
    rlSyslogCountersPerSeverityIndex               INTEGER,
    rlSyslogCountersPerSeverityEmergencyCounter    Counter32,
    rlSyslogCountersPerSeverityAlertCounter        Counter32,
    rlSyslogCountersPerSeverityCriticalCounter     Counter32,
    rlSyslogCountersPerSeverityErrorCounter        Counter32,
    rlSyslogCountersPerSeverityWarningCounter      Counter32,
    rlSyslogCountersPerSeverityNoticeCounter       Counter32,
    rlSyslogCountersPerSeverityInfoCounter         Counter32,
    rlSyslogCountersPerSeverityDebugCounter        Counter32
}

rlSyslogCountersPerSeverityIndex  OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
     "The table contains only one static entry."
   ::= { rlSyslogCountersPerSeverityEntry 1 }

rlSyslogCountersPerSeverityEmergencyCounter OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Emergency syslog messages "
    ::= { rlSyslogCountersPerSeverityEntry 2 }

rlSyslogCountersPerSeverityAlertCounter OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Alert syslog messages"
    ::= { rlSyslogCountersPerSeverityEntry 3 }

rlSyslogCountersPerSeverityCriticalCounter OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Critical syslog messages"
    ::= { rlSyslogCountersPerSeverityEntry 4 }

rlSyslogCountersPerSeverityErrorCounter OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Error syslog messages"
    ::= { rlSyslogCountersPerSeverityEntry 5 }

rlSyslogCountersPerSeverityWarningCounter OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Warning syslog messages"
    ::= { rlSyslogCountersPerSeverityEntry 6 }

rlSyslogCountersPerSeverityNoticeCounter OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Notice syslog messages"
    ::= { rlSyslogCountersPerSeverityEntry 7 }

rlSyslogCountersPerSeverityInfoCounter OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Info syslog messages"
    ::= { rlSyslogCountersPerSeverityEntry 8 }

rlSyslogCountersPerSeverityDebugCounter OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Counts Debug syslog messages"
    ::= { rlSyslogCountersPerSeverityEntry 9 }

-- -------------------------------------------------------------
-- rlsnmpSyslogCollector Table
-- -------------------------------------------------------------

rlsnmpSyslogCollectorTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlsnmpSyslogCollectorEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing Syslog collector information. Internal MIB that configured by snmpSyslogCollectorTable"
    ::= { rlSyslogPrivate 22 }

rlsnmpSyslogCollectorEntry OBJECT-TYPE
    SYNTAX      RlsnmpSyslogCollectorEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines the information to generate syslog messages to
         an aggregating agent or collector.

         Entries within this table with an access level of read-
         create MUST be considered non-volatile and MUST be
         maintained across entity resets."
    INDEX  { rlsnmpSyslogCollectorIndex }
    ::= { rlsnmpSyslogCollectorTable 1 }

RlsnmpSyslogCollectorEntry ::=
    SEQUENCE {
        rlsnmpSyslogCollectorIndex
             Unsigned32,
        rlsnmpSyslogCollectorAddressType
             InetAddressType,
        rlsnmpSyslogCollectorAddress
             InetAddress,
        rlsnmpSyslogCollectorRowStatus
             RowStatus
    }

rlsnmpSyslogCollectorIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..8)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A unique arbitrary identifier for this syslog collector."
    ::= { rlsnmpSyslogCollectorEntry 1 }

rlsnmpSyslogCollectorAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The type of Internet address by which the Syslog
         collector is specified in snmpSyslogCollectorAddress.

         Not all address types may be supported."
    ::= { rlsnmpSyslogCollectorEntry 2 }

rlsnmpSyslogCollectorAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Internet address for the Syslog message collector.

         The use of DNS domain names is discouraged, and agent
         support for them is optional.  Deciding when, and how
         often, to resolve them is an issue.  Not resolving them
         often enough means you might lose synchronization with
         the associated entry in the DNS server, and resolving
         them too often might leave you without access to the
         Syslog collector during critical network events."
    ::= { rlsnmpSyslogCollectorEntry 3 }

rlsnmpSyslogCollectorRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows for the dynamic creation and deletion
         of entries within the snmpSyslogCollectorTable as well as
         the activation and deactivation of these entries.

         When this object's value is set to notInService(2) this
         collector will not be sent any messages, nor will any of its
         counters be incremented.

         The agent SHOULD not delete a row, except in the case of
         the loss of persistent storage.

         Refer to the RowStatus convention for further details on
         the behavior of this object."
    REFERENCE
        "RFC2579 (Textual Conventions for SMIv2)"
    ::= { rlsnmpSyslogCollectorEntry 4 }

--------------------------------------------------------------
-- rlSyslogLastIndexPerSeverityEntry
--------------------------------------------------------------
rlSyslogLastIndexPerSeverityTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSyslogLastIndexPerSeverityEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION  "The table displays Last Index per syslog severity"
    ::= { rlSyslogPrivate 23 }

rlSyslogLastIndexPerSeverityEntry OBJECT-TYPE
    SYNTAX  RlSyslogLastIndexPerSeverityEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION   "Static row for this table."
    INDEX { rlSyslogLastIndexPerSeverityIndex }
    ::= { rlSyslogLastIndexPerSeverityTable 1 }

RlSyslogLastIndexPerSeverityEntry ::= SEQUENCE {
    rlSyslogLastIndexPerSeverityIndex               INTEGER,
    rlSyslogLastIndexPerSeverityEmergencyIndex    Counter32,
    rlSyslogLastIndexPerSeverityAlertIndex        Counter32,
    rlSyslogLastIndexPerSeverityCriticalIndex     Counter32,
    rlSyslogLastIndexPerSeverityErrorIndex        Counter32,
    rlSyslogLastIndexPerSeverityWarningIndex      Counter32,
    rlSyslogLastIndexPerSeverityNoticeIndex       Counter32,
    rlSyslogLastIndexPerSeverityInfoIndex         Counter32,
    rlSyslogLastIndexPerSeverityDebugIndex        Counter32
}

rlSyslogLastIndexPerSeverityIndex  OBJECT-TYPE
   SYNTAX      INTEGER {
        static(1)
   }
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
     "The table contains only one static entry."
   ::= { rlSyslogLastIndexPerSeverityEntry 1 }

rlSyslogLastIndexPerSeverityEmergencyIndex OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Shows Index of last added Emergency syslog message "
    ::= { rlSyslogLastIndexPerSeverityEntry 2 }

rlSyslogLastIndexPerSeverityAlertIndex OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Shows Index of last added Alert syslog message"
    ::= { rlSyslogLastIndexPerSeverityEntry 3 }

rlSyslogLastIndexPerSeverityCriticalIndex OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Shows Index of last added Critical syslog message"
    ::= { rlSyslogLastIndexPerSeverityEntry 4 }

rlSyslogLastIndexPerSeverityErrorIndex OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Shows Index of last added Error syslog message"
    ::= { rlSyslogLastIndexPerSeverityEntry 5 }

rlSyslogLastIndexPerSeverityWarningIndex OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Shows Index of last added Warning syslog message"
    ::= { rlSyslogLastIndexPerSeverityEntry 6 }

rlSyslogLastIndexPerSeverityNoticeIndex OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Shows Index of last added Notice syslog message"
    ::= { rlSyslogLastIndexPerSeverityEntry 7 }

rlSyslogLastIndexPerSeverityInfoIndex OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Shows Index of last added Info syslog message"
    ::= { rlSyslogLastIndexPerSeverityEntry 8 }

rlSyslogLastIndexPerSeverityDebugIndex OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Shows Index of last added Debug syslog message"
    ::= { rlSyslogLastIndexPerSeverityEntry 9 }

rlSyslogPropAppl0LogLevel OBJECT-TYPE
   SYNTAX  INTEGER {
      info(0),
      debug(1),
      warning(2),
      error(3)
   }
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
       "The Log level of the PropAPPL0 Probe
        info - info log level.
        debug - debug log level.        
        warnings - warnings log level.
	errors - errors log level."
   ::= { rlSyslogPrivate 24 }

rlSyslogPropAppl0LogModule OBJECT-TYPE
   SYNTAX  Unsigned32
   MAX-ACCESS   read-write
   STATUS       current
   DESCRIPTION
       "The Log level of the PropAPPL0 Probe
        options:
        none - All modules log disabled
        call-home - call-home modules log enabled.      
        discovery - discovery modules log enabled.
	northbound - northbound modules log enabled.
	services - services modules log enabled.
	southbound - southbound modules log enabled.
	system - system modules log enabled.
	All - all modules log enabled."
   ::= { rlSyslogPrivate 25 }
      

rlSyslogUnexpectedRestartTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF RlSyslogUnexpectedRestartEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table containing errors registered to non-volatile memory."
    ::= { rlSyslogPrivate 26 }


rlSyslogUnexpectedRestartEntry OBJECT-TYPE
    SYNTAX  RlSyslogUnexpectedRestartEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION "An unexpected restart log entry"
    INDEX  { rlSyslogUnexpectedRestartCounter   }
    ::= { rlSyslogUnexpectedRestartTable 1 }

RlSyslogUnexpectedRestartEntry ::=
    SEQUENCE {
        rlSyslogUnexpectedRestartCounter             Unsigned32,
        rlSyslogUnexpectedRestartDateTime            DisplayString,
        rlSyslogUnexpectedRestartAppMnemonic         DisplayString,
        rlSyslogUnexpectedRestartSeverity            RlSyslogSeverity,
        rlSyslogUnexpectedRestartMessageMnemonic     DisplayString,
        rlSyslogUnexpectedRestartText1               DisplayString,
        rlSyslogUnexpectedRestartText2               DisplayString,
        rlSyslogUnexpectedRestartText3               DisplayString,
        rlSyslogUnexpectedRestartText4               DisplayString
    }
	
rlSyslogUnexpectedRestartCounter   OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A counter that identifies this entry - used to differentiate logged
         entries. And the order given is the order of logging. A entries may
         not form sequence of this value. (Time is not a differentiating
         element as logged entries may come in a sequence."
    ::= { rlSyslogUnexpectedRestartEntry 1 }

rlSyslogUnexpectedRestartDateTime   OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time in string (formated DD-MMM-YYYY HH:MM:SS e.g
         14-Apr-2002 10:33:31), when the eroor was logged.."
    ::= { rlSyslogUnexpectedRestartEntry 2 }

rlSyslogUnexpectedRestartAppMnemonic OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..8))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Application that created this error."
    ::= { rlSyslogUnexpectedRestartEntry 3 }

rlSyslogUnexpectedRestartSeverity OBJECT-TYPE
    SYNTAX  RlSyslogSeverity
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Severity of the reported error."
    ::= { rlSyslogUnexpectedRestartEntry 4 }

rlSyslogUnexpectedRestartMessageMnemonic OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Short identifier of this message that created this error."
    ::= { rlSyslogUnexpectedRestartEntry 5 }

rlSyslogUnexpectedRestartText1 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 1."
    ::= { rlSyslogUnexpectedRestartEntry 6 }

rlSyslogUnexpectedRestartText2 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 2."
    ::= { rlSyslogUnexpectedRestartEntry 7 }

rlSyslogUnexpectedRestartText3 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 3."
    ::= { rlSyslogUnexpectedRestartEntry 8 }

rlSyslogUnexpectedRestartText4 OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(1..160))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The text of the logged message without time and date - part 4."
    ::= { rlSyslogUnexpectedRestartEntry 9 }




rlSyslogUnexpectedRestartOccured  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "A flag representing if an unexpected restart had occured
        and has not yet been cleared"
    DEFVAL { false }
    ::= { rlSyslogPrivate 27 }

rlSyslogUnexpectedRestartClear  OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "An action MIB variable setting with that when 
        set to true, will clear the unexpectedRestartOccured
        and delete all entries in "
    ::= { rlSyslogPrivate 28 }
END

