RADLAN-rlLcli-MIB DEFINITIONS ::= BEGIN

-- Title:      RADLAN LCLI MIB
-- Version:    7.36
-- Date:       26 Mar 2004
--

IMPORTS
    rnd                                         FROM RADLAN-MIB
    TruthValue, DisplayString, RowStatus        FROM SNMPv2-TC
    Unsigned32, TimeTicks,
    MODULE-IDENTITY, OBJECT-TYPE                FROM SNMPv2-SMI;

    rlLCli  MODULE-IDENTITY
        LAST-UPDATED "200503280000Z"
        ORGANIZATION "Marvell Semiconductor, Inc."
        CONTACT-INFO
			"5488 Marvell Lane
			Santa Clara, CA 95054
			USA

			Website:  www.marvell.com"
        DESCRIPTION
             "The private MIB module definition for Radlan CLI MIB."
        REVISION "200707260000Z"
        DESCRIPTION
                 "Removed ranges of rlLCliTimeout, rlLCliSshTimeout, rlLCliTelnetTimeout since the range is dynamic
                  according to device capabilities. "
        REVISION "200504110000Z"
        DESCRIPTION
                 "Changed lower range of rlLCliTimeout, rlLCliSshTimeout, rlLCliTelnetTimeout to 0
                  to support 0 as 'no timeout' "
        REVISION "200503280000Z"
        DESCRIPTION
                 "1) Added Module-identity range.
                  2) Changed description of rlLCliMibVersion
                  3) Added ranges to rlLCliTimeout, rlLCliSshTimeout, rlLCliTelnetTimeout "
        REVISION "200403260000Z"
        DESCRIPTION
             "Initial version of this MIB."
        ::= { rnd 74 }


rlLCliMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "MIB's version, the current version is 3."
    ::= { rlLCli 1 }

rlLCliTimeout OBJECT-TYPE
   SYNTAX Unsigned32 (0..3932159)
-- (0..65535*60+59)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
       "LCLI Timeout indicates the interval in seconds, that
        the system waits until user input is detected."
   DEFVAL {600}
   ::= { rlLCli 2 }

rlLCliHistoryEnable OBJECT-TYPE
   SYNTAX TruthValue
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
       "Indicates if command history function is supported."
   DEFVAL {true}
   ::= { rlLCli 3 }

rlLCliHistorySize OBJECT-TYPE
   SYNTAX Unsigned32
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
       "Indicates number of commands that the system will record
        in its history buffer."
   DEFVAL {10}
   ::= { rlLCli 4 }

rlLcliCommandLevelTable OBJECT-TYPE
   SYNTAX  SEQUENCE OF RlLcliCommandLevelEntry
   MAX-ACCESS  not-accessible
   STATUS  current
   DESCRIPTION
       "This Table maps a CLI command to its level. "
    ::= { rlLCli 5 }

rlLcliCommandLevelEntry OBJECT-TYPE
    SYNTAX  RlLcliCommandLevelEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The row definition for this table."
    INDEX {rlLcliCommandLevelCommandName,
          rlLcliCommandLevelContextName }
    ::= { rlLcliCommandLevelTable 1 }

RlLcliCommandLevelEntry ::= SEQUENCE {
    rlLcliCommandLevelCommandName     DisplayString,
    rlLcliCommandLevelContextName     DisplayString,
    rlLcliCommandLevelInsertTime      TimeTicks,
    rlLcliCommandLevelCommandLevel    INTEGER,
    rlLcliCommandLevelActionMode      INTEGER,
    rlLcliCommandLevelStatus          RowStatus
}

rlLcliCommandLevelCommandName OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        " The CLI command name "
    ::=  { rlLcliCommandLevelEntry 1 }

rlLcliCommandLevelContextName OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        " The CLI context ID which the command name is associated with "
    ::=  { rlLcliCommandLevelEntry 2 }

rlLcliCommandLevelInsertTime OBJECT-TYPE
    SYNTAX  TimeTicks
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "The time elapsed until this entry was created."
    ::= { rlLcliCommandLevelEntry 3 }

rlLcliCommandLevelCommandLevel OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        " The level which is associated with the command name "
    ::=  { rlLcliCommandLevelEntry 4 }

rlLcliCommandLevelActionMode OBJECT-TYPE
    SYNTAX  INTEGER {
        set (1),
        reset (2),
        setAll (3),
        resetAll (4)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        " The level action which is associated with the command name "
    DEFVAL    { set }
    ::=  { rlLcliCommandLevelEntry 5 }

rlLcliCommandLevelStatus OBJECT-TYPE
    SYNTAX  RowStatus
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        " The status of the commandLevel table entry. "
    ::= { rlLcliCommandLevelEntry 6 }

rlLCliSshTimeout OBJECT-TYPE
   SYNTAX Unsigned32 (0..3932159)
-- (0..65535*60+59)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
       "LCLI Timeout indicates the interval in seconds, that
        the system waits until user input is detected on SSH LCLI."
   DEFVAL {600}
   ::= { rlLCli 6 }

rlLCliTelnetTimeout OBJECT-TYPE
   SYNTAX Unsigned32 (0..3932159)
-- (0..65535*60+59)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
       "LCLI Timeout indicates the interval in seconds, that
        the system waits until user input is detected on telnet LCLI."
   DEFVAL {600}
   ::= { rlLCli 7 }

rlLCliTelnetHistoryEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates if command history function is supported for Telnet."
    DEFVAL {true}
    ::= { rlLCli 8 }

rlLCliTelnetHistorySize OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates number of commands that the system will record
         in its history buffer for Telnet."
    DEFVAL {10}
    ::= { rlLCli 9 }

rlLCliSshHistoryEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates if command history function is supported for Ssh."
    DEFVAL {true}
    ::= { rlLCli 10 }

rlLCliSshHistorySize OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates number of commands that the system will record
         in its history buffer for Ssh."
    DEFVAL {10}
    ::= { rlLCli 11 }

END


